(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Unseen Servant (Baby 10 Seq)")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./")
    )
  )

  (net 0 "")
  (net 1 "Net-(U2C--)")
  (net 2 "-12V")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(D2-K)")
  (net 6 "Net-(D2-A)")
  (net 7 "Net-(D3-K)")
  (net 8 "Net-(D3-A)")
  (net 9 "Net-(D4-K)")
  (net 10 "Net-(D4-A)")
  (net 11 "Net-(D5-K)")
  (net 12 "Net-(D5-A)")
  (net 13 "Net-(D6-K)")
  (net 14 "Net-(D6-A)")
  (net 15 "Net-(D7-K)")
  (net 16 "Net-(D7-A)")
  (net 17 "Net-(D8-K)")
  (net 18 "Net-(D8-A)")
  (net 19 "Net-(D9-K)")
  (net 20 "Net-(D9-A)")
  (net 21 "Net-(D10-K)")
  (net 22 "Net-(D10-A)")
  (net 23 "Net-(D11-A)")
  (net 24 "Net-(D12-A)")
  (net 25 "Net-(D13-A)")
  (net 26 "Net-(D14-A)")
  (net 27 "Net-(D15-A)")
  (net 28 "Net-(D16-A)")
  (net 29 "Net-(D17-A)")
  (net 30 "Net-(D18-A)")
  (net 31 "Net-(D19-A)")
  (net 32 "Net-(D20-A)")
  (net 33 "Net-(D21-K)")
  (net 34 "Net-(D21-A)")
  (net 35 "Net-(D22-K)")
  (net 36 "Net-(D23-K)")
  (net 37 "Net-(D24-K)")
  (net 38 "Net-(D25-K)")
  (net 39 "Net-(D27-K)")
  (net 40 "Net-(D28-K)")
  (net 41 "Net-(R2-Pad1)")
  (net 42 "Net-(D29-K)")
  (net 43 "Net-(D30-K)")
  (net 44 "Net-(D31-K)")
  (net 45 "Net-(D32-K)")
  (net 46 "Net-(D33-K)")
  (net 47 "Net-(R31-Pad1)")
  (net 48 "GND")
  (net 49 "unconnected-(SW11-Pad11)")
  (net 50 "unconnected-(SW11-Pad12)")
  (net 51 "Net-(D35-K)")
  (net 52 "unconnected-(J3-Pin_11-Pad11)")
  (net 53 "unconnected-(J3-Pin_12-Pad12)")
  (net 54 "unconnected-(J3-Pin_13-Pad13)")
  (net 55 "unconnected-(J3-Pin_14-Pad14)")
  (net 56 "Net-(Q1-B)")
  (net 57 "Net-(R25-Pad2)")
  (net 58 "Net-(R32-Pad1)")
  (net 59 "Net-(Q2-B)")
  (net 60 "Net-(C2-Pad1)")
  (net 61 "Net-(Q3-B)")
  (net 62 "Net-(D26-K)")
  (net 63 "Net-(Q4-B)")
  (net 64 "Net-(D31-A)")
  (net 65 "Net-(Q5-B)")
  (net 66 "Net-(D32-A)")
  (net 67 "Net-(Q6-B)")
  (net 68 "Net-(Q7-B)")
  (net 69 "Net-(D35-A)")
  (net 70 "Net-(Q8-B)")
  (net 71 "Net-(D36-A)")
  (net 72 "Net-(Q9-B)")
  (net 73 "Net-(D37-A)")
  (net 74 "Net-(Q10-B)")
  (net 75 "Net-(Q12-C)")
  (net 76 "Net-(U2A--)")
  (net 77 "Net-(U2B--)")
  (net 78 "Net-(SW12-A)")
  (net 79 "Net-(U2D--)")
  (net 80 "unconnected-(U1-Cout-Pad12)")
  (net 81 "Net-(SW14-B)")
  (net 82 "Net-(U3A-+)")
  (net 83 "RESET_IN")
  (net 84 "CLK_IN")
  (net 85 "Net-(D11-K)")
  (net 86 "Net-(D37-K)")
  (net 87 "Net-(U2B-+)")
  (net 88 "Net-(SW1-A)")
  (net 89 "GATE_OUT")
  (net 90 "Net-(U1-Reset)")
  (net 91 "CLK_OUT")
  (net 92 "CASC_OUT")
  (net 93 "Net-(R43-Pad1)")
  (net 94 "CV_OUT")
  (net 95 "Net-(U3B-+)")
  (net 96 "Net-(SW12-C)")
  (net 97 "CLK_IN_N")
  (net 98 "Net-(U3A--)")
  (net 99 "unconnected-(J1-PadTN)")
  (net 100 "Net-(Q12-B)")
  (net 101 "Net-(Q12-E)")
  (net 102 "Net-(Q13-B)")
  (net 103 "Net-(Q14-B)")
  (net 104 "SEQ_LV")
  (net 105 "Net-(U3B--)")
  (net 106 "+12V")
  (net 107 "Net-(R37-Pad2)")
  (net 108 "Net-(R40-Pad2)")
  (net 109 "Net-(R41-Pad1)")
  (net 110 "Net-(J3-Pin_15)")
  (net 111 "unconnected-(J4-PadTN)")
  (net 112 "unconnected-(J5-PadTN)")
  (net 113 "unconnected-(J7-PadTN)")
  (net 114 "Net-(D34-K)")
  (net 115 "Net-(SW14-A)")
  (net 116 "CASC_NORM")
  (net 117 "Net-(J16-PadT)")

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp 0a4add12-cb60-4024-8630-91bf5e5cec93)
    (at 46 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/13fc8df2-903f-4a19-9c43-a2eaf0c524c1")
    (attr through_hole)
    (fp_text reference "SW1" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3312b392-81c1-492c-b968-78a2183417f5)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f6878957-ffc4-410c-9daf-1b208689d304)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ea2bae7-9b4f-4278-ac10-475d777dad49)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 696cf63e-c249-4c02-9864-0ae6bd21d8f3))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3ed7c7e-d1d1-4eab-90b6-246e343587b0))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65bfb0b0-ef72-4a96-864d-78ea4ef6be88))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 13ce9e98-5046-4cc8-96e6-26a77d85e3b9))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c9538020-ffe8-40ce-9baa-7867461a6d7c))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86523a22-8ff7-4df3-a30a-cd2fd1fc8323))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8965d289-844b-4b9f-8ea3-3c1616cb4719))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32634ef1-c0f7-4f19-bd01-ac821b99bfb6))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f7301e3-6e7c-4f5b-8fb4-de4488b73327))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8652ad4-700c-431d-bcb8-7aaf341a8032))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f763eebf-cc33-463f-9cf8-69c55b26f426))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ba1415f-06c1-4d48-aea7-d988db2c3b15))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 277e26bb-5597-423d-bb8d-a9b9511e2eac))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "B") (pintype "passive") (tstamp 97d121dd-d471-44dc-8f33-4a510014246c))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 923de071-f474-4a99-9ea2-dd5d77889347))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 1127db84-3cdb-4976-a932-0104afc5f138)
    (at 45.5 35.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/86ec99ee-6e7b-42f4-8927-8c38f3f05a50")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.68 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7422b41f-c92e-4f40-b2b0-3ced9012ed65)
    )
    (fp_text value "100nF" (at 0 1.68 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e192010d-cf52-47bc-bde0-52689b475008)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp b0535f5b-0ecb-4a62-8c16-8b5c4c264bbe)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 92ec7f04-93bb-427d-9aa8-8d8c7bd63863))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c90cbbe-1c9f-4d48-a274-70a055f3c3e7))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 165a763e-ed1a-4fef-81d9-ecd965fa951a))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c747e3f3-4207-4c73-95ed-e680cde63628))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bee0dfb7-846d-4507-9663-9015c3073bca))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e405a3a4-8e8d-4e62-a666-eb3a8d3aaf16))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7293f07b-fda7-455b-a57e-b518d9a98879))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31d2ae02-a28a-45dd-9ca8-0db5e25b2478))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 74abebde-d7de-4114-b0b6-58bf85fd7dbf))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7e87312-a772-437b-a6d8-63fd65688a8a))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 81 "Net-(SW14-B)") (pintype "passive") (tstamp 7ab33934-7e5e-4bc0-84fe-1f5830b231fe))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp b485ca92-6774-48e4-934a-8ab2cc9ff9c1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp 16fbf80c-b626-4bf3-83e7-ca3580907c52)
    (at 146 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/ab88720e-19c2-42ce-bc5f-313970ca6107")
    (attr through_hole)
    (fp_text reference "SW9" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68693ceb-05a1-4f48-990b-bca033a848a5)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 847f64d8-2ac8-49d3-a7ec-74741afdc8d7)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d9a7a031-e4fc-4dc3-88d6-0d8baeb95326)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 167842ea-5c91-424b-a4d7-f3a2fddcbee7))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee81118e-cd5f-45d2-bc7b-ea6a5681458a))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 728e0f21-1ae4-4925-b00b-a73a6ae083af))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef296c82-edbf-4344-8950-34f93eb72a14))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5c1aded4-37c5-4b76-80c6-959247bd167b))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a2988b7b-e1e4-4eb6-83a9-f7db06c6a416))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 758f84b1-9c60-4a6b-a88f-c177df28b914))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0beaf048-4ae0-4876-86b4-47dec20765e6))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 45eeaf1c-2748-4e9f-b944-c94db775c836))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9e56793d-3006-464e-b7d9-0bcb7dc3643b))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp edc56213-502e-43e2-af1a-5370dd88abbf))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee64b989-63c5-4c27-9693-55c9b0825005))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp d723cb64-b4ca-4c91-9eb3-f989be62b1be))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D9-K)") (pinfunction "B") (pintype "passive") (tstamp fa6153fd-1dff-40e3-b6cf-ee5f1c4e891b))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp f07c1a49-9fae-453e-a632-68ba0ab65aec))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp 17dc9565-7417-4128-9eba-dc918c5ccfca)
    (at 83.553 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/9662582c-34de-4677-abe1-bb2fc203151f")
    (attr through_hole)
    (fp_text reference "RV4" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a422d269-f560-407d-8211-2c382ba9e48e)
    )
    (fp_text value "Stp Lvl 4" (at -0.171374 1.01 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94a1b737-e04b-4bd8-9a9e-b1a8e65db069)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 35f60d04-e5ce-4fce-90c1-878e8b69077d)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0414eea-72d3-49e0-a962-60cf2be80512))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9f323c5-c09f-4c34-a28f-53ce1134d1e4))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a8006788-5efc-410e-9ba9-81afae6ea295))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99b765ec-7e7e-4379-a40e-443d0b1577f1))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b1eb18e-9574-4f4e-8152-cf2ed765db16))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21b340cc-7cdc-4695-9d5a-7de6fd7070e5))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 636e9d8a-946b-4a59-983d-79da24831f16))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e992ae6-d6e0-44df-9957-97f72ed36bfa))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4de340e1-cee7-4ed2-83ea-4100ec1a117b))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aea30a05-1f33-4015-8fe3-062135bf29d3))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1af61858-1afd-4f2b-9ec2-64d68009212a))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b3ad176-6b5a-41a2-8c87-a91fb769469a))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2982a89-d006-4e0d-a374-272c320129d9))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49a01d70-a408-475d-a363-5eb8aa75e374))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1778c19-73df-42bf-88b7-197b6efbceac))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cd504aaa-9201-4734-8bcb-bc74667e1c9d))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4307c913-1521-4de1-a286-bfaf1be11307))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a20ccad8-9cf6-4714-bbbf-e3673f5bb1df))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6b4ccb78-2a50-444f-bd4e-e37e6c0f61ff))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a97e061c-0a62-4f9c-ad21-93c79ee7f696))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f2a9e520-c9a5-4011-b784-fca74256f5d5))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8616f7a4-8dd1-4c88-b0d8-c54110ce372f))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d663415a-e93b-4ea9-b8d1-3ed47676ee09))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cc223df9-4105-4cb2-aac2-8fcabc4820c5))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3c0b5cc-3e71-4177-9231-9ced070b1aff))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea8130d4-6208-43d1-8b44-3752a2fc0e27))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48eaeb03-9222-4dd3-9e1d-816a61689860))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 57954dae-cdd3-4e3e-9067-e9ed7554fd4e))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-A)") (pinfunction "1") (pintype "passive") (tstamp 34b83aef-1184-47e3-be07-3ea2d7cf8ca9))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(D14-A)") (pinfunction "2") (pintype "passive") (tstamp 2c0290cd-6a2f-469c-a785-ee97b8292dfb))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 052e0889-624f-4d31-aaff-f3d92abf9f97))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 02385b84-c79e-44c4-9950-d2edf7ac0762))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 1857de2f-a28e-41d2-bd60-c30701d30a12)
    (at 88 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/f31ae053-cc75-4425-bb3b-bf149ddc3864")
    (attr smd)
    (fp_text reference "D4" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd5ca85e-c248-4a65-b85a-4dcb20b6edae)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed68ded0-a99f-4d33-b0a5-3293272edeb8)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25ed7fba-2486-4434-9b94-4fbec744a317)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc946e5e-8121-4997-b9eb-17f6d7316086))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83f01079-df04-4482-9f0a-bf8dc20784f3))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1c74474-c3d3-4582-b6b2-25c36cbaebd1))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5ddf7a5-7e45-4251-bc8a-982f2ef395dc))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c5e8487-5e3a-4666-b9df-8fa95d8e5024))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2ae9c488-99fe-4969-a10a-d580b934172e))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f4a03c61-32be-4dfc-be77-d8d1da630869))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2d613c6-c192-4787-b939-a1568950d197))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7587e68d-60b6-45db-8ab7-35a877767818))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8fb1d405-fd40-435b-bf92-06c0d646cc9e))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ef3fe86-95e0-4bcd-9daf-07cf2d57edd7))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e312903a-a6f1-499c-b4fd-4f060132c7df))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1271ed0d-ced3-4669-b947-1116268c30fe))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc6358bd-b19e-4d10-97b9-8ae3b899b34d))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 30ba41d2-9861-4280-8819-33b0b933a822))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f116f315-176f-4380-b3f2-db23fa88ca17))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 766507a7-ead3-4de6-99a5-3b9066fb392e))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c463d51c-7120-457e-8953-2cccd521ed7d))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 9 "Net-(D4-K)") (pinfunction "K") (pintype "passive") (tstamp 59304dd9-a96b-4b0a-917c-c915b146b792))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(D4-A)") (pinfunction "A") (pintype "passive") (tstamp 54cfdc78-b65e-4074-867b-6f74acc50800))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp 1b6ea1be-a50e-4b6c-8ac0-6f97099a6717)
    (at 46.053 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/3d4edbaa-8bd8-46d4-868e-0ee0d827f733")
    (attr through_hole)
    (fp_text reference "RV1" (at -0.091374 2.55 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 181b96a3-0096-4df9-9fc7-e75f316dff76)
    )
    (fp_text value "Stp Lvl 1" (at 0.378626 -2.29 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4713f997-bef8-4be0-80c1-d0620b17fa99)
    )
    (fp_text user "${REFERENCE}" (at -0.031374 2.55 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a32ae980-2770-4e5d-8e6c-73c745154848)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ace239a0-766a-42fe-a8d2-2bd77e7fb6a7))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 329dbed0-e667-4d77-81e1-e75994db2fa8))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 897ac7b7-42ac-4c3f-9d12-8dd203e34d2b))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0a511cac-77eb-43e2-9181-bc03b84826c8))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 497ab768-cd17-449b-a5eb-ab9ff3d15d6a))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5199979e-fcc4-4213-9c1c-8c6ba3073d14))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b367a3a4-2c2b-41de-a4b7-7a07e8abc4ef))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 312e460e-c43d-47f4-93d6-0b1e51ccccc9))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60d65b78-01c1-49a7-9255-4050314d4a8a))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 412fbee4-53cc-489f-91c6-7792ad2f8268))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b94f194e-3160-4ae0-ad36-779072d531f9))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 17440c71-ffd2-4c3c-960e-6e33c6b0ce83))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a565a41-d69f-47a6-a7b6-d55a0ba33640))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c8659bc-d3ab-43f8-8e42-be3e399ce981))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8680ef99-0905-401f-8ad7-39c8d77f3510))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b42083ed-c22c-4c42-b055-0dd4a98706b3))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c364f0d-aa58-4461-b98e-9a5505ded74a))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a610a1b-fc7a-4ff1-8991-c84e38c03291))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b1809380-f319-4b7a-9b0b-da58fd3bd5b6))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c8ef38f3-c192-4dd1-b170-eb23037c3d23))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c26cbe24-5940-4164-afb9-ade4fb6f1c85))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e9d8efd-63d3-42ae-8a9b-3a712d79106b))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09c027ae-0123-490a-9ca3-ddbd6aff27e6))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 887d8218-23df-4857-a05d-c84bbb5055ff))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41fa39df-db6f-4f0a-91b8-525445a28393))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 376fbd75-d336-4306-97f4-efc2526a3fa6))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b75b454-e8c5-4cac-a56c-e1aa0a45c848))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp bdc827d4-cb08-43e8-bbfd-124e33dd120f))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "1") (pintype "passive") (tstamp 8bd507b9-7935-4cf4-87b5-927bc1c10e50))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D11-A)") (pinfunction "2") (pintype "passive") (tstamp 59d15fc2-125c-423b-a0bb-26f5c5b6740a))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 3e2e9027-94a6-4f0f-ac9d-1758c7b637bc))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp b462f498-4b78-4d12-8816-ade42fc35d1f))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 1c8bcea2-ce58-4893-bd9f-8337e2ef39c7)
    (at 138 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/7e7707c3-81fb-45ec-ae38-a1f7ed057147")
    (attr smd)
    (fp_text reference "D8" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1fb176c2-37e5-4873-8720-ed25db405b30)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 651b683c-d41e-4016-915e-b776d67baacb)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1bf65aa-31ef-46b5-8475-3dc51cae0be0)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e054e51c-75b8-424d-a9d8-9eb7409c5ab1))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78822216-06ae-4d4d-9e31-bd2e53f46c61))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c4c1586-c779-41f8-a73c-847dbe7ebd47))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 92eff2d9-615d-4b61-b277-3123f2053d33))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cbf6ab78-7608-4116-adb5-8fdde0d46f79))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc756482-09da-4a90-817f-59b78f1fa251))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c6dcf413-f80a-4e5d-a473-a57e8f478bc8))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46dd8f45-c1ba-4db5-ad37-b5dab8aef57f))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69df6890-33b7-4bd4-909c-ed6f50d8df04))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e144573-8f4a-4489-b84a-905abd3fce44))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 903be3d4-70a8-442c-bb92-9ca7a1a57aaa))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 093ac86f-795b-48fa-b666-809ae152aca2))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp adba68bf-a3e3-44e6-8bad-71a21d8ab331))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 59ed46ad-3b4f-4d57-867c-f09f63ce8a44))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5709bfad-4cb1-4a92-93e5-7c9ec59d04db))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b28de11f-8154-45ee-8c5f-865d7adbb385))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b95c345-9a09-4fb0-a42b-47f397866ba9))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f6961229-150b-49b5-9859-a7f92cf30d72))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 17 "Net-(D8-K)") (pinfunction "K") (pintype "passive") (tstamp dfba2f1d-010c-48dd-981a-946de2d6631f))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 18 "Net-(D8-A)") (pinfunction "A") (pintype "passive") (tstamp 3cb3ce3a-8be2-420f-8c8c-cdbe294268f9))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp 1ea5b7ed-eb8f-4ff4-97da-332750eb1f51)
    (at 58.5 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/162c4dc7-54aa-4eb8-be44-8071a582118c")
    (attr through_hole)
    (fp_text reference "SW2" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 317225b3-f1fc-44eb-bc92-103fe960f82b)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 790fbfd8-7f3c-4771-9a75-48c5267391bf)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b700d3b4-432e-455f-b305-185891210c2e)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00240379-5fc5-4f77-8989-4e9853b456f8))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f68271c-0879-426c-840a-45798396fb54))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3be2f119-02ec-4bb8-a811-7fc990f50804))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a822154-52c9-47ce-a607-0ed4499c53ba))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b9786f80-29c9-4a41-8061-01c5a5728c27))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b51a3b95-4aea-4ce5-96a2-21d0ddd58ecc))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c2cb092-ab7b-4283-8285-89bf67f7cb97))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5014a4de-331e-4693-a99c-ac899e617ced))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 662747fe-85ec-4b58-986b-182cc1e92d80))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 04cc4e03-8c73-46f8-9112-4dafdd12c769))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 506cd608-09ec-4e6e-97a1-1dda8197d5e5))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6e55c98-1a05-4ecf-8519-8d9da11fb49e))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 677cb487-224d-4fed-bc91-033165791241))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-K)") (pinfunction "B") (pintype "passive") (tstamp cc4fee46-14de-4b3e-92e9-a9341b3b1823))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp d66ce8e9-26dc-4544-8511-0b271f3c0b2a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 22e1d633-cb94-4937-a47f-fb4c22e1ebf7)
    (at 69.783 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/696a55ea-fd74-426e-a040-1efcdbac50a5")
    (attr through_hole)
    (fp_text reference "D23" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9bfb1b8b-e74d-46e2-b3e3-1f78d65b5d71)
    )
    (fp_text value "STEP3" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 346aa766-b14b-4b4f-93e2-f10a3468dc6b)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 62d07a42-0023-4f22-9333-3acf2d9142e8)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f82a9bc-9d56-4598-993a-d8a19663bf1c))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 883c1ff1-d96f-4b91-92e4-2bdf16e51918))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8afb379-f8ce-4120-b68a-88cc34f5b7ce))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ddab0fb-d81e-4d5b-8f88-0ddab50e9b9d))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf3c714d-6cc1-4851-9fc5-a46105d1ba81))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fd9357e3-19bd-4f0b-b42e-2f2fdf9b5c0a))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d455d30c-e623-42e0-91dc-35c4dbc14df1))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8b574b32-623b-4cca-8157-66bce9d641ba))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eca90147-686b-4893-ab4d-15fe68a7a244))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b02fd0fa-3c99-4e37-8a7b-6d01fd902bde))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be7b5117-f5b1-485f-93bf-6afdf26027d4))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2ddcc92-171a-4ecc-ab8e-932c3fc85bce))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77c310de-1ba3-410b-b9b1-9a6bc00dbc6f))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ab900ee-afaf-4a18-befb-640be3166663))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2734882c-81b3-4d35-a56a-5ecf244c74ee))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(D23-K)") (pinfunction "K") (pintype "passive") (tstamp 6bb851d6-46bc-4a38-86f7-c2dd647c771d))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 77aaddc4-cc49-4f5e-9e12-a2f5e10ac8ec))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 2a5c15c9-1692-4c45-918f-163f3bc2280a)
    (at 26.25 82.85)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/a438a10b-dda8-48d6-b767-fe99b7b38bda")
    (attr through_hole)
    (fp_text reference "J1" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd8cabfa-848a-4868-a5e4-4f1651af32fc)
    )
    (fp_text value "RESET / CASC IN" (at 3.75 5.9 -90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cacce8d5-bd95-492e-bfb3-55bb0eeadcb3)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp a76b866d-7225-410c-ba27-be99f8af6350)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9491e33-83af-4c7e-8dbb-7dc181f88308)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cd5507c3-53b6-4c78-8a87-f209aed2eae0))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 267be842-ff20-4576-930f-494930d634a7))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9d6dcc38-b3fb-495d-a9d2-61eb9a61aa77))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 504ebb09-bb06-4d70-b542-4b89b76533b4))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 50118f97-fd66-408c-b261-a95aaffd0f3e))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa3f6bdd-dda3-4a3f-8410-f3e85bf18c53))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3793f5bb-d6e8-4c6b-ac73-d088ff9f1c1c))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1facda2-4e13-4b67-9ae6-83f4ec800f08))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 999e5e94-9ffc-442c-842c-8d12dc0de5af))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f760bac6-cb32-4f7c-a098-224a876b5c8c))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3060d356-4d95-4277-a860-ed7aeb401e43))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b1e516b2-dccf-49e7-bede-81cc9cb2f1b4))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3e8d4599-1d51-4c4a-bf87-e4d65f71ac86))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a805b196-0bd5-4cc2-8a4b-31e8aaf96a41))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b87d608-3b5f-4ca0-a050-1b911e7cab57))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9f86f8a-581e-493d-b3e9-83ce7ce791fe))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bbeea66c-c4fe-43b9-b86b-318d273a8db5))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a1223501-b4b4-4b26-9e84-f174529fb483))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp ec8a9878-3cab-4343-8e38-5939056d94ce))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 01d8ee25-7e63-4299-8526-e7a4afd28e3f))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 83 "RESET_IN") (pintype "passive") (tstamp 412a31c3-8d7a-440a-af4c-a4de8f3629ea))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 99 "unconnected-(J1-PadTN)") (pintype "passive+no_connect") (tstamp 8d2d248f-0b4e-4cf3-ae4d-5ecb9288007f))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 62b30080-91db-4905-ab8f-06012c5cbd7f) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 27.755141 89.33)
          (xy 27.73493 89.084171)
          (xy 27.674841 88.844945)
          (xy 27.576486 88.618744)
          (xy 27.442508 88.411645)
          (xy 27.276504 88.22921)
          (xy 27.082932 88.076336)
          (xy 26.866992 87.957131)
          (xy 26.634482 87.874794)
          (xy 26.391646 87.831539)
          (xy 26.145007 87.828525)
          (xy 25.901187 87.865835)
          (xy 25.666734 87.942466)
          (xy 25.447946 88.05636)
          (xy 25.250697 88.204458)
          (xy 25.080286 88.382784)
          (xy 24.941288 88.586548)
          (xy 24.837436 88.810278)
          (xy 24.771519 89.047965)
          (xy 24.745308 89.293226)
          (xy 24.759507 89.539475)
          (xy 24.813734 89.780099)
          (xy 24.906532 90.008634)
          (xy 25.035411 90.218945)
          (xy 25.196908 90.405382)
          (xy 25.386687 90.562939)
          (xy 25.59965 90.687385)
          (xy 25.830079 90.775377)
          (xy 26.071785 90.824553)
          (xy 26.318278 90.833592)
          (xy 26.562936 90.80225)
          (xy 26.799191 90.73137)
          (xy 27.020697 90.622856)
          (xy 27.221505 90.479621)
          (xy 27.396223 90.305512)
          (xy 27.540158 90.105205)
          (xy 27.649445 89.884079)
          (xy 27.721149 89.648074)
          (xy 27.753344 89.403526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 2dd77e7a-46eb-49da-8052-7d275d6018ef)
    (at 100.5 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/ed9e8005-af79-4b4e-bf45-cc16902295cc")
    (attr smd)
    (fp_text reference "D5" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 725cb2e8-d263-4aeb-b790-4bef0b457867)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 38b3d2f0-74f6-4d48-97ea-258b0e820f88)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ad23f3e-c610-477e-84fe-6381283ea2b5)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0213441b-4449-4dfc-b97c-46f552171889))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2b453dc-cf6b-4bf9-b47b-94fec94f0619))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 097d0cfa-580f-453c-b767-7fa00ee26fd7))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 847297dd-4a1b-4fa9-98d6-852d13ac3c55))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 411e6754-0a06-4902-8e4f-271a5170b485))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7a0cf80a-69ad-4e7c-8064-db088308cd09))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a4739887-de39-4a4e-ae82-5f8b521eb823))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57981c04-6d46-41a5-90be-1d681c6ce932))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6670a31a-6a5c-465f-b0d5-12fc9ec9492f))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 230f2d8b-dc9d-48a4-ab62-eebfe5599714))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa4eac88-9840-4121-b936-092d3a0a07bd))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ccf6c60a-8fbe-4cbf-ba2e-627ae7b8fa8b))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp deae3afb-4514-4fa3-ba0b-8e8a784cfa9c))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b670506-6abf-4f73-930a-17e5760518f6))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 514388e9-e261-4512-8b59-03ffec5e445c))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b6412a5-b225-4fb4-a232-e501dfe416e0))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf31019a-30b2-4895-94c1-8d1f1f760b80))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d58a48e-e057-4374-b6e2-b3aa8578c27e))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(D5-K)") (pinfunction "K") (pintype "passive") (tstamp 7c5ad7be-52bf-4fc8-b98a-1b860aa4ccd5))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 12 "Net-(D5-A)") (pinfunction "A") (pintype "passive") (tstamp e20bd404-a87d-4de3-a41c-3825b05535d6))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (tstamp 3482d2ab-5352-49a2-a398-7b4cc725cafc)
    (at 35.56 45.72 90)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (path "/12ba5c77-8f9b-4df9-8167-54da086dc1bf")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.998 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ceffe24-dfc8-4e6b-8541-4df49ee208a7)
    )
    (fp_text value "TestPoint" (at 0 2.05 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53076dca-658e-4a15-91c4-26e3ca3253f3)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e25c426e-5cc7-49ad-a0fe-316c78881925)
    )
    (fp_line (start -1.2 -1.2) (end 1.2 -1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40922d25-fb0f-4b23-b849-b93272fd0404))
    (fp_line (start -1.2 1.2) (end -1.2 -1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5342c9ad-8284-4aad-a51a-068f35d3d323))
    (fp_line (start 1.2 -1.2) (end 1.2 1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b90a25b4-97c1-4e45-ae14-ef8a7f4527c4))
    (fp_line (start 1.2 1.2) (end -1.2 1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0338f5ae-00d6-441c-a7c7-f21ea3b4cd77))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f2d1c59a-3793-4f2b-b6f7-975b45accca8))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 65994f3c-b950-433b-b715-23c0888f5a13))
    (fp_line (start 1.5 1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b1efa8fd-1449-4999-9d06-41336f5d61da))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp de68d68c-0251-4ba6-a687-f306a2dad26a))
    (pad "1" smd rect (at 0 0 90) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 85 "Net-(D11-K)") (pinfunction "1") (pintype "passive") (tstamp 74816a0a-95b3-4de0-abed-70566d632c07))
  )

  (footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 388018df-18ed-4761-9424-3d8727bf63db)
    (at 32.2 16.025 -90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Variable resistor")
    (property "ki_keywords" "R res resistor variable potentiometer rheostat")
    (path "/b766d986-4335-43ed-b9df-41844fee585e")
    (attr through_hole)
    (fp_text reference "RV11" (at 6.45 -4.8 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9c9eca7d-cbdb-4501-acd5-f907fbadb54b)
    )
    (fp_text value "Clock Rate" (at 1.975 9.2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 180c5af4-52d3-40bb-88de-90392909dbfd)
    )
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6296a8e1-a6fd-42bf-bfc6-c6204566250e)
    )
    (fp_line (start 0.88 -2.38) (end 5.6 -2.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 498809e4-208e-4b13-9b39-c4b83b83397b))
    (fp_line (start 0.88 -1.19) (end 0.88 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c60a593b-0620-4db5-908c-aff9dd28d5df))
    (fp_line (start 0.88 1.71) (end 0.88 1.18)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6ee8534-6ef6-4cf4-9dd7-c5f8ad5a8239))
    (fp_line (start 0.88 4.16) (end 0.88 3.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 26a184cc-0b68-4f0d-89b6-5b761cbb4cdb))
    (fp_line (start 0.88 7.37) (end 0.88 5.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f30887a7-6f60-403e-8d1e-22eaf2deabfa))
    (fp_line (start 0.88 7.37) (end 5.6 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3f42c28-0f25-4241-8e07-9eb5c53e2c61))
    (fp_line (start 9.41 -2.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0b9582c2-24c3-45ec-95cb-af00964508c8))
    (fp_line (start 9.41 7.37) (end 12.47 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49a86b98-40f2-45ac-834e-dcf9449597df))
    (fp_line (start 12.47 7.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca8df006-869f-4f1a-9980-da115689e225))
    (fp_line (start -1.15 -4.17) (end -1.15 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eb196010-ee51-4f21-96e0-1ec35eba6e19))
    (fp_line (start -1.15 9.17) (end 12.6 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5cbd8b68-1563-4ba1-8bc4-aee0bfddcf8e))
    (fp_line (start 12.6 -4.17) (end -1.15 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9041d91a-433e-46a6-a4c6-ddf96206fd1f))
    (fp_line (start 12.6 9.17) (end 12.6 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e909d675-e48f-458d-b330-df096d6a89ff))
    (fp_line (start 1 -2.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d43dbb0-12af-4815-8c74-2450478cf137))
    (fp_line (start 1 7.25) (end 1 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 039fdf52-9fd9-4ffc-b4f5-2f5b1bf287a8))
    (fp_line (start 1 7.25) (end 12.35 7.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 399ca681-7e8e-412a-8574-a64ad731afc0))
    (fp_line (start 12.35 7.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b4fae90-7987-40c5-870d-a722f46da7af))
    (fp_circle (center 7.5 2.5) (end 7.5 -1)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp fe93d96c-5415-4d4e-9fee-152db26d2b2a))
    (pad "" thru_hole circle (at 7.5 -2.3) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 4f92f989-d8ff-414e-be57-538cb6f7b640))
    (pad "" thru_hole circle (at 7.5 7.3) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 177c8011-9496-4be6-884f-8692d1cf46c2))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R2-Pad1)") (pintype "passive") (tstamp 9031989c-cc45-4015-a357-fb7fdf90c969))
    (pad "2" thru_hole circle (at 0 2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(R25-Pad2)") (pintype "passive") (tstamp 6ff4425b-46b3-4ecb-bae7-678b3ecb4f33))
    (pad "3" thru_hole circle (at 0 5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 0660a881-baa1-4f56-a92d-27b6899b9517))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 3ab22836-cba0-4659-9623-84087671913d)
    (at 109.343 21.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/ad673740-db19-40ff-861d-9a13fb0c1597")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a10d9438-28c9-474a-92d1-baccdd0c3d7d)
    )
    (fp_text value "100k" (at 0 1.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd2dea7d-0368-4c8e-bc8e-aa2772cfd566)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 4e38d3fe-a4b8-43bc-a85b-b29792d5ccdb)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8041ae95-1a35-4042-a403-472992675d06))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a9d78de-0d0e-4496-90f4-ac75aaad4fda))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a9bbbba-d4ef-4c42-a6a0-2263a8d366d2))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 517632f3-cffd-49a3-b245-30c3d68caeef))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bdf95054-9445-4c8b-abb2-5acf179fdd5f))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2fd8f6f4-61de-4bb5-983a-52d4e9e6c122))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34d5ae7e-7e1d-4ac0-9df2-32c1eac777a3))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d219666b-548c-4111-9243-c676ea80f516))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79717f82-6f48-43ea-8c10-5006de3dc51b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e15298e-c1fb-4c29-b865-03236340395c))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp c841ccda-1c77-456c-9595-cc6e00a2ccc7))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 90 "Net-(U1-Reset)") (pintype "passive") (tstamp 5db22b31-0a6d-4f51-a481-8ad95d05cd70))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 418d1605-764a-4a60-9786-1806e2ddbc63)
    (at 82.283 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/f97fa5b1-6168-41aa-8a8b-19b72a1d874b")
    (attr through_hole)
    (fp_text reference "D24" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ff6d9a5-1882-4e36-a3f2-666788f76cc3)
    )
    (fp_text value "STEP4" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11dc41b7-e236-4cab-9258-67d8dbe6a704)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2c3e4810-7d0f-4eef-8b64-8e880f727ebd)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 587e5f9f-2465-4411-8285-4d89189e059e))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5fc2809c-161b-47c7-8483-0e210f9d82a1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d619b00-a539-4bba-883e-30d618244fce))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23f5d3e9-1ac8-4ebd-a70d-576f9ff650ef))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7aa92683-a223-44ac-91c0-86f8ad56a79c))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16c63bd9-d2c1-4a2f-b4af-1f9b80451a0d))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 85327631-081e-4ad8-95bd-a0e9820c7b72))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3d5d6064-9b3f-454f-b0d1-2656300615c6))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 87f7be29-0cdd-4584-a88a-85f30f8b9402))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e7e1a2b5-4b71-41ed-b598-8952d1221d17))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b8d3f232-82f4-4574-8f1e-5ac11c3d08c6))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 740bcd4f-1cd9-473d-ae1d-84ecd54e89d2))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93cd817e-e090-4a69-bb76-2c1aff90c9b0))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 55df1280-371d-4769-8fc2-2696647365cb))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be0ed2ca-06f4-44d0-ab1c-4bfc870401df))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(D24-K)") (pinfunction "K") (pintype "passive") (tstamp d0d28b75-18ae-47bf-9b75-b740c5381875))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 569cc865-12dd-4e38-bfec-53f4a02e5739))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp 445b6066-bee1-4adb-a651-297b15586186)
    (at 108.553 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/70a8d1d0-a64b-477a-89c0-b15efc124637")
    (attr through_hole)
    (fp_text reference "RV6" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a3e3926b-7242-4d30-9d40-652503768422)
    )
    (fp_text value "Stp Lvl 6" (at 0.078626 -2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47d11857-d02c-491d-a408-e4c8f5a11727)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0d5ee8c-2644-4d46-895d-fdd6a615b01c)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2af6bcfd-fcde-43d2-95dd-8e08e0fffc60))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 111f2bb8-4c27-4f70-b1df-87102f392be8))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 412cf14b-f9fd-42ca-93b9-5b570af837a9))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 091da7d5-31f2-4146-a6cb-44fd4ffd3ab0))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a6cf177-a72b-4f01-925f-640d762f7600))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 17f2dcb8-7161-4607-ace7-bc1d8e65443b))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 097b2443-8fda-4a6e-962d-d223f19e6f50))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da006e10-6930-48c3-a285-1885c03f6919))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f625d00d-64ab-4323-af5a-30440698f1ae))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 27f799d7-0651-438d-a9ef-5526497c53b7))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d39f27a-6dd1-49e8-a865-5484ad3e7664))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 97ace3b4-e151-4a78-9542-ee71977b4907))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58e7d2d1-6519-4d83-a1c6-2a3cdf7a7420))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cfcd3393-592e-4aa4-a216-3c14028f84ac))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b59c795-6e79-4a2d-ba4f-154e9551ff2e))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef686dc2-caee-4811-bbad-e6febcd1de67))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b7b801c2-8d4f-404f-b125-b7cd67b2d4ee))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21ad408a-cfa1-4620-a67e-789cdc26540d))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 97eca5aa-c41f-4eda-970e-041eb8d57cc0))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d787fce5-0dd3-4976-abbf-1b56f0fb2059))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cdf5382a-ac33-4bea-9114-2f212aa429f6))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cf2af8da-2779-4339-84c1-cbd49390a88e))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25d3b472-2f77-476a-8e82-edc9108b43a9))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 035daa1d-7305-4da9-bfe0-d23fe336926c))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a3b97bc1-ccef-4642-9ef2-32864819fa0b))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d870dbba-2a8d-480e-b5ac-ef61e34575be))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d217e67-cc93-41e6-a76b-49df05988881))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 26c2547d-9399-4332-9ad9-0255f9190a73))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D6-A)") (pinfunction "1") (pintype "passive") (tstamp 23805f4f-bcf5-4f4c-8d3d-0627bd6f7cee))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D16-A)") (pinfunction "2") (pintype "passive") (tstamp 7c965127-1e66-471a-ba24-e65a7aa855bc))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp e57d02fc-6b95-41fb-b61d-ec20b89d6937))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 19e0ddf7-ad58-437a-b502-7980f0133bc1))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 4d638c52-18af-4121-9bc4-694d6e5d960e)
    (at 107.283 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/8f5a140f-2f58-4732-83a8-f7d8f7c3aa10")
    (attr through_hole)
    (fp_text reference "D26" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f0b67f9c-fb02-4f95-83bc-3ed9272b5c3f)
    )
    (fp_text value "STEP6" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10e261d3-c662-4a2a-bdba-b63334faa530)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4e81caa5-ded8-431e-a1b9-540ee46e7eba)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc4404df-ac17-45ff-8a13-6c443d8243b9))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a77b28e2-38f6-4741-9bdb-9819222f8cf4))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1517b1c5-35df-4e43-820d-dd70c815c40c))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bc67f56-4193-4b94-ab6b-ed863ae5b6db))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b74d09c0-ed35-4978-ba0a-d7a116322987))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a34dcd4-5982-4c5b-beed-b79de01b195a))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b085db9d-a762-464a-9ae6-ccd4160dd767))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5092b591-b2df-431a-a600-44f19a64901c))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cdb27273-6557-4161-8847-59fb17d7d2c7))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ceaebcf5-f5d5-4682-9968-95ef81b4451b))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e4220f7-72a0-46a7-bc12-fde6cfb55584))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b1b84d1-2dab-405e-8745-dc4c19652575))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9c0f010-c21a-4f89-bfdb-52bf30f28416))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b6cc762-12ae-4c38-aeb1-1c2a94de6f21))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffa88657-d0d1-486a-9ac2-636515a16c88))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(D26-K)") (pinfunction "K") (pintype "passive") (tstamp f66c1630-d54b-4eab-8fed-ee7af3f4b066))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 4bb885f4-3af1-4cba-8f46-2bd013db3fc1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp 523c9110-f6ed-43f5-b342-84757a46105f)
    (at 58.553 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/3557ed4b-6e4e-4655-bfbc-cff98bcefc86")
    (attr through_hole)
    (fp_text reference "RV2" (at -0.031374 2.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2651bd27-1ce8-437c-a950-bcc6e1556152)
    )
    (fp_text value "Stp Lvl 2" (at 0.038626 -2.55 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9ca9718-90bb-4deb-a6d8-84c0caa7d4ae)
    )
    (fp_text user "${REFERENCE}" (at 0.038626 2.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b26aefa5-aad4-437d-b846-7bfe7810c07e)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f6d34527-f48d-4882-a996-c18478b160e4))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4762a965-f489-4c97-95ff-b9b05ea33dcf))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78a643be-ff2d-4fe3-893d-efd9b69d0185))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b817a6f3-5cd7-4c62-8eae-b943eed6b572))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85541d5b-d890-49e6-b4f3-f1faeccd805b))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6de0b6bb-4b18-4114-bb75-524330cdd468))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 565ca86e-c725-4f52-8123-c8c9766c6d4e))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a49d39fd-b607-42ca-a2e9-66faa8067f12))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7a504e7-f029-4092-b221-0704cc74d42b))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1fd43cd4-9bc7-48ca-8f2f-6924815eeb1c))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e20cbe39-688d-4d14-bbdf-aedc8b90ea79))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e143e75-b9ce-4359-8618-d1094cf39c83))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 540d18ac-4829-4590-af66-996b20bbb7bf))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0871e953-1512-4f79-a7ac-0678fec38dfd))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cb269f15-2ff6-42b8-a213-3a396982e3a6))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ea4aee1-4eb6-4be5-9d4c-b2934cf59471))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00f3b010-eed0-4f48-aa68-8d24456d5d5f))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c76f9e40-a4bb-4ad2-a84f-f9a51a6e0b8f))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f91ca43-255e-4ebf-ba89-91a4911a9885))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 33546df0-a0a7-49fd-bcec-41be5555c8e3))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7742571c-cd7c-4a42-8b08-6ffacc8c2d4f))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 11448688-4cee-4b15-94ce-2203b9f9b626))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp efae6fcc-8c98-4fce-bd0a-45b7ccb74276))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 048afffe-a1dc-4e6a-8d11-feb4b1f6777c))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fffad808-7e4d-4639-a33e-21766e584201))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87c2a204-0c64-4c70-881d-0f7d5d38a833))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4cae729-e576-486d-b684-cbfa9ea9a952))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 40b1fe41-9aee-4029-ba5f-020b97170999))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-A)") (pinfunction "1") (pintype "passive") (tstamp 4e0e0c3b-5329-41bf-8462-ad3cf8fe9fb5))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(D12-A)") (pinfunction "2") (pintype "passive") (tstamp 548516a8-43e2-4a4f-8c5f-03d86237205c))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp f9185da4-d798-4ef0-b23b-10721798ce30))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 73912e7a-6212-4af2-a3eb-58588880442a))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 57903993-8135-4249-a2c9-11a5eb2dbb26)
    (at 47.75 16.47)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/e7082dc8-06f5-4bb5-b360-4274f39cdd4e")
    (attr through_hole)
    (fp_text reference "J2" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 728fd62c-93ed-4d49-b002-0cde1ac5803a)
    )
    (fp_text value "CLOCK IN" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef274710-3211-4a90-99ed-fcffef2cb0c4)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp a31318ca-177d-4915-800f-fa352b4b056f)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1d7c6494-5cbc-456c-ae6c-db3b508b8f46)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2d7713c4-be0c-4d86-97c3-e0de9ceb1172))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cac11480-4495-464f-b004-065d0b6c3507))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab893226-b65c-4036-837b-77c18c5b71ac))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 436e4371-b7b5-4544-8001-db176a9b64f7))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2162c231-faf4-4e03-b095-a35688b1be79))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef8abc3a-c06d-462e-90ee-1c508f4740ff))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8271d1a6-b2fc-440d-89eb-37def0ee2a85))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f339bb6d-d79e-45b8-b2f6-c76e146bb3cf))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 124a21b8-cee3-4110-8bbf-0a5c2b35e741))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5a33cd2-9039-4c08-ba90-e811ebbf7ea5))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1449e1ee-2e15-4872-9f41-bcc0b631b7a7))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3e12939b-66bf-4d3f-a475-6e59ceed42ad))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6111cee3-ec16-41e7-926b-5dd8203a1c77))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3640ab02-09c5-4541-a4b4-1305613c6c66))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0100977a-2514-4900-beff-963fbaddf26e))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e966d698-47de-4fd1-9513-8d388e96a1a3))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 26b021c5-79c2-4ba2-9850-2339e48bbe63))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77cea80f-82ea-41b8-9445-61d7cef44df6))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c0ba6ad6-4be0-46ce-917d-4af7fb641314))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp d6329db2-e4c3-4dd0-aa58-5c40734ec666))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 84 "CLK_IN") (pintype "passive") (tstamp 96b9749d-57c4-402e-9310-6e37b062fe43))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 97 "CLK_IN_N") (pintype "passive") (tstamp 695c7c88-d5ee-4399-bff8-6609948cc45b))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp ba8cba15-5360-4cc9-9ade-ea0a4011ead6) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 49.255141 22.95)
          (xy 49.23493 22.704171)
          (xy 49.174841 22.464945)
          (xy 49.076486 22.238744)
          (xy 48.942508 22.031645)
          (xy 48.776504 21.84921)
          (xy 48.582932 21.696336)
          (xy 48.366992 21.577131)
          (xy 48.134482 21.494794)
          (xy 47.891646 21.451539)
          (xy 47.645007 21.448525)
          (xy 47.401187 21.485835)
          (xy 47.166734 21.562466)
          (xy 46.947946 21.67636)
          (xy 46.750697 21.824458)
          (xy 46.580286 22.002784)
          (xy 46.441288 22.206548)
          (xy 46.337436 22.430278)
          (xy 46.271519 22.667965)
          (xy 46.245308 22.913226)
          (xy 46.259507 23.159475)
          (xy 46.313734 23.400099)
          (xy 46.406532 23.628634)
          (xy 46.535411 23.838945)
          (xy 46.696908 24.025382)
          (xy 46.886687 24.182939)
          (xy 47.09965 24.307385)
          (xy 47.330079 24.395377)
          (xy 47.571785 24.444553)
          (xy 47.818278 24.453592)
          (xy 48.062936 24.42225)
          (xy 48.299191 24.35137)
          (xy 48.520697 24.242856)
          (xy 48.721505 24.099621)
          (xy 48.896223 23.925512)
          (xy 49.040158 23.725205)
          (xy 49.149445 23.504079)
          (xy 49.221149 23.268074)
          (xy 49.253344 23.023526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 5f259d13-1382-4454-a954-99d1351c81d0)
    (at 157.283 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/75ca9aa3-60cb-4c6b-b509-7abbfdcaff7d")
    (attr through_hole)
    (fp_text reference "D30" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d07f25de-8a3a-46a9-93f5-d0b656b9f6bd)
    )
    (fp_text value "STEP10" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a720e25-6b85-4c34-ac7d-500885e0491d)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1cac7f2b-4c05-4596-ab02-51cc9fcf5b49)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f88d604-e844-44c1-85d0-1ebb6714efe4))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 130bfd32-93ca-4069-ad29-21379c81b0ec))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7952ef74-feee-416d-af15-495c41b6e849))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51d6c195-be62-41f5-b97d-cecbfda0dedd))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd600066-270a-45a8-9ed3-5c69faf0be98))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32dfb074-95e0-4546-b3fa-4f84ab52820d))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 316a765f-29ac-43de-a41d-41f6d7b38295))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 27c70ded-03bc-45d0-bcc2-bdd303fcce88))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 85bbc0b1-690e-45f7-8c3b-3d65ada8372f))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 00b17b0e-b4c5-457f-95ac-0ad088ad7a11))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4ce0023-bc82-41e6-80eb-4cadf12f06f7))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9181d592-80d2-4169-8eb2-c3b81d332039))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 74e1402c-6801-4832-b82c-35e2030381d6))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 561cca89-142f-4cf9-8b87-626fa48aac09))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 042a042a-4290-44fd-a129-60a9b3215215))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(D30-K)") (pinfunction "K") (pintype "passive") (tstamp 2662bb06-c5cf-487d-a4ea-cff96f8880f8))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 4ace15b8-b550-4045-91d0-a67fb7ca5e6f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp 63f694ff-3f47-41fe-9707-d1eec71b346b)
    (at 83.5 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/7949112f-8149-4d0f-80f1-9f39db374004")
    (attr through_hole)
    (fp_text reference "SW4" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8535a726-f825-4486-be0f-a632019ee4d0)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2b43a948-ef79-4694-b83b-9ff77d9dd601)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 26cbf96f-f3b3-4859-b53c-0cc4b913effa)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2384f5c4-040a-45d7-b442-6aca5ccd7972))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 657bf107-92a1-40f6-a6d0-e1af6ae796dd))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c5791213-0228-434c-b503-ead6b9653406))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 983a628c-5b2e-4e86-a311-2b564c0a9b41))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d7abe413-bbe0-4fb8-8892-7ea3135281a8))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55632257-7302-4310-9896-c1db9da450ce))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c92ca10b-d148-4c4b-8327-46da2266be12))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 18b86972-b783-45f9-a5f1-3976ddd7cd77))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f8cf3bd-24a6-420e-98ee-72c493aa4680))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e0d787d6-c1ce-460c-bbc0-147f17c15d69))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70db0270-0b13-4a9c-a12e-a76a53b41814))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff8fa469-4aa1-42cb-9d3d-dcbda0a1cf10))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp e40a3e5f-5936-4e08-8410-16a21bf4f0a0))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4-K)") (pinfunction "B") (pintype "passive") (tstamp c6807577-9e53-42a7-b76d-7bb6f397a798))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 957bcf11-27c6-436d-b30d-d8b5a73c1a35))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 66774aa2-70d4-44ba-8804-7c19a3448275)
    (at 150.5 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/b27b3e4d-3220-4998-8c24-ce59b4d92104")
    (attr smd)
    (fp_text reference "D9" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8f5b287a-04e2-4eea-ada1-6f9a33663dde)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 57fdde4b-a5f0-4815-8ea2-0ed11fd221ad)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fe61591c-5e2b-41b9-b6e7-ffeffc419fa5)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ea5296c-50dc-4c14-abf1-285f2dbe2515))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7b1ff8c-6ec5-4cd8-9312-0d8ad19cac8d))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d53a533f-4003-42d5-9092-837bfe263540))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 38e61a0a-413a-4380-bf5a-1b37bae117ca))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2274a29e-a8ef-4aef-9f75-8d5442d1a98f))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8373d05b-5986-4ed2-9fea-eebf1a53e398))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0c2a1f17-5416-477b-be49-ecf1f1cbc89e))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84106c7f-3db2-437e-9e4b-57a41da025a5))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4fb8b944-9c07-452f-8c68-03dc7d067149))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d4ce6c15-402b-4491-9847-2c138dfdd76c))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 40e06c08-8a5e-4206-ac45-426f1f91d008))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87d5394e-4135-4368-bf2a-1bb69b8d7134))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 172b3935-c698-4f25-94c2-e179103bf6fd))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2cd242d4-82c9-4c9a-895f-0be0229af890))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed08bf15-6c35-4ca3-9b14-92fb5e3f605f))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0da5ed08-c008-4ac8-b776-699390f57964))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c28e3c29-ef59-4390-840b-3fabafe844f2))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64272142-747a-480a-b577-7455019662b9))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 19 "Net-(D9-K)") (pinfunction "K") (pintype "passive") (tstamp 82953dca-8d4c-47f2-bd2d-f06c33c8d6f5))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 20 "Net-(D9-A)") (pinfunction "A") (pintype "passive") (tstamp 2d1eaf24-6abc-4bd6-9129-62a63ddabccd))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 6a58e902-3e00-4198-8f81-2dff423c9eec)
    (at 113 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/3ccb4da4-fbfa-4aef-bc2f-7ab715fe5c1c")
    (attr smd)
    (fp_text reference "D6" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e67d198-a150-4120-9d69-7001fbe7da44)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c286c2ca-faa5-4761-97ef-9c5c734b0394)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 01d8c3a6-1c2b-4ee1-8d54-2590afc48267)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5e48787-b3de-4f63-bf52-94ed10d2afbf))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b0ccd376-28d4-4383-be26-11e3f4c433ba))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp db15d08b-5c67-4de2-89bd-817d8e0a1f1e))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f65cc10b-e407-4249-8cb5-0444328496d6))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2d4b326d-a308-4da3-9444-212ff3c7bdcb))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a29df6aa-a8ce-4ba0-952c-d32c33ce474b))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f6e34cb-c961-4a4f-8634-0348fef7adbf))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1dad7910-f0e7-4d7a-9543-051f8a0464b3))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb5467f9-5fbf-450c-bbb6-6c7454402767))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 72101c7a-a41f-4bba-b3b2-1227c41784d2))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a522b37-dc09-4f04-a9eb-b72d1cdf3be7))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8d705085-8e09-47fd-afef-c30e1aa40618))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc3d3137-5ff2-4c3d-8218-d81335ffda81))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f7e8e7e-c7d7-44d8-80fb-8c8cde562e0c))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 35e8ca24-55f2-4cae-82c6-7a0f07d3dbe8))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b9ff2abb-cf29-47eb-b8c0-bf417e6866da))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed46bd2f-f654-40d5-aa55-f906da090260))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 035d7a8c-51dd-4e08-8e30-d728fa8db089))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 13 "Net-(D6-K)") (pinfunction "K") (pintype "passive") (tstamp 7afee8a9-c848-4e20-95ce-297bac636f9d))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 14 "Net-(D6-A)") (pinfunction "A") (pintype "passive") (tstamp 053d87e8-a64b-4bbe-8166-32f2515de1ea))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp 76fe937a-d923-4ad0-8fd6-d4a50f32c839)
    (at 133.553 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/2de2c660-4a22-47ec-94b9-24e52fd4c21f")
    (attr through_hole)
    (fp_text reference "RV8" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 93827116-5c79-4d4d-95f4-60b16d109d5a)
    )
    (fp_text value "Stp Lvl 8" (at 0.288626 -2.57 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c5da4fa9-669a-4ad6-8e3c-b51e2b058a6f)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c16ea3e-828c-4361-9552-23cbc3fcf2d3)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 363c87f4-1612-4c74-84bf-572c19bb1f4c))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5544b3fc-60bc-4aa9-8919-e26f2d7d0c52))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be897e93-ac19-4ad2-816b-d2670b40d8c7))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dce55f11-c9ad-484d-b7a1-04477b502c3d))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 988d49fc-884e-470b-b7f0-b383cd0d1c2e))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7a80a05-80c3-4569-bab5-864082d8f5e4))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bd5e9c71-7c67-44ce-95e4-fcd30c762dc9))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5367125f-50c9-484b-9651-75190cde09b8))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 11812f4f-d3fe-4c56-8afa-3a98bf9b8498))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5cd187b-55ba-4848-a6f2-265f80c5c5fe))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7bd959ad-80ac-4809-aad5-c1c494b953da))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a75f91ec-c8a1-4698-8edf-8ef919cf9102))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 259b294c-b2b0-4474-aa4c-bbf81e1a2460))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 279b7ac9-4497-4bec-a4f2-23365b284c38))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ae5a4365-4db2-4820-a491-8a92e9d85a40))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp df973ad9-d8f8-430d-acc4-64dea4ab2c4c))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4cf3c1ac-5a2f-4a35-8559-ef8d17742e3c))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74feb9f4-b027-47a4-8d00-d456d316032c))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 795d1195-7188-4fad-a8c1-5ad63970f5a6))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e045d857-d16c-4527-b173-6c6dcfc21a22))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 07a25b5d-139b-44ea-a183-9399e70c4228))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0888302d-0bb9-44a9-80e5-a5f14aded932))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ac842390-ec47-4f12-a3ef-0b85bdf109e9))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e775f09-0dd7-4516-88be-28f3fcc16b44))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f562e44-f624-4b02-a491-55d7198eda04))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6909ffed-d6ef-49f0-99ad-88f049d6c081))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 826e52cb-a35c-4452-ad97-7139ebde4a71))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 90e4c1ad-1788-459f-bb25-5ad54ac8a11c))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D8-A)") (pinfunction "1") (pintype "passive") (tstamp 1e07ed92-dbce-44a4-9b12-6ec57332a0d4))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D18-A)") (pinfunction "2") (pintype "passive") (tstamp 744df253-319e-44be-b251-2896ec1a0ecf))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp c755e0d2-7448-42f2-8242-a095be0b4998))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 4f08957a-c7d7-467f-923e-1c13b608a1bb))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 79a6d254-37bc-44ab-8d36-7422abc6f764)
    (at 50.5 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/f7f48cb2-98b1-4bb1-a3a0-803ad175e8fa")
    (attr smd)
    (fp_text reference "D1" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 120e378d-e0ab-40b5-96af-132e372f5bbe)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1d1729c-0bcc-4648-89be-a5b0113e66b4)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20d1801a-ab4d-4517-870f-7ab11c0acd09)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2721bcd8-47c6-4db3-b651-df6dbab4a7f1))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7297fb2-5593-4bf4-b66b-dcf934b22b9e))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8fd26b4a-27a6-4fbe-aeca-ac91990289b6))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7db8fdf9-f840-4b12-b879-564d3638835c))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b22ace79-3921-4578-9487-b8d688610790))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7d380614-0d79-478c-9711-c5bdd196ae58))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1193b4d-c0f3-47b6-b0d0-0e61bc32f104))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffaa7622-57dc-422f-8f38-b42447fe1baf))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c3c3213-ebfd-44bc-bdfd-4284461a07c2))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f374164-00cd-4e68-a5f1-c1fe903188ea))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1dc208a5-d45e-4333-aacf-bbccd195da63))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de6e78fd-5cb8-4a92-a34c-d2468ebba5bf))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc48b62a-4740-4ab3-a640-9eebfc9f1082))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3cf93c73-2d46-43f0-8753-13ceb03377c2))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b4612132-9316-4b23-a126-ccc964c951f5))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4199c64-122c-4b88-9bb0-f305740c7343))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f081fbc1-c3d6-4c26-b0bc-32157c916b01))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae573d19-a316-457d-9fb9-2a2d8cf03ad0))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive") (tstamp ed78a9cf-e7e4-4f8a-bfef-38fd44fcbd78))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive") (tstamp 6f5beb13-d11c-446d-b5c2-5b6df147c3f1))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 7a811af9-d2f5-4dac-a360-15388ee358d3)
    (at 177 60.6)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/cf4747f6-1bf7-453f-9a17-2abe64d64352")
    (attr through_hole)
    (fp_text reference "J14" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a5ab83e-a4c7-4142-92b6-8cd8394104e1)
    )
    (fp_text value "CASC OUT" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9e9933c-26f0-4123-9b51-9b7266306fba)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 0d748e03-b777-4e2f-89ac-f9ba43ff878b)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 287fac13-87bd-4c85-aca0-6157d3069e32)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aceca13a-b04a-45a9-a5ef-e7aa5a3e52c1))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4dcacb70-2b83-4c1e-9eed-73f31476b5f0))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c70234f-6d36-41cd-8f07-cc201e7a7e07))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab4f04d2-4480-44b7-9a5d-84130c99109d))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ef73206-6da8-4b89-acec-6275d5b5729d))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7046affb-3b52-40f6-9fa0-0b0b0d0fbbaa))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 920b5ea6-bd16-4e17-89c1-540701e6deab))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45562691-3923-4681-9fec-7b66862f6279))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 4a22955c-ae27-4adb-8940-243f739c9e23))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8af31a08-121e-40a3-8014-97ab4beb181a))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 80f3b248-1e84-475d-9d01-2a5da659290e))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e28bf6f6-5cd7-453d-be25-36c1e34e9328))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d63d2d4c-0ee6-45d5-ab97-b1c8e0d5124f))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49a17678-8c22-44b5-861b-1a12b3b535e9))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77a9777a-b16d-46b2-8448-a137eff2437f))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d39ce22-3330-4c41-9af6-e019fc4ea9e3))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bca1465e-dee9-47d7-9d56-b23629e7dfd2))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e886119d-0741-42b5-a6ab-670ead0d0654))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 60fb9f41-0cdd-4230-b4ca-4bd546332afe))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 93e98c03-5eb3-4623-8b74-c6788d67f124))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 92 "CASC_OUT") (pintype "passive") (tstamp 97f800d4-3091-4bc9-8695-db7c7b670145))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 116 "CASC_NORM") (pintype "passive") (tstamp 87bab10a-c685-43f8-812a-a1eef913c46c))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 4651761b-e2e5-4c83-81ac-5e0cf766ffd9) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 178.505141 67.08)
          (xy 178.48493 66.834171)
          (xy 178.424841 66.594945)
          (xy 178.326486 66.368744)
          (xy 178.192508 66.161645)
          (xy 178.026504 65.97921)
          (xy 177.832932 65.826336)
          (xy 177.616992 65.707131)
          (xy 177.384482 65.624794)
          (xy 177.141646 65.581539)
          (xy 176.895007 65.578525)
          (xy 176.651187 65.615835)
          (xy 176.416734 65.692466)
          (xy 176.197946 65.80636)
          (xy 176.000697 65.954458)
          (xy 175.830286 66.132784)
          (xy 175.691288 66.336548)
          (xy 175.587436 66.560278)
          (xy 175.521519 66.797965)
          (xy 175.495308 67.043226)
          (xy 175.509507 67.289475)
          (xy 175.563734 67.530099)
          (xy 175.656532 67.758634)
          (xy 175.785411 67.968945)
          (xy 175.946908 68.155382)
          (xy 176.136687 68.312939)
          (xy 176.34965 68.437385)
          (xy 176.580079 68.525377)
          (xy 176.821785 68.574553)
          (xy 177.068278 68.583592)
          (xy 177.312936 68.55225)
          (xy 177.549191 68.48137)
          (xy 177.770697 68.372856)
          (xy 177.971505 68.229621)
          (xy 178.146223 68.055512)
          (xy 178.290158 67.855205)
          (xy 178.399445 67.634079)
          (xy 178.471149 67.398074)
          (xy 178.503344 67.153526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 7b969e35-7155-45c2-af71-9a0d9f212898)
    (at 144.783 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/492a6785-1cf7-4f2f-b411-3a2f992d8621")
    (attr through_hole)
    (fp_text reference "D29" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c677ce34-70b1-4330-830a-8ebbee3d109c)
    )
    (fp_text value "STEP9" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 814470af-d66d-4643-8174-2bd6505812ca)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8bc69f88-fada-42f2-a2c4-9c7251bb1e0e)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aeacadb0-5299-4199-b14e-c609727d5aff))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1fbfe99-389f-452b-ad6f-e882326766f3))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fea10e27-ca33-4ba2-8de0-807eeb4a920c))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3b1f959-177f-453e-ad63-adcf266546fc))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 59d84653-131a-4d63-8e62-6e21aedcb30e))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ebbb23e-9ee2-4119-895a-1720467c0654))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 77507f59-05b1-4f4e-a072-9156f8f3f604))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e0f3c30-0194-4535-bef6-4719b67615d0))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f88cb703-1a89-4945-86d1-5ae3f9e984c5))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 90b64bff-85e4-496c-95a2-2984807c66de))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 652da33b-6b1a-42eb-9584-c479f7a8bf32))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19f11c19-52b8-4287-97d1-0f9bf6a67185))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp da511d93-0407-4394-8add-41916f828285))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e310ad9-577e-42ad-bb8e-1641374bd6d5))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48d12069-152a-4c86-8a61-fb855a51cca7))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(D29-K)") (pinfunction "K") (pintype "passive") (tstamp bd06ca6b-a320-4c61-965c-b0504529e6b6))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp e98f45a3-0d4e-4110-b13a-8950b279e060))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 7eb6834c-0518-4139-942e-9bcb5be24322)
    (at 99.25 21.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/48bf121b-ef12-4c51-988f-61a2380d1d40")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.68 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4696b4e5-3241-4757-a524-7087f77f0f2b)
    )
    (fp_text value "100nF" (at 0 1.68 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2290bac1-2e83-446c-9f7f-8b9a7077ad2c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 905480ff-2c09-4216-8f0e-9c96fb666572)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f066434-dd79-4f2a-b088-4a99c0089a19))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78b4a640-9e8b-467a-bef7-d943b5d1b242))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 40d99757-b5d0-4d06-aadd-260bc256685c))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 29860800-092b-4028-a821-e4bee847b5e1))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4dab49c4-5478-4765-9c7d-f079c3b12a11))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2b2d1ca8-7a4c-42b4-96b9-182061479843))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d175bee6-a371-430b-ad9c-ca7f1f95a81c))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b58ab81d-0d7f-4872-ab89-160019393319))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1955e9b-968c-422a-9b42-9c6e3adc44f1))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba75df20-772c-4566-acd0-0beafb965880))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp 13a298fb-9600-4605-8d88-8c0eca7f01f8))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 106 "+12V") (pintype "passive") (tstamp 866ddf1d-fe75-460d-925d-782953704505))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 82a452f4-a215-4064-aa34-d8e5b3e42cb1)
    (at 169 33.06)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/ee255141-3d8e-4ab3-adad-41b21585f52a")
    (attr through_hole)
    (fp_text reference "RV15" (at 0.75 -3.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c925592a-8454-4397-837a-fd75304ec17a)
    )
    (fp_text value "B10K (Glide Atten)" (at 6 10.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa408bac-7094-49e3-a868-e07db133958e)
    )
    (fp_text user "${REFERENCE}" (at 7.62 2.54) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee6d589c-16c5-4f04-a025-aeb2588448e5)
    )
    (fp_line (start 0.88 -2.38) (end 5.6 -2.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b5fcc8b8-94b3-4331-b0d2-be522afb55d6))
    (fp_line (start 0.88 -1.19) (end 0.88 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 90e9ad70-b39e-44ff-9b4b-57fa7f1a830f))
    (fp_line (start 0.88 1.71) (end 0.88 1.18)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a12a7f40-83eb-4894-a1c2-265ede956ec9))
    (fp_line (start 0.88 4.16) (end 0.88 3.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c220f344-c67e-4734-8c33-bee5f7d82fe9))
    (fp_line (start 0.88 7.37) (end 0.88 5.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f4b4cb9-58be-4f22-b75c-3202739a3d82))
    (fp_line (start 0.88 7.37) (end 5.6 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d871689c-2d0c-4876-bd04-0adf7005b9d8))
    (fp_line (start 9.41 -2.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e94e9fa0-6cbc-4275-a346-0546841a44aa))
    (fp_line (start 9.41 7.37) (end 12.47 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d60d1b7-b56e-4ac5-b664-8de5595dc519))
    (fp_line (start 12.47 7.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6d7f9676-41d7-46ff-a441-0bac7d6ea0a6))
    (fp_line (start -1.15 -4.17) (end -1.15 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7667013f-64cf-42a0-a9e1-ee033b22ae6e))
    (fp_line (start -1.15 9.17) (end 12.6 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b47457ef-d236-47e9-8064-725f7963687e))
    (fp_line (start 12.6 -4.17) (end -1.15 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b41e9f18-8be2-4862-8278-a611c6e8ce63))
    (fp_line (start 12.6 9.17) (end 12.6 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a553d85-af27-4064-9e1d-dd9006741da5))
    (fp_line (start 1 -2.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ed0c0a5-f9fb-4853-9bb5-5d78da8b5959))
    (fp_line (start 1 7.25) (end 1 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66d023f2-4e33-4952-898f-48725dde048e))
    (fp_line (start 1 7.25) (end 12.35 7.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2979eb78-ce4e-42ec-88af-6f9b36194f6b))
    (fp_line (start 12.35 7.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa529ded-ee17-4cd8-9de5-bd2c1192dac2))
    (fp_circle (center 7.5 2.5) (end 7.5 -1)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 1245ac2a-38ac-490c-9b87-10761f66f8d5))
    (pad "" thru_hole circle (at 7.5 -2.3 90) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp a8ce7ab4-d07b-4318-8762-fda6551fe478))
    (pad "" thru_hole circle (at 7.5 7.3 90) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp c3e536f4-2e3b-484c-bdbe-927fe36ea7b5))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 109 "Net-(R41-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 20f79652-03b9-4389-a42f-80303c84abb6))
    (pad "2" thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "2") (pintype "passive") (tstamp f9d135fd-9eae-459c-8205-c7f67465d833))
    (pad "3" thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp e9b2314e-3954-434b-a8ba-c9582910e4f8))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp 84a00af8-c116-4bc2-8870-8562bbb312a8)
    (at 94.783 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/6517db95-4136-487c-bf60-8019e65a32e6")
    (attr through_hole)
    (fp_text reference "D25" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d374293-8269-425e-8dc1-29e130865b21)
    )
    (fp_text value "STEP5" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8760d852-3123-417e-9216-39a934f961fb)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 563acc02-23aa-4bf4-9641-710215ef80e7)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6dcfe965-a9c6-4257-83ed-0570d885ec66))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b564e863-ed51-479f-9146-e25283de1411))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65ddfb12-f6eb-4e3e-b71d-385987c4f06b))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bb396a2-63e9-48d3-b21f-d5ee5a85a884))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bdb63b52-ae60-4532-9b0e-8dbc60cbe26b))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 38493b58-9704-4fb7-bbf2-4708f8eb5d27))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6e7d6829-8318-444c-b545-bb04cdd6c0a8))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d0504ae3-0b00-45fe-9a9b-fd1c44f73c7f))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f5574ce-6a78-49ab-8ebc-7854dcdaaaa0))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ac9cbf7e-c869-4d9f-a3ed-50fdc9caa81f))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d3e5495-7a67-4c8b-8ae3-57d572887907))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c1d1262-7f3d-443c-92e2-41b360e16572))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65c2185a-236f-4016-aaec-75d151c02e55))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa19031b-58f6-486f-a89f-092f4832d652))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 633ef047-fe08-403c-991e-4701e6242a07))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(D25-K)") (pinfunction "K") (pintype "passive") (tstamp 11f6d376-3b31-499c-b6df-ad8d93a3b2b5))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp b1992ccf-0f16-4cb4-8420-7b88335464bd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp 8847ba53-717e-46ac-9dd9-a897247aa2ce)
    (at 163 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/93b448d3-58e4-4bb6-841e-b282b22fd434")
    (attr smd)
    (fp_text reference "D10" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8e8af53-ae6a-4099-b28e-2f2da108c5e7)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fe9312a1-14c5-4b89-9628-2c6bf34c5eba)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 95b51462-ba92-48a6-b68e-c47cab164143)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c25c4994-48b4-42e6-a014-6a470febbeec))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 61bb0d51-6d4c-4659-9124-90da17cdeb86))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8aaec37-5bbf-4f03-82ce-73b00cbd6bea))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9c845b29-acd0-44bd-89a5-7eaa56b33df6))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 29cf3926-cb8f-4ed6-b4f1-e428b8533137))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa8a97d1-b45e-46d1-9594-627f48010eb1))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a55deed-b69c-4965-9f83-d19b79e0e373))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp df154714-0948-4290-b474-11d0ba87dfdb))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb67532c-b50d-4b5f-894b-17daa6825592))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c787d24-4846-43d0-845f-b1977af6cb16))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9993dc57-4faa-4fe7-a53c-72cea65a5321))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5562e028-e859-4198-b0fc-5a6e1192668f))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bebb9bbb-54d0-4e57-a539-82d13012ac3f))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b8f2566-2bf2-42b8-9e0c-8b018869dd88))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp caf474a5-fdd1-4c48-b454-b787acd6354a))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 24b0a75e-028c-49a2-998a-3959de179858))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9c70338c-fd04-48c7-aa42-5b5d425f5dd4))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81e3e66b-9f19-456d-88e6-1580d2e67baf))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 21 "Net-(D10-K)") (pinfunction "K") (pintype "passive") (tstamp 099b53ec-b4ee-4af6-bf9c-fc4508fa42bc))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 22 "Net-(D10-A)") (pinfunction "A") (pintype "passive") (tstamp a38933d5-a3dd-495b-9470-be052e222110))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 8c6032dd-79e3-449b-8adc-a54b3abcb078)
    (at 169 61.96 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/25842358-6c9f-4cc6-8114-46b64f4268e6")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12b80213-bbef-4938-8232-1c8935828f9e)
    )
    (fp_text value "100k" (at 0 1.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d069a51-333f-4156-8360-07bf3d419917)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp ad8b0fb6-4016-42b4-ab64-3a725ce326eb)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 61504afe-d037-4886-8710-97a6dab6e026))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9d819d3b-f29c-4086-adae-0f0670ef60da))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a19cc7e-ad25-4de0-a543-73bf44470558))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d614c47-304a-43b2-98a6-585d67031396))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9e04b40-3883-48ae-8e78-7c6a7ceae24d))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 94fe1bf9-598d-43fb-a1d8-727887df8bec))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b8a110e9-3706-4d0f-9db6-973f146f2adc))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 62eff1ac-ef8a-4c8f-b2d1-1d0384b711ef))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp debeb2cd-680f-4bf4-b757-df5ab5683e50))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f2fe749a-4f5b-4657-9e31-60df873f835e))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 207e377f-90f8-4686-8e86-6f5f2192d047))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 92 "CASC_OUT") (pintype "passive") (tstamp 33371d26-536e-4857-b7c3-7339b9b76f65))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Pushbutton Switch (PBS105)" (layer "F.Cu")
    (tstamp 8cbfb993-485a-41bd-b122-2c4967d81ed8)
    (at 36.25 89.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (path "/c21f60d8-7735-431a-9933-e8230c037a10")
    (attr through_hole)
    (fp_text reference "SW16" (at 0.001344 -6.171835 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cecb98a6-15ec-4d51-8ec4-d4339ba9e5e2)
    )
    (fp_text value "Manual Reset" (at 0 5.761533 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d1a885f-53df-4cda-be57-24eaa9c05479)
    )
    (fp_text user "${REFERENCE}" (at 0.014406 7.115765 270) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 965d4722-72dc-469a-914c-d22915013c23)
    )
    (fp_circle (center 0 0) (end 4.85 0)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 5a092ebd-e4d7-4bbf-8833-c8bdeb3bff7f))
    (fp_circle (center 0 0) (end 5 0)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 924d3e17-3ac1-4e7d-9b6a-f9be5aeb36f3))
    (fp_circle (center 0 0) (end 4.75 0)
      (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 2fdd9b52-fcc3-4f83-a0a0-20c3b8302a57))
    (pad "1" thru_hole oval (at 0 -1.75 90) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask")
      (net 106 "+12V") (pinfunction "1") (pintype "passive") (tstamp 066432a1-bd11-41d1-a5e7-40559ac7b68b))
    (pad "2" thru_hole oval (at 0 1.75 90) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask")
      (net 83 "RESET_IN") (pinfunction "2") (pintype "passive") (tstamp aab9c604-c1bb-4059-9668-890b410d0c17))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 8f31afc4-8158-40e5-a377-43bcd38fa947)
    (at 153.9625 26.75 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/9b83c56d-01b5-4a01-8cdb-e2d4fb255a70")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 718d40cd-768c-48d7-8aa2-e7a5a5d26999)
    )
    (fp_text value ".1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da8e9b5b-db67-43ab-80bf-7c136a6566cd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 035b679e-2296-47e4-b7d6-34ce35f31588)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2d941fc-9ccd-440b-ae66-bba06fd151e4))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ced7e69-b77d-4e7d-891c-b135fe7e9439))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fec52514-8c62-4a45-949b-b902de0267d0))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4e8c362b-6c94-499d-b489-08be1c0ace57))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6a7c0f43-1b5c-4fe0-8397-c132d77e1c86))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 689749e5-4f94-470c-a4e1-26402bf08535))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50452693-3506-4b91-9bf8-63804d39b156))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae2fadd8-37a1-4638-8bcd-eafa573974e3))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0f767ef-4256-4aea-b86c-69f117acbd6a))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8122e0e9-9d93-4420-8113-1ce3bf900230))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp be560b05-addc-459f-993a-16483cdadd42))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "-12V") (pintype "passive") (tstamp c92f77db-5cdf-4c0a-945e-888466574a1b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 936c5b69-db7c-402a-84e1-3f4136e16587)
    (at 162.25 42 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/98c95737-efdc-46d9-b3a0-b3b3d8f84a68")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.65 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a529f11c-fa54-447a-9da2-97572a08d9c7)
    )
    (fp_text value "10k" (at 0 1.65 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1e29a58-423b-48c8-bf0f-d26d85f0757f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp c9d6dde2-053f-4785-b83e-c6e1b38beff1)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f115189-1181-4f3a-b0e7-4264645eda81))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35cf56b9-845c-4b57-b9f5-0149f4bc079d))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ca44b758-7844-462d-8515-0885eac7e3ee))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f06c6528-0863-4735-915d-6a2360433060))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43c89c67-cebd-4d86-b739-731491552504))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6f04b163-ce22-41d5-8022-4a8b01f86f9c))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d15f5744-8ad6-4916-b9c9-4a2846323956))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b4004e12-a3db-40ef-889e-19b2662c59f8))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5951bb63-bf71-4e85-b3bb-e5a59aacf51a))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42d1479d-7159-409c-b0d7-e63eb3d89fe8))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 109 "Net-(R41-Pad1)") (pintype "passive") (tstamp 5b8c8cea-0c66-4a6a-a18a-88ae090bf894))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 117 "Net-(J16-PadT)") (pintype "passive") (tstamp 0d0c3d9c-0df0-4486-a568-7383b66f3f86))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp 94895e79-edd2-4bb6-a4a7-34b7e94545dd)
    (at 168.75 17.82)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Variable resistor")
    (property "ki_keywords" "R res resistor variable potentiometer rheostat")
    (path "/112d4e16-2eec-40ba-8650-5cb34528100b")
    (attr through_hole)
    (fp_text reference "RV16" (at 0.75 -3.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 292e4b6e-3062-46c6-99c2-cd5cdc4139f1)
    )
    (fp_text value "A100K (Glide)" (at 5.5 10.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1fbe4aec-4009-46d0-abc7-7a7d3ed3bebb)
    )
    (fp_text user "${REFERENCE}" (at 7.62 2.54) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43bc9bb0-e1b1-4800-a637-d439ba40742b)
    )
    (fp_line (start 0.88 -2.38) (end 5.6 -2.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2001629e-04f2-4277-9842-4c0fb8d339f1))
    (fp_line (start 0.88 -1.19) (end 0.88 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b63e9e3-1b4a-4ebe-a5a3-76cf239b46fd))
    (fp_line (start 0.88 1.71) (end 0.88 1.18)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 084b582e-4329-462d-b986-6e51a06c6f42))
    (fp_line (start 0.88 4.16) (end 0.88 3.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6d00ac74-9712-4047-b73d-db386bdbd563))
    (fp_line (start 0.88 7.37) (end 0.88 5.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 06780e37-6b87-4825-9159-86f32c45c3a1))
    (fp_line (start 0.88 7.37) (end 5.6 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eadfaef5-9670-477f-9f9f-9d9639658199))
    (fp_line (start 9.41 -2.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7a50e30-6383-496c-a2d6-c5601f30af25))
    (fp_line (start 9.41 7.37) (end 12.47 7.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0487b38-6c0b-4b38-8e4b-ea2a905179bb))
    (fp_line (start 12.47 7.37) (end 12.47 -2.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a64f6d8-ef7c-4dd3-bd94-779880e16458))
    (fp_line (start -1.15 -4.17) (end -1.15 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fe2b81ea-1bbe-4287-83c2-63e4e1b69ed1))
    (fp_line (start -1.15 9.17) (end 12.6 9.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3face92c-6189-407e-b3f3-6c0022ebb1a9))
    (fp_line (start 12.6 -4.17) (end -1.15 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4c0c937c-231c-42b7-9e36-a758970317c3))
    (fp_line (start 12.6 9.17) (end 12.6 -4.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ece966db-a2b4-442d-acb7-8b7382710d42))
    (fp_line (start 1 -2.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 866b80fa-06b7-4bb4-ae45-ac2d6d0da5c2))
    (fp_line (start 1 7.25) (end 1 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 28b50175-83b5-497c-bcbd-1f0dc3c03c3b))
    (fp_line (start 1 7.25) (end 12.35 7.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f1cc77da-1444-4c70-89fb-6d719be79307))
    (fp_line (start 12.35 7.25) (end 12.35 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41321e94-5302-43c1-94d6-2f672f765db6))
    (fp_circle (center 7.5 2.5) (end 7.5 -1)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2ae10706-5f61-405f-be1c-f836449a5f4a))
    (pad "" thru_hole circle (at 7.5 -2.3 90) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 63085d22-ee10-44d3-93ff-81d8367e89e6))
    (pad "" thru_hole circle (at 7.5 7.3 90) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 5f48325a-b0b6-44cc-ac4f-6dd764f8b8c0))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 106 "+12V") (pintype "passive") (tstamp 7257a102-6368-45c6-898b-6165ab14d18c))
    (pad "2" thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 108 "Net-(R40-Pad2)") (pintype "passive") (tstamp efcc078c-bb39-4ac7-9132-1ad6fefffdda))
    (pad "3" thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 1043464c-9f7c-46b0-a8af-5438a9d57c32))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp 9a257f04-c3cc-464f-b36d-38f925cf0691)
    (at 108.5 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/9eeeccaf-3c20-472a-a441-789923290aab")
    (attr through_hole)
    (fp_text reference "SW6" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e39fb7e6-978b-4356-ac9a-0888155beefc)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85cddc73-6609-4898-884d-84ba064b0d4d)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf1bcab4-0166-4aba-b7e2-7417d6f5d011)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8183939a-4dfe-479a-ba65-33264a9af49a))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee0efb1b-3f4d-415b-8d81-8d7917e16399))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa806a4c-cda5-424f-be40-dbf3594fb150))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85a5d8a4-a7ae-41d9-b35f-f2a125cc845f))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f45efe81-d19f-4b28-9e12-92af1fd9f3ff))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4e37e981-92ac-446a-8073-46bebed4dfda))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 90fae5cc-5bd4-4d3d-9bfd-82e55a8cec00))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30e6f1ae-46c5-4db7-802d-3f9ce26dc87b))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0884cd7a-5af3-40a3-b37c-bbb4d0d79e7e))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7bb328f6-95ab-4e70-9ec9-b55e81593129))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 21e5f9db-804f-4153-a4a2-a34f4f22539c))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82fd1884-3785-4feb-8295-625120480716))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 4fec4d35-7491-46f2-adf4-0ee41eed38ce))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D6-K)") (pinfunction "B") (pintype "passive") (tstamp cef2caeb-fc29-4684-86f2-933f5b572279))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 44819d17-f8b2-4784-bdca-353f21935460))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 9b3f41c4-9600-4dd6-90b3-4886aee82566)
    (at 100 40.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/effe28f5-455f-4bef-8beb-8eb5beec6907")
    (attr smd)
    (fp_text reference "R48" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2df5008f-eb3f-485c-836f-19bf59055c71)
    )
    (fp_text value "10" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb380b5f-f75b-421e-b24e-5920c1e02e65)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp dda5e52b-ac59-4ef8-9c15-8f5d442d6488)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a9969f0-4b2b-4bcc-bf38-957f34f56b46))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f5152b45-5329-438a-991c-5029b1f0d284))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 095ad872-273c-4a4e-a660-a22a1b47ea80))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 56be44e5-c798-4586-86ca-2307242c834c))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd8093d4-080d-425e-a546-b444caeab74e))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1e204d20-91ae-49b3-8c09-854c1b4579c5))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab2a96ec-b764-43ac-a76e-63a3f76c68f7))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3466a9c-f05c-4601-97d2-9ccf292e644f))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8482bae-9d6f-4862-8328-45ad7a645f9c))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93fe2476-7adb-43ca-82e2-e6517540cadd))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 86 "Net-(D37-K)") (pintype "passive") (tstamp e7fe307d-4196-4dae-8b1d-0ea8d0ca4476))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 115 "Net-(SW14-A)") (pintype "passive") (tstamp 1f845cb6-a690-4ce5-9c67-9e3d434d0afa))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp a25c1b63-3196-452f-9a31-e9dd284904cc)
    (at 168.55 106.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/7c10a238-6ecb-4fa2-a54b-78dbd0178b28")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.82 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c9533487-0ab8-4631-b7fb-2e31d5a05665)
    )
    (fp_text value "1k" (at 0 1.82 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b86322c9-e4ac-4f80-9527-356e5c52a831)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp a24b2895-0d0d-46b4-bc72-3d435d6de72b)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d5a7b79-0cc4-426f-8263-bc1ae1aed746))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3fafc2ac-8350-4595-b749-8c31a3dde218))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f57703a0-7580-49c5-afb7-60d16c03a3a9))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e4a7911a-0f6f-4e0e-8656-40b8b1ee197b))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0929f7c9-b313-492e-be4a-778283ac403d))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 83f43655-1bcf-4c19-9027-4ee012f0bc35))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6c0daced-12d4-45d1-8b77-910c99b8943e))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81392855-2a04-4afb-a2de-b3acc4d8416f))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f14e411-c2c7-44f3-980a-d3162ddc3560))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6bdf8d17-e3c2-46d3-a1b6-e9c5cb96a49f))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 89 "GATE_OUT") (pintype "passive") (tstamp 66a877f9-f17f-48dd-beb4-d9c577ba5883))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 79 "Net-(U2D--)") (pintype "passive") (tstamp db251d7f-a655-4556-841a-b8cb497ca370))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp a41a2412-d2be-4fb4-9b52-43c39abb7e1f)
    (at 44.783 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/ff2e40eb-de5f-471f-9413-ea88cd01eeb6")
    (attr through_hole)
    (fp_text reference "D21" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f6a6ab55-7568-4070-91e4-4bf4a235e782)
    )
    (fp_text value "STEP1" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f68ebdf4-7ecf-4222-990d-3640b642b274)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e89aa99-7358-4b32-a75b-ad6a0645b336)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e1101018-e625-4dac-8623-e9724fd1a966))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b36cee0e-6bfa-4fc2-a87b-6adf80e73c76))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dbaab655-3482-4e92-8d02-a08156a9e2d4))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 92b102c5-2263-4a1a-894c-ea88f114dc7d))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4445ba6e-f7e9-4a7b-a599-21377e4c8172))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b6f3df5-7bdd-4fb8-abb2-29da537a83c6))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 853d8476-74fc-4fa8-8593-0c994ad89785))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9cfa1772-7b33-4c43-a0f9-efca2041dc3d))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3617ced9-feca-40d4-bc04-eaba813f973a))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7416368f-2315-4a18-b312-19d6470786b8))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp feb6ec30-f5ac-44b5-a675-650f6f889d54))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37a7cb16-ea75-41c6-ad8b-898a783abf8c))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b3e4d19b-5e42-478e-a662-9bcd94062cdb))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5555139-3220-4ebf-ac1e-06c0495640f4))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c10df328-e1e0-43de-ae70-52bbc67443c9))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(D21-K)") (pinfunction "K") (pintype "passive") (tstamp a1d72500-059c-4d9e-b7c7-595814cc17cc))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp f78074a9-af86-4253-bb5f-df8341a85f59))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Alpha Rotary SR2511F 12-pos" (layer "F.Cu")
    (tstamp a90178d8-ba8e-4a12-a99e-ecd93612bac8)
    (at 77.5 28.25)
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "rotary switch with 12 positions")
    (property "ki_keywords" "rotary switch")
    (path "/b6e564d3-d51f-4544-90ff-bd8aa7ecef41")
    (fp_text reference "SW11" (at 0 -14.245) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfee37f7-5c39-4d3c-89ec-0fbfaf70f9db)
    )
    (fp_text value "SW_Rotary12" (at 0 14.245) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7e5be8b-35e3-48fd-9575-82a88d9eba1b)
    )
    (fp_arc (start -13.24 2.54) (mid -15.78 0) (end -13.24 -2.54)
      (stroke (width 0.2) (type default)) (layer "F.Cu") (tstamp 689d5cdb-48e6-439f-9d50-3a5615ecf8d8))
    (fp_arc (start 13.24 -2.54) (mid 15.78 0) (end 13.24 2.54)
      (stroke (width 0.2) (type default)) (layer "F.Cu") (tstamp 0d6b846d-e8f2-49ff-8765-ce588bf7589f))
    (fp_circle (center 0 0) (end 12.5 0)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp bac69b8d-4782-49e6-a4b9-512bddabd79c))
    (pad "1" thru_hole circle (at 10.142221 2.7176) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "1") (pintype "passive") (tstamp 3818c358-dc40-4d12-aabd-4f45d720cd91))
    (pad "2" thru_hole circle (at 7.424621 7.424621) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-A)") (pinfunction "2") (pintype "passive") (tstamp 89a19bb1-ed54-4b66-bbbd-3fe3ea59fd85))
    (pad "3" thru_hole circle (at 2.7176 10.142221) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "3") (pintype "passive") (tstamp 1a9abc70-1a9e-4ac7-b011-5ab54715437f))
    (pad "4" thru_hole circle (at -2.7176 10.142221) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-A)") (pinfunction "4") (pintype "passive") (tstamp 87f9544c-1581-4a66-9370-aa1ad48001dd))
    (pad "5" thru_hole circle (at -7.424621 7.424621) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D5-A)") (pinfunction "5") (pintype "passive") (tstamp 22784d06-c02e-4415-baf7-a98a5ce87385))
    (pad "6" thru_hole circle (at -10.142221 2.7176) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D6-A)") (pinfunction "6") (pintype "passive") (tstamp 8730eaf2-8c04-4e6e-9b0b-506472f7bac5))
    (pad "7" thru_hole circle (at -10.142221 -2.7176) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D7-A)") (pinfunction "7") (pintype "passive") (tstamp 17f960de-8964-457e-a43e-bed52d886294))
    (pad "8" thru_hole circle (at -7.424621 -7.424621) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D8-A)") (pinfunction "8") (pintype "passive") (tstamp 80c8f2ab-4ef1-4c09-9922-d4c566e6a4b0))
    (pad "9" thru_hole circle (at -2.7176 -10.142221) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D9-A)") (pinfunction "9") (pintype "passive") (tstamp aeec4591-6776-421d-ada6-fabd7953b954))
    (pad "10" thru_hole circle (at 2.7176 -10.142221) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D10-A)") (pinfunction "10") (pintype "passive") (tstamp 0ab1bf85-6459-4d86-9d83-441a15ecd403))
    (pad "11" thru_hole circle (at 7.424621 -7.424621) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(SW11-Pad11)") (pinfunction "11") (pintype "passive+no_connect") (tstamp c9abff52-be50-430d-acf4-6e12a71a9b28))
    (pad "12" thru_hole circle (at 10.142221 -2.7176) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(SW11-Pad12)") (pinfunction "12") (pintype "passive+no_connect") (tstamp 43a9356c-b6bf-4054-ac69-91c98502725a))
    (pad "13" thru_hole circle (at 5.75 0) (size 3 3) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 030ba767-c6df-419b-8c41-6a9ea5939452))
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp b8e8819c-5075-4526-a397-857ec5753500)
    (at 177 55.325 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (path "/9305d381-d2b8-4946-aa0e-82a67e8d620b")
    (attr through_hole)
    (fp_text reference "SW12" (at 0.013427 -3.1911 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c22f36fe-d6c0-4b2d-87f8-c7bde796cd76)
    )
    (fp_text value "CV RNG" (at 0 12.272578 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a463964a-af36-4aa7-bc91-9aefa4a345f0)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7534c0c8-c9ff-40b9-a279-c88ce891f9b8)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 50476ed0-dcf9-4a54-b881-2b33bf9a0417))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c35c6ea-89bf-4633-a1d1-d280943f28dd))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4835053e-543d-47b6-a8ef-f2f86ca46899))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2871ced6-f653-4f96-987f-fdd73c50b60c))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f0ba900-a44f-434b-815d-8428f076e172))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6f0960cb-f481-4b44-8ea6-a141fa527515))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb8525c4-319a-4684-a32b-391069783dac))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d80a2fd8-1901-4868-b056-8b164e3d078d))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f887d4ad-f7a4-45fa-8db0-1c2fefb01b20))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cabf494-59f0-451a-a5b8-caecf6c8a2b6))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e78adad0-9545-4bfe-b3a0-02592d85ea77))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 865d7d95-d795-42e2-a87c-01b740e4f693))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(SW12-A)") (pinfunction "A") (pintype "passive") (tstamp 54cafcb4-8e1a-40b7-9a58-9c5763679586))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 104 "SEQ_LV") (pinfunction "B") (pintype "passive") (tstamp adf2cad7-46be-44e6-809e-7c079a7c1135))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(SW12-C)") (pinfunction "C") (pintype "passive") (tstamp 710b0086-d48c-43f1-b9d4-addecc8c35e3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp c1969352-5d7e-487b-8459-00939bc40887)
    (at 161.75 24.35)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/78366797-0767-4f76-9b35-3a88ce7c3406")
    (attr through_hole)
    (fp_text reference "J16" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0e0836dd-e021-45d1-b608-cdefc7073a43)
    )
    (fp_text value "GLIDE IN" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d77aa580-6a94-4af6-8862-8e7e131d1f1d)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 7974a01f-1960-4c64-8b84-0542d9b40463)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a71f003-35b8-4209-9705-7bf89c4bda29)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e75f39c-8c79-4d2f-ab9f-e68a89bb38d3))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83be6405-45de-4bc9-80bc-c7dc62c0bcb1))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ec34077-f03b-45ff-bcbd-69d0332a1ba0))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3fb760e-1e09-47d0-be71-90ae1a3659e2))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp faa203f2-c56a-4510-b0db-03ecd3b284d8))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 150b6d46-3e76-4013-a875-dc70ad22c26f))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0aa4545-4a0a-4760-9293-159be2623173))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f2afcfd-2dff-4707-86c6-1f6e85d38070))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ccd090eb-3157-45ea-82e2-ef04d61f3a04))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b69e3c14-8bef-44d0-b6cd-5b4b047b3281))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 670ea280-8367-475e-95fa-ed998d6837b6))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3667ba81-d754-4bf8-bcd4-b6d1be927011))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 461dd5d1-0f90-42aa-8210-960953246327))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9d4eb74-2a94-42e2-8fce-cf125a682be2))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 80a921af-b6e9-417e-acb5-aa0e06eaf29b))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 316b6e8f-d6bd-4617-b766-715e0972be87))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f0ba7a97-fbd4-429e-ad5b-732cb73f2b74))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50214dd4-83c2-4280-84f8-5ee6f81631b6))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 494911db-e84a-4e95-9674-22f0feae3171))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp eb546d5c-3331-4928-9a29-3e5d7a854e44))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(J16-PadT)") (pintype "passive") (tstamp 854df489-e5b3-4108-9cbc-6ef45a4fb068))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 7321d688-ba59-4bb8-ab2d-ff30d28b510e))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp abdfe7a5-d3b1-444c-a327-6b0d3117983b) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 163.255141 30.83)
          (xy 163.23493 30.584171)
          (xy 163.174841 30.344945)
          (xy 163.076486 30.118744)
          (xy 162.942508 29.911645)
          (xy 162.776504 29.72921)
          (xy 162.582932 29.576336)
          (xy 162.366992 29.457131)
          (xy 162.134482 29.374794)
          (xy 161.891646 29.331539)
          (xy 161.645007 29.328525)
          (xy 161.401187 29.365835)
          (xy 161.166734 29.442466)
          (xy 160.947946 29.55636)
          (xy 160.750697 29.704458)
          (xy 160.580286 29.882784)
          (xy 160.441288 30.086548)
          (xy 160.337436 30.310278)
          (xy 160.271519 30.547965)
          (xy 160.245308 30.793226)
          (xy 160.259507 31.039475)
          (xy 160.313734 31.280099)
          (xy 160.406532 31.508634)
          (xy 160.535411 31.718945)
          (xy 160.696908 31.905382)
          (xy 160.886687 32.062939)
          (xy 161.09965 32.187385)
          (xy 161.330079 32.275377)
          (xy 161.571785 32.324553)
          (xy 161.818278 32.333592)
          (xy 162.062936 32.30225)
          (xy 162.299191 32.23137)
          (xy 162.520697 32.122856)
          (xy 162.721505 31.979621)
          (xy 162.896223 31.805512)
          (xy 163.040158 31.605205)
          (xy 163.149445 31.384079)
          (xy 163.221149 31.148074)
          (xy 163.253344 30.903526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp c204be8a-8258-419f-bbdb-7cc9eff5fb4f)
    (at 177.5 108.5)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/ce58c901-eaf7-4ea7-80d6-cc2774f56ea8")
    (attr through_hole)
    (fp_text reference "J7" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c4d3ce3f-7c92-45c2-b206-db4b1c12063a)
    )
    (fp_text value "CV OUT" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20dd176f-ca34-4b30-acbd-4ff201cfe85f)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 960c9259-aa87-4b32-ba33-e462d502fec6)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9a3dc341-4d90-4dbc-a8ed-f33e86ec2325)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a703e51e-2da6-4125-bc28-cfb9994d817b))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e199e050-c693-4a02-962b-4245e80e7a2b))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66e37a75-24b0-4c7d-a610-145d2de80b3d))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 08efe53d-5cac-4105-aa60-9ae0e29db5ae))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0558a70-a1ea-4e80-ac0b-e971bb6d4b58))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8222a6a7-abc0-46e4-ab22-a21aaa82cb70))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f65a1ef-5175-4206-a0a2-1e86b9e1e87b))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0c26fec-c835-45a2-b9eb-17aaab997071))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp bab26b73-78ed-41c4-9608-3a8d6f34f24f))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5772ed80-9acb-47af-8115-07f4a0ccbdbc))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1b486ec-a9f0-4254-a38a-a726d8bbbd76))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01eebfd4-1984-49e4-82fb-2977cac52012))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9405f3f7-816c-4057-99c1-3caa4b490b20))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3d53f3a-89a1-4ab2-89b5-b20a76a3c5e3))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 03c7cef0-5cb4-45db-ab60-997bacee4307))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1645fbc0-ff10-47af-92d4-304296848385))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8b2ca29-6c4c-476f-8735-c25b0d9481c4))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f1b14a8e-1a94-4906-966a-d58dd2ce95b0))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp d97bfcd7-e9fe-42a2-9442-a1d0e6e2c9b7))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 5e8477f6-b19c-4e4c-aaea-c6e4268ceda2))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 94 "CV_OUT") (pintype "passive") (tstamp edd10e7b-be5b-456a-bc68-21ac1a3e2b3d))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 113 "unconnected-(J7-PadTN)") (pintype "passive+no_connect") (tstamp ccfbf7ec-81eb-42e1-8a00-d86b7a3ca813))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 94ce9871-a1a2-4986-b56a-54fad50c2430) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 179.005141 114.98)
          (xy 178.98493 114.734171)
          (xy 178.924841 114.494945)
          (xy 178.826486 114.268744)
          (xy 178.692508 114.061645)
          (xy 178.526504 113.87921)
          (xy 178.332932 113.726336)
          (xy 178.116992 113.607131)
          (xy 177.884482 113.524794)
          (xy 177.641646 113.481539)
          (xy 177.395007 113.478525)
          (xy 177.151187 113.515835)
          (xy 176.916734 113.592466)
          (xy 176.697946 113.70636)
          (xy 176.500697 113.854458)
          (xy 176.330286 114.032784)
          (xy 176.191288 114.236548)
          (xy 176.087436 114.460278)
          (xy 176.021519 114.697965)
          (xy 175.995308 114.943226)
          (xy 176.009507 115.189475)
          (xy 176.063734 115.430099)
          (xy 176.156532 115.658634)
          (xy 176.285411 115.868945)
          (xy 176.446908 116.055382)
          (xy 176.636687 116.212939)
          (xy 176.84965 116.337385)
          (xy 177.080079 116.425377)
          (xy 177.321785 116.474553)
          (xy 177.568278 116.483592)
          (xy 177.812936 116.45225)
          (xy 178.049191 116.38137)
          (xy 178.270697 116.272856)
          (xy 178.471505 116.129621)
          (xy 178.646223 115.955512)
          (xy 178.790158 115.755205)
          (xy 178.899445 115.534079)
          (xy 178.971149 115.298074)
          (xy 179.003344 115.053526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp c255f42b-a83b-440e-803b-ca31e85b9de1)
    (at 132.283 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/72c232fa-c169-49a7-8e29-97297fe32301")
    (attr through_hole)
    (fp_text reference "D28" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19bc43ec-6cd0-449b-9440-9d8935a2d588)
    )
    (fp_text value "STEP8" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdf466da-35dd-4aa6-8900-7be53bcadb0b)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b3201b8-88e7-4100-9977-256bfa2c31e8)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bfddeaf6-3edd-45fb-a14d-2d0c2a17503d))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce2f81c8-a7a0-4964-bb75-db0904a05913))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 36143981-e4fa-4e1c-bf62-d91c628c65d9))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp abd5b476-e03d-4d71-bee8-6553db566cf3))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce0d9434-2505-4391-8734-352eb449f94a))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp db0e93d5-dc22-408b-9e90-d801d1863a12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 613368e2-1c94-46a0-8d37-a127af038251))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7ed3e33e-4442-4322-aac0-611f02627ad7))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e0c53528-1a99-490f-847d-bebf680e8d57))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c46aa247-64e6-4a27-850d-56c9cf32cb00))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4ee8c758-8fb2-474d-b0ee-24d743d948b5))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f05e0ba-7e10-4bf2-bd49-e0e48419d761))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b8799852-1488-416d-9a18-640bd0cbb64a))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3573c88a-ce2c-427f-b01f-0643a946aac5))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0509fb79-09f0-4d3d-9ece-887916de0880))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(D28-K)") (pinfunction "K") (pintype "passive") (tstamp a1bc409d-9589-4f4d-8f1d-539e42d95b19))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 572b763d-a8e9-4a4a-8b7b-6aa397737e83))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp c616b747-c6fe-4ab9-89c8-e3b3d03c2fd0)
    (at 96.053 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/f6167992-35a9-4e7f-98ca-e3c0979e35a5")
    (attr through_hole)
    (fp_text reference "RV5" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9faed22-e779-4d75-94d5-d0579fe030b9)
    )
    (fp_text value "Stp Lvl 5" (at 0 -1.94 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b976aa36-ca46-4dca-8bd7-b814bf433c29)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp def8796b-7b98-4dcb-a628-61093beac73a)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 44b6c31f-5591-47f3-9b95-4c4219449e43))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0226430d-85ca-48a8-b58a-43f624cb59da))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e279dc4-654a-4c06-958b-6938c045977b))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7bce5e7-4d50-4944-8375-61917c20b145))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 33dc28ec-d556-4607-b9dc-a8d821b14a18))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b87f5b3c-e1ce-4a6f-ac25-8ed65e4c2ece))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58e9d47f-4bf2-42b9-9e96-effc56ff180f))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 580a91ed-7e25-4ae1-8fb9-a16a6221dc22))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5abcc618-7c26-4a0a-8950-2d6d0706768c))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d1ceaad-1bd1-4768-ac84-454de4b44bb3))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4eef20c7-525f-4cca-8415-e46b6b19169a))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa830a6a-0296-4786-a192-1b218d1bf416))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc0d492d-2fd8-4acb-82b6-c83c6816df94))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 961d24ff-4362-4a70-99e0-791dbc536cb0))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f31c18f-8b84-4114-bad6-898b28ae2969))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9b5d1a8-271f-492a-9f0f-28c6db3930ba))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7fbc4a59-e09b-404f-abc9-7b108ec2a3a0))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b7043bc-5e27-442a-a402-68615a1a9232))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c4ff86e-ea80-48ed-8437-46eb448c6ff6))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4cee3857-02bb-4c34-8be7-de0f687ecaaa))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1918c063-a3eb-4fd8-a489-e7d69c538c43))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 478c5275-94fd-43b8-a9c3-fa91e4b2dd7c))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e58180c-aebc-4968-aae1-d8bd1f499b1a))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15427fe9-bb9c-4da3-a430-9fe4da3ecc92))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp becfed25-1c22-433c-9e1a-b42d3428e57d))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d5d5872-ad38-418a-925e-70c01dcb8f05))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d4b3b2b0-7f7d-4a06-a739-04946f9e9e21))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f926b42a-c2a4-4bac-8068-ec2ad41f1847))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D5-A)") (pinfunction "1") (pintype "passive") (tstamp 0c971680-4e9d-4c3c-9693-2c204a10580f))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D15-A)") (pinfunction "2") (pintype "passive") (tstamp fa95a7c1-9cf6-47ca-b9b9-7c8e1db17677))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 1f0e6002-9337-4a15-b8e1-64b586ef647e))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 202c0e9d-b73e-4017-8c83-502babf2620e))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp cbbae1ac-d5b3-4f41-be04-c66d6558c047)
    (at 121 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/6138155e-f95d-4aad-ae55-63ea51c95985")
    (attr through_hole)
    (fp_text reference "SW7" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 738d8b5c-e080-4efd-864d-e4e61533a1d9)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 23d7ec92-05cd-4036-8d55-6faefb0c01d6)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 669b6a22-8bdf-4c06-a4a3-82e2a4fb58d8)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 39d76f1c-317b-4585-9f61-1b934df079ba))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4bc41af-0b9f-49ce-8a5a-50a7cf36b198))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eaec5aec-d692-4c11-8f43-11a6d490df44))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 48ecc078-43e7-4cdd-96bb-0d77c56f4039))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 29708364-d743-4671-b8b1-59e675d29351))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 140e541d-ce3b-4ff6-9e78-181f2247a19a))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 609d46e7-789c-4690-a5fa-27fb864badde))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7df885c4-d87c-4d91-a9f1-9e4bc7850df9))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1118e1ec-d088-4175-9cc8-f471bc0d11ef))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4815395c-d720-4617-9dc9-9061ba2af530))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1bc819b-ae7e-4eb0-a747-62f9a62163df))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff4e98d0-e8af-4c93-9499-73b619766922))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 0eae0d42-fc85-4e6b-9116-e1f10d59637c))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D7-K)") (pinfunction "B") (pintype "passive") (tstamp a3266a12-0b47-40eb-a0b9-0584b0ce6b1d))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 064735c3-de6d-46bd-90be-00fd0728e460))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp cd641c0c-8fe0-46ea-9844-431f2665eb2f)
    (at 57.283 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/e5cc5492-f90b-4dd3-b491-707a83d07a19")
    (attr through_hole)
    (fp_text reference "D22" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1db92c3a-bdde-4481-8299-b2ff2a61d5a5)
    )
    (fp_text value "STEP2" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3ab7e05-42a0-4824-bab8-815c485c7820)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b0f08d6-0849-4e0f-a4d1-4b286545957b)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b955a5c1-a317-43ab-8fb1-4e7d704bff7d))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 68168a63-aaf1-4f0a-b76e-d80ffd0328d3))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a59895a2-c069-46e6-a4dc-30d5bae31b5c))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2224549a-d7c6-4216-bf2c-a160531ecb1b))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81472d26-3617-4b35-b1d1-60a66a1b92fa))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec4dee49-865a-4981-915f-c91b11205a80))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 20945f8f-fe98-4bed-83d2-344d27191c53))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 77a0311f-42e2-4009-aa33-c3b600575477))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3b1f9d17-ac9f-4bd1-b86b-18acfd636f05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8b5a1bb0-3889-4df3-8acd-a49add37da53))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6065ab3-d4a0-4ec1-8ff0-6603fa34bc89))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8fb6e41-b8b5-410c-b9b8-85926cc08ad0))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4b3c92a-25a4-4194-be4f-94930cc5385e))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93ddbab2-4cb9-4d31-b88a-a8779737cebe))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff63b12a-cb67-4a4a-82be-568b282ffef6))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D22-K)") (pinfunction "K") (pintype "passive") (tstamp 7a05b5b6-e345-46ef-b334-e8c51ea3aa61))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 15a71a69-d9f4-4075-ad43-d6ee7b41a416))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp cfce936d-df44-46e6-8ce6-c82adcdd2e3e)
    (at 63 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/c1eb7edc-8cd1-43f6-8838-a6a39ee23eef")
    (attr smd)
    (fp_text reference "D2" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8e1149b-3f30-4315-a2d5-0e24ea562a14)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9cffda0-9f41-4117-93b1-e134e47c1b80)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14871bc2-1a81-4989-b710-be87e7c24b8c)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9e99a022-1b6f-47d5-8dde-f29454ab5f54))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa5924b6-9ef5-40a9-b847-26f190106153))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 310082cb-8292-44fc-b649-a50b2c7dba8d))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b8dd2739-8abb-423d-93f2-b76257505821))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5fb6f19-b652-4c48-a351-699cfe7f7202))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7afb0596-c686-48d6-bc08-0364f94d3577))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 11f99640-5a7d-415d-958b-0b8cb7a75a36))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4bc2db99-34ea-4d4e-abe8-1dc43598c144))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8e86f37-b36c-4fb0-8bf6-4f67925ac954))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e759a64-9e91-482e-a0f0-1095680cbbb0))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19e21787-0175-44d2-a356-05f743bab2b4))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48b69428-3082-41cd-a6cd-5cf9f445ba6f))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db5f1ca4-82ac-4c8c-aee2-c7ecf70e6121))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 073e460f-99a1-41f5-97a8-ed9385d13f99))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp da2dc432-1c6b-4379-9e11-96077ffd8a64))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7bc5fdb5-af0d-4e0f-acf1-143acb0c3dc7))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4af67aae-f383-4b9c-9ffd-5bfa3d7c47b3))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee36bed6-c417-4f93-a2ab-0f9848d113e3))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(D2-K)") (pinfunction "K") (pintype "passive") (tstamp f882a43f-ef2b-4b99-a0cc-0011d6492d3d))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "Net-(D2-A)") (pinfunction "A") (pintype "passive") (tstamp 9880ea06-bb5e-4338-b7dc-b537d652af65))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp d0eaa78d-c8ec-4f4d-abbd-ac0756afd2b3)
    (at 121.053 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/e32c6856-42fb-463a-a463-39781323f9c3")
    (attr through_hole)
    (fp_text reference "RV7" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1a2924c-834f-4da4-b92c-1bdfb6fdeaaf)
    )
    (fp_text value "Stp Lvl 7" (at 0 -2.12 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f5fe7a83-50ca-46f5-8fbc-1cb7dde4e015)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7b1f3a9-a119-4b44-a738-3025368783fb)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f3d26d9-fbf1-46b5-80e8-c462e32c3724))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9fb3b11d-c3ab-4aa8-a362-a4e7a8e34b99))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf32862e-71f3-4d93-9a55-fa8ac8c42055))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b93e9501-7c36-4fe2-a91c-9089707ead56))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d856340-05af-4f64-b3b3-b02c1842885d))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ecb5ac1-0674-4751-9851-30d0b9bd4a3b))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af9134e1-483f-4bc5-8bbb-58c485516f58))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d9f4eef6-a927-40b8-95af-c3fbad4a9d2d))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3c247ad9-9632-4c17-9921-ee7a34e930f2))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9237b906-7b16-4bb6-aea4-fa9f292ac0de))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56401588-29df-41ca-9ac8-377bf6248282))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0c14de9-62e8-4cc0-abd3-6815fe5b8eef))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fcf39bda-7001-40cf-8c91-6408a43b59a7))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f06a9351-6166-4680-9623-44b60848f790))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a8341ab0-426d-490d-a9ef-4519b8dd9480))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9fbedb2-5eed-4577-bb4d-ac825171e914))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce843b30-7f75-4956-9a32-6aec84d45887))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8331790d-b8b5-4419-87e5-a4d24e27fce5))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71b6d87b-ec00-43a2-a673-0d8804d9d49a))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 781eb297-d44c-4645-b90f-e5f08ec70989))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad751142-9bd8-4bd0-8e74-7bd02a0e0f6d))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0afa7c67-000c-472f-9b77-dd14f7208eeb))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d49b7348-d809-4582-b507-e0158d60a8d3))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 94b59474-0550-4834-b00d-1879694721e6))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92196f5f-004e-4f4d-8bd6-01a72fa6b878))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e886b4d6-1b38-40af-911c-b0de5bf299ad))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 10d60baa-f450-4dd1-a3e9-66373137910b))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 48032bd2-cb4e-4070-afae-3268d8197a89))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D7-A)") (pinfunction "1") (pintype "passive") (tstamp f09a88d4-e18b-4e49-9e0d-538b4d637d43))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D17-A)") (pinfunction "2") (pintype "passive") (tstamp 6d397df1-93f5-41fe-af34-1f5a4b4e6081))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp ef8d5d0b-59b1-4709-b539-06da24e2eeae))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 5ba1baa1-bbce-4ce4-99e7-42979e893656))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp d3a5b36a-8362-4c3d-9bb6-2fa17b4a4225)
    (at 177.5 91.5)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/432f910e-dc82-4075-8857-172d7b00b6cb")
    (attr through_hole)
    (fp_text reference "J4" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a186ac1-2b55-425f-901e-11eabb0b58dc)
    )
    (fp_text value "GATE OUT" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0aa0dacc-cf94-48aa-891d-7104eabbaf33)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 87261cab-67e0-4def-8766-cc42980db49a)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 184fdf17-0b39-417c-b5be-4084109793fc)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 02e052a8-ba3d-4032-8562-ab591f68d7ba))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f3d2cb16-3239-41f3-8cef-b4c5e3e7186e))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8cbe9743-9862-4768-8dfa-95c0d15c6079))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f56a89b1-0a09-4d18-958d-b23d3fd6b34e))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f91e6297-1485-4c2b-b09f-6d5e4039fda3))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b82eafbd-8d84-4dc2-a582-8294f311c46a))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c64a167d-fc10-40d0-8fdb-066bb1809a5f))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 30ed978f-3241-4842-83d1-bdff100f45e8))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp adffb031-a597-4e6a-9d83-3262f368a183))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 157e9a9d-e0e8-4b51-9a87-d5e01bc37d94))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 199e5a48-76ad-40f1-8766-97c958f61a24))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 681cfadb-5de1-4f5e-a74e-c35fe43130ac))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f022a6d-a0d9-4c0c-86f5-829baadbce52))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77e6d55c-7358-41e5-a76d-72f521297e21))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc97a31a-b8bd-4ef1-bd4d-8327ed6e751f))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 80e2adce-cd8e-4c9b-8292-f76f2f354b36))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 192c1559-a6b7-4355-b172-329228fbf37c))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 971bb029-b419-46c4-9655-74caae5705db))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp a83e5876-1907-4384-bcb7-bcf195d5131b))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 27b695d0-17cd-4a07-8879-8be6c51cc5d8))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 89 "GATE_OUT") (pintype "passive") (tstamp ff1395d9-6f40-447a-af4b-1afedace23e5))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(J4-PadTN)") (pintype "passive") (tstamp 0ae27a94-2f34-45ce-8df5-e5360a9d8535))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp ea55d978-d00b-4de2-b353-4f5c0f67628d) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 179.005141 97.98)
          (xy 178.98493 97.734171)
          (xy 178.924841 97.494945)
          (xy 178.826486 97.268744)
          (xy 178.692508 97.061645)
          (xy 178.526504 96.87921)
          (xy 178.332932 96.726336)
          (xy 178.116992 96.607131)
          (xy 177.884482 96.524794)
          (xy 177.641646 96.481539)
          (xy 177.395007 96.478525)
          (xy 177.151187 96.515835)
          (xy 176.916734 96.592466)
          (xy 176.697946 96.70636)
          (xy 176.500697 96.854458)
          (xy 176.330286 97.032784)
          (xy 176.191288 97.236548)
          (xy 176.087436 97.460278)
          (xy 176.021519 97.697965)
          (xy 175.995308 97.943226)
          (xy 176.009507 98.189475)
          (xy 176.063734 98.430099)
          (xy 176.156532 98.658634)
          (xy 176.285411 98.868945)
          (xy 176.446908 99.055382)
          (xy 176.636687 99.212939)
          (xy 176.84965 99.337385)
          (xy 177.080079 99.425377)
          (xy 177.321785 99.474553)
          (xy 177.568278 99.483592)
          (xy 177.812936 99.45225)
          (xy 178.049191 99.38137)
          (xy 178.270697 99.272856)
          (xy 178.471505 99.129621)
          (xy 178.646223 98.955512)
          (xy 178.790158 98.755205)
          (xy 178.899445 98.534079)
          (xy 178.971149 98.298074)
          (xy 179.003344 98.053526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp d4bbca42-e2ce-4544-a1e9-236a758fc41f)
    (at 158.5 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/7dda46dc-84a6-4969-8074-f6adc742ce52")
    (attr through_hole)
    (fp_text reference "SW10" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43b8304e-17c2-488f-a02d-39da608c51d0)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f8052dc6-911b-48e3-9aea-7445afd61e1a)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9f520cf1-bf82-4f4a-92a7-84b909cd47a6)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b275def2-7d21-4d98-a873-10cf7ca99c2c))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7bcf49a6-04db-4ce3-bea6-a73a67c5a305))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8559aae5-915e-4366-a000-ad86607a62f3))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 29d21f28-44ba-4ccd-bfca-21cd69ebd88c))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3c8df005-dc5f-40b1-86ee-2008edd25d92))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1f586429-1bf7-4a69-84ef-ab6671550c33))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 602fa9f2-12e6-461e-9fc4-4910fce46f8d))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 27cea2af-8f6c-4566-8b67-831b08e1a720))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b03536a8-2f9e-4c58-a7fb-599f9363d15c))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c6e0afe-61a5-48a2-ae2e-2a148918225a))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06e72c30-90fa-4ffb-b1b6-a66ef12e6753))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a448fa48-f8ce-44cf-8979-0a01694b7ff3))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 5418a947-2815-4b77-978e-d970640a47ed))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(D10-K)") (pinfunction "B") (pintype "passive") (tstamp 0295bad9-5385-4b35-b4a4-3ed287898d18))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp f125d765-7274-4346-9107-ed7e179c9380))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tstamp db507a2d-fd7b-4067-b336-d1fdd44ccdab)
    (at 150.053 37.671374)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/edc26770-57fc-4994-963e-5b99ff469e6d")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.82) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a2b020b1-7b12-4396-8c48-12b3e0610266)
    )
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0bca669a-1f42-481a-a5ee-b515727f7810)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 8dfb19a6-ae7b-4a53-b53e-a911ce00988c)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea877f93-2f66-4bb0-89fe-ac27591b5db5))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46c8be47-b92b-4c1b-8522-5251996fd25c))
    (fp_line (start -2.45 -1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aaca7f6c-bfa3-4617-a2f0-2852518761ca))
    (fp_line (start -2.45 1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9d8eaa8a-1873-42c4-b03e-3718b98a1efa))
    (fp_line (start 2.45 -1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76145f0b-2617-448e-8044-e04ce754e34e))
    (fp_line (start 2.45 1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b65c2929-f22d-41e1-a6a6-101ac4b3a99b))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8fa0c3a6-d0da-4645-9ba7-acbbffca2cb8))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60326e9b-76ec-4355-9224-0ce86ac5cbe2))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0574c9f2-cab2-4bb1-a9b7-eebfbbdce5b1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e89162d-f42f-40e0-8f7e-a304b4bdeccd))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 106 "+12V") (pintype "passive") (tstamp c874e5c5-1634-4dc9-b03c-038dccf31bf7))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 34 "Net-(D21-A)") (pintype "passive") (tstamp 414d09d1-f760-4c4b-aea0-00d32f50a839))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp dc573af7-2217-4eac-b3bf-67718f6558a2)
    (at 25.4 60.405 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/d89f63bf-5bfe-4dd1-bb0d-f76fceb6ee8a")
    (attr through_hole)
    (fp_text reference "SW15" (at 0.013427 -3.1911 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7a1bb007-1d3d-49f5-b906-b71ca3ab6e69)
    )
    (fp_text value "Once/Cont" (at 0 12.272578 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba2468a0-2dcf-406c-8769-9da924d701dd)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f72a5f6d-5711-4214-a06e-f7d3c117c1a6)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1d7446ed-ab16-4df0-ac52-62a15ca1447a))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7dada07a-4750-453f-a961-fef1ca2be3ba))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35ccab9b-f3ca-4568-969e-b03fbf516d65))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d0bec646-f5f8-4ecd-ba51-a4fff2adf71d))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aeae11fb-69ac-4a48-b7c8-1b8afb49b52b))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7fbe2904-99f8-4ca6-bece-697cd7b0bde4))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e15489f3-a121-4176-995f-066c6462970e))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 48ff34be-b544-4241-b334-907db4f5f7f1))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 11f2a92d-13d1-4d89-9a50-0a84d9f0e2c2))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 092fbfa1-0139-4dc3-abe8-646ab6f9fc91))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e494b5b6-fc1e-473c-9245-6f0a72a58283))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a8dbaa6-d55b-48c6-886b-ad2b0a303110))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 116 "CASC_NORM") (pinfunction "A") (pintype "passive") (tstamp 8e3ac7a8-2c3e-4794-a46a-3e14ee780494))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 83 "RESET_IN") (pinfunction "B") (pintype "passive") (tstamp d668a954-4414-4d10-9f22-d5b01bfbc040))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 734f47b0-deca-4adb-bb6e-951d730c967f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp dcfd4596-d33a-47dd-9e25-1416cb8fcc33)
    (at 75.5 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/0ddf3f0a-d098-4a75-80da-49bb2dc26a1b")
    (attr smd)
    (fp_text reference "D3" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04936a4c-9e50-4292-a568-35ed392326d9)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56b174ec-6d35-4d76-84d8-e4105ca7e398)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp eff5f4cd-0d26-4550-96b9-ea13d5651750)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5382164-487f-4926-989f-994a080c5a19))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d55f57ea-2b55-414d-a84e-0b5af85a9497))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ece2fc2e-5598-4dec-ae4a-a5d615ade9d7))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 364e13da-2835-4f7f-9023-64cb3a651054))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25c5dab0-4548-494f-beca-48608ad86aa4))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd7d9db7-347c-4c36-93bc-b10346d0a9a9))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a33af14-0a59-4e16-9a19-ebc64525f15a))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4385987d-f53d-4e56-8dd7-4e6d7aa59ba9))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af8e33ee-1bec-4a98-bac6-adf4327d02db))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 58112176-3560-4dda-ba21-f8b36091c7cd))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 044febf5-7043-4989-be33-605d74cb5538))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66608391-f847-4089-ae6c-f4c13e82e680))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8511bd40-cd84-4000-842c-4d16aa6ac2ab))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 539bcdce-7268-45ac-97a4-e45f4b49246e))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c2b487c-4c7f-4cb3-8ac7-0a5f9da21205))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b53496c-7cac-4161-a53c-639382a40462))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cc87ab82-b6b7-4554-98f6-aee2acd4cfbd))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cfe8a75d-9a48-4b8e-896e-df4d74800e66))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "Net-(D3-K)") (pinfunction "K") (pintype "passive") (tstamp b225a78c-b089-4ac4-965b-984a83b33be5))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(D3-A)") (pinfunction "A") (pintype "passive") (tstamp c374e5f5-b59d-496f-9957-1d48aadf91ff))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp dd3454e9-8fa4-41cc-b872-898b4ef338e9)
    (at 158.553 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/30edd45b-b170-4f89-923b-026487de14bc")
    (attr through_hole)
    (fp_text reference "RV10" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e49641cc-674c-4dea-9d22-e8c86fc80951)
    )
    (fp_text value "Stp Lvl 10" (at 0.078626 -1.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ea57aac-0f07-4cbd-a8ae-a22d5509ccf6)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 71778453-0606-4c72-8bec-ca285ea1f925)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2bcb410-a744-42db-8dd7-6b9165f9f7cb))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 689114b3-48e1-4163-8d8b-8a3a2811f3f6))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89ee7ab2-ff36-4a58-bf67-ca512543f99d))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5220ce4e-4773-43db-bef7-4a8dbe1e2603))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp abc89f11-e8ec-407c-b5b1-e782e1cc3656))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2195677-0187-4438-8b3e-de3c82e69da3))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c466011-5204-416c-9106-b6f93d1b99d8))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb82b70c-bae4-452a-b634-b653ce27f7c3))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e9155ad-8a0c-4601-88e9-73f94756623b))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6a6fe145-302b-458c-b128-9836d244067a))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7192a6a5-e39d-4c7f-aa44-c2e35ba3561e))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a996362-d863-4a70-bd13-59fb47c2b8f6))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8754ef9e-e571-4a97-8c38-c1a4b665ce8a))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1a6f8ca-2e5e-4dc1-b697-4ff69feb510e))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 762fb6bd-ed57-432d-8c97-381c3d671b49))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f608aad4-0875-48c9-ba83-12b122c01610))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7542216f-3bcb-4483-828d-122ee94fda7c))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b128b4fc-7b11-4c85-ac84-7bac5e55dfce))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f014c6f2-b383-42de-974a-1c633fee79d2))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9e20c56-2478-4a36-abfd-a54cba9867cd))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68e14ce1-8c69-4c15-ac18-c96000ca42ec))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0eae5e03-83d3-404e-acc0-7867581c2d6b))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a66d0d08-0e30-43b0-9716-dacedbb91250))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3a5af22b-f7f6-44a1-a127-35ce41cd57f3))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57403a30-52e2-4dca-8449-137a7ea65000))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0ffb20a-60e8-46d7-a272-69528399478f))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a09a8b8d-b8c5-4c2a-8be5-a96d25b2d869))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c16fb302-fb0c-42f7-bba6-5251406a7204))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D10-A)") (pinfunction "1") (pintype "passive") (tstamp be942f77-218f-459e-90ba-4eeac3e580cd))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(D20-A)") (pinfunction "2") (pintype "passive") (tstamp c4dc1731-8d53-4d8e-925d-96e8a7c2acdc))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 82d04cb6-b519-4b1a-8b44-ae9876021136))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 407ca0d0-fab7-4c99-9cbe-9b8ad516a8d1))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp dfd18163-acb6-4656-800d-2a6023cb6af7)
    (at 33.02 60.405 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/358df635-958d-4c16-bec0-273c1553b3be")
    (attr through_hole)
    (fp_text reference "SW14" (at 0.013427 -3.1911 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba3b9f52-18c5-4d46-996b-18c00a697f32)
    )
    (fp_text value "Run/Stop" (at 0 12.272578 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dce04788-bf86-4c29-9345-2f7716577517)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a3ad349-e9a8-417d-8df2-3ba6e5094225)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c9dd78e-ae6c-4eba-a648-1d2d9b27c772))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bec09ee-6ebf-4153-9431-b1c55a89f726))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01ce56c0-8207-4bbf-b310-2fd3cb0b67e7))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba94a1cc-fcdd-4f40-a561-f76b8d3ccbfe))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 031921c0-8aa1-4d4b-b541-c967b9ae03c9))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6f3828e9-9540-4fa5-9fd8-164894033edb))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c4b53463-aedc-442b-b48f-79a1af24c552))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6bba1d4a-77ea-4463-b0bc-fa11059d827b))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38624dbe-14d4-42ec-b600-63f2330befaa))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 13d81984-14de-4d45-8c00-2b5b6611ae21))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1599b38a-7e69-4a69-a324-f37f7fdc9c59))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ef76ec4-a6e3-40ca-bf90-334cb442ee50))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 115 "Net-(SW14-A)") (pinfunction "A") (pintype "passive") (tstamp 96367ed6-8fb7-4b14-9eab-a81789be5a50))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(SW14-B)") (pinfunction "B") (pintype "passive") (tstamp a0aa7b33-1181-42c6-a729-2ebe372796f8))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 7e6aef62-a5c2-42bb-bef7-b7865e8fbfd3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp e0078af8-230c-4f44-b9bf-5f8488cb9ff5)
    (at 146.053 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/141ae23b-0c7e-4a00-bcd3-58431a3e9784")
    (attr through_hole)
    (fp_text reference "RV9" (at 0 2.34 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c2f9be0-0999-4ec1-8695-d0fdac5f2f18)
    )
    (fp_text value "Stp Lvl 9" (at -0.161374 -1.17 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 75dc8fc0-f65a-487f-8c5d-9e402b24ffef)
    )
    (fp_text user "${REFERENCE}" (at 0 2.34 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 018efe0a-965e-4512-838b-13d3e56c4c08)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bdd7ea93-9fce-4f8e-830f-158b7ae059b3))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7b78c8b-99a5-48b2-928f-226ef0be190b))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e0a18fe-8f1f-48bf-b551-cfbfe5574aac))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c26c641b-75dd-4775-9e20-423eaffec1bc))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c46e0f9d-d8a0-4869-96d3-13f083cb8158))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 64e88566-1f57-49f9-934c-aecdf9122719))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf67503c-9ff6-43a3-b8eb-d2ca4101a35f))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e03b4e3-0ff7-41ac-ab21-a0a68aab152d))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f601142-1b77-4b51-8053-d03bd25b2316))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c00a06e-0dfa-4990-8b20-a48686bb6b75))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ecb2cd7-f964-42cb-887e-99b86bce0a7e))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ea4e0f5-bdab-458b-a0da-ec442ecfdadd))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e555d654-bfd1-4a8d-a644-081b2d9fdab9))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 76bc2689-5dab-4753-878b-42b289f00eab))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0402c15c-d1b4-4555-92c3-a19c5e4a258a))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1ee7e0a-3c0d-4ca3-8edb-476cbe3e482c))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40e8b696-fd03-4334-930f-501501bd5fb8))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41c9d289-da8e-4c95-bbe8-83d940403bcf))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43ee7a19-1f87-494f-ad56-5bb0e8a65d1c))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5d5c9cd5-9bee-482c-9536-d0ea22eb8d6d))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3feca8e1-0cc1-4353-b1bc-c11786df285d))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 69117eae-d14d-4fd8-a6f0-1e5ab10295da))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9a15d3c9-8673-4db8-8ac3-94f835204493))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 47efa1e2-0cb3-48c0-b4cb-92da4c490881))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5088fe04-3e3c-4e39-98c2-c47a0726a79c))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6839b5ca-1617-4b9b-aede-a79f4cc6f286))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18bce09f-1e7b-4786-8389-fdfcc626019e))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 66a1343a-53b7-41c6-8c6e-5d75c8fec37d))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D9-A)") (pinfunction "1") (pintype "passive") (tstamp 5067cfa0-c31b-4ea0-ab4c-fdd66e8d0a00))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D19-A)") (pinfunction "2") (pintype "passive") (tstamp cec2852d-fff6-42a9-a062-14e55cb7c22d))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp e7d2a6f4-abea-489d-a651-20b9412a3e2d))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 2c151789-04e9-4958-b2fb-306455cd627a))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp e5961717-cc66-4c0e-a75a-7d68eb6d427a)
    (at 26.25 67.97)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/70cf3b7f-0059-424b-ac15-a1ffac78cd9f")
    (attr through_hole)
    (fp_text reference "J18" (at -3.5 -0.22 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 434a3fd1-6490-4359-83f1-0674520e5f98)
    )
    (fp_text value "PAUSE CV IN" (at 3.75 4.78 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f5afa580-3fc2-4a52-9778-aa0d643ad4c1)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp bb1dac2a-1aba-4e4d-ab75-70330ecdf764)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5e9aa96-6dde-4f6c-aa35-87da393bb33e)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 31be8f13-7d59-46c1-8b5c-d313f0d91fbe))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4c723bc-9d49-42a2-859c-1c9bd80fab68))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cbfd6904-cfe3-404c-bf68-eb01aa7a935d))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f64d479a-3ff1-43c0-8b10-aaa0f0c5624a))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 379787c7-0e30-441c-ac20-81bed3dcabd7))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16fdada8-3083-4c65-a734-169db0f22754))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f762da7-8cf3-448d-8cdf-ff7d10247363))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 932dddd3-975d-4abc-a973-212609be5ae9))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp c9c2ade8-733f-4ab0-b5ca-408c61f03a26))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9ce124cd-89f6-46bd-ad5d-91be282582fd))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55a2638e-7ce8-44a8-b35d-967140f605e1))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f597b85-a3e1-424b-871b-a38d6c35bc22))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a5c69c66-7873-41c7-bf6d-74420084b2d8))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1af1194a-62c3-4dcc-9304-9b07ce045b04))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea37ee26-bbd5-401e-9c09-24d31ceb1bb3))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 29b2d7df-092c-4834-91cb-fc333a55d23a))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e4218bd-abcd-4f63-902b-dbb08d5325c3))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6143a863-e1b0-4a46-8a99-0465747f1d67))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 0efc1a1f-b4a0-444f-bfbb-1a42440e6f94))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 7ab94fa6-80e7-4ae3-88bc-ceb4226a5dcd))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(D34-K)") (pintype "passive") (tstamp deb7a6eb-7f18-4cca-88ff-d8b4e037c20d))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp ace31f88-47f3-489c-8ae9-aadc3047db72))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 91015a47-6a99-4b90-a893-485f8b4a80e8) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 27.755141 74.45)
          (xy 27.73493 74.204171)
          (xy 27.674841 73.964945)
          (xy 27.576486 73.738744)
          (xy 27.442508 73.531645)
          (xy 27.276504 73.34921)
          (xy 27.082932 73.196336)
          (xy 26.866992 73.077131)
          (xy 26.634482 72.994794)
          (xy 26.391646 72.951539)
          (xy 26.145007 72.948525)
          (xy 25.901187 72.985835)
          (xy 25.666734 73.062466)
          (xy 25.447946 73.17636)
          (xy 25.250697 73.324458)
          (xy 25.080286 73.502784)
          (xy 24.941288 73.706548)
          (xy 24.837436 73.930278)
          (xy 24.771519 74.167965)
          (xy 24.745308 74.413226)
          (xy 24.759507 74.659475)
          (xy 24.813734 74.900099)
          (xy 24.906532 75.128634)
          (xy 25.035411 75.338945)
          (xy 25.196908 75.525382)
          (xy 25.386687 75.682939)
          (xy 25.59965 75.807385)
          (xy 25.830079 75.895377)
          (xy 26.071785 75.944553)
          (xy 26.318278 75.953592)
          (xy 26.562936 75.92225)
          (xy 26.799191 75.85137)
          (xy 27.020697 75.742856)
          (xy 27.221505 75.599621)
          (xy 27.396223 75.425512)
          (xy 27.540158 75.225205)
          (xy 27.649445 75.004079)
          (xy 27.721149 74.768074)
          (xy 27.753344 74.523526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp e68d5c35-d597-4cc2-93a1-8a52e0707469)
    (at 37.75 38 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/74f88b89-0e58-4337-99f4-05e52e182a58")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.65 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 29ad75f5-a23b-4124-b177-e125e452a8e6)
    )
    (fp_text value "10K*" (at 0 1.65 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 679b1828-1a41-4b38-89d5-ef03dda1736c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp bce56a00-220b-4566-b56c-72f562e816d3)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2a236e23-31e6-44dc-bdaf-10d48cc3bc5c))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0a20938-643a-4435-a879-52ae2415731e))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 651e3fe5-cf09-40e2-ad04-62c78926f5e4))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f7eb1d25-1472-4ca7-b5e2-4e2b193f49de))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78871e57-3119-41ff-95b2-45d67b278990))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bdcb07c9-74fe-4ce0-adfe-b3ec85a94117))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 903d409d-fae8-44c9-88a8-3fe141a2ddd5))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c34f106-8b7c-4796-b03c-e80e1a4b4081))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87c73448-d24d-49fa-8863-2c29c63cdc51))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc614738-cef5-4764-b6f1-e382c55a043b))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 93 "Net-(R43-Pad1)") (pintype "passive") (tstamp a27527dd-c15d-4831-9aeb-853c92055145))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 106 "+12V") (pintype "passive") (tstamp 012319a3-9105-4af2-86fc-3f869b229a44))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles" (layer "F.Cu")
    (tstamp e97cd623-d681-4cfe-ab4f-78e95c61e462)
    (at 177.5 75.85)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (path "/3a61bb28-c157-43fc-8817-19939f91613c")
    (attr through_hole)
    (fp_text reference "J5" (at -4.03 1.08 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6ab29eb-236c-4378-a96e-7afeafe2f9b6)
    )
    (fp_text value "CLOCK OUT" (at 0 5 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 35dfc22b-9c43-4ecf-8279-20d25c9e051a)
    )
    (fp_text user "KEEPOUT" (at 0 6.48) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 6f3b5b6a-8097-4460-aa7a-20ddc6054244)
    )
    (fp_text user "${REFERENCE}" (at 0 8 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c406d87a-7dce-4f70-864a-a29f74c59a63)
    )
    (fp_line (start -4.5 1.98) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83331cd2-a462-44a0-931b-0b3da9b4bbac))
    (fp_line (start -1.23 -1.17) (end -1.23 -0.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 145472f1-84d1-4920-ab0f-ee1d4f623fe2))
    (fp_line (start -1.23 -1.17) (end -0.37 -1.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 97951394-f921-4f83-860c-9b65ac5434aa))
    (fp_line (start -0.8 12.48) (end -4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f24da9f2-8f8b-4fc3-add6-e67e5d8af7fd))
    (fp_line (start -0.72 1.98) (end -4.5 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cb1de558-56a4-4b6f-aa37-9bf07f09f24f))
    (fp_line (start 4.5 1.98) (end 0.72 1.98)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb921b5c-66e4-4561-9483-575c1b8bc47d))
    (fp_line (start 4.5 1.98) (end 4.5 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eab0efba-7704-42b5-bec2-0b77b86ce0cd))
    (fp_line (start 4.5 12.48) (end 0.8 12.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4413ab4b-1cbc-47a2-8d15-7bdd4eb99f4f))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 2e829e26-9cc0-49a7-ae88-22e61f09703f))
    (fp_line (start -5 12.98) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 775aff55-8f3f-4df8-b315-9b1855c5736b))
    (fp_line (start 5 -1.42) (end -5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 59c0d033-0f13-458d-a9ba-a3526348b7cb))
    (fp_line (start 5 12.98) (end -5 12.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c8e90ee-347d-47c9-a0f2-0f3ad6009f47))
    (fp_line (start 5 12.98) (end 5 -1.42)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81c57d3d-3545-4a05-aae3-68211b1eaf72))
    (fp_line (start -4.5 12.48) (end -4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2a22667-6a57-4de3-8788-c2e8d4d29daf))
    (fp_line (start 0 0) (end 0 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22c6fb16-e846-4c6c-bb54-9ab2ebe95bcc))
    (fp_line (start 4.5 2.03) (end -4.5 2.03)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15613b8e-3bff-4cf3-a26b-d2316f22d97e))
    (fp_line (start 4.5 12.48) (end -4.5 12.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 115f8f27-63ab-4589-a862-314b8d7cc340))
    (fp_line (start 4.5 12.48) (end 4.5 2.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aca5be16-03f3-4045-8f22-2cd0c95092a0))
    (fp_circle (center 0 6.48) (end 1.8 6.48)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp a21ad95b-bf00-43b0-9c53-d86722e464aa))
    (pad "S" thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 6627bbca-ec86-418c-b8ef-f12355c2aab3))
    (pad "T" thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 91 "CLK_OUT") (pintype "passive") (tstamp 58751ab9-e90e-40f7-981d-9df44a2cea82))
    (pad "TN" thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(J5-PadTN)") (pintype "passive+no_connect") (tstamp 064d296c-5ada-4ed5-a8b3-27bac181ff3e))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 57ef3e89-58f5-442e-9ade-a4cd20ec2077) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 179.005141 82.33)
          (xy 178.98493 82.084171)
          (xy 178.924841 81.844945)
          (xy 178.826486 81.618744)
          (xy 178.692508 81.411645)
          (xy 178.526504 81.22921)
          (xy 178.332932 81.076336)
          (xy 178.116992 80.957131)
          (xy 177.884482 80.874794)
          (xy 177.641646 80.831539)
          (xy 177.395007 80.828525)
          (xy 177.151187 80.865835)
          (xy 176.916734 80.942466)
          (xy 176.697946 81.05636)
          (xy 176.500697 81.204458)
          (xy 176.330286 81.382784)
          (xy 176.191288 81.586548)
          (xy 176.087436 81.810278)
          (xy 176.021519 82.047965)
          (xy 175.995308 82.293226)
          (xy 176.009507 82.539475)
          (xy 176.063734 82.780099)
          (xy 176.156532 83.008634)
          (xy 176.285411 83.218945)
          (xy 176.446908 83.405382)
          (xy 176.636687 83.562939)
          (xy 176.84965 83.687385)
          (xy 177.080079 83.775377)
          (xy 177.321785 83.824553)
          (xy 177.568278 83.833592)
          (xy 177.812936 83.80225)
          (xy 178.049191 83.73137)
          (xy 178.270697 83.622856)
          (xy 178.471505 83.479621)
          (xy 178.646223 83.305512)
          (xy 178.790158 83.105205)
          (xy 178.899445 82.884079)
          (xy 178.971149 82.648074)
          (xy 179.003344 82.403526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp ebb3b4e9-aade-4e2f-9749-71bc9e09db65)
    (at 133.5 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/09ff6b9d-9f05-4967-8c64-24881a24bb90")
    (attr through_hole)
    (fp_text reference "SW8" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 93409ed6-164c-4938-8364-79a434de2c62)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e97533f4-db8d-4889-ae2c-a9cfeee36084)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b78a73dd-cd00-46fa-83c0-6f495b825a63)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca8968df-d3c5-401a-981c-29fb28f3e68f))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 297835c2-9b23-4bfc-9629-e8896769d495))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 673e706b-34f4-4d45-970d-88aa0f92a2eb))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9925392-f422-45e6-b072-d056292a9d0d))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e04fc9ba-bba3-479e-9092-ff04fa21c015))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2b2f4b32-6235-405c-a8b1-e87d33085d3c))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bd9517f7-33bc-4661-b9ef-7e8eef67f161))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0cba1e98-23e9-4bb5-b509-2c9bbe3523c6))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb4fb985-196c-4a5a-8375-02044e865ea2))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c259aed-0893-4123-930b-1e1562037001))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a834bf5b-56b6-445d-981a-b30460629d4b))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 71810270-fe32-4878-96bc-f5e4c220ac4a))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 5f149d8b-d108-4577-92b9-aa426c3c216d))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D8-K)") (pinfunction "B") (pintype "passive") (tstamp 818b5560-fbd1-4007-ba79-f34a5a2e529c))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 86fbbd84-e6a2-4419-82f4-0a30beb86774))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:SLIDE_POT_0547" locked (layer "F.Cu")
    (tstamp ed4eadb1-7205-4c68-b193-ab0d212f3b9a)
    (at 71.053 78.921374 -90)
    (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 45.0mm")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer with a mounting pin")
    (property "ki_keywords" "resistor variable")
    (path "/6dba6fdf-0ee7-44f1-865c-f3b990443d33")
    (attr through_hole)
    (fp_text reference "RV3" (at -0.031374 2.22 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ce11d51-f1ca-4a3f-88a7-237e48fed990)
    )
    (fp_text value "Stp Lvl 3" (at 0.038626 -2.01 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07802ccf-a058-4db5-9077-b8afebdbbc37)
    )
    (fp_text user "${REFERENCE}" (at -0.091374 2.22 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9b720e8b-5106-4c4b-9427-45060f5aaf22)
    )
    (fp_line (start -30.4 1) (end -30.4 2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78956f08-4a20-42e9-b96c-1a9df2ed7e04))
    (fp_line (start -30.4 2) (end -29.9 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 95ed9f71-5326-4640-adb4-7a696e385524))
    (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f4d7edd-cd40-472b-a34c-34293ffcf849))
    (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 256d3714-1fad-438b-984d-a847b7545986))
    (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 998138ce-3268-4c0d-9e3c-c153fe24a4ae))
    (fp_line (start -30.12 4.15) (end 30.12 4.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a975bb46-6907-4e93-8b20-0b2039e4028d))
    (fp_line (start -29.9 1.5) (end -30.4 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 838c5c71-b4f6-4398-8fe5-6d5dd6c75747))
    (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb6b94f3-a831-4d80-a213-f45677bb6116))
    (fp_line (start -22.5 -1.5) (end -22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6bab364b-381d-451b-aa43-6d0fc46d4141))
    (fp_line (start -22.5 0) (end -21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4faf93df-c51c-4538-9598-03240474070b))
    (fp_line (start -22.5 0) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d2241f25-7427-48f9-a5c2-d2788f2f3b59))
    (fp_line (start -21.75 -0.75) (end -22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc32bb4e-00ee-4fad-a03d-a50521a81726))
    (fp_line (start 21.75 -0.75) (end 22.5 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e09e4abe-3cf3-4570-bf20-17ae3a5807a7))
    (fp_line (start 22.5 -1.5) (end 22.5 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00a407e4-aba8-4429-a87b-3fc6def7bd32))
    (fp_line (start 22.5 0) (end 21.75 0.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4cf5641c-92b9-482a-8576-745ca8b9e7e0))
    (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56cfe858-afd8-4938-9032-84ce476a2623))
    (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f01e0093-ce0e-4fce-9077-2d3e0ea50307))
    (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a57f58e7-5be7-43a4-bf81-3977153cbbad))
    (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 989252a0-dd4d-4648-8889-82effadcf41a))
    (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d48cc47f-c806-4098-85d8-896e8f9f8e8f))
    (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8a875764-ea85-4c65-a063-d6f1e35b30c7))
    (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eed68e12-18fb-4a7a-a966-756892569baf))
    (fp_line (start -30 -3.004122) (end -29.25 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91f8e2f1-241f-4535-89c7-3dfadd2ad8a3))
    (fp_line (start -30 4.054121) (end -30 -3.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 068df562-e64d-4d15-b74b-4e9d05a60c41))
    (fp_line (start -27 -4.004122) (end 30 -4.004122)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c958e918-6de4-44df-818a-2dbae24f430d))
    (fp_line (start 30 -4.004122) (end 30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18a552c9-ce80-4419-8344-b077df796d69))
    (fp_line (start 30 4.054121) (end -30 4.054121)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2602f20a-c42c-442f-82e4-9dfa8e1bceaf))
    (fp_circle (center 28 0) (end 29 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp b4e65f4c-cdf8-4a53-823c-668fddd3b51c))
    (pad "1" thru_hole rect locked (at -25.171374 1.5 270) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "1") (pintype "passive") (tstamp 281274e7-a426-477f-946a-b0760c57e053))
    (pad "2" thru_hole circle locked (at -25.171374 -1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(D13-A)") (pinfunction "2") (pintype "passive") (tstamp d546018b-804f-4abb-b534-7dd2a67acfa0))
    (pad "3" thru_hole circle locked (at 25.5 1.5 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 37176437-bbe8-426c-9ed9-3d676376d686))
    (pad "MP" thru_hole circle locked (at -28.12 -4.195879 270) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp e6e52cf1-14fc-4a6a-ae21-a5c7ca9e93c3))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp ef768e81-8723-41ab-9d35-17a39428a3e3)
    (at 96 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/e17e3783-c43d-43d6-8ef1-f6d8fa49fcb4")
    (attr through_hole)
    (fp_text reference "SW5" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d045429c-2fc6-4267-ad0d-faa8f512dbce)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d592d88-7312-4da4-9c75-65e84b7c37d7)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a5ddb4b3-6fdc-41e2-88b8-0c45e1288295)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 824c8702-5fed-4959-b788-810da3828d08))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 970aa85f-bdc3-4918-a1dd-91f96da1ca8c))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de06d515-5d21-4621-b053-3ddb71f4edc4))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bcd3e4b9-b730-4add-8e2f-3dd878d6d681))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 792266bb-e9dd-4480-8eb4-7ea44b878013))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp da5f64b3-e723-4507-b895-4cb69736d571))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 52b62856-f768-4f7c-85f4-f181b5827d66))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 89360851-0e4a-43ce-b605-c52dcb675806))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4605e753-64cc-435a-96e1-ee8dad4e7e3a))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bee3dea0-ba3e-46aa-b351-e7ef99c79baf))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12b83d74-bee1-42e3-96bb-d835fca2dfef))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8298ab2-5185-4483-8e38-83b9a737444b))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 876580c7-fc46-49d9-9b73-22245a91e1f2))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D5-K)") (pinfunction "B") (pintype "passive") (tstamp 95255205-3824-45a3-9635-1c4fe4059c22))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 3a67611e-fdfb-4b19-be74-1cba914b557c))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Pushbutton Switch (PBS105)" (layer "F.Cu")
    (tstamp f5976b18-9a7d-448c-9309-c87c887d7f12)
    (at 29.75 39 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (path "/29519676-a70b-4873-a763-fa053ddd3e3d")
    (attr through_hole)
    (fp_text reference "SW13" (at 0.001344 -6.171835 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7769b90a-cdb1-4f40-82fc-b39c012f215a)
    )
    (fp_text value "Step" (at 0 5.761533 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f2007dbe-6800-4e9b-bc4c-e4e428944bab)
    )
    (fp_text user "${REFERENCE}" (at 0.014406 7.115765) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f1efba2-04d2-4f2a-957d-979229a11ad2)
    )
    (fp_circle (center 0 0) (end 4.85 0)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 7641cd80-0abb-4ffc-90fc-1570f36250a8))
    (fp_circle (center 0 0) (end 5 0)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 87c1f880-29fc-4417-94b5-97a08f928bdf))
    (fp_circle (center 0 0) (end 4.75 0)
      (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp c9d83567-cfd7-44ef-8669-d22bf2926167))
    (pad "1" thru_hole oval (at 0 -1.75 180) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(R43-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 90905f16-4968-4601-ae8e-f5aee6f80827))
    (pad "2" thru_hole oval (at 0 1.75 180) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(SW14-B)") (pinfunction "2") (pintype "passive") (tstamp 2d8d3f73-65bb-4f11-b991-3365ebc20db8))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp f604886c-d122-4d86-80ae-5805d44f0a6a)
    (at 136.7125 27 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/e2c4323d-1dee-4722-8abc-8aedc3b63988")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b4bb7771-6b62-46a8-b672-26e8a4bdf3ff)
    )
    (fp_text value ".1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d2c4f3c3-65dd-486d-be03-471a923863f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 9dd51074-cd3d-4fe8-a189-6798543e77cb)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ba1b140-1e0e-4a8f-a279-4e0982e5ed1a))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56b1e171-9c7f-4532-a6c5-42006f15a7e5))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea4c593e-f4c6-4268-8096-eae80f486d44))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4b1f3c8c-9a11-40e8-9d3a-d5a4112ee4f7))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f09216b3-9a77-4c7c-b014-78777deb66b1))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb8137ee-d458-4911-b373-0c838c0e70f2))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd55b522-40f0-4bbd-902c-0c218c00642f))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86aba876-a6d4-4424-81fb-7e88dd50fcd2))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5cd7ba60-ef59-478e-9fe0-7c0afdece3bd))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 357fefe6-c7ad-4aed-b453-526bad2bc344))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 106 "+12V") (pintype "passive") (tstamp fcd163f3-9e08-4df9-869a-6303aa2063bb))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp c0bc7b65-1c26-4fc5-89b1-8abc946c40d8))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tstamp f62ae841-a9bb-43d4-89d8-c0de1a79beb1)
    (at 125.5 114.75 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/1214b6fc-2612-472b-a0d6-6cddbef01b99")
    (attr smd)
    (fp_text reference "D7" (at 0 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e4430e5-60e1-4f27-b8cc-4228d618ccc7)
    )
    (fp_text value "1N4148" (at 0 2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2f7d349-3ebb-44dd-8fae-0524707d63ea)
    )
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6fe92d0-a87b-4e71-af38-4216e3b50f7d)
    )
    (fp_line (start -2.66 -1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46d05fbd-ab18-42ce-a375-3ed89debdcd8))
    (fp_line (start -2.66 1.11) (end 1.75 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 266cd858-9119-4d22-92fb-234b18824c46))
    (fp_line (start 1.75 -1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 639b1567-0af5-436c-a05d-77b9d132445b))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6d44d9d7-1afb-4358-93ed-4ccdf1243210))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30da27b5-9d11-4dc9-bfc5-679eee861437))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9dffcd7-e671-4a8d-9702-de0e0eb96856))
    (fp_line (start 2.65 1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 07afdfea-649d-4f23-ba70-d345b95cfdbf))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5daba66c-6bb0-4680-b0c6-4f3d5020a14d))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 08d92db7-daca-40a0-9bef-2f962f31f8e9))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be54d282-5aba-45cf-8681-89ede4b4f03d))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cc436a96-8969-4d17-abd8-a84aaaad2be8))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 83633b89-1496-4fc7-a548-32ef664bd40e))
    (fp_line (start -0.35 0) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 94252d34-bb02-452d-96e7-a972360814e7))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7265fafe-4aea-4b57-a539-e83d6f873ebd))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 95afee21-34c2-4d55-a75c-c76ce57db5b2))
    (fp_line (start 0.25 0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0cebf39f-10e4-41fc-ab16-166b1600a6dc))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb1f2f05-e527-45a9-9b73-707024164c14))
    (fp_line (start 1.65 0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 217b4bf6-8cec-468d-8f8d-92d1e275761a))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 15 "Net-(D7-K)") (pinfunction "K") (pintype "passive") (tstamp 3b8683ae-c72d-4386-bf78-a77af6a43ad3))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "Net-(D7-A)") (pinfunction "A") (pintype "passive") (tstamp 65156471-db31-45fa-b975-eec4c4d925ea))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Mini SPDT (3 pin)" (layer "F.Cu")
    (tstamp fce8a21d-229c-4b57-9e95-ef2da6d38056)
    (at 71 121.05 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/e88a8d6c-c334-4a04-8bd6-549d5d38bd47")
    (attr through_hole)
    (fp_text reference "SW3" (at 4.013427 3.3089) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2c4e4bdc-5481-4d8d-933c-72b283dc39e6)
    )
    (fp_text value "SW_SPDT" (at 0 12.272578) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 958ab3b7-5620-4bb5-8cf7-ea00dd048d56)
    )
    (fp_text user "${REFERENCE}" (at 0 13.811214) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8b039540-b9f0-42a8-bd45-a74785cb691d)
    )
    (fp_line (start -1.605 -2.105) (end -1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 211ad985-e9a5-4a34-83d7-13a42eb60ee9))
    (fp_line (start -1.605 -2.105) (end 1.605 -2.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 90f17f22-e575-4c50-a35f-7e5f681f693f))
    (fp_line (start -1.605 11.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1ba5ebd-5403-4838-a396-e11f794248d6))
    (fp_line (start 1.605 -2.105) (end 1.605 11.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 026d6b92-d344-4667-88e1-ca80c17fef41))
    (fp_line (start -1.8 -2.3) (end -1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f916fa48-8081-4b44-8c1f-507fce94bf2a))
    (fp_line (start -1.8 11.35) (end 1.8 11.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4ba56045-7f66-4bc6-a567-f50d350311ee))
    (fp_line (start 1.8 -2.3) (end -1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6492c547-252c-4682-9b2a-e8af37e9f607))
    (fp_line (start 1.8 11.35) (end 1.8 -2.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f879466-2707-49f2-a319-6ed4a4bffa2a))
    (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70133e83-0c5d-45a1-8d9c-50b927dedce4))
    (fp_line (start -1.545 11.045) (end -1.545 -2.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b0df6e6-e867-4f47-9b35-5cff1291fc1c))
    (fp_line (start 1.545 -2.045) (end 1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43aafec6-ebe2-464a-ae0b-fe80934235a0))
    (fp_line (start 1.545 11.045) (end -1.545 11.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6716de5e-fd14-4d60-99e9-9f841431334e))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(SW1-A)") (pinfunction "A") (pintype "passive") (tstamp 97a49788-7593-4615-9d4b-8463c7fedd34))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D3-K)") (pinfunction "B") (pintype "passive") (tstamp beac765f-8703-41db-b370-995ad06a517d))
    (pad "3" thru_hole circle (at 0 9 180) (size 2.75 2.75) (drill 2) (layers "*.Cu" "*.Mask") (tstamp ca397ff9-a7c9-4b9a-bdf1-fdb1e7ee41d1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp fffecc72-9f45-4587-98cd-7cc0b8dd5e1c)
    (at 119.783 46.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Infrared LED , 3mm LED package")
    (property "ki_keywords" "opto IR LED")
    (path "/ef055a2e-3125-4c24-8d1e-3d9072abf9be")
    (attr through_hole)
    (fp_text reference "D27" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 501a8058-9583-4307-9463-a082969b9e2a)
    )
    (fp_text value "STEP7" (at 0 4.87 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 72ececc1-c1c1-44d2-84d3-70db84364c22)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3416f74-82ff-4043-9914-c733a56bf193)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b158ab40-b26d-40ce-ba01-06825c1bebdc))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c499983-7aba-4381-91c6-e94bc3f5e506))
    (fp_line (start -1.33 1.27) (end -1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88327c5d-1ec3-43c2-abee-0dbb8054cd8f))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c920d954-a4d0-484e-b6dc-6475516837ab))
    (fp_line (start -1.33 3.87) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 87fc518e-dc4a-4c5c-87ac-2de34dd2642f))
    (fp_line (start 1.33 1.27) (end 1.33 3.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3d15d79-4f3a-49fd-abae-cede4450d9a4))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 46d71b80-fc85-4818-b07b-99708b25653d))
    (fp_line (start -1.8 4.35) (end 1.8 4.35)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b9f9daef-a01b-41f2-a043-b90b7e2644b3))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ce3012e2-5026-4cb0-b363-f6808e1f3aba))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e59f77eb-87d1-4aba-8e7e-ebcca5dac896))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a07917af-e0ed-4f1e-bc5f-4b36f4ef7b0e))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 362fadbf-71c2-49a4-82c0-d5e2f7f656dc))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7af9dfc7-f1d1-4318-90ff-56ac625e3fcc))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc7fa424-5500-4134-a990-c7952ff5b6c8))
    (fp_line (start 1.27 3.81) (end -1.27 3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0621d9c7-e0f8-49dc-b92d-aa99ed071607))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(D27-K)") (pinfunction "K") (pintype "passive") (tstamp b5032494-8f13-47cd-8fbe-b887cbe393b1))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D21-A)") (pinfunction "A") (pintype "passive") (tstamp 47ca9cf2-2eb1-4946-9323-9b02220bbf12))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 08f855e3-a0f9-46b3-b808-d99c03791982)
    (at 64.77 41.91 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/4f7109cc-20a9-4f15-87ed-b0d0ef1c7d10")
    (attr smd)
    (fp_text reference "D33" (at 0 2) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 01f80351-6078-4ba4-9bf4-2dcef0fb5fd6)
    )
    (fp_text value "1N4148" (at 0 -2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8281a954-0377-4a54-9927-f84030c38d40)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e09610c2-c1a8-414f-b59b-3b9383808dfd)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d6d5f1bd-9353-49f9-826d-482e0c76797c))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp af6a8e9a-c673-463a-bf50-ca5b5dfde9bd))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0a7d4fef-d2e7-42ae-ba54-b6ce2108c2a9))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 147ff928-3693-4b90-8cae-897aab4f0833))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 22a69bf7-23e7-4ed1-8760-40e53021ee4c))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 212b30e0-846c-4864-a6db-fdd4cea96a36))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp be67ca22-99dc-402e-9108-47fcfccfcb44))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp acd6854d-233d-457b-81a1-46706d8afb16))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8872230b-20f6-40cb-8242-790bd7b5d24d))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5433b68a-3ebe-4cc7-9e24-b2d58823930d))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eb2fd261-8a78-41ce-97ab-1ca2c1183c41))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d682e701-15c9-4945-9c15-af9defccd1bf))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eae3dc2b-6e09-4802-8322-d778d74a3bc5))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 27beb90b-630b-47e0-8524-baa6151270c0))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2e887172-aaa8-4850-9bc9-81f18d5442d1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d2e2fef2-30b1-461b-bb9c-c639f0af52ea))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ba713963-a564-4ec5-8fc4-2e1896d09a47))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ce374990-ca15-4e10-b3b4-56b78af39dba))
    (pad "1" smd roundrect (at -1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 46 "Net-(D33-K)") (pinfunction "K") (pintype "passive") (tstamp ee4664b7-2727-4261-9531-52eaa8ac8be7))
    (pad "2" smd roundrect (at 1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 84 "CLK_IN") (pinfunction "A") (pintype "passive") (tstamp 0cf9408d-e459-48c5-8673-ff87504efbb5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp 13cd98e5-55bc-477f-a1c7-00c5ac01dd28)
    (at 135 84.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/475c3e3b-02f7-4558-bd70-eea2025d4a9a")
    (attr smd)
    (fp_text reference "C13" (at 0 1.68) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cf212312-93e3-4f51-bfd2-be178282774a)
    )
    (fp_text value "10nF" (at 0 -1.68) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2be65ee3-2a79-41ca-a28a-e3a959ef0828)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 088fe2aa-56e3-49b9-b716-161867c6c0b8)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9dfbef42-9798-4ecb-a751-a8e7d17628e1))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23f64217-e8a9-46b6-bb44-4eda09f7d465))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 21d189d3-4dd1-469f-870b-9a66a242c42d))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c6f25e9-dfbc-4442-a7ed-bb7761aa704f))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 02fe250e-b38e-474c-81e5-9e6117912fac))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3c0a8fa2-64a7-4b91-8960-2a54561e2377))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 49a53286-4ee3-45a6-ac96-af4b2eea551c))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 80330264-194a-405a-bc54-359d1abef816))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c6e97948-c04a-4202-8e45-52341fb77941))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d13a3107-5d16-425a-8b25-e09eb8080432))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 75 "Net-(Q12-C)") (pintype "passive") (tstamp b51fb2f3-454c-4318-a441-61aeaaf18b73))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 95 "Net-(U3B-+)") (pintype "passive") (tstamp ecfd8c95-c519-42f6-a5e6-70a65260964d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 162a3dea-1f51-41e6-8eea-7960fcf2511a)
    (at 63.5 32.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/58c54839-a6c7-4470-bda0-d6e51071cbaf")
    (attr smd)
    (fp_text reference "R8" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9049cf85-e5c9-4f80-8cbd-5398c367eb7d)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 60856054-cb6f-46e8-a1b1-4d6419172036)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 8248b5b4-336d-4367-9d93-3a9fc7ef16be)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 14dffdab-9af3-4ea0-927d-eb7d33ffa011))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d8f6d4bd-55b4-4974-81d8-28ef19b291a3))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp edfa5637-6dcb-4525-b7e1-03819727d052))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6131c218-5520-41ff-87c6-cf75e9cdb9c2))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2b6b4ea9-c3a2-4c61-b5ec-e4c46980de09))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a6410d2b-9f78-43a7-ae9b-afbe56e2c71d))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 51eeaded-bfdb-4265-9a78-3ead5a957500))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cf476f70-cbd2-4478-822a-d40644c7595d))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a3403180-9959-4c96-bcce-fdf1263ba1d5))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9446904d-b05b-4903-8609-e3511fea6557))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 88 "Net-(SW1-A)") (pintype "passive") (tstamp c0a51eec-9c68-4f20-b05e-4d11369573f1))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 73 "Net-(D37-A)") (pintype "passive") (tstamp d5b8b71c-6269-47b0-a301-71a16cb01459))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp 1648de1a-56b6-4ead-a365-152756613dbe)
    (at 120.495 40 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/5304680c-3375-4198-a13b-f42d362a48ad")
    (attr through_hole)
    (fp_text reference "RV12" (at 0 2.33 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 90579809-c98d-40e5-925c-96ecb0e99a4f)
    )
    (fp_text value "Adj 2.5V" (at 0 -7.41 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f7123104-8b51-4ff3-8483-f822afb137b1)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8f489dd9-5fd7-44c9-9cdf-02e4d68b869e)
    )
    (fp_line (start -1.33 -6.41) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b666068b-ba9c-4742-a218-874d816bf5fa))
    (fp_line (start -1.33 -1.27) (end -1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d3d7f645-aedf-4578-ae08-64207a965558))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 428f08d7-f135-41e6-89f1-c2766a8fcea5))
    (fp_line (start -1.33 0) (end -1.33 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 75ff2c66-2242-4b7a-9375-fd0f250fdbf7))
    (fp_line (start -1.33 1.33) (end 0 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da9cb525-ceca-49ac-9b95-12df8e090d82))
    (fp_line (start 1.33 -1.27) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8d1f751b-deef-4530-8034-1244be9d624c))
    (fp_line (start -1.8 -6.85) (end 1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp af65f66e-9094-40c2-86eb-c664dd69f81a))
    (fp_line (start -1.8 1.8) (end -1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1d803f50-0026-46af-9427-5cd8fb7387cb))
    (fp_line (start 1.8 -6.85) (end 1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bd117e67-ed0b-445b-a493-45c069532837))
    (fp_line (start 1.8 1.8) (end -1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e8911d8c-f55a-4f58-870c-1fbb064b49e2))
    (fp_line (start -1.27 -6.35) (end -1.27 0.635)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9334a6bc-088e-4239-8f97-b12e01555607))
    (fp_line (start -1.27 0.635) (end -0.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fba8ffe0-6a3b-4924-88dd-35803948817f))
    (fp_line (start -0.635 1.27) (end 1.27 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c9fd4f83-29a4-46da-97a8-5a1aca0229a4))
    (fp_line (start 1.27 -6.35) (end -1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3c4cd5f8-8d25-4716-a407-acdc7e1d5654))
    (fp_line (start 1.27 1.27) (end 1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4aa49de9-c50c-4d3f-8836-38f4b77fa340))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "1") (pintype "passive") (tstamp 4cd59bb8-3063-435b-9153-72f0ce678f9b))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "2") (pintype "passive") (tstamp 757e38e5-5379-4a0f-84fb-99a5a79bdc36))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(R31-Pad1)") (pinfunction "3") (pintype "passive") (tstamp d171664f-98ec-4dbe-9fe1-b7e7aa632a90))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "B.Cu")
    (tstamp 1a83c681-d10e-41d4-b261-5846e927842d)
    (at 138 32 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/670d908c-9b0d-4cdd-9acb-b7fb4827e770")
    (attr through_hole)
    (fp_text reference "C3" (at 1 3.75) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 49c527ef-c1f2-41c1-b688-d6f63642b65c)
    )
    (fp_text value "47uF" (at 1 -3.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7b4ec382-f739-41e3-aa27-5ab87d34592b)
    )
    (fp_text user "${REFERENCE}" (at 1 0) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1c8a0ebf-fa59-48c1-9765-19ab206e74d3)
    )
    (fp_line (start -1.804775 1.475) (end -1.304775 1.475)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4fa4bd95-b3bf-42a8-b5f1-9eebb6ab1986))
    (fp_line (start -1.554775 1.725) (end -1.554775 1.225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e879cabf-f29a-484e-830f-17ac0424d981))
    (fp_line (start 1 -1.04) (end 1 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6c203b77-3b1d-4e31-b9bd-a0230fd2811f))
    (fp_line (start 1 2.58) (end 1 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eaaa0522-5a10-4d23-8b2d-02dc47dadbb1))
    (fp_line (start 1.04 -1.04) (end 1.04 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b9514e39-21fe-45ae-bc9b-63a2759d184f))
    (fp_line (start 1.04 2.58) (end 1.04 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bed45d03-6d72-40bd-ae5b-a6e2e4a6051a))
    (fp_line (start 1.08 -1.04) (end 1.08 -2.579)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2570adbf-5fb6-4f48-9330-03dfea23a70a))
    (fp_line (start 1.08 2.579) (end 1.08 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 24df3dd0-df5e-41fb-a31a-6c6c8634c6f3))
    (fp_line (start 1.12 -1.04) (end 1.12 -2.578)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a90ef953-a871-4824-9562-94738ab865d7))
    (fp_line (start 1.12 2.578) (end 1.12 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2d79a8df-81c1-48e9-91e9-99aaa2d844df))
    (fp_line (start 1.16 -1.04) (end 1.16 -2.576)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2034f5aa-5ae0-40af-8450-e18aa7368c0c))
    (fp_line (start 1.16 2.576) (end 1.16 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6d7ecad4-4e20-484c-b55f-fc0c44484112))
    (fp_line (start 1.2 -1.04) (end 1.2 -2.573)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1b6e8414-fc14-4a9b-ab3a-7e8829ef70f0))
    (fp_line (start 1.2 2.573) (end 1.2 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d80bdede-aa0f-4835-bd7e-eab49cf0cd2a))
    (fp_line (start 1.24 -1.04) (end 1.24 -2.569)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9c87f1e0-4bb4-4a76-b9d7-08ad26464e71))
    (fp_line (start 1.24 2.569) (end 1.24 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 75752737-2818-489c-838f-155623360ca0))
    (fp_line (start 1.28 -1.04) (end 1.28 -2.565)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 29f1eb5c-1331-4ab2-b4cb-d2728745a94a))
    (fp_line (start 1.28 2.565) (end 1.28 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ac14a2f0-7f88-4d7b-ac21-de22008761ab))
    (fp_line (start 1.32 -1.04) (end 1.32 -2.561)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a0b6e257-3e12-43bc-95ec-c7caa807ce5a))
    (fp_line (start 1.32 2.561) (end 1.32 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6fa54fed-26fa-4d7e-b233-b8ad5ffdb1cc))
    (fp_line (start 1.36 -1.04) (end 1.36 -2.556)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8c7f509e-59b9-4724-9f73-156725ce4c28))
    (fp_line (start 1.36 2.556) (end 1.36 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 44e7da97-6323-4baf-9bd1-490bd2598c91))
    (fp_line (start 1.4 -1.04) (end 1.4 -2.55)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp abb770c7-b0d4-45d7-915b-b4986396d36b))
    (fp_line (start 1.4 2.55) (end 1.4 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 025789fd-330e-4675-b5f2-d911d1229d8c))
    (fp_line (start 1.44 -1.04) (end 1.44 -2.543)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4f1745f6-0574-4bea-bbd7-343f8e8c1e1a))
    (fp_line (start 1.44 2.543) (end 1.44 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0f5fd710-2736-4462-a0be-28a55a30e479))
    (fp_line (start 1.48 -1.04) (end 1.48 -2.536)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 259f3b42-24ed-4b7b-a4b6-128e016e3cde))
    (fp_line (start 1.48 2.536) (end 1.48 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eda8b643-7134-49f7-923c-56803eced2fb))
    (fp_line (start 1.52 -1.04) (end 1.52 -2.528)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d688d814-d655-48db-974f-e05b19163340))
    (fp_line (start 1.52 2.528) (end 1.52 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ff9735c2-7f06-43e6-aa2b-dae952510f8d))
    (fp_line (start 1.56 -1.04) (end 1.56 -2.52)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bb9a3261-0e28-4c10-833d-9ff9b50e0878))
    (fp_line (start 1.56 2.52) (end 1.56 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 73b2ed85-8bbe-4c06-8252-7a6bac0e77b8))
    (fp_line (start 1.6 -1.04) (end 1.6 -2.511)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e598cab2-9a9f-4688-8a7c-273a3588b819))
    (fp_line (start 1.6 2.511) (end 1.6 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6881a3ed-974d-49b8-a952-abf639c06645))
    (fp_line (start 1.64 -1.04) (end 1.64 -2.501)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2c6be03a-c65d-40c3-8b12-87ee85a6ceed))
    (fp_line (start 1.64 2.501) (end 1.64 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c69dd538-57e8-40c7-887f-4e9d853e223d))
    (fp_line (start 1.68 -1.04) (end 1.68 -2.491)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 39170ecb-2414-453d-84b0-84177986e576))
    (fp_line (start 1.68 2.491) (end 1.68 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp efa4ecac-073c-4d69-9f9e-9853963dc752))
    (fp_line (start 1.721 -1.04) (end 1.721 -2.48)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 674da62f-13d0-4310-88dc-137453540e20))
    (fp_line (start 1.721 2.48) (end 1.721 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 488477c4-a878-43db-a405-31afe18bd6d1))
    (fp_line (start 1.761 -1.04) (end 1.761 -2.468)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fb9ad61f-308e-4f50-a5a4-c1bcfd630be7))
    (fp_line (start 1.761 2.468) (end 1.761 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 89d630f4-4962-417b-9507-e9ee84c99dca))
    (fp_line (start 1.801 -1.04) (end 1.801 -2.455)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d387961a-47e3-4397-93e7-4de9d84ab7bd))
    (fp_line (start 1.801 2.455) (end 1.801 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d858396b-d37e-4a2f-bc0f-b3535b626550))
    (fp_line (start 1.841 -1.04) (end 1.841 -2.442)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cbacb957-c916-4bcf-b921-d590d44a7b85))
    (fp_line (start 1.841 2.442) (end 1.841 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f07cfc21-e124-495f-b202-bddf4c2f9bb9))
    (fp_line (start 1.881 -1.04) (end 1.881 -2.428)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bbe12188-38d0-45e4-bc33-bc51722ff85e))
    (fp_line (start 1.881 2.428) (end 1.881 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ad2a61c6-6d93-4134-9a82-297d35fdb186))
    (fp_line (start 1.921 -1.04) (end 1.921 -2.414)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 153a3dd0-f97e-485b-a241-d06300e71c39))
    (fp_line (start 1.921 2.414) (end 1.921 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 98ab315f-fe3a-44fc-bd6c-c19515af9ffa))
    (fp_line (start 1.961 -1.04) (end 1.961 -2.398)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0ddb9579-7531-4f71-bb3b-7a3787bff5e0))
    (fp_line (start 1.961 2.398) (end 1.961 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8dedff8d-9fb1-449a-9c39-d477b2aea742))
    (fp_line (start 2.001 -1.04) (end 2.001 -2.382)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 706248bc-ce49-48e9-91fe-47ad6e4f432f))
    (fp_line (start 2.001 2.382) (end 2.001 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 772247a3-6f02-4272-b438-bda1673c5092))
    (fp_line (start 2.041 -1.04) (end 2.041 -2.365)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 811822e5-f351-43e8-9c5f-944023eea827))
    (fp_line (start 2.041 2.365) (end 2.041 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 97cd6372-0df0-4ebb-8efd-d64b44a1d4a5))
    (fp_line (start 2.081 -1.04) (end 2.081 -2.348)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8b134df0-85c6-4d3d-809d-7c5ebc5744c1))
    (fp_line (start 2.081 2.348) (end 2.081 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 54620aba-680e-41a3-b6d5-126e73d892d6))
    (fp_line (start 2.121 -1.04) (end 2.121 -2.329)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8297623-af04-4225-a8cb-1ed4c319353a))
    (fp_line (start 2.121 2.329) (end 2.121 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e5d3ea24-aebf-4d49-b669-9344a81615f4))
    (fp_line (start 2.161 -1.04) (end 2.161 -2.31)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 00ca791a-728a-4420-8377-6f642ab3782b))
    (fp_line (start 2.161 2.31) (end 2.161 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2b61fbb0-a691-438d-b4ac-78e69405e13d))
    (fp_line (start 2.201 -1.04) (end 2.201 -2.29)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 793de36b-9bfd-4352-aa68-8a9344db71cb))
    (fp_line (start 2.201 2.29) (end 2.201 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 12ee8dad-a122-43ec-b6f8-1b7b4b07a93f))
    (fp_line (start 2.241 -1.04) (end 2.241 -2.268)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 15229736-5867-4987-90e1-512179df4ecb))
    (fp_line (start 2.241 2.268) (end 2.241 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 058161da-717b-4e31-8001-27c21d8a525c))
    (fp_line (start 2.281 -1.04) (end 2.281 -2.247)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6317fdd1-b570-41ba-89b0-72773d05e767))
    (fp_line (start 2.281 2.247) (end 2.281 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 37b9963a-5fee-4c25-9449-8784f7e433b6))
    (fp_line (start 2.321 -1.04) (end 2.321 -2.224)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8f5cc2ec-223b-4a9f-add8-3eed0af8fb4d))
    (fp_line (start 2.321 2.224) (end 2.321 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0de89ec3-1684-414e-b889-7898fcdabebf))
    (fp_line (start 2.361 -1.04) (end 2.361 -2.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 409b16cd-fede-4423-a79b-54ea31b6f0a3))
    (fp_line (start 2.361 2.2) (end 2.361 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3d234047-36ad-4ccc-9ab7-17bd24bd0f31))
    (fp_line (start 2.401 -1.04) (end 2.401 -2.175)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dd182ffa-9dbc-40ef-8474-5beb402b7249))
    (fp_line (start 2.401 2.175) (end 2.401 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f721030c-b256-4bfc-96fd-de9c08093247))
    (fp_line (start 2.441 -1.04) (end 2.441 -2.149)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b93a23b2-c137-4ceb-bbb8-abe6f9475038))
    (fp_line (start 2.441 2.149) (end 2.441 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6781a207-b784-4530-8734-cd9309bbc455))
    (fp_line (start 2.481 -1.04) (end 2.481 -2.122)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8975d6de-c7a2-4955-9616-f59c1ed40a09))
    (fp_line (start 2.481 2.122) (end 2.481 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 483dbf7a-efa4-4d5a-b160-0dd3cbb27d01))
    (fp_line (start 2.521 -1.04) (end 2.521 -2.095)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d07787dc-cd0e-47de-820f-327262f4e07d))
    (fp_line (start 2.521 2.095) (end 2.521 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ce10863c-8e72-477f-a232-bb0c3c983178))
    (fp_line (start 2.561 -1.04) (end 2.561 -2.065)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a187738e-6155-499e-be3c-25f3eb0a7c5d))
    (fp_line (start 2.561 2.065) (end 2.561 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 930735fd-4452-4f00-9b61-a1f1c1240886))
    (fp_line (start 2.601 -1.04) (end 2.601 -2.035)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0598adf6-d04f-44f3-a21c-3eea900512aa))
    (fp_line (start 2.601 2.035) (end 2.601 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 93758e9c-db8f-4f80-9480-e5fca37a277f))
    (fp_line (start 2.641 -1.04) (end 2.641 -2.004)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b8b0e0a7-5e86-41d3-89b4-760aacb7178b))
    (fp_line (start 2.641 2.004) (end 2.641 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0ddd04c8-7a71-4a77-9edb-f95525612005))
    (fp_line (start 2.681 -1.04) (end 2.681 -1.971)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9e9895f7-0f9a-4d94-8edd-7665aac91f40))
    (fp_line (start 2.681 1.971) (end 2.681 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 21542601-eb78-4086-9df0-63c9c084a6f1))
    (fp_line (start 2.721 -1.04) (end 2.721 -1.937)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5b82590f-5fbd-4b55-b120-dfd7d21b0565))
    (fp_line (start 2.721 1.937) (end 2.721 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0b96bb10-5626-4f2a-859c-9d2005a1a156))
    (fp_line (start 2.761 -1.04) (end 2.761 -1.901)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 289ddfe1-435e-4157-a13f-ba469a5db15c))
    (fp_line (start 2.761 1.901) (end 2.761 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9cebc464-5aac-490c-80d5-6ec7c5b08ae0))
    (fp_line (start 2.801 -1.04) (end 2.801 -1.864)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7202a64a-d996-4d45-8ef2-822464a4098e))
    (fp_line (start 2.801 1.864) (end 2.801 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 925faf40-217c-46eb-8997-9090b963b207))
    (fp_line (start 2.841 -1.04) (end 2.841 -1.826)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b1916553-e515-4d9f-a807-f936cdc008c4))
    (fp_line (start 2.841 1.826) (end 2.841 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c51dd701-7a88-479e-b01e-0ea974bc1b61))
    (fp_line (start 2.881 -1.04) (end 2.881 -1.785)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5c2d6fe5-2989-41c1-a06a-69e3e25c796b))
    (fp_line (start 2.881 1.785) (end 2.881 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 814c13f4-5351-497e-8c62-d6de110a6959))
    (fp_line (start 2.921 -1.04) (end 2.921 -1.743)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 786b6843-33dd-412c-b2bc-9716d8e010ab))
    (fp_line (start 2.921 1.743) (end 2.921 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5c6e5eb3-2d1c-44b8-980b-7360fa9d7a47))
    (fp_line (start 2.961 -1.04) (end 2.961 -1.699)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ead35a85-b333-4451-a90e-a4c90bc9d8e0))
    (fp_line (start 2.961 1.699) (end 2.961 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 47eb2863-630a-4baa-bbdc-ebb0e8c4767e))
    (fp_line (start 3.001 -1.04) (end 3.001 -1.653)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f2a2b58f-6989-4fc7-a917-58bb0afe660a))
    (fp_line (start 3.001 1.653) (end 3.001 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4fc1c91-cb9d-485e-9e43-d5b3bd78f385))
    (fp_line (start 3.041 1.605) (end 3.041 -1.605)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1300fb1c-5155-483d-b08a-75ac333037c5))
    (fp_line (start 3.081 1.554) (end 3.081 -1.554)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 14c757de-734c-4d86-bfb7-6db158b991ab))
    (fp_line (start 3.121 1.5) (end 3.121 -1.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fed608cc-ba04-42fd-bf1b-034fdd50606a))
    (fp_line (start 3.161 1.443) (end 3.161 -1.443)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b670ad4a-e3a4-47c9-a351-c1f598983246))
    (fp_line (start 3.201 1.383) (end 3.201 -1.383)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f9ff8719-7d66-4adc-a969-cc1aba268375))
    (fp_line (start 3.241 1.319) (end 3.241 -1.319)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2703d5ea-1680-49ea-a2b7-9c015e3efe51))
    (fp_line (start 3.281 1.251) (end 3.281 -1.251)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9dd07845-1101-4a11-8f50-c47bc76e352a))
    (fp_line (start 3.321 1.178) (end 3.321 -1.178)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48158afb-af8d-49a6-941a-a0389b3768b4))
    (fp_line (start 3.361 1.098) (end 3.361 -1.098)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 67463738-7c73-4f52-b4c0-af58b0a5a040))
    (fp_line (start 3.401 1.011) (end 3.401 -1.011)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 54e6eaff-5847-4be3-97c8-2dbaf374916a))
    (fp_line (start 3.441 0.915) (end 3.441 -0.915)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c9012735-8c1a-4f4e-9211-b66a29d929ae))
    (fp_line (start 3.481 0.805) (end 3.481 -0.805)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e5149edb-5d8f-4d61-ac78-2a69dfebba87))
    (fp_line (start 3.521 0.677) (end 3.521 -0.677)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2099f25e-8fde-42b0-bf12-4da03af7de72))
    (fp_line (start 3.561 0.518) (end 3.561 -0.518)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f14dfdf7-467b-4aad-9d3e-c6d5b0243f01))
    (fp_line (start 3.601 0.284) (end 3.601 -0.284)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 497aae66-ac1a-4bf3-b8b3-8e5bf696b4f0))
    (fp_circle (center 1 0) (end 3.62 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "B.SilkS") (tstamp 4422fd07-96ef-45a0-a165-812f025dc307))
    (fp_circle (center 1 0) (end 3.75 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "B.CrtYd") (tstamp 657f50ef-a7ca-4151-9678-b3d89243fea0))
    (fp_line (start -1.133605 1.0875) (end -0.633605 1.0875)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6107788c-a32e-4d7f-8807-2c92a362845b))
    (fp_line (start -0.883605 1.3375) (end -0.883605 0.8375)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 19da329c-0fd8-4865-9d60-455a96c3433a))
    (fp_circle (center 1 0) (end 3.5 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "B.Fab") (tstamp c2ca4420-76ee-4b19-bdd5-c6d40eaee885))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "+12V") (pintype "passive") (tstamp 4829229c-5b6b-4872-9b4a-b64493c60717))
    (pad "2" thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp f41914b3-44a4-47b1-a4b1-b17eb4eb06cf))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 1a93a079-658c-4fc7-a433-8c0fa43e97cc)
    (at 52.5 45.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/0fc55645-96ff-4e1b-bada-2ca05af9a52c")
    (attr smd)
    (fp_text reference "R1" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 37618873-2fe4-45a4-b872-edab3c8afe59)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a1781a2d-99eb-4224-919e-8c12c5573a62)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 1e367e1d-d1e1-4a82-9790-5edb158a08ee)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9a954217-2a32-4491-8b0d-3528e8e567d4))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ed0e6ee3-2db7-468c-bbc8-657416111716))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f78f548d-ab09-47ea-b761-a4c9dabce61e))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2bfc90ac-0e03-4147-9c78-ad0f5baa030c))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 71bbb703-0734-41a1-ab31-b32df012289c))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3e057262-cfec-4fa9-8736-5229d169d8c6))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp de0efc75-0cd6-4a49-9df9-ed646627154b))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 486cefe4-f333-4868-a703-b138933881f0))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 256607d4-cf7a-4fb4-86a4-bb647f5520cd))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a80936e0-187b-41a7-9f98-ea8f2d5bd813))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 97430e0a-e4ad-47f4-9266-c583171b6528))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 87 "Net-(U2B-+)") (pintype "passive") (tstamp 48bbc0dc-4ba2-4efc-8c4c-af16075673c8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp 1afc19f1-87d3-4ad8-89e1-f34a0dccc709)
    (at 164.5 16.25 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/bb5e3d14-876a-46bc-80d3-0c67a17ba9a5")
    (attr smd)
    (fp_text reference "R46" (at 0 1.82) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a8a86987-96a2-497c-b3bd-0d2a91789570)
    )
    (fp_text value "1.1k*" (at 0 -1.82) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8df91e96-fc54-413b-a695-7d5d34b5c5df)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 834acd2c-95bf-45f8-ae4c-14d4992592a5)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 155b8359-5e61-445f-b8d7-a5ef0192e727))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48df3c69-3e8e-4021-80db-21cca3cb1722))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 13761956-174f-4260-bfbf-619c4aa35de2))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e447d89f-a392-44e9-bc9b-35a7c75b00d7))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4ec1759a-9701-466f-9135-30e219e962ab))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0c38b30a-f9f0-416f-aeda-9c256c1414bd))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 97e4c7fd-9b00-4160-b202-230c71a6579c))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9f4fb15d-80d7-42c7-ba25-2101c38458ca))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 366d6191-206d-4650-a364-deaeec1b75c1))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9cce8f6f-55c6-4d27-be4e-65a6134755a7))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 102 "Net-(Q13-B)") (pintype "passive") (tstamp 34530532-37df-42ce-8979-1999addbaba7))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 48 "GND") (pintype "passive") (tstamp f85e51f5-39cc-4f8e-b7f5-289de162264c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 1cb615b6-d05a-4e47-bd51-e1c11936a1c5)
    (at 140.75 100.75 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/55cfc94e-fc23-46ca-9910-42844a68d4a4")
    (attr smd)
    (fp_text reference "R37" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b446b9c9-bdd9-4b7b-a96a-7d559349be11)
    )
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cdee2a02-093d-4148-896c-9ddc44c20d17)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2d776129-5f04-44d2-b305-5be300145f80)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a6b64079-24e9-41ed-8a0b-a046b3952195))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 72ebdb07-59e8-4d97-84e1-0c0ae2d15fc0))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0fb9b90f-b532-4d82-8bb5-01d25b47ef70))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f9b604c6-670b-47d4-9461-d22a848157d0))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 26b6050f-d8ca-441b-8a62-a176974be666))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0a51cf03-db30-4fff-a029-6f993e37fe7e))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 610a3785-6983-475d-bb43-30c8ea3b0ce2))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 25ff785f-bf78-4ea5-8732-2328b5d8f4b6))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c9a01178-e09c-4a2f-a9ee-bad578810d49))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 44451632-171a-4235-953f-895163b8d6f3))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 101 "Net-(Q12-E)") (pintype "passive") (tstamp 09d394ea-95a3-43e8-a60f-91717ea40e93))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 107 "Net-(R37-Pad2)") (pintype "passive") (tstamp a7d28f5c-a3e2-4c8f-a352-b207ecde4b64))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 21e2d08e-8a7a-4963-a659-c32e475485bf)
    (at 132.593 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/74da4a7a-56ea-4fbd-a45a-ec4a4ed24c54")
    (attr smd)
    (fp_text reference "R18" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 20b68c19-9bf6-4a1d-badc-7d6a928c8534)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp da23eca1-4d63-4e32-bfbb-4a673ad4f4c9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2eac3907-83b4-46cf-aede-e9c95c84de5a)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f3a0c3f9-3b76-414c-872f-eab606bfdb29))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8cc2b872-b971-4636-bcff-a56689e49078))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3dc97b04-07ab-4949-a517-705da211cdf4))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2cb9ef53-8677-4d62-880c-6b00d0c11589))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7166ab06-de29-47c7-aff1-4fb3dc93ffc6))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1f02e90d-7446-474b-8752-93a64b2ec6c2))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4d3eccc7-d461-4857-9b93-c3501586d235))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 71b4c95e-194d-4e2e-8ee8-d17ae4b8601e))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8e326be7-f341-47a5-9401-6477502b3a5a))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dfda7771-b372-4813-b569-e3db3ad9f1ec))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 70 "Net-(Q8-B)") (pintype "passive") (tstamp 5058c21a-def8-4d31-8cae-680924ab8dbd))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 18 "Net-(D8-A)") (pintype "passive") (tstamp 1f55379d-e179-45eb-985b-bf5da9119e1e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (tstamp 22567adb-1787-4f9f-9b1f-feb84d2ec52a)
    (at 57.225 26.21)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (path "/f41372c1-8ce9-43e6-a304-668acf7a5dd9")
    (attr smd)
    (fp_text reference "U2" (at 0 5.28 180) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp aaef9edd-ff06-45af-bf20-8f75b99f4070)
    )
    (fp_text value "TL074" (at 0 -5.28 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1220116e-8f7f-482d-bee5-06443bf1936c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)) (justify mirror))
      (tstamp 8f3f6179-c698-4b7a-b024-5c727b084352)
    )
    (fp_line (start 0 -4.435) (end -1.95 -4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 70f2ce49-ed6b-4116-a2d4-e6fe5476c76a))
    (fp_line (start 0 -4.435) (end 1.95 -4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d8c517b8-5c32-42a3-9d3f-745f96a144fb))
    (fp_line (start 0 4.435) (end -3.45 4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6357e62e-b979-42fe-879e-627ce8ffc664))
    (fp_line (start 0 4.435) (end 1.95 4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a15c6d83-4459-44e5-9fa8-c21b99348415))
    (fp_line (start -3.7 -4.58) (end 3.7 -4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4e2a0c05-3666-4906-9982-e995aa4279cc))
    (fp_line (start -3.7 4.58) (end -3.7 -4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bf14dc69-0605-46d3-aaa6-49d659ffa459))
    (fp_line (start 3.7 -4.58) (end 3.7 4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 91c85dcb-545d-4506-84cc-682b1fe2d961))
    (fp_line (start 3.7 4.58) (end -3.7 4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 63a1692b-bc87-4860-ade1-306c68ecec6e))
    (fp_line (start -1.95 -4.325) (end -1.95 3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6bc25a62-9b17-420d-a814-4cd1c76d833c))
    (fp_line (start -1.95 3.35) (end -0.975 4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 84c58622-8706-4396-9f4e-62fa4a8bac65))
    (fp_line (start -0.975 4.325) (end 1.95 4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3890d9b0-6092-47c5-94bf-fda4f02d97ed))
    (fp_line (start 1.95 -4.325) (end -1.95 -4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1fe08bf6-f4e3-4e00-96a3-58080237b587))
    (fp_line (start 1.95 4.325) (end 1.95 -4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3f50bfcd-ef0c-4480-82f7-99f895d2e89d))
    (pad "1" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(D37-K)") (pintype "output") (tstamp 11be1a1f-605a-45e3-9d4b-fb8f71a9a685))
    (pad "2" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U2A--)") (pinfunction "-") (pintype "input") (tstamp 32c0bf54-3b71-4a53-b339-674b7b009492))
    (pad "3" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(D33-K)") (pinfunction "+") (pintype "input") (tstamp b5b098d8-7287-4e42-8cbd-c75228a10ce2))
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "+12V") (pinfunction "V+") (pintype "power_in") (tstamp 803ab2f1-5565-4655-8b1a-66a352ba9eb5))
    (pad "5" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U2B-+)") (pinfunction "+") (pintype "input") (tstamp c1bd3a8f-6ae7-47c2-9fce-0df446dc0355))
    (pad "6" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(U2B--)") (pinfunction "-") (pintype "input") (tstamp 74cf88d8-dfd3-4205-8c1e-4accb0cd8095))
    (pad "7" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R25-Pad2)") (pintype "output") (tstamp 51a96254-3d47-437c-ae49-0a83235dfa99))
    (pad "8" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(D35-A)") (pintype "output") (tstamp 24b75e61-3070-47b9-ad01-2d3f3900fed4))
    (pad "9" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U2C--)") (pinfunction "-") (pintype "input") (tstamp c76f63aa-28fc-4904-9bb7-60c59aef10ff))
    (pad "10" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(D37-A)") (pinfunction "+") (pintype "input") (tstamp 29c37064-ed52-44b2-b3bd-ff0bbb21e1f3))
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "-12V") (pinfunction "V-") (pintype "power_in") (tstamp 2efa7c9f-55ef-4363-b275-f50a3b3a05dc))
    (pad "12" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(D35-K)") (pinfunction "+") (pintype "input") (tstamp 2d225194-3677-434a-8a59-318986d3e35a))
    (pad "13" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(U2D--)") (pinfunction "-") (pintype "input") (tstamp b2d828cd-a572-4d68-96dd-4ec5aa1d7692))
    (pad "14" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(U2D--)") (pintype "output") (tstamp 911dd90b-76ab-4599-97f2-7e66e8d61079))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 23418de9-1035-43b6-b026-9d3630238d15)
    (at 59.25 34)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/c77bac33-1f86-4d83-9cca-b591dd9fe68f")
    (attr smd)
    (fp_text reference "R28" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 363161be-8ef4-48bf-8be9-60aad47e1b18)
    )
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 20d27f73-8ee1-4d35-99bf-3a7e92010809)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 06507b39-93b9-4638-90bd-bb2a8da98310)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f0e98bda-6213-487a-ae21-120d734c630e))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b247c487-d07a-445f-a2f3-f67a8981193a))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 21d9b168-d2f8-4cab-952c-eb663e80cd25))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f9964f3c-da9b-462a-8721-4827c5c72334))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5f2b5cd7-6aa7-4a43-a816-aec43baf7b25))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3c93f042-5b78-4000-bb19-923acd460f86))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 134d96be-c6cf-47f6-bd0f-5c55f2c0a89b))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3b2580cd-6854-4ff4-a816-2f2471880753))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9ca8a2dd-b117-429b-b912-23352abcc7f8))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1155492d-dc80-4d1e-8eb6-8641b8afbe49))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 86 "Net-(D37-K)") (pintype "passive") (tstamp 1dfb46ca-ce8c-4a51-ad1f-83a221838b08))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 76 "Net-(U2A--)") (pintype "passive") (tstamp 9ebb6a38-7e4c-4a56-8f36-3b3d9ed4e994))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 27006b3a-335f-4cfd-9209-fdfd19dbeeec)
    (at 155.7 83.25 -90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/59a8f123-cd8e-46d3-89c7-b055ffc27c9b")
    (attr smd)
    (fp_text reference "Q12" (at 0 2.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3b6cf588-2bc1-4f1e-9d19-41bde7ce5c9d)
    )
    (fp_text value "BC548" (at 0 -2.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bd00a824-d9a4-4ccf-8831-1f5588eba1a4)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp dec0ef3c-1684-4bf1-9d93-3db1f02dd505)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 573e9487-8eec-42eb-b1d5-4bd18b64dc48))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1d3b1d2e-c4e1-4795-afcb-7a9091c301ad))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 81f43259-606a-4c7d-9f4e-86c88fc1dd2a))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a85dcabb-c051-4e40-be07-f4dcda9fbf4f))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e1e8a299-86f7-4cf5-811f-102759895531))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6f6901a0-febb-49f1-b603-57e52de2a97f))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4ee3397c-1f9d-4c3d-8bc0-389d12655e63))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4e84057b-d2e0-4a04-8a3c-ce7e7013f0a6))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e3712762-de89-4ec1-a94e-bd80cd224557))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4940d5b8-3fd4-4428-90b1-f3f185b61c20))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 86b8dcdf-a3ba-47ec-a617-c7898c06a010))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cbb17937-a3dc-47c4-8c7b-2acde5be1d72))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a7b396b2-9e96-4434-9440-9544e873e9e9))
    (pad "1" smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(Q12-C)") (pinfunction "C") (pintype "passive") (tstamp 61ec5f5b-a62a-4256-b168-ebed48d24644))
    (pad "2" smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "Net-(Q12-B)") (pinfunction "B") (pintype "input") (tstamp 58d7c130-8a13-459e-bf86-b02fb38561f0))
    (pad "3" smd rect (at 1.5 0 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "Net-(Q12-E)") (pinfunction "E") (pintype "passive") (tstamp a822a727-f1ea-413f-a529-9f855cac4f88))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "B.Cu")
    (tstamp 2ee0b133-e46d-4d33-b83b-424d62a7a928)
    (at 142.75 27 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 1A Schottky Barrier Rectifier Diode, DO-41")
    (property "ki_keywords" "diode Schottky")
    (path "/c381024f-bfd2-4784-b640-9ef1fb462618")
    (attr smd)
    (fp_text reference "D31" (at 0 1.85 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9009d45d-361b-4964-846a-f25cc06a4104)
    )
    (fp_text value "1N5819" (at 0.1 -1.9 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fcbfe823-b172-4d60-8f9a-744e85cf085f)
    )
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ee1a4aeb-c7c7-48f6-bcf5-990d1d773560)
    )
    (fp_line (start -2.01 -0.85) (end 1.25 -0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 45e9c894-2ec8-4e31-bb65-79d1565468d8))
    (fp_line (start -2.01 0.85) (end -2.01 -0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 90a85206-e610-4a3c-9e8c-5cdfae43ae21))
    (fp_line (start -2.01 0.85) (end 1.25 0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c6ea09bf-c735-4073-bc03-bee7b1c28a8e))
    (fp_line (start -2 -0.95) (end 2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 78011c05-e9d1-4dca-863c-9a25074d866d))
    (fp_line (start -2 0.95) (end -2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9b016957-c5e1-4a60-ae90-ff550e2d4ca2))
    (fp_line (start -2 0.95) (end 2 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5a124ff0-360a-4c3f-8ab8-3096f4d89851))
    (fp_line (start 2 0.95) (end 2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6bb78f94-b0a7-46d0-98b0-cf760ca76212))
    (fp_line (start -0.9 -0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a389c297-d6c3-4fe2-b816-6dad585c6eb1))
    (fp_line (start -0.9 0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c9ffcc0f-8abc-4072-bc54-8ab4afbbe8fb))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp af1f22d2-fa5f-42c8-aac4-308414f32e28))
    (fp_line (start -0.3 0) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2964db0d-f791-49a6-b2b8-22dcbac3d63b))
    (fp_line (start -0.3 0.35) (end -0.3 -0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c501ed1d-cc0c-4dbf-b520-acf620ed535d))
    (fp_line (start 0.2 -0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a3ea37d0-b67e-4fee-bd03-24a58c45703b))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f85eb3ae-3f16-4d0a-9b02-f4a7a6366988))
    (fp_line (start 0.2 0.35) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c7b1eb5-5cc9-48ec-9af9-bcd8f5795b41))
    (fp_line (start 0.9 -0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7ad12ff2-c29b-4948-bdbb-4b2d3cd8b3a1))
    (fp_line (start 0.9 0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dd0c40fc-68d2-4cab-8ba1-0a5026e0d483))
    (pad "1" smd roundrect (at -1.25 0 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D31-K)") (pinfunction "K") (pintype "passive") (tstamp b183e3de-2485-4d52-92f1-798be35f80ef))
    (pad "2" smd roundrect (at 1.25 0 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(D31-A)") (pinfunction "A") (pintype "passive") (tstamp 2ab74992-2b52-4031-97de-4e8b2bf76fcf))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 309227ef-f5e4-44ea-b409-b95ffae57bd8)
    (at 70.093 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/b4b51c74-b835-4318-902b-8f1d36ce9770")
    (attr smd)
    (fp_text reference "R13" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a009e00a-2fc2-4c3c-9a8e-c1adef997c15)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e76791a8-c5a3-4d75-9a78-4bdb3934505f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 1dc3714b-524a-4254-a1c2-5725db152a9a)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 752e606d-24b2-438a-a193-cec4fd66681c))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3596223f-a8d0-4ca9-b8c3-e1fd0568e8e0))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e742f738-e917-44ff-8223-850decb66627))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp efd5c6a5-b426-48cb-8dd0-84fc376a436c))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96c3bdb7-69da-48ed-b212-fbcbc71045d8))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c602777-c982-49f8-8ffa-7d91f9f00e70))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ebb9f3cb-223d-44a7-9eb5-7cf0315a5e8b))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 286ac034-f201-4729-b4d7-09fd3fcaf625))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bef2fb02-85db-4576-a84d-473b9cab1154))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e3bb4817-4e5c-456c-b0d5-a01397b12b27))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 61 "Net-(Q3-B)") (pintype "passive") (tstamp c4681d5e-8fcd-46df-af6d-2d08ffbdbd9e))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 8 "Net-(D3-A)") (pintype "passive") (tstamp a4e03452-6dcf-47b8-9eb2-9ecc656384eb))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 33c31c56-13d0-4f40-ba59-24349702988e)
    (at 23.5 80.75 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/aeef4800-7cfd-4ab5-880e-aac1a4abd155")
    (attr smd)
    (fp_text reference "R47" (at 2.25 -1.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1f9d4d61-e66a-4451-acf6-217864175074)
    )
    (fp_text value "100k" (at -1.25 -1.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 831a8626-a425-4f6e-bbe3-30fbe6779f7f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a88dcf4f-ab6a-4a33-872f-70ffc159f211)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ffc1124d-7633-4987-931e-8cf872eafddd))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6cf2bbdf-ed35-4705-82bf-919c7ed8654a))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2e353f04-ed14-4a72-854f-1d0b78538aba))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e9c6c372-1142-4874-9eda-fac3d02ac7ae))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6c55771e-3bb8-4b0f-895b-86ffc4a022ff))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f1f6015a-cf75-4599-863e-f9a69492f754))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4264e4e8-94b2-48f0-a905-d20529287241))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3f2a48e6-d330-4735-9611-fde64cfa1fc1))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e334f6e3-5017-4a39-b1f3-a200dad6d8d2))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 65e09f72-c05e-4445-ae28-d96b8bbc4f95))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 076dc5e7-7e66-40a6-a0a0-c59f13f540e2))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 114 "Net-(D34-K)") (pintype "passive") (tstamp f9edc1bc-cfd9-44d5-a83f-96884e1eeb09))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp 341ee6bb-7c9c-4bc2-80a1-4be85aada0ab)
    (at 54.75 38 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/0880a800-306e-4e15-971e-207a608e1893")
    (attr smd)
    (fp_text reference "R25" (at 0 1.82) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5603529-4ba2-40b9-99b0-306d4c035bc7)
    )
    (fp_text value "1k" (at 0 -1.82) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fe653f1f-e7b3-4dda-bca9-d8cfb6d0baf0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 1286b2e9-6d91-4c23-9506-cb2e4bf5c3b3)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3a065402-6f4f-4219-a9ef-b856ed5a55e6))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 95117a9e-0e54-4cb7-aa52-498d43682952))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 19255826-efbc-42fb-af4d-d5aee1ebf65e))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp cd03809c-41db-4282-af50-89904478e9c4))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 69bc6bf6-67ab-4866-9549-a4f00463aa51))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1fd45744-6bf4-4be0-9128-37223f529123))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fbf8ad99-2148-4f80-8f6c-abd85429c0e2))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 56bab482-ee3f-4715-ae35-21e7b884681a))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 508707ec-b048-4bf1-bd23-ccb96121bd2f))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 688a7787-6931-432d-892b-802117273673))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 97 "CLK_IN_N") (pintype "passive") (tstamp 6cabb077-ab92-4ca6-89b1-f51de037d483))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 57 "Net-(R25-Pad2)") (pintype "passive") (tstamp 273607fd-f668-4eda-93f3-ec43337671dd))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 3454b447-aaea-42bf-b823-68643d5dd713)
    (at 108.593 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/3b8a68e2-9b42-433a-b4c8-db28126752e7")
    (attr smd)
    (fp_text reference "Q6" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3ef78052-e28c-4229-9ddb-83116d694927)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d6e97797-2abd-4e50-87d4-9f5b4a40114f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 5e7f2914-5fca-414f-825d-55bd6da3a3d7)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c7098f12-51a2-4bc0-a375-b941db2af17d))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5d193bf8-5d6c-4e03-b0b2-22be7cc73806))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0e9d1b31-762f-431f-9ad5-12d65307cd7e))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a3c7f1fb-1a22-4a50-b0a5-8f6db2ddd476))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6c9cec27-ad31-4bcf-908e-2a077029e96d))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 414111a5-50b6-4664-b7dd-2b4edf46ddd3))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 196c513b-cdd9-477a-8de3-ce2d2c054b50))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 50aca275-81f2-4994-8ea2-9d56d332a807))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp efaecbee-ec83-4bc3-ab69-c61695a8b8e5))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 70c5c466-9beb-48e0-8df0-e690ac197053))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 82561df1-1a35-4bd2-8c09-13f9c96c78ca))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b85037ba-e201-4e3a-a28a-a1ae1ead6719))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4c4f1362-04e3-4103-8b05-3e28f83a144c))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp a73b50e9-32e5-40ce-9075-451693224dd0))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "Net-(Q6-B)") (pinfunction "B") (pintype "passive") (tstamp fbe77f18-a491-42c9-b65d-d343c8c6b9a4))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "Net-(D26-K)") (pinfunction "C") (pintype "passive") (tstamp 8efaa475-9485-4805-9b1e-64ad19068487))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 357de24d-cc3d-4c78-8433-d11f55b7f1c6)
    (at 131.29 40.64 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/afe0965b-e44f-4a5a-a375-9b0a82cbe052")
    (attr smd)
    (fp_text reference "D36" (at 0 2) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c242d479-9041-40df-b512-0d75b63ee74a)
    )
    (fp_text value "1N4148" (at 0 -2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 91324b5a-a3fa-4746-bbe5-bc3e23d7cd00)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e106f452-914a-4da6-978b-ff238bc62185)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eafdfd19-75bf-456d-a25b-a54ec1524e77))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8aded92-8e2f-439f-8c89-3169ba507e0b))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f6e6a078-efbb-4d12-a7df-d47e8bb4bdab))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c26a3fa2-c141-449d-bb9a-d4bac7186b5b))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 42802a3d-a209-4bb3-82a8-1c7733f13a8d))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f2c081d0-5988-4bde-ad1e-5bad5a324665))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 077dc14e-3638-416b-a7b7-c46f279bcbe0))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 654b0506-229a-48e1-97e2-73c34b72cc8f))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 46a8a4cc-a3f1-4255-a70e-e99b2ada05be))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 64131551-44cd-4ac3-a7cb-8bb32244a8a8))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dc1656f4-88ed-4dac-8e9d-8ccaba24e4fe))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d88d3966-7f09-478d-a8d9-71b5d8c5b385))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7f7c9a4c-62bd-4239-9051-e2f70f61ba18))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1f9387dc-b52f-43c7-ae87-1cb9fe965c1d))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6754704b-2d4a-447e-9f52-d338d2cd7fe3))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 01c057f9-d2cf-427d-8514-02a01e331f02))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0555886e-d491-455d-8c4d-5e5194611a9b))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 02450b56-bf2c-47eb-9d80-7abae2f6b40d))
    (pad "1" smd roundrect (at -1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 92 "CASC_OUT") (pinfunction "K") (pintype "passive") (tstamp e2e51430-0659-419b-85ce-145ae20b90a7))
    (pad "2" smd roundrect (at 1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 71 "Net-(D36-A)") (pinfunction "A") (pintype "passive") (tstamp cd0fbf09-c7bb-42fd-a241-f5cf4c446d35))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 3595e6b5-3eab-4788-bcf9-470c6bcca5db)
    (at 36.75 16)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/8d205633-a34c-47c5-b49a-17b06a5ccceb")
    (attr smd)
    (fp_text reference "R2" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ecdc5054-6419-4587-80c9-9cfa9c015d6a)
    )
    (fp_text value "6.8k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4864e1e3-f0ca-45fd-914e-d157b43242ab)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp f3eb9050-fad7-42b2-9d7b-2922bc67fc97)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c52be2db-3005-4005-a645-932faf46208e))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6e106b10-d106-4530-90c5-ad9b0f894b1d))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 794eb0f0-7f43-426a-a705-533954b2cf4e))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 74c38c0d-fc61-41f3-9cd3-74c86927cee9))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 381fdfe0-b0da-4d5b-858e-9288f359f03f))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ff394fee-0382-46f6-ac80-faf1b67a1270))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4a8725df-687f-4ae2-a53f-121304c92708))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f13ee8b2-a751-4ffd-b1a0-86ef6f0500ad))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 80174bd8-f9e8-4be8-a4d7-b1035057689e))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7243d0d5-3aa7-44ed-8e4e-e0a41e0732fa))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 41 "Net-(R2-Pad1)") (pintype "passive") (tstamp 5936121f-b634-4952-ba72-48ea783cca79))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 77 "Net-(U2B--)") (pintype "passive") (tstamp e54d8648-ec66-4cac-b327-5c891d04b781))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 359c4c1e-efcb-4a90-b9f2-d96498136123)
    (at 69.75 43.25 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/36a04c0a-ad88-4907-ab47-ce951f51aa64")
    (attr smd)
    (fp_text reference "R26" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f7ab1f80-c446-476a-9f4e-9a7e25ab51e4)
    )
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd85620d-6101-489b-b377-3e316bcdbe38)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 5ee0e4e4-69fd-4c48-9281-c5dfe84c72b3)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ab934741-8a1d-472c-81d1-c2b3f96f798e))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eb97889e-b0ca-44eb-bac0-b91991679e86))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 26dae291-6583-407e-af0f-8c37af76ba61))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ef2ef71c-cf5f-49ba-b4f8-3a3ea6d58d92))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a37a8823-954e-43f8-9eb0-9b74fdae461d))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c09e8680-a248-4870-b79b-c7e10894d41c))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6cc102d7-0f9f-480b-8052-aa8b06f681f7))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 70aaf1fa-fc45-4d77-8107-d488221960e9))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp db8f9b1e-1078-4aab-bd65-aecb5ce33ab9))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f4fcc30-1aad-4c3a-963d-ce5da61ae4d4))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp d73d1684-b1f6-47a6-9e63-5531fab5310e))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 46 "Net-(D33-K)") (pintype "passive") (tstamp 481aeb2a-5fa2-4597-9120-ff68a2e65900))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 373147bb-6417-456b-8307-9fc313ac0a17)
    (at 71.093 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/30430be0-b2e2-4a8f-bac5-c897f7e54d11")
    (attr smd)
    (fp_text reference "Q3" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a7a948a0-8c28-4917-8909-4da7831c82e3)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2895d597-06f6-45f1-940c-16710fd51dfb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 63b4fb3a-c3e3-4874-9199-753beed11678)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 10cb2e61-d9e8-4417-aa83-b67d9054106b))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9933526b-7a27-46c5-ba2f-91e1dac0d32b))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e51ded0f-6ba0-4171-ab79-6770f6b301b3))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4e25e180-0ca6-4854-991d-99b8c46f6834))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5fde8403-79b9-45a0-ab38-e0e0db3aa753))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 936cca49-edd9-4db6-80e2-1d41f9bf3ff1))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e0e3d514-8f73-42d5-ab73-51ce5e29d9df))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 99654b03-3f35-4b3c-898e-18aaf7d53a19))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b4b5a064-6a3b-4b6f-8f93-5ee16f8d49a4))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f861fa03-d215-4a51-a7c5-edf7c5a4e3f7))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 21a498ed-c2e6-45a6-979d-7b0052c8f70a))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b661fb47-f069-4823-ae2d-9922bbd42ce7))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dc3fab8f-ca25-49ff-a118-71c114a13373))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp 46696385-c280-449f-84d4-c2e42af532cb))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "Net-(Q3-B)") (pinfunction "B") (pintype "passive") (tstamp 195c0bd3-7110-4fc8-9fae-d850aa30a108))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "Net-(D23-K)") (pinfunction "C") (pintype "passive") (tstamp fc7f8773-caf1-44ec-a315-75c17e476b12))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 3ae0ce85-0c4e-40a8-8179-d399ade63c70)
    (at 161.45 83.25 -90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/39341e5d-9d91-4279-88e4-546b1354e7c1")
    (attr smd)
    (fp_text reference "Q14" (at 0 2.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d28262a0-3087-4e71-bc3d-8ff15bba86e5)
    )
    (fp_text value "BC558" (at 0 -2.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9dc2d21e-1e21-44de-ac97-7f9e098fa0ea)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp c64ec7d8-06e3-47e7-bfe4-88d7b420b74b)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 83eb6204-e01f-4535-84c4-a97ab1165021))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ae00cd6b-a9f1-47b6-8aaa-294b4c3f97ac))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1af13e27-1f17-4d2c-972d-6367ddd9e6bb))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp abedcefc-9b59-4d9a-a103-e1ff213cae95))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp cfe7fcfa-44e7-425b-8e12-d844115a42bb))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a591f986-70c5-4eec-8292-e99f876c252d))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2e043613-3f41-4ac7-8ba3-1232274e5fd1))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7b582aa7-8ebf-40ea-8af7-df39be0dcb39))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 09474464-278a-405f-b457-75669d1ebb39))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d2cbb0a6-6d78-4e53-b0df-d3157b3513b1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 26e37232-cc56-40e1-8ea7-dc25007490bb))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 35db94d7-c2bb-4dbd-9c63-57bb181c4ef4))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4e14a444-4e44-4009-adcf-31326faab40b))
    (pad "1" smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "C") (pintype "passive") (tstamp 6c7a2ed1-22c3-40f4-9ddb-e7a35fe60998))
    (pad "2" smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "Net-(Q14-B)") (pinfunction "B") (pintype "input") (tstamp 5208a720-4822-4048-834c-68ebe4710e2c))
    (pad "3" smd rect (at 1.5 0 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "Net-(Q12-E)") (pinfunction "E") (pintype "passive") (tstamp db7cae23-e119-4410-8e7b-2437f97ebe73))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 3f4c0512-7762-40ba-929b-e6dbce915990)
    (at 110.75 34.25 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/e7b449dd-41fb-4414-83f3-745fb801f612")
    (attr smd)
    (fp_text reference "R32" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2cb26d5f-4229-46a9-8d2d-555ab027796e)
    )
    (fp_text value "51k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 150de5bb-ff01-400c-9abb-86f120d58414)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 443f1d21-d5a7-4d2d-962b-71402041ebdc)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp be5ebc88-2250-4d44-a671-84a11a810e07))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b17dcb0b-617e-4406-ab3e-66bc80e02fbc))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f2367c8b-fa0b-4d1b-a4e1-8d384c91c752))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp db01cfce-fbb8-443b-af42-cc4275edb803))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96ea0a0c-a834-4524-8c33-1a45e056bdc3))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b7e9eed8-3953-4eb3-923d-57cfe0e264ba))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9007a9c7-745a-438e-b202-ec4c1c53c562))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1a21c40a-dd16-4f56-9b90-43f9ee939003))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bfae7501-640d-4d60-90e0-3c6aa475d946))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2a6c8d8f-4aa2-4c0d-9998-5ccf5a7ed6ab))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 58 "Net-(R32-Pad1)") (pintype "passive") (tstamp c7c969bb-1583-4db5-9e6f-7d1393daef7d))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 78 "Net-(SW12-A)") (pintype "passive") (tstamp 02fa86d3-c9cb-4bdc-b0b6-99dad5b16c53))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp 41601c1e-3a35-40cc-9663-9fc696765472)
    (at 148.2125 94.75 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/60d46157-43e3-49f9-9283-e18503e8b10e")
    (attr smd)
    (fp_text reference "C2" (at 0 1.68) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97d8da11-2ce4-4967-8c0b-a11b507b6933)
    )
    (fp_text value "1nF" (at 0 -1.68) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0e52f5d5-104f-423e-8559-0853539d7b63)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp f383a15b-153e-4e1e-a113-6dc5c82b9feb)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4b93a5b0-3218-403c-9a6e-a9a64684cd49))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 50afcf87-eee4-4062-ab2d-bbf9cc3195d5))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1f652949-d1a3-47ab-a592-2dd12a92d639))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 83bebbc0-aee7-4966-8d2e-133c463869fb))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d7281d41-4827-4eb6-8534-4dab61f39fa9))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4262e809-c3ef-40c0-b872-64fcb22fc46b))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 902d0900-e172-429d-9946-ad6da451aeb4))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f5d21eed-7dea-4115-ba07-2663517bf337))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp aa3dd79e-10cf-4cc2-ac35-9d8e2c5c9993))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e5954d1b-643f-4293-9844-a5a26e69ea97))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 60 "Net-(C2-Pad1)") (pintype "passive") (tstamp 1bd3ec73-7024-40e9-a28f-f144fc107f25))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 82 "Net-(U3A-+)") (pintype "passive") (tstamp 3db24143-f654-4b42-b23a-f85d2915bf6a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 4444cf5b-281c-4271-8835-ec38c830ace0)
    (at 153.25 92.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/da7d2601-bdff-4b23-86de-7575f1dee312")
    (attr smd)
    (fp_text reference "R36" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 550acf88-7a10-4b13-8150-5e00a3703b5d)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f2396fa-e37f-4bff-abf5-d6979813dfeb)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 1797fc02-025e-499d-8da8-9be2e0db8cbd)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8a4c08c1-f033-4228-b91c-dcdf6ede26cc))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3af92df5-f568-45fc-aa3e-24c88a0161f6))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b73e124f-c228-4e9f-acc6-094c346d3514))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 56c50805-ce9a-4fa9-b9f3-a39439398024))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 60305910-106b-4977-8242-e795657e37a2))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8319662d-e183-4e5a-a9d6-6ca0df90f49d))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fad76e90-c58d-4a78-a635-122efc268635))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c901f11-0d81-4e3d-97dd-13a3498bef23))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3dd7e2d9-2d8b-4cc3-a5fd-ca6f98b1b28f))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 349515e9-314b-4f73-a122-83d8bb551757))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp cbd28727-b531-4aed-888a-f53eb603ad1a))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 60 "Net-(C2-Pad1)") (pintype "passive") (tstamp 3092ff55-23f1-4b62-9c91-32bac25a3686))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp 4676b329-b2f6-4426-adca-9a6f007a3080)
    (at 166 80.05 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/82c3541f-c4c9-4165-abb5-cd2b8642bcad")
    (attr smd)
    (fp_text reference "R38" (at 0 1.82 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f276823f-23f3-4653-b27d-3adbdf8aa09b)
    )
    (fp_text value "1k*" (at 0 -1.82 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ff6a882a-ecc1-40a3-98f4-4acd2de27fd4)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 9881c1bd-0aab-41ba-a431-28e2ccd05bb8)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5e868093-78bd-4ff2-9b7e-ba394ebecfce))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ea505a64-1f0c-4014-ac3f-0cacea1cb9a7))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 030d8495-e530-4247-82ea-55455cd8f4fd))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4d47186b-fc81-48c5-aff1-3a8e7daee753))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0cbe16a1-0bc4-4536-97a9-dbe7912265c7))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bcea9879-1a45-4b87-bbf0-b0d954b33ed5))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 05bbbf06-9357-42e3-9139-bc5a793420f0))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a1bc2c24-bc33-4e68-89c1-62036258d2bf))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8052b65d-c8cd-4211-bc48-a6d49e1bd049))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3609f1fe-9fa3-4d30-aa3b-a17202c3b689))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 103 "Net-(Q14-B)") (pintype "passive") (tstamp b541bff6-3aae-4ee9-8223-f6c602804551))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 48 "GND") (pintype "passive") (tstamp 3bf430f2-e845-482d-a009-b5f847915670))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 4bcb6a29-2923-4264-b674-c38aae4d2619)
    (at 146.093 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/1d0eaf09-9fbc-469a-b78c-d9bff4c8f7b3")
    (attr smd)
    (fp_text reference "Q9" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 81e7b5ab-1cbc-4d8e-8725-0fa71e6921f8)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ba3b9a18-b310-42e3-a77a-49f9fb38b5bc)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 8694da8c-c03a-434f-9bc3-ed93359cbce2)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0caa90bf-8eef-427a-afd4-0684c819d560))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b651ce65-ace4-4ac7-9374-9b29052e045f))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 96eda49e-4c8d-40d3-ae70-7ce4c32546d9))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b95c42a3-d2e8-4293-aa6f-bc9f72cdcfcd))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c4aab734-0352-44ac-b3c6-e04f73ccf0ee))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp dc502425-805e-4878-a814-9b1565cbfdba))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3d52efa7-01f7-458d-9b1c-4e71c1c58fb4))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c5af279e-5109-4828-8c6a-a475cb72783e))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5a082c4a-bb7c-470d-9166-ae52ed6fada5))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5d5a2d14-cd1f-4075-8c68-767f2c8ad0b8))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2c1e2d85-a8ab-407a-8cad-cd2452b52ef4))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 98807ab5-4a9c-45d4-a92b-58b99db31d67))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fd4f5ce3-11fb-4654-a282-9ff365008129))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp d7bcebe4-9c58-4215-9263-df5c6a9481df))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(Q9-B)") (pinfunction "B") (pintype "passive") (tstamp e7a1148c-c3cc-4163-b849-432eec8c20b5))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "Net-(D29-K)") (pinfunction "C") (pintype "passive") (tstamp fc16ce91-4c26-4378-8ab4-674794b3d9d6))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "B.Cu")
    (tstamp 519b2781-60d0-41f4-9057-657818959182)
    (at 148.75 27.5 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 1A Schottky Barrier Rectifier Diode, DO-41")
    (property "ki_keywords" "diode Schottky")
    (path "/d1d56d0a-85fb-4062-9847-6ee8da3956a3")
    (attr smd)
    (fp_text reference "D32" (at 0 1.85 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp db8843aa-7924-4062-bb5d-bd1cf06a72f6)
    )
    (fp_text value "1N5819" (at 0.1 -1.9 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a5710a17-6de4-465b-b079-72426ff938f6)
    )
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5a60b720-df6b-46d7-a3d2-89976ee900c4)
    )
    (fp_line (start -2.01 -0.85) (end 1.25 -0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 96270ade-be2d-4bcb-8cad-fd8fd3cdf8c2))
    (fp_line (start -2.01 0.85) (end -2.01 -0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 419b65d2-a309-4f01-a921-342ba800d174))
    (fp_line (start -2.01 0.85) (end 1.25 0.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 21f5b823-8e0e-4042-895b-4c104a8b317b))
    (fp_line (start -2 -0.95) (end 2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ed657f60-c293-45ca-b6c7-5a7ec8cbb8ae))
    (fp_line (start -2 0.95) (end -2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d40fdd68-02b5-4545-9d33-d6f2aaf28468))
    (fp_line (start -2 0.95) (end 2 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 50a1617c-919c-40e9-89d1-8e59701dd535))
    (fp_line (start 2 0.95) (end 2 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d662f056-f9ec-456c-b071-dae9f50f9eb7))
    (fp_line (start -0.9 -0.7) (end -0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a64864e1-9ecd-44e4-aff6-d9d5472b01d7))
    (fp_line (start -0.9 0.7) (end 0.9 0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0b1d49a6-44e3-468a-b9a0-5d0911cae1fb))
    (fp_line (start -0.3 0) (end -0.5 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 36f0295a-f7be-4347-8c02-4c70c0bb802a))
    (fp_line (start -0.3 0) (end 0.2 0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cbcf06b4-0f9c-4d3d-9e46-40729a8f5d86))
    (fp_line (start -0.3 0.35) (end -0.3 -0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1d853a88-368e-4978-97d5-2c1e76a048db))
    (fp_line (start 0.2 -0.35) (end -0.3 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2b65ba8b-cc30-432d-abd1-ddc3919c1f09))
    (fp_line (start 0.2 0) (end 0.45 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 01519d04-eab0-4b4c-ba17-a066c093f336))
    (fp_line (start 0.2 0.35) (end 0.2 -0.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d1ce3733-97ac-4385-a8ba-daf2b764d6ba))
    (fp_line (start 0.9 -0.7) (end -0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e6ec4761-76cf-452f-a376-5ff18baea5be))
    (fp_line (start 0.9 0.7) (end 0.9 -0.7)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 12b28360-3e72-437e-8248-d0b9c3f5a49d))
    (pad "1" smd roundrect (at -1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D32-K)") (pinfunction "K") (pintype "passive") (tstamp 4374d7ef-38cf-4b75-b47e-353ab9f0fe94))
    (pad "2" smd roundrect (at 1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(D32-A)") (pinfunction "A") (pintype "passive") (tstamp 38a0a686-3343-484d-9de1-ab4d229b5bb6))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 546002fa-6d06-45e0-96e2-67c550b87504)
    (at 172.302855 15.967968 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/567f60ae-06cb-487f-a8ce-8f3c0f4702fd")
    (attr smd)
    (fp_text reference "R40" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 43ea17f2-16d8-44e9-93b5-e753baf941d4)
    )
    (fp_text value "47k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2107e373-3d6e-4084-b90b-80e85d751a32)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 239768ab-91aa-4af2-94d1-df2c9f29be8f)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9be71e8c-090d-4b5f-9a0f-5697621b8adb))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2c90ec2d-24ce-4b1a-861f-a1014c1cd189))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a2b74fc8-83ed-4663-8315-bdf374a33077))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 76f674aa-d5af-4b07-9a4d-17f9fc984c0c))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 67139c96-7367-44c2-9c07-d8fd89a50115))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a61e1e10-6392-4995-9074-f521c27d4f0a))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 601abb26-879c-4c51-a9e8-11316e4e9459))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp aa53f4e3-0f71-49e8-9eac-854d9c727a5f))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 05d94211-5aae-4d18-af34-86a3adc929eb))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 253534a2-8305-44fc-adee-d6b698e8d78c))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 102 "Net-(Q13-B)") (pintype "passive") (tstamp e4b89d2f-9259-4dbc-b194-0ed6a4e83714))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 108 "Net-(R40-Pad2)") (pintype "passive") (tstamp 63fa26ea-7069-44c6-8e35-cccc6ae7da99))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp 55a53e7d-35e1-40a7-a0a3-d2cb862b4b7d)
    (at 135 90.0375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/6fbd5aef-97a3-4a73-a4b4-b8be7bf399c8")
    (attr smd)
    (fp_text reference "C11" (at 0 1.68 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a5370b1b-d8ac-4182-b0e6-7cd3f2dbd92f)
    )
    (fp_text value ".1uF" (at 0 -1.68 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3716672b-0753-4d56-89da-7bde9ff68fbb)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp e4233311-4e35-465d-9e11-c661f6adc10f)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a1c18f32-7533-4690-9d7e-46dda8ad4c52))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7d328e14-75d0-4728-8afa-f284cb7e6201))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 83e15f2c-efa0-4465-9d5a-14ced5d23708))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e2e46d3d-a769-41d5-a13e-d1af61f05a8d))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 920cf73e-f3ef-45b5-9f18-e2ebfc1debc3))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1b6fe57e-9179-4f2a-a057-9354c3caa622))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0fa4cd4d-ceb3-4790-9fc9-008227f348a4))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c80b57b2-42f8-40fe-8b58-b0f5c2009a0f))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 109e2e3f-f6ba-4d5f-a618-faaa929e6fbd))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2cc72a6f-f3f4-431d-a563-0fa67229d778))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp 59e074c5-5f61-416f-b2ed-7859ee0fa617))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "-12V") (pintype "passive") (tstamp 99d25eee-2426-4738-9b7f-21f377c1cedb))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 58a67a0a-8871-4b7f-a57f-a0cf49767f19)
    (at 46.093 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/c5183d24-2684-4c18-9bd3-e1d7ebec0b53")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8f633376-e3db-479d-8219-8c60d4a5185c)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5275f67-c23c-4575-afce-2ad19378335f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp e715375f-fac3-4f70-a83a-2bee026ebb5f)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a80a4943-6c16-412e-8c3b-fc943f9c3b5b))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 14550b4b-4826-458b-a910-7f55b241efe3))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 05405abd-de36-4dd0-8f2a-ea050e25e259))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 75f222cc-ffa4-467f-b77a-96b30dd010bf))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 38ec7857-f1bd-4ab6-a458-78b0fadf2465))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6b4f1572-72ab-4f9f-a79e-026c3e3d4e07))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b1c2a435-cfb1-4150-9283-6ee466710aff))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 62eba6e2-b6bb-4ef1-baf6-ee8b34994aa4))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a5e3cb65-5d46-4485-8f5f-245cbb34c0a6))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 262731b6-55d2-4a3e-81d3-6eb275138c86))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 070aa15a-765d-4dad-8bf5-28f21129f0cd))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4ffe08f8-8e15-48df-afac-469e96282e09))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 75dde10e-1d7a-4043-9820-a51ecf3ef927))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp 4e34bfd0-2424-46ab-8db4-483bed68fe64))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "Net-(Q1-B)") (pinfunction "B") (pintype "passive") (tstamp 06fd7bef-b6a2-47ba-a8c8-a67d22d58d5f))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "Net-(D21-K)") (pinfunction "C") (pintype "passive") (tstamp 7fd4f006-0239-48d8-923f-d526b4311fcb))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 59d7e28c-fea4-4a6c-833d-2fc31d197191)
    (at 82.593 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/6635e795-5934-462e-a753-64d3eb6657bb")
    (attr smd)
    (fp_text reference "R14" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 74f00426-0939-48ff-b061-38aa722b96a5)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e3313d25-27ca-4de7-a023-08f5cb10e6bd)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 79818949-1eed-43ed-b94f-42792e3b911f)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 082d5743-eb81-476a-8af5-e62aacaf15a1))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8800f69d-7eda-495e-91d3-54ae22081f3a))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 22fafe67-903c-4f53-9b49-b87f64191277))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b521fbbc-bed4-4eaa-9075-83e29dfa8281))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp caf49e31-2991-4fca-8496-674874c6c42b))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f5565508-de8f-4c39-b774-e364860d70f7))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 03da8444-32db-4b9b-b287-a16eea9c8e7c))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a5f4fd42-16ad-441e-8cd8-b056e43b9a9b))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e5f7a02b-e61b-4970-8c88-50fa192ba0ff))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 32d31eb4-d1d2-4257-9832-38f037fd8be2))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 63 "Net-(Q4-B)") (pintype "passive") (tstamp b39a6a81-61b3-4486-8578-ff73d4bc3f96))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 10 "Net-(D4-A)") (pintype "passive") (tstamp 6f8261ef-e308-4cf2-b554-e7deca8f0a35))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_Socket" (layer "B.Cu")
    (tstamp 5bfd4074-8e42-4392-add8-7f975a134498)
    (at 103.12 17 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Johnson Counter ( 10 outputs )")
    (property "ki_keywords" "CNT CNT10")
    (path "/705687c8-56b2-4621-8cb4-9cfc96fa7822")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 76f6097b-b717-4e0f-b854-866814dfa600)
    )
    (fp_text value "4017" (at 3.81 -20.11) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 08618611-e724-4d18-88b8-1dc241fc6f60)
    )
    (fp_text user "${REFERENCE}" (at 3.81 -8.89) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 75486a38-5db6-469d-b6a8-fd33dfa9b805)
    )
    (fp_line (start -1.33 -19.17) (end 8.95 -19.17)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 29351964-bee3-4b10-99ac-177b2c874d1b))
    (fp_line (start -1.33 1.39) (end -1.33 -19.17)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ee52adc2-648c-43ee-b5ca-129382406969))
    (fp_line (start 1.16 -19.11) (end 6.46 -19.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5947d8a3-f20b-4b27-9b8b-3f04afe006b2))
    (fp_line (start 1.16 1.33) (end 1.16 -19.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 756265c0-1734-4316-81a5-e59a5c363c61))
    (fp_line (start 2.81 1.33) (end 1.16 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b6d3bf7f-9a98-4028-a713-29f6893d9c9c))
    (fp_line (start 6.46 -19.11) (end 6.46 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 918358f1-fdf7-457e-b248-761ad1462145))
    (fp_line (start 6.46 1.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5caf9192-22e8-4984-aea4-7f8555dec3e0))
    (fp_line (start 8.95 -19.17) (end 8.95 1.39)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8e9667ce-bc52-47a1-84a5-135e1d16481c))
    (fp_line (start 8.95 1.39) (end -1.33 1.39)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eb3bad39-9214-4334-8aeb-af4bd2d7eae1))
    (fp_arc (start 2.81 1.33) (mid 3.81 0.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e48df57e-38ba-4a6e-b8f0-1e715018770f))
    (fp_line (start -1.55 -19.4) (end 9.15 -19.4)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b0f1c047-2044-4e05-9a71-10d74dde0bf4))
    (fp_line (start -1.55 1.6) (end -1.55 -19.4)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c7fbfa0-180b-4032-ade7-bcf163647d24))
    (fp_line (start 9.15 -19.4) (end 9.15 1.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1fcd2702-97d8-41db-9395-d26f92184289))
    (fp_line (start 9.15 1.6) (end -1.55 1.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6dddf258-4a59-4b88-8aba-d62a909f7098))
    (fp_line (start -1.27 -19.11) (end 8.89 -19.11)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6183b0ba-6425-428d-97fa-f00de92e8cc3))
    (fp_line (start -1.27 1.33) (end -1.27 -19.11)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ed496121-d02a-4c56-b601-6f53312d9ef5))
    (fp_line (start 0.635 -19.05) (end 0.635 0.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c703023-54ff-4ed8-8704-9e268415105a))
    (fp_line (start 0.635 0.27) (end 1.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 34f78896-0e96-444f-8761-c7101dcc00c3))
    (fp_line (start 1.635 1.27) (end 6.985 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d9a170ab-2c63-4264-9209-e33a6466798c))
    (fp_line (start 6.985 -19.05) (end 0.635 -19.05)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a34f4762-fff4-454c-a7b6-af9a9463e793))
    (fp_line (start 6.985 1.27) (end 6.985 -19.05)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d3fdfd72-d7ab-4170-85f6-4fc8ea66f604))
    (fp_line (start 8.89 -19.11) (end 8.89 1.33)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4fd0eea3-ddf9-42e8-a0f9-e16e6c828aac))
    (fp_line (start 8.89 1.33) (end -1.27 1.33)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bcd8d57d-f0f1-4b0e-a5a0-4020a388207a))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D6-A)") (pinfunction "Q5") (pintype "output") (tstamp 88c177c8-5eb4-4ef3-b3c7-3815209a39e9))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-A)") (pinfunction "Q1") (pintype "output") (tstamp ee48c337-e018-4e14-8f83-7d3a2ec33430))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "Q0") (pintype "output") (tstamp 0cfef230-bfc5-4234-96fd-7e3181316f30))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "Q2") (pintype "output") (tstamp c544ca38-625f-4d78-a0bf-f026ae30a828))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D7-A)") (pinfunction "Q6") (pintype "output") (tstamp a9b7ce35-6109-4de6-b054-084d20081a8b))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D8-A)") (pinfunction "Q7") (pintype "output") (tstamp f42b381d-b6b2-42a6-9b82-c961c8aec99e))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-A)") (pinfunction "Q3") (pintype "output") (tstamp 888c175e-96f5-4d1a-bac2-60ea05440882))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 33e3ba93-f991-47ec-992b-8fa1992e7639))
    (pad "9" thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D9-A)") (pinfunction "Q8") (pintype "output") (tstamp d92022f1-8691-438f-9295-e7464585c7fa))
    (pad "10" thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D5-A)") (pinfunction "Q4") (pintype "output") (tstamp 2a86503a-1f8b-498a-9b62-60c61f4d6611))
    (pad "11" thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D10-A)") (pinfunction "Q9") (pintype "output") (tstamp c6bd1ae8-d5a2-4548-8697-0d4b0a6617ff))
    (pad "12" thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(U1-Cout-Pad12)") (pinfunction "Cout") (pintype "output+no_connect") (tstamp 3d262ed6-429d-4293-bc15-f0fea6dc0b21))
    (pad "13" thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(D34-K)") (pinfunction "CKEN") (pintype "input") (tstamp 15d783ea-04ef-47db-a9ba-5a9145402332))
    (pad "14" thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(SW14-B)") (pinfunction "CLK") (pintype "input") (tstamp b6ef4c79-f5f3-43af-a4ca-52418bd55ef9))
    (pad "15" thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(U1-Reset)") (pinfunction "Reset") (pintype "input") (tstamp f74b27c5-20c6-4269-ac8b-12a102f9ec6e))
    (pad "16" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "+12V") (pinfunction "VDD") (pintype "power_in") (tstamp 9f2bda8f-9285-45e1-a602-781152fd1914))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 5d523ee2-0a56-47df-8494-386df23c7382)
    (at 88.093 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/f997c2e6-eb30-4218-828f-505e274d346d")
    (attr smd)
    (fp_text reference "D14" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b7d3e5f1-3f3e-4c43-bea5-6027fd864873)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 66baca37-42e1-4a1c-9a89-cb9d343e6148)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5215baa-3808-443f-a24c-512e5739ce76)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2b9bfdba-1dba-4fd6-9092-88212c4c6581))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a0058058-de16-4a55-89b8-d545aa3b771a))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5117a745-49ff-4a12-8730-52a0c3c5c077))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b9563d0d-36d4-4276-9741-bd506a00bf27))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5df31f36-3b21-47bd-ab6b-baccd639ff1a))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9fb33099-3d5f-44dd-a1af-1d08a26e83ab))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ddd7bce0-4422-436a-8e87-4d0392399515))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 11ef7f22-ff79-4413-a7ec-b76719b93ec9))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bcc36044-6880-42ea-9000-7b36e2a5af0f))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c68e9417-5b91-4557-911d-f026eac51c1a))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ce8b41c7-4ea6-4663-b8a9-d04ebf318783))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a56a7cdc-9bf1-4cc8-a713-5753626dfe53))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ba4dec95-be79-497a-93b2-d3b5b2c5b75a))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 685428d6-77d6-4255-b21d-e8aab2a82329))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8970e66e-47e4-4ad8-910d-3bb5d74b338c))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 044f84f8-a649-43ef-acfb-e1e20aad740b))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ff679540-80b9-422a-9b6a-ebb83edfd774))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c6255fac-fef6-4d0c-9d94-2e8c2365253c))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 17dcae87-e1ed-4ecd-baf3-09986a4e4321))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 26 "Net-(D14-A)") (pinfunction "A") (pintype "passive") (tstamp c3bfa208-3ed5-49e5-b705-6f9c0ec42e96))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 610f2b0d-9062-49d2-9c7c-1039c0ea211e)
    (at 138.093 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/32e9d9e6-c353-4ec4-ae51-d9cfc9f519f9")
    (attr smd)
    (fp_text reference "D18" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4fd2df2e-6e05-4530-870b-962f93112e15)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1649adfd-d52c-4fd3-845e-37bf936a457d)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 879674a8-66c9-4678-986a-8c02c4fa7a6a)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3eacd138-e17c-4848-80dc-c512ff1befd6))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp af4aed0b-0207-4a65-9e52-b59c14546446))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1bfb0109-bde5-403d-a90c-1b5af6c3c436))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a3dca42c-c8b4-457f-b3e4-0a5c174ac7a9))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e118def3-011e-42a3-8414-6c321fd1aec9))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f66f01e9-c680-4740-822e-62fa53ae47a5))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d460a69a-b4c4-4a41-9edd-3be162c4d1a4))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6dff3c07-2916-4477-9f94-07e7006aa4a2))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6050f229-74bb-4abb-94d1-31b703f21f61))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ffee9570-2a25-4c60-a8da-32471ae65c39))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ed8c82a8-f4d8-4179-b528-ae0df8ee693f))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4ad39c75-2c3d-4c92-9d95-d94295e7b198))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8fe78ee6-b58e-46d2-8f90-b58b38d77dae))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 62427d27-ea3d-49ee-8fd5-2b497a4adb30))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 021b1a50-0ca3-4e1e-84d5-6802f46373f4))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 213032fb-a7b6-4260-a880-5fab915ee00a))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eeddda10-fb98-4b2a-bf09-acbaa02541ed))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 16bb3256-1678-4d86-b0c0-86d05abb2666))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 06311c94-aac1-45db-ab7c-bc5ce2bd9852))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 30 "Net-(D18-A)") (pinfunction "A") (pintype "passive") (tstamp 6e7aa3a7-7070-46e0-b82e-f664b8d22c77))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 647dedc0-0f13-48d9-98fa-218fe5f9f7e8)
    (at 113.093 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/708a44f9-8839-4a4c-b06a-cf9847eb9ba1")
    (attr smd)
    (fp_text reference "D16" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 43503ace-3694-4f6d-98cc-60d994c323a6)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d6d53728-3c0e-4c84-b1f8-7a5a92a05fe0)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp db7c011f-cc9b-42b6-b384-24b85713e310)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b8817eaa-9b26-46a9-bf8e-8bfc67b4ceb3))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d2f3663f-42d3-487f-bef9-8b1e4dac43a3))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 407985da-26e4-4037-9f27-5b1b719d472e))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a966a062-0cc5-4833-8bed-8ce61e2dea5d))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp cc1c6daa-7263-4b2d-abf7-63f052c46134))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 59a04c27-b74a-45d2-a46b-c10e04bfb0a8))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f93193f1-3376-4865-ac7d-efa9290aa204))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 64aed797-7d4f-4205-9290-0c1e5023794e))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7f77f307-f847-482f-9e33-1bda6dd63298))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp be71df5c-aac5-46ae-b097-dfe8614d5d71))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 74a89b48-8a80-481b-9109-f691967d7aba))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fdc82fe3-7888-49af-9aba-18b368fee749))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3f3dc2ce-48f2-412c-9b9f-e1fe8da30a42))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 90199200-29b9-4d3c-99d6-72a97459a125))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7d0d1416-8f61-4d4e-ac85-ddfb2f65cd25))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5c9559d3-cb34-4095-8dc3-ce260c2e0046))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 769d1e9a-2f79-427a-bffb-1b2d34bfd124))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d4e3c39c-5bcb-4810-b97a-18e990aa0eed))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp a2807ea9-3303-4eb7-b7cf-ba10a01cb630))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 28 "Net-(D16-A)") (pinfunction "A") (pintype "passive") (tstamp 84d6da14-d99a-4108-b88c-38d82e9d81cc))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 67c8492a-6d25-4aa1-8f62-5e235852d61a)
    (at 152.5 99.75 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/277c77b4-af86-4ee3-8703-b9dba6ca4b47")
    (attr smd)
    (fp_text reference "R29" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c2e006df-7a84-4e86-9471-6963eb1cabce)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5bd4e5d0-dd47-4c1c-981a-be4986b875f9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 5cbf6012-a44b-4cff-bc48-e006571efcc8)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0ff3eb0b-905c-4693-9aa2-70b5a63b62e4))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4f46b674-b389-4afd-963d-c2f66f0426cd))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c333c386-6a9b-4864-9b4b-8a819d88af66))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8964fa9c-aec4-4a1d-83ef-511854ebfe95))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ee13a0a7-0278-4f19-81c0-ceae5765bc73))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b8b21c46-7683-4360-b571-9048bb50e779))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4d689a44-05fc-44ec-9329-96fac98a79f8))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp db57a64c-ca6e-453b-82e0-a38e875ce004))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0a3ae062-d6c1-47c9-8897-3e0e28dc99de))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 699feb6a-bb42-4b03-b2d2-396e32c9eb30))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 4adaacfd-03e4-4597-8fa5-02b0ede6ef67))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 82 "Net-(U3A-+)") (pintype "passive") (tstamp 8ef7f784-01cf-46fd-ba0d-697aa8661b3c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp 6b87a48b-29ff-419c-88c8-33f7f5c8e518)
    (at 168.25 99 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (path "/9e9e0b2b-5026-43dc-9c1b-8197d4f88035")
    (attr through_hole)
    (fp_text reference "Opt1" (at 0 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b85c16f3-fc5b-493e-9115-f098a4b10a2a)
    )
    (fp_text value "Normal to IDC 16?" (at 0 -2.33) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eead7fcc-efec-4e51-9408-4a243252680d)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e95e91d-6b2a-47c9-87d0-34a8de21d1eb)
    )
    (fp_line (start -1.33 -1.33) (end 1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0fc68874-c5c4-41cb-8ac8-66b012aeb517))
    (fp_line (start -1.33 -1.27) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0eb09b7b-832d-446b-98d2-173fc7a3e5c7))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7dade1a7-de50-4e02-a5ce-d04c0038e9de))
    (fp_line (start -1.33 0) (end -1.33 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e29ff61a-d7a1-4112-88b1-098d18b5c368))
    (fp_line (start -1.33 1.33) (end 0 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d1f0c7c5-7cd4-4dc6-a054-f1c169d6aa80))
    (fp_line (start 1.33 -1.27) (end 1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 81c02bb2-56fc-4662-9dc2-6147cff30143))
    (fp_line (start -1.8 -1.8) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 573a0bc1-dcf1-482d-a8ef-42d55738cf71))
    (fp_line (start -1.8 1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5b97a359-469e-46a8-88e4-d08f0a760563))
    (fp_line (start 1.8 -1.8) (end 1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2ec9c0b7-a09e-40c9-ac1a-a6c262716058))
    (fp_line (start 1.8 1.8) (end -1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b708b3b0-7535-4a7f-820f-a62ef199a369))
    (fp_line (start -1.27 -1.27) (end -1.27 0.635)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 900c16fd-f304-40a9-9973-530f76351227))
    (fp_line (start -1.27 0.635) (end -0.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 513d819f-5298-451d-9529-77412ce88ff2))
    (fp_line (start -0.635 1.27) (end 1.27 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f7c1457c-1c2b-4804-bf1e-a2d62336050a))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9389b4b0-4571-4094-8329-ce17989387d2))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 231a2cf5-a639-46d6-a94b-9217d080a020))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(J4-PadTN)") (pinfunction "1") (pintype "passive") (tstamp c370a58c-2d42-40f5-a672-d1b8869d4ac0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 7328431f-80fa-4dae-90ab-4f9ac4a43f64)
    (at 57.593 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/e5dff7b4-a9a1-47a8-93a6-7e8a24efec39")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0b9a39ee-d056-48a4-a343-267b396e496e)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 995b5802-57f8-4123-bbb9-8b654c28e219)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 3621c3a9-0d2e-4042-b227-6e2721868df2)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 62229d0d-b531-4879-8754-e4011558233d))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e8d69798-4fde-49ea-8fb4-043bd1b15c7c))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 32cbb4a9-d0ec-4a06-a1ee-8f038b14ff58))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 52de32d1-5cbd-44ff-a377-aa74c8da0496))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2970f80f-a55b-4648-8b7f-b34eb7f3b1d2))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3c6f0981-aa91-4a89-bcd7-6a412bdf2436))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1cb01e26-e1ba-44b2-ba98-816408ae0944))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d705ab49-7018-46ef-b4c3-d3526153b6eb))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 45daf79e-96bc-4956-8b95-fe36fc2fee13))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6a5ce6a4-4188-4ef3-94b1-5ecdfe142fc8))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 59 "Net-(Q2-B)") (pintype "passive") (tstamp 6e7d6bd4-cb94-4984-a288-913b7861120e))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 6 "Net-(D2-A)") (pintype "passive") (tstamp 2919fed2-7263-40f5-9893-c13ebeb7c982))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 7428eaba-6d3b-426d-8cb4-2d00ba3bb2dc)
    (at 51 25.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/ca7daf9a-7768-4eb4-9559-57d529227923")
    (attr smd)
    (fp_text reference "R3" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bb519ad0-eb71-4a3f-8fe4-f0c7c16b75f7)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bc227b5e-e9e0-4c86-9aff-f19c73ac86c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 8ea5b2b6-43d6-4264-acb2-557198703f6f)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4154ee7c-3138-4f17-8e61-d87d23af7a28))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6f6db291-20b7-48f5-83e2-f84b7ae72353))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2d52933a-aee4-4513-b37c-fa50af992316))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ca203f02-d502-4964-bbc5-69ba36fd8f3a))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d2ad3444-48b7-494f-8488-c2c3cda2db73))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6d62a1c4-fa41-40b1-a21c-2d13f5bbbac1))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d3d60b22-3d2f-47cb-bea0-8f9e376e2b90))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9cf1f295-b440-4d72-84cc-45ab7ab06107))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 497872e3-0ec0-4fca-b2cd-56e469fc17e6))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9d451fba-8d36-4f8f-b7b7-cf8d602f655d))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 57 "Net-(R25-Pad2)") (pintype "passive") (tstamp e122aaab-7543-46c0-94f7-8bc9f966fe1c))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 87 "Net-(U2B-+)") (pintype "passive") (tstamp 0a3f6e7b-70c2-47b8-a5b9-dc1f19bb3d09))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 79866c03-127d-44dc-9163-b94a7496c2e1)
    (at 65 15.5 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/3e795fb8-eead-4b9b-9c17-59e079172ed3")
    (attr smd)
    (fp_text reference "R9" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e2f4ced-6841-4e9c-a6b8-a59aa6250626)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1df3937c-ee0f-4d27-9409-27e4fd31f68b)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a62efd73-3d69-4cd9-8af5-313e6f5624e7)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2f39e950-da0e-4720-99e9-e6500fd7b547))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 926f1c15-d0fe-497b-b194-01b4deae851a))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp cdf9651a-f489-48e1-87b0-187bc30a9643))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 181ce5fd-9045-49dd-ad03-ac41df3b00fa))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 862d1227-ad87-4b4f-a159-d54b1cc4ec98))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c7c532fb-7e50-4759-b472-8e2c0c96f076))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8775e702-2308-42f1-9019-e417964597d9))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b500c4eb-f872-45d8-b9d5-eb2361590fc3))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d0e7acb4-3c03-4264-ad4b-855d956b1e1e))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f153bb0a-6a0b-44ab-a4ae-09bb1505737e))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 625704da-95a5-4f73-b5ff-895742dda8df))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 73 "Net-(D37-A)") (pintype "passive") (tstamp d718a87e-acba-4a54-b087-4cc86149f050))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 7ad4ad89-851f-4b19-a3ae-149a107ab24e)
    (at 95.093 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/8a421989-81db-48c9-82fa-c9802a4fd719")
    (attr smd)
    (fp_text reference "R15" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5e26fa5a-b46c-4d61-a907-78dba821467c)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e50f7f49-ed39-426a-80e1-712647f5b559)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 4ca2c05a-744e-42ea-b5f3-367c0cae7d85)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 78c326dd-75c2-4b2f-98b6-853f82e1416b))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ecaacae5-1ff4-4f27-ae20-d2c15add6876))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 962d9409-3571-42c6-a28a-e1efe3e970b3))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c8f43053-8402-4145-86bf-0f1d49e6470e))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp aba6da09-1e6a-413f-b34d-01cb60ba411f))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 64889c82-c961-4eac-9da4-76f194a678a8))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b258d276-5cea-4721-a5df-3461e3a52cc2))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e2bbba6b-aee2-4fc9-ae0e-db877e35a823))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3ef81095-195d-4aef-b6a9-4f4ab6402f94))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6db39b25-d079-4471-942c-cb73cca25176))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 65 "Net-(Q5-B)") (pintype "passive") (tstamp c895a0a1-ece6-4231-bd6c-9a5a9015064e))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "Net-(D5-A)") (pintype "passive") (tstamp bdf802db-b909-4b36-bafa-3b9811998853))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp 7b59c8ed-9688-48dd-9943-ff3e681e47d0)
    (at 168.05 72.25)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/5d34b4be-69f7-4241-8dfc-3f813e8db163")
    (attr smd)
    (fp_text reference "R24" (at 0 1.82) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp becb6dd9-5b3b-4416-99ec-2eed07b66eba)
    )
    (fp_text value "1k" (at 0 -1.82) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a4ac0eb4-b095-447f-94b1-b0c25978336a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp afcb1e78-4c49-4f9d-8afe-9a2e62221e9e)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp defc2741-066c-4c9c-aaf8-d62f72f3e0cf))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f7d67394-00c7-4d29-b140-2dfacf86b02a))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f8b66a38-5b3b-4b6e-8da4-371f114dcafc))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 178be03b-88c6-4ffa-b188-e14f5fc9485f))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9262db6a-b38a-496b-bb46-5789d248f6ed))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8eb79bb6-597c-4980-b87c-8557e1e627c2))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c5e97167-b69c-476f-9b7c-4ca3fc66f612))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 81a5a6a9-23c7-411c-91d2-eefe9b49685b))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c8aed3c-d55a-466b-ada9-4f0c9a2ff262))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1eadb8e6-107d-4f10-a843-85767e37341f))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 86 "Net-(D37-K)") (pintype "passive") (tstamp c43be2f4-73af-4755-aae5-da639c72f77b))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 91 "CLK_OUT") (pintype "passive") (tstamp 74caa798-2645-4bd8-bdb0-75551395f37b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 832a625c-4480-4479-836d-9dd21a31e18d)
    (at 61.25 15.5 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/f7250d8b-a366-45b0-a345-a8e3e95fd641")
    (attr smd)
    (fp_text reference "R21" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f04cbf9-17cd-497c-9e56-5e1dc8bfe149)
    )
    (fp_text value "47k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fb8a70e9-4864-413d-9c18-d65c757c8aee)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a405c75f-44a8-4818-8bb5-65efaa345eac)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0314b462-58ea-4fda-9cad-3452da1d42dc))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a6edab01-df88-4d3f-9fdb-596841698fe2))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2b19c366-9509-454a-b328-f40523734006))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3107b567-e435-48d4-a888-fc9ad5129c63))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ac9c26af-5246-438d-ba0f-e1572a0afa1b))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2c50a1e6-00d3-4fa3-8793-1cc6a7bc7ff6))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f0be3210-1f45-4de7-bc51-3a2f9d138f79))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 039e7167-d5a8-4ccd-916b-fbcd2337d04a))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 69576eb0-7ed8-4cbd-9d6f-fb6106d81d75))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 718be3e0-00f0-4f39-8475-a6c797ddc3e7))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp f8e04cc9-44b6-434a-9820-8ae50d9a747d))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "Net-(U2C--)") (pintype "passive") (tstamp d820067a-10a8-443c-b97f-d655a5b34dce))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 83dd7237-9931-4d1e-91d9-9975e31216af)
    (at 143.25 83)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/854cc8d8-4dde-487f-b82c-f9bc62627a1e")
    (attr smd)
    (fp_text reference "R34" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2ee182d9-b855-4b0b-8599-9561305193d1)
    )
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 38139076-324d-4ecc-93b1-725d903acf59)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 0172d0f5-3859-48d8-ba61-17dc49736c12)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23103ef9-99f5-4d61-9f0e-247383b7a85f))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8ee0ee2-f951-44dc-bf68-2a949035da9c))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp eae4f05a-75fd-4022-a0fb-f2d54ed55b19))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp af9c117a-17dd-46ed-96ce-c307f8a13c5c))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 025ce340-8a5d-44df-80a6-7f3d2350d587))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5525183b-4c94-4876-8ef2-b33a0e08abae))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ebbfe1b8-d71a-47b4-9f1d-90a245e5ba39))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f50b6bea-5aa1-4462-b3c3-3ab9f28399fa))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 581c1801-4a2e-4332-b7eb-1625a29b340b))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a3cb0004-4a37-4882-aa2c-5308b55a7985))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 106 "+12V") (pintype "passive") (tstamp f57438cf-dbc9-49ac-9c60-24014ed01320))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 98 "Net-(U3A--)") (pintype "passive") (tstamp 86805b5b-d18f-431c-8143-24ef24bab26f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 851b7d49-e7da-4283-b57e-a050bd428472)
    (at 64 37.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/392667a3-1d73-4ab9-b765-9383508e6918")
    (attr smd)
    (fp_text reference "R27" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b4a7762e-735d-4a25-a7ac-e8baea7b2f73)
    )
    (fp_text value "100k*" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7a5f0d35-e0af-414a-ae84-cf0046f44c34)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 54e8ead1-42dd-4d4f-9495-ca11e9865600)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a7c47f6c-8a2f-489e-b3b1-fec7fadf20a2))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e37c4d6a-dac3-4298-acf5-0d41f7fdb268))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5ccfb246-20fb-44ad-99f9-fde5f75afa2a))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0ffee3d3-113d-4e7d-bd89-dacb62afe2d6))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp aa7d4fc8-c673-42ee-a851-175fc516bb39))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9c29dc82-537f-4310-9ad1-c6f6a6e59a73))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8978cb7b-2051-4e9a-b7f6-7b9c67b17a96))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d7d600db-92c9-480e-88c1-bb8ed21b4d66))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d0f942b3-b5f2-4524-b214-1a589f50e949))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp acdf3bbb-adbf-4bda-8f9c-afac75f0d856))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp a4e06525-4b78-4edf-a21d-5fdf4a5534e4))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 76 "Net-(U2A--)") (pintype "passive") (tstamp 118fcafc-2c37-4a26-9032-ed64b97a927c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 8571f7f4-a82f-4e8c-b097-afbd679200d2)
    (at 155.7 77.75 -90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/42349f29-92fd-4759-b7d2-ddb86ce4d569")
    (attr smd)
    (fp_text reference "Q15" (at 0 2.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 059c2218-9208-4c8f-ad27-e8acba4d0648)
    )
    (fp_text value "BC558" (at 0 -2.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1450c584-2fc6-403d-80e4-b06c8ac527cf)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 59b9988d-ef77-4dc7-81d3-cad3d57658e6)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 60842536-342e-41eb-ab92-b2651c58e0ad))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 51892156-dda6-4bcc-9293-a315c4e62ec4))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 65077ae9-98f3-43fd-9ee9-edb81838a2e0))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b93f1074-1333-44e3-8607-54ba489e6da7))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 52d1a06f-f018-427d-89be-78e92a859100))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b67de459-adb0-472a-9774-957357dd485a))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c2ecc60a-3dd6-4273-b7a8-4e2d097ea72a))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 845c2ff3-e3dd-4da8-9197-b1446d99222b))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 25824ee2-b45a-43e3-8a60-5219899e4674))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 585373a9-ccb7-439d-a434-da07076892f2))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 109f2828-b168-4c17-acf7-8387dd8ac4c8))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3ed4f05f-dfa3-497b-bd55-486fb80d4ea9))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 516a1e2b-7ffd-475f-a270-873af8c0704c))
    (pad "1" smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(Q12-C)") (pinfunction "C") (pintype "passive") (tstamp fce63051-bf3a-438a-9d93-49ddf59278f6))
    (pad "2" smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "Net-(Q13-B)") (pinfunction "B") (pintype "input") (tstamp 51929046-8a2d-4c65-b084-e7cd1a79ba1e))
    (pad "3" smd rect (at 1.5 0 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "Net-(Q12-E)") (pinfunction "E") (pintype "passive") (tstamp 85a3dc84-22e8-4ad9-bb83-0cd27994ce2c))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 8616fe63-e3e4-4b90-81e2-deda7534ea32)
    (at 125.593 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/235f9e7b-c925-424f-8ec6-3deb198121b0")
    (attr smd)
    (fp_text reference "D17" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bcf79e1b-feed-404d-b0b5-b3a281d40da2)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3b45e23a-e52d-4de5-8c12-df537a9b31be)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ccf28835-440e-4405-8df6-4561df67c8df)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 62243ddd-924e-4d5b-a0b0-17b0e93f5049))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d5446761-a115-4930-b5ce-faa3ad2798ca))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8a204a0a-40f6-4d3d-9e53-881c08ee32b7))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp fda884f3-4790-4061-983e-71535b39bb33))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 573d2825-ef7b-4421-9a44-cdfca1875887))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b2350f2d-6911-4b77-adfc-48e0b4db8d13))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 194f6721-5b92-44f4-b51f-130060de8e67))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bedf0ae1-b0c4-4b9e-99e6-066a89611788))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 69c15f0a-0064-48cd-b490-8c4f29a797d3))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7a908dcd-7ea3-4366-af89-55833c027f50))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e2166028-7929-4ad9-ba18-e60055c622f1))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0efc8f25-3540-44a2-b208-a65a705fecc0))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 38ca0441-8ecc-4121-8ed8-f2679e99a8b5))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9ddfc048-85f9-4ec3-a9e9-3b177fb91c38))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 81c3a540-6b02-494b-bb04-810a5482c8da))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a888729f-f75c-41b2-a7e2-6aba7e3ed00c))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 237e5a85-86c6-41eb-acc8-f2006bd4b2f4))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 15303053-bc1f-4deb-bf08-e00d3815bc07))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 1d71ab34-dfeb-4116-8727-2b067354adc9))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 29 "Net-(D17-A)") (pinfunction "A") (pintype "passive") (tstamp 80e3ce84-36c6-4eeb-b5ae-ffb0a1609f39))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 8786cc6c-fc7d-4e12-8f57-d36fea98f622)
    (at 63 20 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/2bb75604-92ee-4f71-ad6a-a7699c82bf3c")
    (attr smd)
    (fp_text reference "R49" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2ead8b4d-d669-4a59-a191-9de6a0f6efc9)
    )
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d0747bc4-dbd6-4e12-925c-3d7064c3bd96)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2490ce98-61a1-4b48-9dcb-c23a9d9896a0)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 70fb0b09-c1d6-4f66-a08c-d630765d15ab))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0cf11cb7-2dec-4286-9ec0-f3e048d73e09))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4e7e91e9-e305-4e12-8b46-8f8818c6386b))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a1c9656b-674f-4d30-8083-1729dd5d0500))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 69ba4c1e-1b18-4d89-8af5-53c561a5afd3))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b9baf2c8-fc30-47dd-80be-3be59b642e67))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 469aede3-4e31-422e-a2ed-d273ac1e79b9))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3b1fabc5-5933-4168-aa88-34d7e09f5f90))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 98539a7b-fb05-4c21-8a28-4638ae288a2a))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2f25ec0c-b320-4ccd-ab4c-fbea05b47f95))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 48 "GND") (pintype "passive") (tstamp 4fe189d6-9c12-4623-a75f-936363baa9c5))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 51 "Net-(D35-K)") (pintype "passive") (tstamp 73c77e29-968f-439f-9a99-3c05280d8f68))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 880280ff-2707-4cfc-bfd8-8f12b7feb59a)
    (at 75.593 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/a30bbb0c-fc8b-491b-8846-a6660a224cb9")
    (attr smd)
    (fp_text reference "D13" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9ffa7f01-8702-4baa-9e6b-5a82ad795cda)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8ebeb970-bc7a-477b-b8d9-6d75e74d2060)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 02a81d9a-7699-439a-b3c6-dcb0098a2eba)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d53e1a4c-cfeb-4cca-9e39-9ae73aa111ca))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp be3de5d5-7f0a-4529-8797-0581914efbe2))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e77d6671-4c01-4dc5-85e5-416c1d91b865))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c0acf679-1377-426c-a00e-4d5801060aab))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3ecbafcf-a14f-4ca1-9306-94efa150be45))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7478e3b4-972c-45bd-8ec5-d19318cb59b2))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4ac86a9d-1605-4214-9629-c3a918f7bd6b))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1575f2a1-33e8-482e-8feb-51f2628aa7ab))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 03b23197-556b-4089-938d-69ea812d961f))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ee73cd62-7db9-4f3a-a07a-9acd2848602f))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5e89106e-b10c-48e2-a489-41ef11f593b1))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f7e98cd-99f3-48b4-a9a0-3092a6ad7c4a))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2ab4bd05-60df-4c98-809f-e4eadc484422))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c511db57-b3c2-4291-accf-859eab2f3b6b))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 095ed21a-e33f-433b-a76f-f3167f606f05))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cc934552-6a12-45c9-a3de-13f3f191cf0a))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c996bf82-a1a5-42b4-b743-64c427a65cfe))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5ca5695e-00a0-4362-9a93-48313772b82e))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp cdd4458d-50af-4e56-bf06-8dfeacf6ab52))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 25 "Net-(D13-A)") (pinfunction "A") (pintype "passive") (tstamp 6a80b6d1-fb24-4c18-800f-349ef3978dc5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp 88b42e4f-f51e-4951-8902-949980f498e5)
    (at 31.75 98.425 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/14f848bf-80ca-4a9f-96a5-4b967b593461")
    (attr smd)
    (fp_text reference "R5" (at 0 1.82) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8136fd09-a8a5-4b06-b099-87b18415af69)
    )
    (fp_text value "1k" (at 0 -1.82) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7c8410d6-a98c-4724-b88f-72f7ce8e334b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 5fef70e8-a3e4-4d8a-bb41-53818a765957)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2b54647d-2b78-45a3-ba22-4766c977a3f6))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 13f4c5da-04ba-45c7-a7ea-7c46acf04ac5))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d2fbcfea-dfa7-463c-aec5-a10b1620c02f))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a206601b-4a45-4f74-b21b-e7a5cc59517b))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ec1654ef-60b2-47b6-9902-1e79c7af098c))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp afd0964f-c474-482e-80b4-8488751114b8))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d96f88a4-e22c-4a15-91e7-758ac98a3027))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ac53f3c5-440d-4737-88b2-051b25109695))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 84e78f67-e59e-4856-bcb7-b35fe611f0e3))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f59487d-fbb6-4590-8ac9-6b612692754d))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 60 "Net-(C2-Pad1)") (pintype "passive") (tstamp c07f4893-5ff8-4c9f-aef4-f3e2d6b98d1d))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 83 "RESET_IN") (pintype "passive") (tstamp aff2990e-d7f9-4d7b-98ca-f601cdbe2998))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 8b781065-3e4b-43a4-8f8d-79a5560b0e1e)
    (at 147.5 85.25 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/b70cc4c3-6da7-45d7-b498-24e65121db21")
    (attr smd)
    (fp_text reference "R35" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 81b9c367-5c58-4759-8cab-5f52fdb780d0)
    )
    (fp_text value "10k?" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fa5464ac-1715-4840-a20a-2fb720a53ef4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 9130e24b-1448-4118-b8cc-6d027dfffb7b)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6d2ce08a-bcd1-4440-ad8e-5f252d59526e))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d2a46c5e-d29b-4755-adc1-c710ebde112f))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 272fe5a5-6497-45da-82a2-4a016b91c861))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7c6601df-df57-4fb7-86bf-4c9680a60ca2))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 23219ebb-12d5-49cd-b11b-030faa7ed943))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3d6dec6b-cd65-412a-82cc-089d22c28f33))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a2b2d25a-fe1c-4b41-b6c9-fdbb50821498))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 066db8cc-c563-4452-b78d-651b0915de0b))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 112070b1-eb6b-4228-b5b1-39b05b0344a5))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c9d8330-23e7-494c-ac32-7edf574813e2))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp 77e66d7a-42a3-4a97-8155-b95a306b6f3f))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 98 "Net-(U3A--)") (pintype "passive") (tstamp 816d998a-7ffb-4e2f-a819-e251fc432715))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 8b96d3cc-a068-4880-beeb-3a2de1c08243)
    (at 51.75 18.5 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/123bbc67-9a03-4a85-a7ed-f657856c4f8b")
    (attr smd)
    (fp_text reference "D35" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 52af69fa-fdb0-4387-9f71-bf8055611d94)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e042fed0-88cf-438b-9f55-e361ececc2c2)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6f4128d3-02ca-4e7a-ba34-84a7a5bed832)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6e17f972-6411-4973-8c30-078190174a96))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e609185f-953f-439e-9470-2186712bcbf3))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4977e54b-0a5d-4321-9aaa-60502d97c3a1))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3a924448-6ca2-4dd2-a923-33b4c0249fab))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 431ebdfe-3d51-4827-aba7-7690d5954317))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d61a39c9-197e-4e11-a1cc-740f8210a239))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1425ff45-ec9f-486f-b218-850289f3184c))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9bd3a46f-ed48-4c21-b583-4123d79584f9))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 58019f09-2547-4855-a3f9-f74321489c78))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ac799f0b-3745-415c-98b5-34ed4ff740d1))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d75af2ae-5292-4782-91ff-ffca88fa5c20))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c60fca6a-ba91-4791-81b2-b8c640fb1f18))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp aef5899e-ccfe-407f-a4d7-9e5e7e2b983b))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e2ac04ad-76d8-470e-b6e8-f0147f3e7bf8))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9f7fdc4d-7c5d-48f3-89a2-927758106090))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4454353d-4386-4630-bbf4-24b0c21f3378))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d70ce99d-7b0d-44a8-b244-2d860f029580))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8889aabc-4bdb-40f6-a5f8-deb8fdb978fe))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 51 "Net-(D35-K)") (pinfunction "K") (pintype "passive") (tstamp fbad1c46-2b35-4332-a8b8-24c4bffd6835))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 69 "Net-(D35-A)") (pinfunction "A") (pintype "passive") (tstamp d2e1f6bf-00b8-4310-bd1d-ac7c6d97b309))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 8d0e9504-0de1-4d0e-a712-f83de62585f6)
    (at 133.593 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/8fdef195-c528-49c3-a542-8050a0f76e00")
    (attr smd)
    (fp_text reference "Q8" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 450963fd-1409-4a99-9e5f-7419d84f1891)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b56f7b64-4094-489b-ac74-aa5271faef49)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp dfa3351c-36b0-4afb-9278-2c551bfc3c59)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b988e2af-1512-434e-9919-74f777800880))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e3c025ef-f7c4-4653-a85f-f94bf20b0623))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 50bfbc5d-512f-4d2a-bf82-633f1cf7f436))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a28e320b-3025-437d-9bea-f22c38eaf3ef))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4f9fe3dd-d97c-4bee-9f80-c182c55ed09d))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 892fbc80-44b4-4182-beb6-bdcf8db1f289))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7941aec4-bfde-4deb-bb7d-d88c6baf8006))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d0e2bc87-69e3-47ab-a506-36047f4511f6))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4495ab3f-2432-431e-b71b-5be400b516f3))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 989f261c-e3ca-4ffd-9c3f-498c04e513fb))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6d149b4a-8606-4909-a35d-7f27b53f9de4))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 97ff682f-2d95-4e78-bed5-ad15b7d30f5d))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 08b86171-2e5f-4d96-916f-97f32ba46f2d))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp 3842907e-7836-4cbd-a827-4b7afe983b83))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "Net-(Q8-B)") (pinfunction "B") (pintype "passive") (tstamp 7ee8eb9d-03ae-4897-945c-614629f0209e))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "Net-(D28-K)") (pinfunction "C") (pintype "passive") (tstamp 9ac4780f-d622-4f69-b49b-c905c42b1ca4))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 8dfa1edd-9a16-4125-b937-c7630b3581e1)
    (at 150.593 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/594b08bd-44c4-4721-9d5b-c10e5b7a2c29")
    (attr smd)
    (fp_text reference "D19" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6dc83e06-841a-4cbe-85f7-75781ff764e2)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eacafdeb-ad7f-47a8-b4cf-ac11da8ced1f)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d44ee61a-222f-4f47-b59e-82ce70d242bc)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 738930e6-fb99-44b2-adb9-573d7d693ad7))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1fc82867-591b-48a1-9679-2eec229c42a5))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 25d307ba-0c60-448c-a589-55f16bf5185b))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d6eab8a4-b206-4411-8eb3-96e1b496e3af))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ccd3516b-039c-4402-93c3-ff6c32dd70b2))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e80189f5-f0f9-4c03-959a-6d897ef6839f))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6ae52140-51a3-41b3-a6e9-11eeeda70a4e))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 008a8790-7b33-411c-9560-d51eaa38d56f))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c27dde1f-e24f-4962-8671-2f8af4a57370))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 31b18422-f535-44b0-9b6c-b2a203da0f68))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5865a18d-8046-4b38-a1e4-dba178ff3525))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 830f716e-4459-4b48-bc8b-c36eee0f5507))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2ecc3613-bd59-42f5-97ec-6400157e6614))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c3815721-1441-43c8-a210-2da04b741124))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 98d871e7-9176-4cb4-b509-9e1ac2ad19dc))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0484ed97-e579-4ae2-9fe1-d8fbb83ae3c9))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ffeda29c-fa90-4fb9-ad28-786bb9d9a66f))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 652b5524-2e30-4bdd-b51a-a6fd16d271cb))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 8f481866-1d81-4b55-850d-f6ff3e8a7abc))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 31 "Net-(D19-A)") (pinfunction "A") (pintype "passive") (tstamp 844ac2c0-c69e-4cd0-a049-d130bc2c7d0e))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp 8e2042b9-2de6-43b4-a0d7-95c171e18690)
    (at 161.5 77.75 -90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/bbcaf5d8-47bc-4128-98f2-fb0bdc6e3102")
    (attr smd)
    (fp_text reference "Q13" (at 0 2.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 94a664e5-88d8-467e-9fd3-33d430720051)
    )
    (fp_text value "BC548" (at 0 -2.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fab43763-b8f2-4365-b084-179910da47a2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 3b6f0372-0319-4209-b687-e0e93a01c54a)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 174c54f1-906e-4472-97ef-3cf8e6c5d2b1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a6fbf919-c48e-4314-a2ae-3e0e383d3675))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 99dce650-8140-468f-9700-9908a6501d02))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8c6677f3-3872-465f-818e-99e07b52f9e2))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 31c8d066-459f-4f91-8ad7-7f051f77c1d1))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e310c9cc-6266-47ee-80e7-8328cb2282bc))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8a84795f-3935-4c13-8b1e-cefcba29a693))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2c8c7afa-dbae-4cc7-ba0f-b572d50f4977))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a90f04c6-ed54-4cfb-8c67-b23f334ebbcc))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 66fd16d1-6d62-4c1e-aba0-bb8323b6ac84))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c486ee39-b894-4c9a-bcf8-96f6ed996fdf))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ed34db0c-6d32-4837-999c-7cbb70e98301))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cdfb66d3-44c1-4969-8d0a-6a6dc7dfba2d))
    (pad "1" smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "C") (pintype "passive") (tstamp 5d593863-54e1-46b7-b4b3-858cd2a59b9d))
    (pad "2" smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "Net-(Q13-B)") (pinfunction "B") (pintype "input") (tstamp 668851e9-936f-40fe-8c03-9c0b425b7919))
    (pad "3" smd rect (at 1.5 0 270) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "Net-(Q12-E)") (pinfunction "E") (pintype "passive") (tstamp 5c28958f-4080-4cc5-aca0-ce7dcef938ab))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 8e554d7c-6402-46aa-b266-df135d6e143d)
    (at 63.093 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/724ad879-e26d-4b00-8e2d-4e024821fe9d")
    (attr smd)
    (fp_text reference "D12" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1cfc889f-3cc9-4fbe-aac9-eef3a4195de1)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f8548bb1-942e-4ab9-95e9-ca346412fa8b)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 22652388-b251-4c72-a545-815c115ad5fc)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ae1dd4ec-2ea1-4991-b806-8f4a871a70a6))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 18c28860-56a7-49d1-aa76-75754a5c2bda))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a552ac26-3e60-43fc-be72-a163c396bfed))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a99f9aa5-4fd5-4e6b-8844-a458830918fd))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96bba11b-8d5d-42af-bfe1-64fd8b06eeb2))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a9e072f4-fcaf-4396-b15e-d49fed792067))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b8a473b6-4035-4786-8242-f33d4c49520f))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f471bf0-e2c6-4c99-88c3-928bc036b216))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 09aeac2b-f891-4d7d-a73e-dcafb753ed04))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 81836593-b4b6-44c3-b036-0e985f575703))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1b70de80-b51b-4563-acd0-a35af746fc75))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 96ffec40-6253-4c85-9589-fdc7578ce0af))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 47ee3430-9960-4bf0-84aa-42066d6c7f60))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0ae5d23d-a08b-4075-a4b3-d8502ec8b4c1))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4157a874-ca9e-4599-90c6-581b5773b5f2))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a68ad3f9-e541-40a0-87ae-cf3228e12185))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0084617b-c1fc-4bd8-acda-97d58bb23c6a))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2d8a1548-566d-4638-b079-5576854b620a))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp fa109e35-77d8-40b4-87f8-eb98c2e3334b))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 24 "Net-(D12-A)") (pinfunction "A") (pintype "passive") (tstamp c96f9bab-1ce8-4252-9550-7d4c8f56e3fa))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 938a71ca-cc5a-4dd3-a0f4-037041ec66bb)
    (at 100.593 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/c3e5375c-8862-4cec-a89a-a1410768a390")
    (attr smd)
    (fp_text reference "D15" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f26cd007-2672-4a98-86f7-9c9a939add6a)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e8bcae74-53d5-4a0d-967f-c2f3419c76c3)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97bbfd16-6f35-472c-9a99-bd91486c631f)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 86eb1df9-a2f9-42c5-98a6-3e8f87167114))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b9b0fe00-1a0b-426f-ac50-d959fbed4f9a))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 172419d0-b786-460a-a3ff-e064227993ad))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9d162e25-6c10-4914-80a8-e67d5dd585b3))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 813995e5-8e3f-48db-bb01-81bcdd2c69a0))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f7d6bbd7-5f5c-42ee-b7ec-3ba3c702ac62))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4fa1f267-63d0-45b2-b393-da811f7f7ad3))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8690760c-3fe4-4685-a1d3-4f8d48757cf2))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 04998047-b209-4c8b-9ae4-cd772d2adb38))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9f6cf0cd-6ebf-4690-962d-74ef2a4dadbe))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3bec9e38-f9e4-47b5-97eb-73b9145df65d))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 52b520b8-c84b-460f-9566-5697f9148805))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6dc5d9ff-9d75-4964-aa43-28adae6a7990))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 213b8774-2cfc-46f2-ade6-d43ac934b8dd))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp de98d1a5-c22b-4b53-a044-f9060da02b4e))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 55af4dfa-01e4-496a-a065-e8d739669b79))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 904d5bb6-fa30-4d90-8169-9324c12e3f34))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a7c5606d-3344-4550-8e7d-812123757570))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 9423e3b9-0aef-460b-8fee-b2f125a18a85))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 27 "Net-(D15-A)") (pinfunction "A") (pintype "passive") (tstamp ae1c5928-9c17-4d20-8027-274ecdedda13))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp 974d2c8a-04dd-4580-8853-700b675fdf4c)
    (at 120.093 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/41296ac2-162b-4f30-80d2-7ac2664161c9")
    (attr smd)
    (fp_text reference "R17" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 82e7467b-7066-48ec-86ec-a12ec6293265)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8aa9af09-0a20-4a4a-ab83-75c406812188)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp feff1ba2-5000-48d4-b0f8-cf22eca2be20)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9b0f2263-c9e6-42f2-8ddb-c306b5802596))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e4c7dddc-38b4-4c08-a3a2-bb44a56625cd))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4a2aed9b-cef5-4e4e-94e2-2f3f895ba9a7))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 31249bd4-5671-4d39-805b-6a3f5e737c9a))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8c1c7161-515e-4c18-9bae-35f24a13d017))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 08020370-158f-4dc6-bd37-7d258b306649))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 204d67e4-b6fc-4ee3-be35-445043f55f27))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1748ba2a-03a1-4e2c-99fc-05c07cebd32c))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 46490074-2717-4774-b4ce-519b6ce63df7))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fa3b622c-cd0d-4259-a184-9c674c75f0ef))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 68 "Net-(Q7-B)") (pintype "passive") (tstamp c0cd9b66-004b-4218-ada8-9f10626bb990))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 16 "Net-(D7-A)") (pintype "passive") (tstamp e78c9698-9285-4efd-865e-ff6e492cea70))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "B.Cu")
    (tstamp 997b2586-7878-4be2-b914-d90526667c3c)
    (at 155 32 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/ad32d57b-e5c6-4450-a9c5-5ba8200fdd13")
    (attr through_hole)
    (fp_text reference "C4" (at 1 3.75) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 557666ec-f293-407e-8925-9aeaf55a7f4e)
    )
    (fp_text value "47uF" (at 1 -3.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5d59ce0f-9add-4730-af03-1f8db5f1b957)
    )
    (fp_text user "${REFERENCE}" (at 1 0) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ad252187-06ce-4de2-b7ff-4af0476587d3)
    )
    (fp_line (start -1.804775 1.475) (end -1.304775 1.475)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d54b0379-e7e8-4744-b2c6-c5d60c874863))
    (fp_line (start -1.554775 1.725) (end -1.554775 1.225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ca5e4207-45d1-4fe6-888d-c5830b1b8e0c))
    (fp_line (start 1 -1.04) (end 1 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c989acdd-8d81-415b-88c5-5d1a3a6dea8f))
    (fp_line (start 1 2.58) (end 1 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ccec14dc-6fbb-414e-8b45-50ca3fa3b80c))
    (fp_line (start 1.04 -1.04) (end 1.04 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d59c391c-1274-4d3b-a5c6-87dc072a0440))
    (fp_line (start 1.04 2.58) (end 1.04 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 14f78f0f-39c6-4746-91c2-5b0c89242762))
    (fp_line (start 1.08 -1.04) (end 1.08 -2.579)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 37c09929-bdc4-49dd-9dfc-02e4aa3e68fb))
    (fp_line (start 1.08 2.579) (end 1.08 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dc2e6f10-c9d6-4503-ac14-893179608108))
    (fp_line (start 1.12 -1.04) (end 1.12 -2.578)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b011d9a1-c87d-4c25-bf61-f45d80d24f5f))
    (fp_line (start 1.12 2.578) (end 1.12 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 73b0827c-f58b-487c-a418-f512faf522db))
    (fp_line (start 1.16 -1.04) (end 1.16 -2.576)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 822318c5-8f06-4961-8950-09898d0acf85))
    (fp_line (start 1.16 2.576) (end 1.16 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 29f3c08f-618f-42d4-8166-6e4db04213b1))
    (fp_line (start 1.2 -1.04) (end 1.2 -2.573)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 99eabbbf-37d3-4618-aafd-cb47621edf0e))
    (fp_line (start 1.2 2.573) (end 1.2 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f7d39b58-c27e-4fb3-b743-754a07003575))
    (fp_line (start 1.24 -1.04) (end 1.24 -2.569)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fccc8ba7-4eab-4687-bb90-e6c5c1833b5d))
    (fp_line (start 1.24 2.569) (end 1.24 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 49965d97-a804-4ecb-afcf-fb2c000891c7))
    (fp_line (start 1.28 -1.04) (end 1.28 -2.565)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3fef7136-c188-48a4-9e24-b077c8ca316c))
    (fp_line (start 1.28 2.565) (end 1.28 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d83f56cb-0b13-41f7-9088-1a4302464047))
    (fp_line (start 1.32 -1.04) (end 1.32 -2.561)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 380cb713-d172-4ddc-81ca-243ae8d5e573))
    (fp_line (start 1.32 2.561) (end 1.32 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5cbf567a-8154-4500-a937-6709991cf74f))
    (fp_line (start 1.36 -1.04) (end 1.36 -2.556)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d1816eb1-06b0-4980-8a0b-19f4189183ac))
    (fp_line (start 1.36 2.556) (end 1.36 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a294867f-02df-4042-9008-f83bf9a9407e))
    (fp_line (start 1.4 -1.04) (end 1.4 -2.55)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 12ee5338-fb4a-45e2-a526-a6e4d03a3034))
    (fp_line (start 1.4 2.55) (end 1.4 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4c3ea356-7497-4f9b-b8fc-1333890564bc))
    (fp_line (start 1.44 -1.04) (end 1.44 -2.543)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3a9f53d1-d807-4396-835c-a2be1182d9cc))
    (fp_line (start 1.44 2.543) (end 1.44 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 20263360-ef0a-4a80-ba72-c880cefe6cf0))
    (fp_line (start 1.48 -1.04) (end 1.48 -2.536)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a0fca139-0de0-4b17-8f0e-5f9c46012a64))
    (fp_line (start 1.48 2.536) (end 1.48 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d27693cd-0aa0-4e08-91d5-6abe2652ab3f))
    (fp_line (start 1.52 -1.04) (end 1.52 -2.528)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 704a9e64-8cb9-442b-82b0-f8ce4bc0a6a8))
    (fp_line (start 1.52 2.528) (end 1.52 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a8ba4f24-eb86-4530-93c6-3b0c1b7a07f9))
    (fp_line (start 1.56 -1.04) (end 1.56 -2.52)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1e0c7b15-070b-40e1-bd40-51850d9ca906))
    (fp_line (start 1.56 2.52) (end 1.56 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 529717ff-d5ab-4ed0-8427-2f7ddddd665b))
    (fp_line (start 1.6 -1.04) (end 1.6 -2.511)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cb305fc9-0fdf-45eb-bdcb-4ca415ae44ca))
    (fp_line (start 1.6 2.511) (end 1.6 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8eec3a8d-7514-417e-a482-e71b0e54ac61))
    (fp_line (start 1.64 -1.04) (end 1.64 -2.501)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e86b9a3a-431f-4f78-a8d3-8c4899daf739))
    (fp_line (start 1.64 2.501) (end 1.64 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fbecd8d4-a86a-4492-8faa-a5139f644a73))
    (fp_line (start 1.68 -1.04) (end 1.68 -2.491)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c4028c28-3e64-4b3c-9fb5-dc5914d446d0))
    (fp_line (start 1.68 2.491) (end 1.68 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b8cc8f93-6bd9-4f53-983d-4d946ad4f51c))
    (fp_line (start 1.721 -1.04) (end 1.721 -2.48)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 36950a2c-ec43-4d89-a778-249f6a10793f))
    (fp_line (start 1.721 2.48) (end 1.721 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 25bc32a7-ca7f-4d1f-9ae6-b71fad4b1889))
    (fp_line (start 1.761 -1.04) (end 1.761 -2.468)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 594a6217-fbd7-470a-8baf-e9f5b483a397))
    (fp_line (start 1.761 2.468) (end 1.761 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e94d5a65-e939-4c60-ba51-b2d02f383a78))
    (fp_line (start 1.801 -1.04) (end 1.801 -2.455)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9a9ee99b-71c5-4cf5-8293-337028b95103))
    (fp_line (start 1.801 2.455) (end 1.801 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c667c0f9-55c3-4107-8999-71beffd734d0))
    (fp_line (start 1.841 -1.04) (end 1.841 -2.442)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7c843fab-89df-4a86-984c-d068daf5f0ea))
    (fp_line (start 1.841 2.442) (end 1.841 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8d62aa22-7617-4805-95ae-16992ba5cf93))
    (fp_line (start 1.881 -1.04) (end 1.881 -2.428)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a21c5f28-9acc-4207-a9ea-1fd21a389969))
    (fp_line (start 1.881 2.428) (end 1.881 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5fab72f9-852b-424a-ad82-63dff8c5e1cc))
    (fp_line (start 1.921 -1.04) (end 1.921 -2.414)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ce76a1e9-559e-4db7-b793-d7623ad68434))
    (fp_line (start 1.921 2.414) (end 1.921 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3d25e09f-8562-4ece-a163-4ee15c27b90e))
    (fp_line (start 1.961 -1.04) (end 1.961 -2.398)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7187fca9-d9d0-429a-8ff6-12d22d31deb2))
    (fp_line (start 1.961 2.398) (end 1.961 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4da8232a-7674-450c-bcc1-fa61e06d28a0))
    (fp_line (start 2.001 -1.04) (end 2.001 -2.382)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6bdba2b7-3a95-4df9-b92f-e27be9ad7c0b))
    (fp_line (start 2.001 2.382) (end 2.001 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b61f1386-8c7d-4f10-872e-2a6df54a6077))
    (fp_line (start 2.041 -1.04) (end 2.041 -2.365)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da633886-9686-4b76-b900-1f042d624a30))
    (fp_line (start 2.041 2.365) (end 2.041 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2046a72b-58be-485f-9402-a5e4b85d3292))
    (fp_line (start 2.081 -1.04) (end 2.081 -2.348)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 31ec53c3-eef0-4fe9-b27e-e5631aa9c591))
    (fp_line (start 2.081 2.348) (end 2.081 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4d6e9baa-e6be-4099-9e07-1cc4fae78297))
    (fp_line (start 2.121 -1.04) (end 2.121 -2.329)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c7369306-29b3-4c54-99be-52930a662fc8))
    (fp_line (start 2.121 2.329) (end 2.121 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b1814fbe-5e08-461d-af5c-af9bacde410a))
    (fp_line (start 2.161 -1.04) (end 2.161 -2.31)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8a589db2-dac0-4d29-89d6-d7c7ead0d226))
    (fp_line (start 2.161 2.31) (end 2.161 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ec055dfa-e940-4c41-93f2-4540b10b4ad2))
    (fp_line (start 2.201 -1.04) (end 2.201 -2.29)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 991189c2-6e35-491c-8de1-20064c79c3a0))
    (fp_line (start 2.201 2.29) (end 2.201 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2a29f3a7-1bd0-4ca5-813f-a39120608056))
    (fp_line (start 2.241 -1.04) (end 2.241 -2.268)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8a20cb77-43e7-4028-910d-c8fcce584c44))
    (fp_line (start 2.241 2.268) (end 2.241 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 78587f1c-aa7c-4994-b392-f4d334f4dc80))
    (fp_line (start 2.281 -1.04) (end 2.281 -2.247)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 102514fe-a761-4f9b-9c9b-d83ea8860f03))
    (fp_line (start 2.281 2.247) (end 2.281 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d5e71ec6-6e0f-48c7-88e1-965b7ce7f540))
    (fp_line (start 2.321 -1.04) (end 2.321 -2.224)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fb67dc04-ec4d-4500-a1a0-8259aa08b513))
    (fp_line (start 2.321 2.224) (end 2.321 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1abd8f74-7173-4e2b-9d94-3e79b731ee82))
    (fp_line (start 2.361 -1.04) (end 2.361 -2.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fd8e873d-29cf-4fd2-b8aa-0afd452ea6f8))
    (fp_line (start 2.361 2.2) (end 2.361 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f0bad355-29d8-48ff-b855-5ffe2b80a21d))
    (fp_line (start 2.401 -1.04) (end 2.401 -2.175)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 072c9f09-b04c-4678-8af9-c1cfa12125ca))
    (fp_line (start 2.401 2.175) (end 2.401 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b2e5156c-5f0f-45d9-9b85-e930c8ff6a6a))
    (fp_line (start 2.441 -1.04) (end 2.441 -2.149)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8f8f75ea-b0b8-4f32-ae92-7bca9bd807af))
    (fp_line (start 2.441 2.149) (end 2.441 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 874b3461-d61c-4938-8dd8-6a408fb4a83b))
    (fp_line (start 2.481 -1.04) (end 2.481 -2.122)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2f6037bc-af68-4444-9686-d7f28b20f916))
    (fp_line (start 2.481 2.122) (end 2.481 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a562d3ab-59b5-4a25-9e9b-d3e6a3da0ecb))
    (fp_line (start 2.521 -1.04) (end 2.521 -2.095)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c7a6a163-2507-4a2c-86a4-252dd8bfa024))
    (fp_line (start 2.521 2.095) (end 2.521 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4a126274-e7d7-42e7-b282-d71dc1bf54f2))
    (fp_line (start 2.561 -1.04) (end 2.561 -2.065)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1a1f79eb-5b73-4d4d-aea9-03399a8533a2))
    (fp_line (start 2.561 2.065) (end 2.561 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2794b5e0-0742-40e9-8d4e-eef60ed67317))
    (fp_line (start 2.601 -1.04) (end 2.601 -2.035)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ddd8b8d1-e64f-4fa1-910b-57813007047e))
    (fp_line (start 2.601 2.035) (end 2.601 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ed1fc9ff-e932-44fd-af27-abf546fd6a61))
    (fp_line (start 2.641 -1.04) (end 2.641 -2.004)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e20c99b2-662a-4677-b036-ad033dd52dc7))
    (fp_line (start 2.641 2.004) (end 2.641 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp aa544bf1-2f12-43f9-9f0d-709d159186d2))
    (fp_line (start 2.681 -1.04) (end 2.681 -1.971)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6c9b6b44-57ed-4ccc-bb2d-39e0a8c4cf50))
    (fp_line (start 2.681 1.971) (end 2.681 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 53c33679-b997-4291-b64f-de1472bcfe52))
    (fp_line (start 2.721 -1.04) (end 2.721 -1.937)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c2bc08b3-d8c0-4b21-aba2-759be243c92b))
    (fp_line (start 2.721 1.937) (end 2.721 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1d1b85cc-f345-465c-a0bf-77ebcf4e345c))
    (fp_line (start 2.761 -1.04) (end 2.761 -1.901)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp feef544b-c500-4753-b40d-15ea1907d602))
    (fp_line (start 2.761 1.901) (end 2.761 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c7a1340f-eaaa-4cfc-8210-c44b6d5ba845))
    (fp_line (start 2.801 -1.04) (end 2.801 -1.864)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d9afcc00-f464-475e-bff0-4d830a43b01b))
    (fp_line (start 2.801 1.864) (end 2.801 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8345cb37-209d-45de-9d2e-cc82ff38aa10))
    (fp_line (start 2.841 -1.04) (end 2.841 -1.826)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 00946916-1ec8-4e74-a94f-9662efae5b88))
    (fp_line (start 2.841 1.826) (end 2.841 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 61f967c6-6fbf-43be-a474-4de69875a172))
    (fp_line (start 2.881 -1.04) (end 2.881 -1.785)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dde717f5-5f4e-4ca6-957b-4081aa4d9297))
    (fp_line (start 2.881 1.785) (end 2.881 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 82fea10d-8b1a-40e9-952f-dff03d544498))
    (fp_line (start 2.921 -1.04) (end 2.921 -1.743)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d2059534-86e4-41a5-aa0f-dac9a004e96f))
    (fp_line (start 2.921 1.743) (end 2.921 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 25b18f5b-3b20-4ec0-98d9-0e84a290261e))
    (fp_line (start 2.961 -1.04) (end 2.961 -1.699)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4c469f9c-83ef-48e9-9b2c-ba41ffb1b26e))
    (fp_line (start 2.961 1.699) (end 2.961 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 674a24e9-a2b2-419b-869d-683549b67e81))
    (fp_line (start 3.001 -1.04) (end 3.001 -1.653)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5e73ded8-0409-413a-8501-cffc4a34f9d8))
    (fp_line (start 3.001 1.653) (end 3.001 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7f2068db-bcff-4261-86da-3ee595842fe5))
    (fp_line (start 3.041 1.605) (end 3.041 -1.605)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d4962ea5-efb7-4e95-ae78-732756271f1a))
    (fp_line (start 3.081 1.554) (end 3.081 -1.554)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4af88de5-82ca-43d5-a243-80777e5922fc))
    (fp_line (start 3.121 1.5) (end 3.121 -1.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cd6b6bbc-4f7c-49e8-949e-c8067975301e))
    (fp_line (start 3.161 1.443) (end 3.161 -1.443)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 51f93d69-9ddf-4c20-90ee-49ed69bf7969))
    (fp_line (start 3.201 1.383) (end 3.201 -1.383)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp af62a110-36a5-4d1f-a3f6-6953df92278e))
    (fp_line (start 3.241 1.319) (end 3.241 -1.319)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 17a39fba-69f9-4232-adc0-45dfcf88be03))
    (fp_line (start 3.281 1.251) (end 3.281 -1.251)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 233dbb86-df20-46cd-9ca6-1a164af25b60))
    (fp_line (start 3.321 1.178) (end 3.321 -1.178)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp df491503-9cea-4aba-98cf-552e7f03d10e))
    (fp_line (start 3.361 1.098) (end 3.361 -1.098)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 00628ac9-f3ad-492c-b12e-f62ce8b8d5d6))
    (fp_line (start 3.401 1.011) (end 3.401 -1.011)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0c1a8e34-ebd4-437f-a7f4-3f80774551d4))
    (fp_line (start 3.441 0.915) (end 3.441 -0.915)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e217dfa6-8535-41e8-9dd5-276859f85265))
    (fp_line (start 3.481 0.805) (end 3.481 -0.805)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 73ed4cc9-b686-441f-bb97-2e93feeb2f50))
    (fp_line (start 3.521 0.677) (end 3.521 -0.677)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6ff06341-f055-4e77-bd53-730a633849e2))
    (fp_line (start 3.561 0.518) (end 3.561 -0.518)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4585b653-c50e-41f1-8609-5ca0cd2bcecd))
    (fp_line (start 3.601 0.284) (end 3.601 -0.284)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4d87f257-bb20-4802-b9c0-8e9595426f1d))
    (fp_circle (center 1 0) (end 3.62 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "B.SilkS") (tstamp a65a7ef8-6f11-46b5-923a-bece9fa4715d))
    (fp_circle (center 1 0) (end 3.75 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "B.CrtYd") (tstamp d01d5997-e832-4933-b467-1e4018f0e42e))
    (fp_line (start -1.133605 1.0875) (end -0.633605 1.0875)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a901632e-da5f-496a-b0c0-ebda782b04af))
    (fp_line (start -0.883605 1.3375) (end -0.883605 0.8375)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 86098799-7ab6-4f17-8304-c9a1fcf4f868))
    (fp_circle (center 1 0) (end 3.5 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "B.Fab") (tstamp 72df31ea-3181-4b4e-bc91-466889547d31))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pintype "passive") (tstamp 47f9b701-a802-433e-b3f5-3b17cf10a119))
    (pad "2" thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "-12V") (pintype "passive") (tstamp 7c502d9e-158d-4cf5-a5c9-fa2e1b995c7c))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "B.Cu")
    (tstamp 99c8327d-0837-4115-9f29-ed25e010f047)
    (at 165 67.25 180)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (path "/03050a54-e7f3-4b7b-81b4-e33abaf10142")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 1.998) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2751812-ad42-4247-bbb5-905a6318bec7)
    )
    (fp_text value "TP5" (at 0 -2.05) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp debd8b3d-23ca-444a-874d-b3e18a366e70)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp acb6ac86-1080-4490-bf6d-03df6c99e15d)
    )
    (fp_line (start -1.2 -1.2) (end -1.2 1.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 18152128-174c-41af-a138-a4e22d88b94e))
    (fp_line (start -1.2 1.2) (end 1.2 1.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9ef5a5b2-9465-4065-b4cc-3fff94a40a68))
    (fp_line (start 1.2 -1.2) (end -1.2 -1.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 029c685f-a141-4318-848e-9da03d388a99))
    (fp_line (start 1.2 1.2) (end 1.2 -1.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 856b8aee-a286-4663-b8cf-c7449c730ac0))
    (fp_line (start -1.5 1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7a21614d-4cb3-46c5-a285-65b4ef712aad))
    (fp_line (start -1.5 1.5) (end 1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f450261e-b038-47c6-aced-f6feafbaaea3))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 909b9db2-a3ab-4edc-b308-993a19168a09))
    (fp_line (start 1.5 -1.5) (end 1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1b39aeb3-c4ae-497a-8e20-48bdcb88941c))
    (pad "1" smd rect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 86 "Net-(D37-K)") (pinfunction "1") (pintype "passive") (tstamp d2499d8f-932e-40ef-8909-dec1d6583437))
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp 9a2ccb44-670e-4743-81b9-1a98927f128c)
    (at 50.593 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/2c57aa10-cd60-47f3-a892-3c982cb2d946")
    (attr smd)
    (fp_text reference "D11" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 65853d65-e3b8-4ede-9ad1-f0cae53bfbdd)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b4af36eb-bdd3-4eb7-939d-a68cdf9b06c6)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2c808417-2b6d-41ec-b090-62704171801f)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 19b51fa1-9df7-42f3-ba5b-572111786204))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c8419c3d-88a6-4354-8697-a91e898ea22c))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 87eafff7-880a-4f73-9e90-1901145d2d69))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e3e4827b-65ee-4f0a-ac59-d932ab4838e3))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 76758f6d-d9c5-4295-b0d6-40defb0d21a8))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 13eac4b1-b62e-43db-adef-3a3c5bf686e1))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp de9eff58-eae9-4a57-b449-936d118cef74))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6040ae98-3cca-42a9-aae0-6d42c8e19caa))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e0ce68db-a676-4ae1-a07e-bc6cbc3e8010))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 722ba1f5-fe3d-47a1-861f-82e159b53f15))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 837af8aa-df79-463d-87dd-5456931f0032))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f2809e5a-d9e1-452f-a6a4-d2b76c8c1d48))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b3c8aa6d-e6ba-4675-9659-b4ca604f7116))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 325addc2-c71b-4c84-8068-b7f1377675e6))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b1b2680d-650f-4aca-9ec6-ca3cf48454ac))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 49f00035-8f79-47e7-982a-7d5576aaf6a1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9fea8538-3cc4-4476-870e-310c5924bd92))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a129e396-f8e4-4c6c-aea8-b4f29d13c87c))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp 14fd8e2c-da5f-4a1d-8133-b0bbacf6b194))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 23 "Net-(D11-A)") (pinfunction "A") (pintype "passive") (tstamp 619696d1-7cb7-4297-9521-440af1574f62))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp 9b155abf-363c-4997-a9aa-c9555fded028)
    (at 149.53 20.25 90)
    (descr "Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x08 2.54mm double row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/c1212be2-06f2-4b84-a8d0-ac95770dbd0e")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 6.1 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 163baad9-6428-478f-b5d4-0ba7e5b3a852)
    )
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 -23.88 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b7522265-42e2-419a-8287-3059c7203ed5)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -8.89) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 16c66e45-349a-4446-9ef3-f70a45208c60)
    )
    (fp_line (start -4.68 -0.5) (end -3.68 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c4fddf38-81f0-4510-aa60-9880be5e400b))
    (fp_line (start -4.68 0.5) (end -4.68 -0.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3afb8580-d44d-4ff8-bf6f-c4f461ba0a20))
    (fp_line (start -3.68 0) (end -4.68 0.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp aac22d9f-be89-4b29-94a1-82ddae27e8cd))
    (fp_line (start -3.29 -22.99) (end -3.29 5.21)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d519dc63-e239-42e3-8ea9-68005badaddd))
    (fp_line (start -3.29 -6.84) (end -1.98 -6.84)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1f10fb2f-a76d-45f3-a2da-ba61f884364d))
    (fp_line (start -3.29 5.21) (end 5.83 5.21)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2388af17-4046-49e3-903f-4e464e13841c))
    (fp_line (start -1.98 -21.69) (end -1.98 -10.94)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7d61e59a-0a9a-4528-b1d2-5be63f9b3d7a))
    (fp_line (start -1.98 -10.94) (end -3.29 -10.94)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ee2d767a-c797-4a85-98ec-5f86f6695cc7))
    (fp_line (start -1.98 -10.94) (end -1.98 -10.94)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0021e358-9074-48fe-bc5e-67f6ad093af8))
    (fp_line (start -1.98 -6.84) (end -1.98 3.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0eec0da4-1020-49c6-b73d-d69cf1324768))
    (fp_line (start -1.98 3.91) (end 4.52 3.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 57575555-e52b-4a32-8745-5268d1837669))
    (fp_line (start 4.52 -21.69) (end -1.98 -21.69)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c4a760a6-2fb2-4144-ba77-a7ca89f0670c))
    (fp_line (start 4.52 3.91) (end 4.52 -21.69)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c580b3c0-d526-46da-a4bd-9781c40f12b0))
    (fp_line (start 5.83 -22.99) (end -3.29 -22.99)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1182332c-0ff0-463f-85cd-5f65d9a6cac1))
    (fp_line (start 5.83 5.21) (end 5.83 -22.99)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c2af640f-fd48-44ee-80e1-7622d22d039f))
    (fp_line (start -3.68 -23.38) (end 6.22 -23.38)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8006f298-dc85-47b0-a94c-9d47897ff631))
    (fp_line (start -3.68 5.6) (end -3.68 -23.38)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7ba5bb51-edea-409a-9f60-124388edf49e))
    (fp_line (start 6.22 -23.38) (end 6.22 5.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6568044e-2a89-470b-9a81-05cf6b9e13ef))
    (fp_line (start 6.22 5.6) (end -3.68 5.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 580aca25-e1f5-4a8e-8730-0866c804716e))
    (fp_line (start -3.18 -22.88) (end -3.18 4.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4166f914-c140-406a-bfa4-c7e07cec6643))
    (fp_line (start -3.18 -6.84) (end -1.98 -6.84)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6ca1d757-46a0-4fe1-a808-8c0b3607a526))
    (fp_line (start -3.18 4.1) (end -2.18 5.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ba14a822-f870-421b-bdaa-7f7f8a8550c4))
    (fp_line (start -2.18 5.1) (end 5.72 5.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 29cae05a-6f8c-4d52-b7e8-8e316484ace9))
    (fp_line (start -1.98 -21.69) (end -1.98 -10.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c26a83d3-931b-4c99-8a23-805914c8f4f5))
    (fp_line (start -1.98 -10.94) (end -3.18 -10.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9b6e2181-9a3c-4ac8-9173-cd0bc2b5d275))
    (fp_line (start -1.98 -10.94) (end -1.98 -10.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 851a2284-65ba-4aed-89e8-8eb6c97aeddb))
    (fp_line (start -1.98 -6.84) (end -1.98 3.91)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e0f00add-46af-4edf-8cc0-186d92db3911))
    (fp_line (start -1.98 3.91) (end 4.52 3.91)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5de6b8a8-73ca-4c3b-be4b-cb8163ab3f34))
    (fp_line (start 4.52 -21.69) (end -1.98 -21.69)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 32c7790e-3f82-45e2-9c31-732f2f987f4d))
    (fp_line (start 4.52 3.91) (end 4.52 -21.69)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 373a650c-239d-4cd0-894f-a8c382f6c092))
    (fp_line (start 5.72 -22.88) (end -3.18 -22.88)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 23bd40a9-8d2f-4f3e-aeca-d8650a0acfe7))
    (fp_line (start 5.72 5.1) (end 5.72 -22.88)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 52527b9d-40c9-486f-b64a-0fd1a6e96285))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.147059)
      (net 45 "Net-(D32-K)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0d706f00-e169-4eea-943e-e2dc513231f6))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(D32-K)") (pinfunction "Pin_2") (pintype "passive") (tstamp 9d7b3400-7579-4820-8c73-9da33e15507c))
    (pad "3" thru_hole circle (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 99f2a8df-9d63-4d14-a8c3-bb9a7246cdec))
    (pad "4" thru_hole circle (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 66b1a514-8c21-4344-974b-594de9ec365b))
    (pad "5" thru_hole circle (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp 86712382-b68a-4e26-9e3c-f127bce30696))
    (pad "6" thru_hole circle (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_6") (pintype "passive") (tstamp 651a02e5-cac9-45e4-b9e3-1f4e2abb60dc))
    (pad "7" thru_hole circle (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_7") (pintype "passive") (tstamp 702fa692-0307-4783-89c8-11000919128f))
    (pad "8" thru_hole circle (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "Pin_8") (pintype "passive") (tstamp ed87f2d9-13a3-4fdd-b849-9938e168083c))
    (pad "9" thru_hole circle (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(D31-A)") (pinfunction "Pin_9") (pintype "passive") (tstamp c8e7f3cc-7251-49c4-9b6a-94fe27cc78d1))
    (pad "10" thru_hole circle (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(D31-A)") (pinfunction "Pin_10") (pintype "passive") (tstamp 4e19e838-3a9c-47c3-a286-d6fdf6946a5d))
    (pad "11" thru_hole circle (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(J3-Pin_11-Pad11)") (pinfunction "Pin_11") (pintype "passive+no_connect") (tstamp c583e7b4-9850-4bd9-ac3a-2a08509f9f87))
    (pad "12" thru_hole circle (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(J3-Pin_12-Pad12)") (pinfunction "Pin_12") (pintype "passive+no_connect") (tstamp 83cafb82-8fb9-4032-b082-865338a7b9f5))
    (pad "13" thru_hole circle (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J3-Pin_13-Pad13)") (pinfunction "Pin_13") (pintype "passive+no_connect") (tstamp 057294a3-73af-49eb-b851-db7b0fb22d9c))
    (pad "14" thru_hole circle (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(J3-Pin_14-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect") (tstamp 4981a206-46a2-4a4e-8ed2-96a1d6056179))
    (pad "15" thru_hole circle (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(J3-Pin_15)") (pinfunction "Pin_15") (pintype "passive") (tstamp 5858bb96-a77a-4a13-92b1-2dde8bf18617))
    (pad "16" thru_hole circle (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(J3-Pin_15)") (pinfunction "Pin_16") (pintype "passive") (tstamp 1484bca3-1057-478a-b6ab-1a5d77a704c1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp a4888190-00cf-4e96-b1d6-7fefb418efd5)
    (at 121.093 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/64adf459-8bb2-4b7a-9eef-d1fc3c14d6cb")
    (attr smd)
    (fp_text reference "Q7" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b3af5bc6-9770-4dc7-aa20-3ccad9d0f1d9)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ef084f5e-3196-403b-8073-e30fdd759647)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 2fac1b88-1710-43d5-b160-1be351604421)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ca03c073-eda9-4c18-a8d7-604b0c34a4f1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 004212e7-0775-43d7-81a7-b33028981dd8))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a8ec5cf5-37f5-4f15-aa81-ea5101604c05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b81f919e-f348-490b-a4e4-97b7218d4dae))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5ce88247-608e-4de5-9123-f8d2d5e95fd0))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5674e349-7c86-46ec-abc0-6d2e76c6508f))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp aa2cb5d2-0416-4e0c-83e5-fdfbc409ed33))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp eef0f62c-f6e6-4bac-accc-b8ac8947a77e))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 34dc20b7-5206-4205-bc49-57c0f9c2dd75))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f2e146a8-172e-4f85-9e2f-11e7905d57c5))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0e514638-9e98-4818-b66b-500cad49b635))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cf1d0e91-291e-4826-a573-9b43532c98b1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 40ed4759-5b04-4760-8538-837412b56447))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp c88a5d20-17a7-44f3-9243-1c596dec1b49))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(Q7-B)") (pinfunction "B") (pintype "passive") (tstamp f3557234-9a93-4eca-a45d-aec34ac6f616))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "Net-(D27-K)") (pinfunction "C") (pintype "passive") (tstamp 16ce7424-de40-4fc6-8c8b-938321260494))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tstamp a720ae47-0e21-402e-816e-a22cbc70d732)
    (at 168.55 118.75 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/a98347f7-1669-47bb-92e8-ed30c1dd4cb6")
    (attr smd)
    (fp_text reference "R33" (at 0 1.82) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04728ba7-e21a-4a9c-960b-6f6af523be10)
    )
    (fp_text value "1k" (at 0 -1.82) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 57224a3c-6276-4326-9618-2149aa3059fb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp b4121b20-66aa-4c21-a36e-31dff3067983)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 88db56dc-e4d5-4d54-ac2d-2dec7b7ef683))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 09d6698a-61a3-4c18-9394-56b19a51e998))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5f181978-be6e-402a-a6b9-b7d7ac07af19))
    (fp_line (start -2.45 1.12) (end 2.45 1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9d86a336-f2ec-41ca-832d-5ee1080bb299))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 87c88a78-ed56-4969-8d5a-505a744fde20))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2e6d9de0-de50-4f99-a41a-5a99365e7eb7))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f1e885e5-0952-4e4b-9d1f-e86ed2e9875e))
    (fp_line (start -1.6 0.8) (end 1.6 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cf1ef92c-d006-4a28-91bf-05dfe8a851f4))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d39a87e2-c3ea-4509-a9cc-20a7f513145e))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 39e39ed6-040f-4657-8f99-e92e0c3f0782))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 94 "CV_OUT") (pintype "passive") (tstamp 770dbd70-a5ef-4c17-bb98-fb0ac9674b45))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 105 "Net-(U3B--)") (pintype "passive") (tstamp a7ce7ab7-88b4-4282-b7a6-540f2c9c87e8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp ab2f2562-1478-4932-8859-ed78d8b630ce)
    (at 96.093 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/e7cdcf51-8254-44e5-80b4-ff1acc81d93f")
    (attr smd)
    (fp_text reference "Q5" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8e62b4b1-b592-4a31-b245-100eec0b28b3)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a33fb907-2476-4e34-9d59-ca4da72675fd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 5497fe07-5a99-490f-a480-b350e01f4aa6)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 49b66a95-46b8-4c39-b877-0900ff09bc97))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d1be6fb4-9b7d-4e27-94e9-60dcf4147c93))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 46106e06-d8d2-4503-a2d2-8956c1634f00))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 01df6335-ddcc-404a-94ff-9093c3cbe46f))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 35407b85-d543-43b8-ac38-15063ee5c27c))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7a651023-d001-4aec-82f5-27f09e4ea849))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 41f1361a-f42c-4a8c-b43b-fca1b06d2496))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1abecd02-014e-48a3-899a-f5360af35a8a))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 633f0c85-77a5-4925-9b5e-b4425147a306))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e0ee974c-1d1e-4149-ab40-75f286105e62))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 33072f64-6de6-41ea-9721-51876ccbc9a7))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d1fb9336-0fcc-4fbc-b0ef-5859e18a747d))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 990a3785-9c1d-4785-aa31-d667d9aecf98))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp d4fc4cec-fe07-42d9-8e8d-8dc1f83e0746))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "Net-(Q5-B)") (pinfunction "B") (pintype "passive") (tstamp 1c4028ad-f7ed-440c-8c4f-f85c2f85fba1))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "Net-(D25-K)") (pinfunction "C") (pintype "passive") (tstamp e5271e34-1f38-4875-b049-d5ac982c6b5f))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp afdadfe9-da8d-45e4-8699-c4c76d9d2d1f)
    (at 62.5 25.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/bf63cf98-d848-449c-aa1b-9d062ece4fca")
    (attr smd)
    (fp_text reference "C9" (at -2.5 0 -180) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5a0199eb-8001-4120-b646-d786e5af27bd)
    )
    (fp_text value ".1uF" (at 2.75 -0.25 -180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ca268e67-1577-4dcb-900c-5a558e52345f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a1344d5d-ce5b-4721-a2d9-7371ab8caf48)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7077d903-59ad-4939-84c8-1a30dad98cb7))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e4d51207-74a9-4c66-a5b0-5111970675cc))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f8462912-bed8-48b0-a156-febc437cc5cf))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0fd0e121-74d1-4005-bad3-bae9304a88fa))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f8d77ab1-4a75-47ea-ac6f-f8d4c3ba3134))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6606a3a7-0d98-4df0-971b-8505446102d9))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7ee22c67-2f66-4422-aa86-870e6dec00a5))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 66136797-2856-4fff-8d93-137229e62a19))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8a174485-2f5e-44c9-8707-ec01a4d31cbb))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 582a3c2e-4036-4eff-9749-bf2d6aadd316))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp 8ba2cd7d-1c2a-45f6-9574-89f5712369c8))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "-12V") (pintype "passive") (tstamp a2524517-8c1d-47b4-ae3e-f3a3ae156878))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp b4f94bc6-6483-4244-af42-c726c78238d0)
    (at 83.593 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/2762e21f-0e01-44ff-9838-b02ce69e3b2e")
    (attr smd)
    (fp_text reference "Q4" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a02b9495-1534-4f68-b0ca-2eae923cf12f)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8ed9095e-0ae4-4202-8e47-042998d226b5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 845484d2-288a-450a-906c-74c73646faf6)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c712747a-c1dc-4064-949e-2a180fb4bd04))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4719a5d-efbc-40a5-bf47-6cabdb8d1e3e))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2a3578a3-c894-4f39-9012-70dd6f0fadfd))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2bc5e98d-9f7e-4bfa-b529-4805d83d7958))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bea46354-5d04-42cc-a09a-33c88811a502))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f4dd821b-74c2-4a21-b297-6dbef816263f))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 812af6c4-872f-4d56-86e6-79586a5de574))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp fc6bc2cc-f5a2-4e1c-b7b3-dfbd6e83b4da))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 828e72d6-a424-4d2e-993c-6d460cabcc65))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7a0683de-b653-4212-8f33-44fc29b180b3))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 07b2ca17-7c13-479b-b608-172ad986a651))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 69ffe95f-da31-4e04-b2fc-b73fb913f911))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0f55b881-e24a-40a1-b1b2-d7e7fc0dd0ef))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp 03f8aa85-d1c3-4932-9dfc-52af9c02d850))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "Net-(Q4-B)") (pinfunction "B") (pintype "passive") (tstamp da1bfbb5-6510-4019-94de-d23bc8c3feca))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "Net-(D24-K)") (pinfunction "C") (pintype "passive") (tstamp d668a8ed-7e9a-469e-963c-3b890b620fb2))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp b800fac0-3227-44d1-9f06-6c9c60f75d9d)
    (at 169 55.25 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/54e2f5c9-c589-483a-8986-280a763ed21d")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5d58ad54-1e92-4d98-8ec9-edea12aa1b9a)
    )
    (fp_text value "68k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fb56fa7f-ebdc-4023-b7d2-6d7f2f39f4bb)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp ef33e339-eb16-4468-8d17-b68c6ac4ab67)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23df755d-b0cf-4cf3-b47e-c0098b40d5a0))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1ba31662-3ac1-44a4-b67a-4d131857477b))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c877e572-d8e3-4035-a13c-5a43c8197890))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96fdbfa8-e9d8-416f-8527-7d6c66f5d1e4))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 745036fb-0542-406d-ba7a-41a63f4ce254))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9ea0c757-2809-43bb-bde2-9180db621028))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c41f89e0-434f-4909-ba16-2c9ab539bc48))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6a70d752-9d3e-4d3c-ab9e-702fc996a78d))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f4b046d-c553-451f-bcff-627ffcb5ce90))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b6d40058-f8b4-4053-ba62-746bdd2ff0cb))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 104 "SEQ_LV") (pintype "passive") (tstamp 5963f9dd-a9bb-421b-957f-c48e7de358f5))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 85 "Net-(D11-K)") (pintype "passive") (tstamp 2e961397-eeb1-40cf-9143-bfee25aa2298))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp b805ed46-c211-42a3-b520-ec16e854495f)
    (at 142.75 31.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/68805cf6-ba90-4885-ac5f-1d331d4465d6")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9ec757fd-1452-41d2-946d-369d4f7c47c2)
    )
    (fp_text value "10" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5a76bc2f-1969-4a75-83ef-3421dd6fb593)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp edbfc9cb-0083-4293-a8f1-760b419a2054)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 70e617ae-bfd1-4ab2-8197-0d2aaef30248))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 49c6c9cc-cd2c-4b40-98cc-06cad1ca6726))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7732094e-31aa-465d-9b2b-f222b719ffe5))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a0a0fbf1-b9dc-4ed4-a67b-5a841d9e596e))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f46d2f01-1637-470c-80cf-5ce138479c46))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9abc40ad-87f6-4ded-8940-73c64941be67))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ed6f4eed-9fc2-4a2d-bed4-1b8242801bf3))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 16a21c4c-7d04-4ddd-b4e4-1de68614f5e6))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ecf15bad-7bc2-445a-86c1-4ad379bf3d8f))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4bc2db25-a4eb-4014-8b6f-891c6f1cf6be))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 106 "+12V") (pintype "passive") (tstamp c6d3ed48-1593-4766-884a-3b861d6725d6))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 44 "Net-(D31-K)") (pintype "passive") (tstamp 39f8791d-48d0-4870-a6e2-f17d3ab020a0))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp b8f0443f-5795-4b49-885e-0151cc90c251)
    (at 147.25 90 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/f50e8134-d22d-407c-8977-4a241a71e145")
    (attr smd)
    (fp_text reference "C12" (at 0 1.68 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5b70796-5ede-45bf-8ff6-f0450f47d2a5)
    )
    (fp_text value ".1uF" (at 0 -1.68 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e4d7549e-5d94-4e5c-bcbd-f1bb04f52ca0)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 5afc0c32-d15e-4b48-9432-0452389fa642)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a1aa821e-aed1-4aa8-9c30-d1038afd4c6d))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 310af9e1-29a7-4566-87d4-35ff1183baf8))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 168fe740-fe40-4d52-afc8-2737dc924e63))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 53622694-d0ea-4566-9ca1-53cf82b5d7ed))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 16ddaf97-95f0-4062-ab4d-9d73ee519015))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d52ff6af-b8bd-4f69-ba5f-83f0a0a80c95))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 37b20f9a-64b0-4943-8174-895d132fd833))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b74b96ef-5ef6-451b-89a8-81c352ee439b))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c2298641-0d0b-4c8f-a073-9780b3eb652d))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 19f0124b-e707-4fed-a5d6-695028374269))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 106 "+12V") (pintype "passive") (tstamp a15bd2a1-f13a-404f-bce5-7e7dfdcda1e7))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp a595cdbd-ee02-46b1-93d0-9d63819e7bd8))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp b96c02da-4fde-411b-b467-1cb57e77b943)
    (at 171.5 28.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/f56f4d03-8aad-4352-b5a9-b66f2ca3f68c")
    (attr smd)
    (fp_text reference "R42" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 50d657df-6443-4108-8529-0a9de4bb2fc6)
    )
    (fp_text value "6.7k*" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c4efb70b-7a30-4cf7-b637-1312a6f29ce7)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 998e4fb3-cc58-478f-a0d1-6554af14f58c)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 25c7dd02-f1e3-43fe-9d89-23ee2c9325b3))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9cffa738-bd5e-423f-ac0d-d7e60f3d3f34))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 39e0badd-6cff-45d0-a0bf-3aa32032db17))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1c0a1f85-2c81-4ad7-b018-b02ac26d8e1d))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2b814534-fa7b-43de-96b7-9b5838f046e0))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8bc2ad9a-95a0-4db7-b427-a64b7735812b))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8d08e5d9-673b-4bf8-87d9-ae69cdc2d8e6))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp acf58c98-8076-4bcf-8eaa-f1f6f3875cd4))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp de052145-ad49-471d-a469-4a4d6b773ff6))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 384332d4-df9c-4071-94ec-426932583cad))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 102 "Net-(Q13-B)") (pintype "passive") (tstamp cf154e4f-e82c-411b-b3b7-04217f492590))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 109 "Net-(R41-Pad1)") (pintype "passive") (tstamp 11db5af1-2495-4197-af47-90784cdd4a7b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (tstamp bb71141a-b89d-45f7-afba-d0b171b2d450)
    (at 141.225 91.06 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (path "/e4cfe4ac-e228-454a-be18-2830f05a0093")
    (attr smd)
    (fp_text reference "U3" (at 0 5.28) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e2c62361-df04-43b3-9ba6-35805766237c)
    )
    (fp_text value "TL074" (at 0 -5.28) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 007ea1c0-4821-4a9f-924a-9ff9f5814408)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)) (justify mirror))
      (tstamp e0e191d7-a1b3-476b-9af4-d05342e76963)
    )
    (fp_line (start 0 -4.435) (end -1.95 -4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2212fe9c-4690-4f83-b8ec-024cf3e66ad1))
    (fp_line (start 0 -4.435) (end 1.95 -4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3fb272bb-13c7-4389-bf34-e935d72feee2))
    (fp_line (start 0 4.435) (end -3.45 4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da90d6f0-7a8a-4a19-b602-ae3351e76805))
    (fp_line (start 0 4.435) (end 1.95 4.435)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 978896fa-6484-4294-8278-e7569d8f5084))
    (fp_line (start -3.7 -4.58) (end 3.7 -4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 52ef6cd2-bbef-4fef-8ca1-067f7fd68744))
    (fp_line (start -3.7 4.58) (end -3.7 -4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ff80a301-b1f7-4e3e-bf0e-1471c2c203fd))
    (fp_line (start 3.7 -4.58) (end 3.7 4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d8f30ef4-bc73-4bb4-b23f-a86099e10695))
    (fp_line (start 3.7 4.58) (end -3.7 4.58)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4eac7024-b6ca-4d39-a633-2aa7d2a694c8))
    (fp_line (start -1.95 -4.325) (end -1.95 3.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 11d40354-a41a-4296-ba69-ea8f1428b0b5))
    (fp_line (start -1.95 3.35) (end -0.975 4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 568a0397-9112-47da-ae97-0471a9fdb489))
    (fp_line (start -0.975 4.325) (end 1.95 4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3d3a90c0-cb6b-485a-a01c-42ecbcfd63b1))
    (fp_line (start 1.95 -4.325) (end -1.95 -4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 095530d9-6889-4d85-88db-05ba89928fa0))
    (fp_line (start 1.95 4.325) (end 1.95 -4.325)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp abf1b205-28cf-47d6-b9ff-ae1d2d64a652))
    (pad "1" smd roundrect (at -2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U1-Reset)") (pintype "output") (tstamp 89c275a2-b6d5-4a14-9de4-9eed405c66bc))
    (pad "2" smd roundrect (at -2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(U3A--)") (pinfunction "-") (pintype "input") (tstamp 418064c0-c9bf-453b-93a1-abc91dbe0f91))
    (pad "3" smd roundrect (at -2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(U3A-+)") (pinfunction "+") (pintype "input") (tstamp b3a09d09-4935-4933-859e-5153902ce80b))
    (pad "4" smd roundrect (at -2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "+12V") (pinfunction "V+") (pintype "power_in") (tstamp bb1b9c94-57da-40f3-bfa1-84bb7f31699c))
    (pad "5" smd roundrect (at -2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(U3B-+)") (pinfunction "+") (pintype "input") (tstamp f98f3010-97e4-4509-9873-e616e10618b5))
    (pad "6" smd roundrect (at -2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(U3B--)") (pinfunction "-") (pintype "input") (tstamp 3839e067-73d7-4545-9237-8324b114832d))
    (pad "7" smd roundrect (at -2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(U3B--)") (pintype "output") (tstamp 401e37e7-8368-48b0-beda-f0ab7be0ddf0))
    (pad "8" smd roundrect (at 2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(R37-Pad2)") (pintype "output") (tstamp 4f473e73-4487-4c58-85d4-b911b59ad39c))
    (pad "9" smd roundrect (at 2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 104 "SEQ_LV") (pinfunction "-") (pintype "input") (tstamp f25dd849-4199-418b-a8b0-fd36dbd37c7c))
    (pad "10" smd roundrect (at 2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(U3B-+)") (pinfunction "+") (pintype "input") (tstamp 21eca2e2-0c99-4e47-8537-b4a8f369e23b))
    (pad "11" smd roundrect (at 2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "-12V") (pinfunction "V-") (pintype "power_in") (tstamp 2bc8f082-0069-4904-843f-6d36c12203fa))
    (pad "12" smd roundrect (at 2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "GND") (pinfunction "+") (pintype "input") (tstamp b430ce12-8018-4020-bac9-988b6b66d061))
    (pad "13" smd roundrect (at 2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(Q12-C)") (pinfunction "-") (pintype "input") (tstamp 2063c57f-ae24-456c-b090-6df17371b4b2))
    (pad "14" smd roundrect (at 2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(U3B-+)") (pintype "output") (tstamp fc8d7f7d-e8ef-417f-84a9-4348c7c50836))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp bc783bc0-1089-4405-a446-fe02c87de0fb)
    (at 120.44 34.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/3320ecf5-3082-46a0-8236-d946712b3c97")
    (attr through_hole)
    (fp_text reference "RV13" (at 0 2.33 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 429dcf24-da6b-479a-bf4d-0a4bbc9911fa)
    )
    (fp_text value "Adj 5v" (at 0 -7.41 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp dc5accf9-6540-4a14-aac0-c280e130abea)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cd20b44e-36fb-482f-b075-566ed8bf3bea)
    )
    (fp_line (start -1.33 -6.41) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 076daebb-d941-4081-b87a-b2d2f3d76e41))
    (fp_line (start -1.33 -1.27) (end -1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 256c85dc-8bf4-40bb-9728-715cecc807e0))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 27aea7cb-5ad7-40d5-942a-ee365dffbfab))
    (fp_line (start -1.33 0) (end -1.33 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 42b82e73-b145-4857-b477-2a42a535d45a))
    (fp_line (start -1.33 1.33) (end 0 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cbc661a3-de53-401e-bf44-0e51335a26f9))
    (fp_line (start 1.33 -1.27) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5008f4d1-2c63-40c4-974a-e92adbe13681))
    (fp_line (start -1.8 -6.85) (end 1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5ecb60d8-bfff-4d49-9cee-23a810e81369))
    (fp_line (start -1.8 1.8) (end -1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a734a59f-5216-4446-a5d6-d58ea112dbe0))
    (fp_line (start 1.8 -6.85) (end 1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b451ba01-aa98-4b8a-b770-089fbcfcdef0))
    (fp_line (start 1.8 1.8) (end -1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c87b5297-8ae2-48f3-b9ce-ad3a06c73cf3))
    (fp_line (start -1.27 -6.35) (end -1.27 0.635)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 95f7b1e1-6294-4197-9f97-1c52eead3cae))
    (fp_line (start -1.27 0.635) (end -0.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 619d48a4-4c57-4a15-9767-7e2440f46af3))
    (fp_line (start -0.635 1.27) (end 1.27 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ee651fec-9b56-4b72-a004-680f242869d2))
    (fp_line (start 1.27 -6.35) (end -1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bb5105ef-02ca-4535-a8a8-f491c3eaaaf7))
    (fp_line (start 1.27 1.27) (end 1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f627f525-b7f8-4484-9a1d-350245848d82))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "1") (pintype "passive") (tstamp 5ef323dd-65b4-4737-9ccc-f3c7a8725011))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "2") (pintype "passive") (tstamp a3678eab-ae1b-466b-9318-5bd66eb7affa))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(R32-Pad1)") (pinfunction "3") (pintype "passive") (tstamp 2b9d3096-314e-48eb-a1f9-69db5ba7bf67))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp c0878ba5-905b-4f2e-ae62-031b2f6e6e5b)
    (at 148.75 32 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/75831602-f56f-4580-b4ab-6aef002c1795")
    (attr smd)
    (fp_text reference "R7" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 66229101-5330-460a-b0a3-9560c3e6d58f)
    )
    (fp_text value "10" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d5ed216d-9edd-4831-a662-ab349dba562a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 4df102d5-9872-46c9-8992-6824b88beac5)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp daf76389-ea96-42ef-afcd-3d1bacbea621))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bc86c7dd-11e9-469b-ac9c-06632773a471))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2447f251-3976-42a5-b98a-6779f139291d))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3dc378e2-4880-481d-b114-fe46d31d583a))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d711cc24-834c-490f-97c2-af598af6f9a8))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8eb614f5-75de-4f3d-9b5d-93e905020103))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c6e592d8-deb2-4e58-be25-5db276aa3ae9))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6c0349e5-121b-48dc-97d3-b47f44e8c366))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1208abec-e6a0-4355-a4ee-782de0ad3e0d))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bb5f5a99-de46-4594-87a3-d4dc4af96f74))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "-12V") (pintype "passive") (tstamp 22ddecf2-6312-4431-bf20-9ce63c679ee7))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 66 "Net-(D32-A)") (pintype "passive") (tstamp f653bae5-bc80-43fc-88e6-615f4b584e7f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tstamp c6e55ab6-2c9d-475f-adae-65ef5b7d1370)
    (at 51 29.9625 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/cd3ee726-d313-4027-8a08-03373ef97914")
    (attr smd)
    (fp_text reference "C8" (at 0 1.68 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1a9312a2-fd93-4763-8785-24d36e27d1bf)
    )
    (fp_text value ".1uF" (at 0 -1.68 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f6ae45a1-dc65-428c-84be-db64d8949682)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp cf23ebe9-685f-4ccd-ac2e-a0756a321ff2)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9b89ee28-dbc5-4332-a5f2-9fa0c6283611))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8baca5d5-43b2-486f-8d40-e77d2aef5650))
    (fp_line (start -1.88 -0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5ed78204-2b3c-4ade-b339-19dbbc08e442))
    (fp_line (start -1.88 0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e34c0f9b-93b4-41da-93fb-3c619bd478de))
    (fp_line (start 1.88 -0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 26618ba6-9514-4d5c-b759-1bf491b57b02))
    (fp_line (start 1.88 0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b3fdccbb-9888-42bd-a288-42e7525377e8))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1d984540-a1ed-4204-a65b-b9c31107b22c))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 52a87758-c1b3-407d-b104-836fddb35190))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b138a8ec-5182-419b-98ea-30f350e24029))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1a393a33-b422-4328-b395-87629b56222e))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 106 "+12V") (pintype "passive") (tstamp e7249fa8-2adf-407a-98b1-03dd2c8635c0))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 48 "GND") (pintype "passive") (tstamp 73569c7b-654a-4a31-a51a-113d02ccd2fe))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp ca30f2ea-d54c-4257-8793-86fb2fbe41d0)
    (at 157.593 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/f2eb88a5-9326-444a-8c3c-3a39f75d8210")
    (attr smd)
    (fp_text reference "R20" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c808833e-e27e-4537-b67f-c3150ceb103a)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9f7a69fb-9f10-45db-9032-937ff8be3325)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 59e3637e-b94b-42ec-848e-50af228c66a1)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 43b31deb-c43c-4ad3-8c47-1eeef6ad8c6b))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0d470127-8759-4cbd-bb35-c743c9af8006))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6d2a9bbc-e58f-4679-99c9-432151234b67))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 968acc2d-449f-4834-a73e-a6d0e7d3530c))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f3adc1df-c886-482c-8cc6-ccb6dac13791))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7a1de0f6-47e9-4dd5-8e3c-ed54dacb9668))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d982b00e-8f19-43b4-adf4-771f5fb17ce3))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 38557221-d908-404f-945d-194723474cf0))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 15220713-583e-4aa5-876b-f093530f10ed))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b551ca1f-d4d8-41fd-a21e-5b0b399e9a32))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 74 "Net-(Q10-B)") (pintype "passive") (tstamp 19f42c93-cde0-4b57-a99e-dbeb12e4dcd0))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 22 "Net-(D10-A)") (pintype "passive") (tstamp b3910954-06e2-407d-99c4-1436f5b80ef2))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp cafbe16f-dab1-4f19-823d-faf64a604b1a)
    (at 107.593 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/852bf9b8-5501-4a35-8880-eaa9354c852c")
    (attr smd)
    (fp_text reference "R16" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c58941c5-9aff-4bd8-9c2d-3f2acaf8e2da)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a49e2831-4a41-42a7-8866-3e78c571c062)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp aa78fbec-4bd2-4c64-9b8b-a15d5518bfb9)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bafac23b-0531-4ada-9ec8-339660690bd8))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 46fee6cd-2107-41f7-ba5e-82758ba03379))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f152350f-5437-49d9-8d8f-3ed66c2016aa))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b4f52ffe-e5fb-4ca2-a3d3-66308b2496c7))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 22b216b3-cf6b-4a16-9a70-b69a8d4c0697))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a2be5d9b-cc5b-4072-bbf7-b0483cd90ef7))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 42cc1f78-70dc-4b00-9ff1-691b3f13ec13))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 08e0fd2a-5abd-4a37-a28e-c6f02f25762f))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 17fe7fe4-5d5b-4e9b-8d08-1bb5179e4acc))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 06d0c2ed-e6fa-4112-b61a-b6cd1f9b487b))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 67 "Net-(Q6-B)") (pintype "passive") (tstamp 0424323c-173b-4c8f-969c-b62cefbe5eff))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 14 "Net-(D6-A)") (pintype "passive") (tstamp 07deadc2-cc7a-4f08-bf50-6c7b2cb1195a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp cca5e37f-4abc-4b59-9f0e-4a5943b4e5c0)
    (at 163.093 60.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/50c8e302-9ec1-4b0e-a8b9-b06ddf04b2f0")
    (attr smd)
    (fp_text reference "D20" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 29469ca3-4743-4fed-816b-bc97f71f9a79)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0fc8ee63-ff43-421e-8915-fde6fe2cc124)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 40c656ed-be85-43b0-981b-faff6f067041)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 04369bc7-76a4-43c6-98a6-32fc0ac8c555))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b805b742-4b75-4189-80b9-5c0de008bb8d))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ed3d196e-85af-46c8-91bb-7b090d054ebc))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 13757321-cb84-4100-b6ee-2c074ef6ffc6))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 094350f5-ed50-400a-98f4-646cbaea72a1))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5752d2eb-2b67-4f31-bf13-bbf9b6b96006))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c8e07393-507b-464b-ba92-ed1525ce6455))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 191c809a-f5d6-4660-802b-15585fa05334))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 03437009-3369-4603-939d-49b249b46e5a))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2d6f2710-8136-4be4-8578-c90ae8782f21))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f8da5bd8-97f6-454d-94d1-4960d17b8ee9))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0224bb6e-b163-4842-9de6-74f67db1959a))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 18d1d65d-ebe7-439b-a671-37de7cdcdd2f))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0c297d19-b86b-4a44-b8fd-5cfb65e51213))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c0145c8d-4f6a-4695-8a47-a817a38935c2))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a7b0bea7-ea30-49e1-b453-357b80984223))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d5cc5efe-7358-4f2e-8608-01136898a855))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f52cc80a-d04b-449d-9885-7d1977c42c9c))
    (pad "1" smd roundrect (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 85 "Net-(D11-K)") (pinfunction "K") (pintype "passive") (tstamp c3172aaa-9e53-4dfe-a951-31482d590f76))
    (pad "2" smd roundrect (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 32 "Net-(D20-A)") (pinfunction "A") (pintype "passive") (tstamp 24a8eedb-eaa0-4499-afd4-e118051dedf5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp cf1d381c-1ed0-45f8-bf1d-2770ebf47e7e)
    (at 118.25 18.5 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (path "/2a7fe0b7-68f4-415e-aa4d-44e07cdf6490")
    (attr through_hole)
    (fp_text reference "TP10" (at 0 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e2f45a90-7180-4dfb-bab0-25658cdd34a6)
    )
    (fp_text value "TP10" (at 0 -2.33) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b8312721-903d-406b-a9a6-49f8757c6e16)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6efd6017-dc77-4c9a-9b2d-9d1c58202f43)
    )
    (fp_line (start -1.33 -1.33) (end 1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d6cfb2a1-1e5d-49e0-9fa9-2ce3c48270e5))
    (fp_line (start -1.33 -1.27) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ceb4c766-1ac5-44f3-bbcb-f7359fb9c183))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ed207c79-ff78-4348-9e9f-db36e85857d0))
    (fp_line (start -1.33 0) (end -1.33 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9cc3d750-40fd-4726-877e-266f0e1203c9))
    (fp_line (start -1.33 1.33) (end 0 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2dbf59aa-d8cc-4e31-b99d-b10de887600e))
    (fp_line (start 1.33 -1.27) (end 1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 60087456-bb1e-4f5c-9cb9-e7917b5b6124))
    (fp_line (start -1.8 -1.8) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c5faa895-5a5e-434d-beae-916b01fdc41c))
    (fp_line (start -1.8 1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 537eaf9e-f8c5-4cee-b2d1-1fa81ea48da5))
    (fp_line (start 1.8 -1.8) (end 1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 37ffb1c3-5928-4a36-a04b-6f53122c31f9))
    (fp_line (start 1.8 1.8) (end -1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d5faf04b-1ca4-4e13-9721-71039a508d52))
    (fp_line (start -1.27 -1.27) (end -1.27 0.635)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a8bab893-7618-4500-b6ba-7c1f0121cb7d))
    (fp_line (start -1.27 0.635) (end -0.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d5746763-08e7-4018-9ac3-cf8b8ad19c9e))
    (fp_line (start -0.635 1.27) (end 1.27 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 87a16d37-affe-45b0-b865-7811fbe45634))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fb11ed04-4ba3-4e1a-8299-c5011ed65e40))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 61822605-e39f-4ed4-9ebe-1386819d1001))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(J3-Pin_15)") (pinfunction "1") (pintype "passive") (tstamp c04e6050-82fb-4278-9c03-383d4f87e54b))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tstamp d82ac8ab-e2cc-4ee7-ab01-566d19cbc1a8)
    (at 40.6125 16)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/7728db11-17c2-45db-8c8f-a4164cbb06d3")
    (attr smd)
    (fp_text reference "C1" (at 0 1.43 180) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8d930d02-6bc1-42be-a1a1-35ebd60657e2)
    )
    (fp_text value "1uF" (at 0 -1.43 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0b7c41df-9147-463b-8dcc-740ec6326c24)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 038639e0-3fbb-42b2-8f1b-10578edb6618)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48d2aaf0-ad68-4607-95d1-6d320310c038))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0165ebf8-941a-4009-9556-6d63f8980c8b))
    (fp_line (start -1.65 -0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c9acc675-325e-4374-9c16-71abfa5b29d9))
    (fp_line (start -1.65 0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 92c9c521-6aab-445f-bfe6-4e3c3698ad59))
    (fp_line (start 1.65 -0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b221e44e-beee-4200-bedd-a73dd44c4396))
    (fp_line (start 1.65 0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96f4932b-92fc-4217-87a4-7bee0d7d9e8f))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 79a4fea8-c1b1-44fe-9b3b-df288ebb2303))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d360c684-592b-4576-8a26-a79fbc93ae6e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7385ef36-b03f-4f9b-89f9-06824ce7cfae))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3a8afd05-62ee-4c2a-b356-dc3be29d6ce8))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(U2B--)") (pintype "passive") (tstamp e2205828-7a93-4b64-9a2b-b287caac1693))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "GND") (pintype "passive") (tstamp 22c7717d-1240-4f6d-b3ec-37ef4e7e7be2))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp d8f1e905-7d6b-42b5-9c0c-338427c9d15c)
    (at 158.593 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/17f6c459-1f89-48ee-81b9-98c410d2d707")
    (attr smd)
    (fp_text reference "Q10" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 256d6d79-7ec0-424b-b265-9ff3445bbeaa)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 37c83c17-eb49-44d9-b2c9-d9392ca07479)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 72652a04-d8c5-4fb3-91df-89b7547a86f7)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 84cf1494-cd4d-41a2-bb36-2ca2cfa3d860))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 43d37586-c4a0-4705-a24b-f34230a77469))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4d1aafe2-cf56-47ad-a4d4-64b5518d9c39))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ef888817-ca81-4876-8a5a-ffac7f211a4b))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f8875ef5-8105-4f0f-9c31-d388cd98cf21))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ff3ebfbd-33ee-4b6d-b2e5-fe8fdacc6646))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 98d9762a-50fa-4d11-84a3-4d9b9bad84a7))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4d259865-1a40-4d76-a3d4-025168ec1639))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4cc3dd3f-359e-434f-812f-3977fa4ccf6f))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 74044908-f1f2-4e6b-a6b2-4aacc675b06b))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 34ea0096-4980-4497-9667-e3b55d6c0805))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bb62827c-4a67-4035-889b-a447b68e8ca7))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 00c92d60-bdfc-428f-962e-457f4e36cf9b))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp 1c9fca9a-06fe-410f-a689-124acd560b7f))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(Q10-B)") (pinfunction "B") (pintype "passive") (tstamp a9e18faa-7041-46f5-a81b-423097698fcf))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "Net-(D30-K)") (pinfunction "C") (pintype "passive") (tstamp 092a2809-d96d-4122-9e91-0832fd857feb))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp d9f9b246-9005-4976-bfc2-30f824d907a9)
    (at 45.093 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/1a354c41-0296-402e-8de0-7e6d3aef4059")
    (attr smd)
    (fp_text reference "R11" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5415ea19-f025-49e3-b9e8-7963b7962e8a)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 52444b6f-deb5-4c0d-8040-13fda8518f8b)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 65e808d9-1d9f-44c5-a3fd-7c9d59da6210)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e869eb1e-67f5-43a3-b7a0-3e6823984efa))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7eb0da8e-d2f2-45f5-96ef-d73210eefafc))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c961c4ac-bf61-4d03-b549-1aebf31cacba))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 46d95536-8e56-488e-9096-d7de7adb6a0f))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 58978eee-401a-4071-9661-8e8eea804dce))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d74711b6-6c87-4540-a8f7-47b67c94b4d5))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0d21c5ff-c131-47eb-a405-a7b200ea5a84))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c724a2b3-15dd-45da-ad32-b317bb55ffe2))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ff2e6222-c985-4ed9-81f4-2dbb52a1644b))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c1a77929-0f77-4def-aaca-e14cd9340351))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 56 "Net-(Q1-B)") (pintype "passive") (tstamp 4a9cdd2f-2599-4fce-a9f9-841bd3e26fc6))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 4 "Net-(D1-A)") (pintype "passive") (tstamp 60792c64-3a40-4cf5-befb-bcf26a977d75))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp dd887468-17b9-4dc3-b1f1-3eb7f04edcbb)
    (at 145.093 60.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/827375fe-b8a3-4e7c-bffe-7006c020fd47")
    (attr smd)
    (fp_text reference "R19" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 74fc2cb0-2838-403c-b7d0-38f99513d349)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c7f12f18-22cc-4033-82c9-edd13fc2dfaa)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 64c777ac-a3a1-403f-b572-02932e8dbf73)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 61d2dfa0-28de-4bb0-8928-1b6d3a1ee626))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dd6a243d-ab37-4586-932b-24e932aabe36))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 065042bd-1e18-45ac-b4fd-0d0da13ef615))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 567997c6-193c-4bc6-9f1d-88d508faf188))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 090122a1-2423-4755-a5f9-026aa861c025))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c8d817d6-2762-460f-888b-bd4198d8f684))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp de7a7d11-b97c-4bcb-8eb9-4cfd7558dcb3))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2f86cb2d-c733-4007-950f-2cb0ed4c3128))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 24ca2801-9ce8-4ef1-8a40-3b3360ec0bcf))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ab3dd246-50ca-43ab-a70b-5aac4b00269b))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 72 "Net-(Q9-B)") (pintype "passive") (tstamp 10422670-b404-4f51-9012-74b1c28f3e35))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 20 "Net-(D9-A)") (pintype "passive") (tstamp 7e2a0617-9667-418c-ba9f-a1c274e2bec4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp df01ae58-1bac-4879-ab35-bb7cb67fb4ab)
    (at 56.5 16)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/c3f14ced-6ff2-4b0c-8e5a-3d3a5719bbd9")
    (attr smd)
    (fp_text reference "R10" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b3b6b429-2413-41e2-ab6e-6dbe963507b3)
    )
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1e814c88-b836-4e1e-afd2-b96a9eae7556)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a4c7d606-ebbb-443a-964a-d8d6ba9ec7d6)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b22a124e-36dd-4bea-8e7c-1c3867ae982c))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d59fd351-3df0-4a60-ad20-ce6bdd97477f))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9ce66f26-64d0-4230-b515-a4316728ed54))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4e2a9318-24a9-46c9-bc93-073b55d34cd3))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c0471bb2-24ef-49c8-84d7-4768de1fd53b))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6ccb8235-90ef-483f-ac9d-cf44096fa6b1))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 64622d84-7837-47bb-b3f1-1bae518fec13))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7c971078-9f35-43c2-b2ba-f25e21509ab9))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fc453979-8962-4ca0-ae44-4483d3c643f1))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5d983da5-cbcd-47df-a1d5-deecffdf8bf3))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 106 "+12V") (pintype "passive") (tstamp 4bc68381-1a99-483d-ab65-34158a491ecd))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "Net-(U2C--)") (pintype "passive") (tstamp f3a82546-00b9-4077-a855-2a874d4c6755))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp dfe636ee-f8f0-4c65-b68a-f14d6c0a2627)
    (at 110.94 40 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/32f4c72b-06a7-49b3-9f2e-860485474b59")
    (attr smd)
    (fp_text reference "R31" (at 0 1.65) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9a2babd3-453b-429b-8cac-39fb56001675)
    )
    (fp_text value "18k" (at 0 -1.65) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 75ff7bdf-f42e-42d7-915a-0aa2d9e26758)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 8e124a52-05a8-48f2-9396-cdbdaeaf9af7)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c6092786-d5a3-4e8c-8838-cdc839e851f2))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2eb0e971-b20c-4c9d-9b46-d9febc15ccb4))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 36f036f3-78b0-432d-a70f-01321dd068c1))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 18042142-3bef-4978-af9e-6d248606ea5d))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e168b278-2b5f-43c0-bf7f-210f7f54cc56))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2e5b2cd5-8574-4113-a940-a83a0ea55b4e))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a828b1f8-4f45-4141-b2d9-51f0a8736028))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1902774d-e9ae-4e73-8f68-7c916612ca34))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1c3bc750-afc3-4302-8788-b96b3ee1499d))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b837e902-4662-4c77-828e-7bce1cf2f4d3))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 47 "Net-(R31-Pad1)") (pintype "passive") (tstamp ec3091bf-f2f0-49bc-a824-9219fb0c0c73))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 96 "Net-(SW12-C)") (pintype "passive") (tstamp 9f2e16e7-7eab-40e1-aec9-a74cf46b20a8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp ed4aa89b-93be-4255-bb47-83b12183c8d9)
    (at 59.055 40.64 -90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/0ceafdd5-13d4-4351-b058-a490fe6d4a6b")
    (attr smd)
    (fp_text reference "D37" (at 0 2 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6bf1bcb9-0ea5-4308-a511-bde555a25282)
    )
    (fp_text value "1N4148" (at 0 -2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 19625cfe-61bc-47d3-bef9-7f9cd4addfab)
    )
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp dbd44cbc-524b-40bd-81ca-ad6e7fbbc96d)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8c7f2dd-c2c2-46d5-83d4-e8f764291afe))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ff4e95f4-fcfc-422f-a0fe-e04c79451e1c))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d3b112bd-250d-40d3-8c21-8e0a2e322d85))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e23d598a-cac2-4c88-8b9d-698df55909af))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 52842241-6eb1-4e35-b33c-590c936670f0))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4d61bd00-283c-4977-91fc-6481a252b917))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c0871721-c8fd-4c4c-b621-b996908a10da))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3b1c314d-9d0d-4de5-beea-2be5fef3d11d))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 19805d06-6bc3-4d44-ae6c-471e0c6cf0bc))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d341b068-b62e-472f-aa77-ba773e62dded))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7d08108b-768e-4df0-b2f8-6a4f4f59eaa0))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 381b65af-9982-42ab-b79f-afa1b6cf87c4))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a76ae72f-33a5-45d8-b535-77ac886b8df7))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a3d1f3cb-b840-4548-a249-edce515cd875))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp be2a0d49-ed32-49c7-bd5d-866fe4c82e9e))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e75f1348-7540-48ed-a12a-1dfe9dafb9d6))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b5095e18-489a-4681-b2a3-046789eb1a2f))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6750f7bf-78d8-4bff-94ea-4ea89628684f))
    (pad "1" smd roundrect (at -1.75 0 270) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 86 "Net-(D37-K)") (pinfunction "K") (pintype "passive") (tstamp b8cdc552-7901-4352-9adb-67fae96e7d83))
    (pad "2" smd roundrect (at 1.75 0 270) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 73 "Net-(D37-A)") (pinfunction "A") (pintype "passive") (tstamp 7c5eff33-24da-4374-b3f5-8faa8e01a6ca))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tstamp f1cb0eb4-51bd-4d62-80e3-7988f2fdf8f9)
    (at 180.75 70.5 -90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (path "/a326d5e7-3480-44d4-9ddd-0441b468c66e")
    (attr smd)
    (fp_text reference "D34" (at -0.75 1.75 -270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1e3bb310-e519-4ac5-996b-2c4f05589ab9)
    )
    (fp_text value "1N4148" (at 3.5 1.75 -270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6c98d4e0-adef-4a72-8f98-b40cb8b57b02)
    )
    (fp_text user "${REFERENCE}" (at -0.75 1.75 -270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5c2ec00e-f746-4028-b688-f1bd95817a9d)
    )
    (fp_line (start -2.66 -1.11) (end 1.75 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cfdd9cbc-0c76-42fd-ae00-c69f7d602845))
    (fp_line (start -2.66 1.11) (end -2.66 -1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4c07e1d-f63b-4c8e-9c04-88a8635dfe2a))
    (fp_line (start 1.75 1.11) (end -2.66 1.11)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1d4a6ac3-a6ca-4213-b5e4-e458477292c9))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 684e3bf4-3a19-45ea-b73c-a4a6e37977b7))
    (fp_line (start -2.65 1.1) (end 2.65 1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f41a189f-cfd4-436b-a8f6-766b3ce0e2ca))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 82ed329a-2af5-438f-9459-fefabb5920bd))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 9a62a9b5-5f6e-493e-aea7-6c066262d666))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 86941b57-8d51-46cc-8fb3-14196b5c933d))
    (fp_line (start -1.65 0.8) (end 1.65 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp afc27e15-dc81-4aa8-85f8-9e709976a514))
    (fp_line (start -0.75 0) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 075dd4bf-1dd2-4f87-b884-dbf76c3c1b8d))
    (fp_line (start -0.35 0) (end -0.35 -0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a9595eb7-64f1-4e1b-b899-9196a01944ce))
    (fp_line (start -0.35 0) (end -0.35 0.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4aabe96d-8e97-4c3d-8572-c20de1afaa05))
    (fp_line (start -0.35 0) (end 0.25 0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bfe6720f-eb48-4dc4-bfd9-15746384613a))
    (fp_line (start 0.25 -0.4) (end -0.35 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eeb28918-5e1a-44f0-9c0a-523ba98fe05b))
    (fp_line (start 0.25 0) (end 0.75 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c74b3345-7817-4efe-b9cb-a2335964a864))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b86e93de-2b53-4132-b825-1c245599bbfa))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 22f65a1c-6713-4423-92d7-d7b2278e65d9))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 76b4a9e4-69ae-4f92-92ac-42daf7bfe8d7))
    (pad "1" smd roundrect (at -1.75 0 270) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 114 "Net-(D34-K)") (pinfunction "K") (pintype "passive") (tstamp 21a65f11-b8c5-4265-bc6b-d1e46f0f6090))
    (pad "2" smd roundrect (at 1.75 0 270) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 92 "CASC_OUT") (pinfunction "A") (pintype "passive") (tstamp adc3f93b-e027-48a8-a204-0704df70fba4))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "B.Cu")
    (tstamp f404110f-92e8-44a3-a465-06bcb7a8479a)
    (at 58.593 65.5 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (path "/632699c7-3460-4e03-baea-1b8892451fca")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.5 270) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bdd7308c-dcfb-45c1-85e8-2bab61f1b392)
    )
    (fp_text value "2N3904" (at 0 -2.5 270) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 38c134e6-63ca-4d94-b3f1-e103adb1a9d8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 29624861-06b2-46a8-8dd7-23ffdce4ed04)
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3ce8e6ff-0a0d-4001-9c68-0e80d6c71af6))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b4915130-2a78-4abc-8bd2-98cb851b912f))
    (fp_line (start 0.76 1.58) (end -2.4 1.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3f67f257-8994-4bf8-9148-e6ab66c64cf9))
    (fp_line (start 0.76 1.58) (end 0.76 0.65)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp caa198c2-f2dc-47cb-be1f-206eccf762cc))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5774abc8-0046-4a96-bf40-9902a037ed3e))
    (fp_line (start -2.7 1.75) (end 2.7 1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ebec0ced-718a-4e64-9ff9-01e735a2cb2c))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 79f6d093-470c-4676-9df8-4b768ad2e31b))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 229ee4c2-cb8d-4b30-9a0e-c43bf32c39e5))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 91141b91-4dd3-4bb8-ba5e-9a963e790d71))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cde2c1bf-6363-4324-919a-e9ecd58621df))
    (fp_line (start -0.7 0.95) (end -0.15 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7910140e-d268-4704-959c-5b85b9dc7e33))
    (fp_line (start -0.15 1.52) (end 0.7 1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a829116f-aa95-4584-80ae-e46d5e4d2705))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2ad62318-b77e-4d4d-a470-19e48cb191a2))
    (pad "1" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "GND") (pinfunction "E") (pintype "passive") (tstamp ed1623a7-51b3-4bfc-9e92-e2e20427b913))
    (pad "2" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "Net-(Q2-B)") (pinfunction "B") (pintype "passive") (tstamp cc715bd8-0cf4-459f-a15d-6d3ce0336241))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "Net-(D22-K)") (pinfunction "C") (pintype "passive") (tstamp b50c4a71-cc89-4411-9cec-54e360104151))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tstamp fd3a4dfe-94b1-49d8-8a99-b8664c363445)
    (at 54 33.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (path "/9faca8b0-9329-4dd6-a332-efba6efadf51")
    (attr smd)
    (fp_text reference "R45" (at 0 1.65 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5779f98d-056f-4753-b90f-aea5e47c91c0)
    )
    (fp_text value "100k" (at 0 -1.65 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 877a7415-cbfe-48d5-a29b-a2dddaeea111)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 603000f0-fa13-4fb2-843a-c1bab54b5558)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 36984242-dc45-43b8-b0e8-2f68415146b2))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7fc92cc0-24b0-4638-90f6-7e3861cd945c))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bebd6793-3458-426b-9a60-febee36fc5dd))
    (fp_line (start -1.85 0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c4c9641-3f49-40ce-85c0-6ed0d0b565bd))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c94950b1-87aa-42e4-8d68-bc7f8ce943ff))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 26a19630-eff2-4b1f-bdf6-5d36fa05cb92))
    (fp_line (start -1 -0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 658edf06-0975-42f9-82a7-e05db9ecf966))
    (fp_line (start -1 0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e4116325-fbd2-46c0-b846-b106da14e586))
    (fp_line (start 1 -0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a0a45297-ed74-4c80-9e7e-ea836cead808))
    (fp_line (start 1 0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 38e985ab-eb3c-4837-a3be-01e045fecdf6))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "GND") (pintype "passive") (tstamp fa6ee6a0-4365-424e-b7bc-749fb3ac1701))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 86 "Net-(D37-K)") (pintype "passive") (tstamp b18a7e88-0da2-4763-a24f-5c50ec48d098))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tstamp ff14425e-bfdc-4df0-a48d-c2e35d5a849b)
    (at 167.5 86.71 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Unseen Servant.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/93ddd4ed-b4c9-4e00-81bd-411cace69865")
    (attr through_hole)
    (fp_text reference "RV14" (at 0 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8b09491f-d113-4543-aa8a-b098873474b3)
    )
    (fp_text value "5k" (at 0 -7.41) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5de6309f-b6b3-4877-a656-503b41b97361)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2e3b69d4-6d5f-4d78-ac90-078e1fa2bcb1)
    )
    (fp_line (start -1.33 -6.41) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4d6abe84-4511-42cf-b1a6-57ad7a947a98))
    (fp_line (start -1.33 -1.27) (end -1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1179959b-1189-4142-a7b9-f020e2d1b93f))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 077cff55-6e6d-4b09-ba76-1c8e417af23b))
    (fp_line (start -1.33 0) (end -1.33 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ebea4b94-6161-4297-a777-79de2c35b34d))
    (fp_line (start -1.33 1.33) (end 0 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cc169d15-be4e-443b-be61-960ac27df9e5))
    (fp_line (start 1.33 -1.27) (end 1.33 -6.41)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7d72e183-d9d8-4c99-8794-50f172095b87))
    (fp_line (start -1.8 -6.85) (end 1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp dd9e8a3a-3f62-4ade-8076-d8dcc4f10625))
    (fp_line (start -1.8 1.8) (end -1.8 -6.85)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 891f8504-4429-46ba-a582-25063a4a8536))
    (fp_line (start 1.8 -6.85) (end 1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2202d1db-3549-4217-b023-3202758d42c1))
    (fp_line (start 1.8 1.8) (end -1.8 1.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0b19885e-8166-49fa-aca6-1aff9a4d4498))
    (fp_line (start -1.27 -6.35) (end -1.27 0.635)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 64c5fb39-faec-4f08-984f-fcdc3e37218d))
    (fp_line (start -1.27 0.635) (end -0.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 05cf6235-dbf5-43c9-b75d-c92f2f14d925))
    (fp_line (start -0.635 1.27) (end 1.27 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a369e24d-6d7d-4b55-bbbe-48a20c2a9ba2))
    (fp_line (start 1.27 -6.35) (end -1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 516eefd2-d58f-4165-8924-fd416f219aef))
    (fp_line (start 1.27 1.27) (end 1.27 -6.35)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 34188b03-8adc-437a-88d2-8443cb572ef1))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(Q12-B)") (pinfunction "1") (pintype "passive") (tstamp 923e5036-6410-4b9c-91c8-05030a7e5291))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "2") (pintype "passive") (tstamp 0c7b8dae-5bcf-440b-be0b-53ec2c497d42))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GND") (pinfunction "3") (pintype "passive") (tstamp 1c4627b3-e742-4bf9-9aab-0f8c265da172))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 21.043 13.5) (end 182.663 123.5)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp 38a52bbd-f414-4a79-8c9f-e11bc4d4f3bf))

  (segment (start 115.11 34.25) (end 115.36 34.5) (width 0.3) (layer "F.Cu") (net 58) (tstamp b6d31b9b-4ba0-4b14-98cb-80b3e684fe18))

)
