(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 84.5 17.5)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers")
    )
  )

  (net 0 "")
  (net 1 "+12V")
  (net 2 "GNDREF")
  (net 3 "-12V")
  (net 4 "Net-(C5-Pad1)")
  (net 5 "Net-(C10-Pad1)")
  (net 6 "Net-(C10-Pad2)")
  (net 7 "Net-(C11-Pad1)")
  (net 8 "Net-(C11-Pad2)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C12-Pad2)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "Net-(C13-Pad2)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 "Net-(C14-Pad1)")
  (net 16 "Net-(Q1-Pad3)")
  (net 17 "Net-(Q2-Pad1)")
  (net 18 "Net-(R1-Pad1)")
  (net 19 "Net-(R2-Pad1)")
  (net 20 "Net-(R3-Pad1)")
  (net 21 "Net-(R3-Pad2)")
  (net 22 "Net-(R4-Pad1)")
  (net 23 "Net-(R4-Pad2)")
  (net 24 "Net-(R5-Pad1)")
  (net 25 "Net-(J2-PadT)")
  (net 26 "Net-(R6-Pad1)")
  (net 27 "Net-(R6-Pad2)")
  (net 28 "Net-(R7-Pad2)")
  (net 29 "Net-(R10-Pad1)")
  (net 30 "Net-(R11-Pad2)")
  (net 31 "Net-(R12-Pad2)")
  (net 32 "Net-(R16-Pad1)")
  (net 33 "Net-(R19-Pad2)")
  (net 34 "Net-(R20-Pad1)")
  (net 35 "Net-(J4-PadT)")
  (net 36 "Net-(R23-Pad1)")
  (net 37 "Net-(R23-Pad2)")
  (net 38 "Net-(R24-Pad2)")
  (net 39 "Net-(R25-Pad2)")
  (net 40 "Net-(R27-Pad2)")
  (net 41 "Net-(R29-Pad1)")
  (net 42 "Net-(R31-Pad1)")
  (net 43 "Net-(J5-PadT)")
  (net 44 "Net-(J6-PadT)")
  (net 45 "Net-(R33-Pad2)")
  (net 46 "/FM IN LVL")
  (net 47 "Net-(J3-PadT)")
  (net 48 "unconnected-(RV7-Pad1)")
  (net 49 "Net-(VD1-Pad2)")
  (net 50 "Net-(VD2-Pad1)")
  (net 51 "Net-(C14-Pad2)")
  (net 52 "Net-(D4-Pad1)")
  (net 53 "unconnected-(J4-PadTN)")
  (net 54 "unconnected-(J5-PadTN)")
  (net 55 "unconnected-(J6-PadTN)")
  (net 56 "Net-(J7-PadT)")
  (net 57 "Net-(Q1-Pad2)")
  (net 58 "Net-(Q3-Pad3)")
  (net 59 "Net-(R37-Pad1)")
  (net 60 "Net-(U3-Pad3)")

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tstamp 0a6da648-8ed6-4fb3-89d1-2fffe35a4330)
    (at 144.85 124.15)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/5cec58a4-ff2f-4d89-ac51-f7259223375b")
    (attr through_hole)
    (fp_text reference "C16" (at -0.258162 -2.071892) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfa52eea-193e-44bb-8866-06bda5d987bb)
    )
    (fp_text value ".1uF" (at 2.666655 -2.120912) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d5da71f-cee5-4781-950e-97d789082938)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ab02c3f-68e3-4cb5-af83-9d41342b6a03)
    )
    (fp_line (start -1.37 -1.37) (end -1.37 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1fa4ac14-bad3-452d-a8c1-e7eeb6ec75dc))
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b55e2ad-e932-4553-b1ec-09b6131c87a7))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32c6b13e-36f5-49e5-87e0-e72d233b2210))
    (fp_line (start 3.87 -1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2f49ea9-ccf9-4e11-a110-ea74be4f9d0f))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 26031999-9526-4199-8920-e9cf3314591e))
    (fp_line (start -1.5 1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86df606b-f618-4030-9f59-21f3e91be886))
    (fp_line (start 4 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 910f47fa-29a9-4e5b-b0bc-4257edbbd457))
    (fp_line (start 4 1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e40e1be-2653-4bc9-b226-57a22b80e272))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 659fb018-5364-4e45-9418-5642101bb67f))
    (fp_line (start -1.25 1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56d1a675-dc95-491a-8691-f0d633d7fb81))
    (fp_line (start 3.75 -1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 726914e9-0e74-47d7-ae60-698d83d0249c))
    (fp_line (start 3.75 1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 779734d6-10d5-4479-b54f-6e7ef82544f5))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp f0fd12a9-3620-4185-b464-21f5837a596e))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp ad7fb963-4918-4740-89e3-7975ec38df33))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 0a9f96ae-26f6-4357-bf55-5e40bb135755)
    (at 136.05 117.9)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/f2055e72-3ea7-495b-ac86-171496a7ac87")
    (attr through_hole)
    (fp_text reference "J1" (at -4.03 -5.4 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f546e8d3-7ba9-4a7a-9101-8e9bd816d8f7)
    )
    (fp_text value "FM_IN" (at 0 -1.48 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b40d961d-bf89-4482-981a-5c22b6c44b6e)
    )
    (fp_text user "KEEPOUT" (at -0.05 0.3) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp f023daef-858e-494a-9dfa-8382ab07740c)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 581be911-96a7-48ad-9d11-628b381aacbd)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ddef303-b468-4e85-8b5f-43e9db9f1acb))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1ca58a6-0765-4c05-b52d-71076a7edd6e))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd0a0aff-78ed-44d1-82c1-789268f7d360))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd0d9419-1d11-49fb-81e9-0aa4899a085b))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a52aeaf6-711e-4822-88f7-2bdbdd128afc))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3648fac5-361c-40ab-b8d8-6827f0ddebbb))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5931c4ce-6e2e-46bb-aaf1-bb28d1ff30a3))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7889511e-fa47-462a-8629-ad86876afd71))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp e549aa39-f671-4191-ac9c-3705813ae233))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9c1cf014-fa95-43f3-a99f-336742230592))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0d66922f-92f1-4071-be8b-acb0e892c710))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68811e58-1d38-45df-86a8-35ee2ed28608))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25122fbf-539d-4522-b462-b0b129b4280b))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ed5c716-ac31-427a-b14c-100a82dccc55))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2540ad92-919a-4d16-9c97-fe1b975e7c57))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76067e52-d1a9-4184-8220-f5da1efeaca2))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e8192f02-ac19-42bd-8e67-3558c38787b0))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 24ca2d4a-0176-439c-99c9-28a64b7394a8))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp dce543b5-79d5-4cd3-b3cd-dc131f24301e))
    (pad "S" thru_hole rect (at 0 -6.48 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp f9b03c5f-987c-404a-a613-77353131f030))
    (pad "T" thru_hole circle (at 0 4.92 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 46 "/FM IN LVL") (pintype "passive") (tstamp 5a21c995-7861-48e5-af5f-ab36334148f9))
    (pad "TN" thru_hole circle (at 0 -3.38 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp c8e8accc-0e09-4c99-87b3-e5ea846327a7))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp de1d3b20-4620-4bae-8cd6-1b6ce24b0b62) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 137.555141 117.9)
          (xy 137.53493 117.654171)
          (xy 137.474841 117.414945)
          (xy 137.376486 117.188744)
          (xy 137.242508 116.981645)
          (xy 137.076504 116.79921)
          (xy 136.882932 116.646336)
          (xy 136.666992 116.527131)
          (xy 136.434482 116.444794)
          (xy 136.191646 116.401539)
          (xy 135.945007 116.398525)
          (xy 135.701187 116.435835)
          (xy 135.466734 116.512466)
          (xy 135.247946 116.62636)
          (xy 135.050697 116.774458)
          (xy 134.880286 116.952784)
          (xy 134.741288 117.156548)
          (xy 134.637436 117.380278)
          (xy 134.571519 117.617965)
          (xy 134.545308 117.863226)
          (xy 134.559507 118.109475)
          (xy 134.613734 118.350099)
          (xy 134.706532 118.578634)
          (xy 134.835411 118.788945)
          (xy 134.996908 118.975382)
          (xy 135.186687 119.132939)
          (xy 135.39965 119.257385)
          (xy 135.630079 119.345377)
          (xy 135.871785 119.394553)
          (xy 136.118278 119.403592)
          (xy 136.362936 119.37225)
          (xy 136.599191 119.30137)
          (xy 136.820697 119.192856)
          (xy 137.021505 119.049621)
          (xy 137.196223 118.875512)
          (xy 137.340158 118.675205)
          (xy 137.449445 118.454079)
          (xy 137.521149 118.218074)
          (xy 137.553344 117.973526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 141f9d43-90b6-4ef2-b9fb-ab46e8ef02df)
    (at 145.85 130.07 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/67042882-28b0-43e2-bc7c-aca17614c507")
    (attr through_hole)
    (fp_text reference "R22" (at 3.33 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da5573f7-be92-46f2-aec4-b15127510470)
    )
    (fp_text value "10K" (at 6.58 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce863558-108f-4551-8f83-c8beb6980933)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fc87698e-8307-48f3-8e1e-e62aa3fa02b6)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 533b6223-d663-4198-b7dd-86e388a00776))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f97ae523-265f-4efa-a5fd-203910bd2ec8))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab76fb61-a23e-42fc-9d98-9ec6d12f08e6))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e3f3bc8-bff0-403c-9f39-ed5c73cbc7bc))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d0794ce-e4f2-4dbf-822d-03dfa20ebff0))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a95a82df-fd49-4f00-b2ec-eb93c8a830b9))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f2dca5a-687c-4062-8641-6c649d7738f6))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f2308c4-7459-4d29-a0a6-5f08f033565b))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c2054d2e-89fe-47c1-ab23-e30b29710e66))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 50096a4a-87c8-47d6-9522-ed9d76315a42))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57601abd-c62f-4250-aeb1-f94f47f12112))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f39addfd-91aa-46f3-b674-99284bdfaf01))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b84a2c6c-0230-4080-aaa8-ed0feaed838c))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5575d42-e87a-410c-a7ac-d7dc5dfc9d25))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e091400f-4f20-4aa6-9b36-c64789b73593))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f0c8f3f-e45f-40b1-b4c5-154e0527b5de))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C12-Pad1)") (pintype "passive") (tstamp 604bfcc9-84ae-42b6-b924-3444de77618b))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D2-Pad2)") (pintype "passive") (tstamp 893b499c-ed09-40ed-8649-0fc12eeaf788))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (layer "F.Cu")
    (tstamp 14a3d088-f1ff-46b4-9224-94cb58b749ba)
    (at 158.6 76.9 -90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/2888c230-cc65-4349-b0d4-dfd4d7e4274f")
    (attr through_hole)
    (fp_text reference "RV2" (at -5 -5.75 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cad203bd-f55c-4c47-8973-6d64a6b56be4)
    )
    (fp_text value "100K" (at -5.25 5.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a2e8a9e6-738c-468e-8b49-9ce3f37ae3f2)
    )
    (fp_text user "${REFERENCE}" (at 0.12 0.04 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 66522276-2398-4fd0-918a-f6e7e9dbe6eb)
    )
    (fp_line (start -6.62 -4.88) (end -1.9 -4.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 345dc0d3-db0a-492c-8244-8d53412f64e5))
    (fp_line (start -6.62 -3.69) (end -6.62 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4f11ecd-b553-43a0-ae3f-ed0b20832770))
    (fp_line (start -6.62 -0.79) (end -6.62 -1.32)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2442958-9277-4132-8513-d827c74532d2))
    (fp_line (start -6.62 1.66) (end -6.62 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd153b34-3cc6-410c-b87b-cbe132afcfe8))
    (fp_line (start -6.62 4.87) (end -6.62 3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7345384-904b-4b2c-b65f-f890da5e433e))
    (fp_line (start -6.62 4.87) (end -1.9 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4dab38d-1600-497c-9dfd-841551d67f0c))
    (fp_line (start 1.91 -4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55d6f1b7-762b-4986-848b-89b2a867edb7))
    (fp_line (start 1.91 4.87) (end 4.97 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee2d7df8-9e9e-41dc-814d-f8e01656b90f))
    (fp_line (start 4.97 4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 629a72fd-ca2f-4a44-ab51-c0a6cf658941))
    (fp_line (start -8.65 -6.67) (end -8.65 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3c5161ce-037f-4a6f-babd-8c3b2df6627f))
    (fp_line (start -8.65 6.67) (end 5.1 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cf10d943-c7a8-4ec4-b22b-fd82988c8ff4))
    (fp_line (start 5.1 -6.67) (end -8.65 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5b9420b4-739a-455d-921d-950c1e2adcb1))
    (fp_line (start 5.1 6.67) (end 5.1 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0c886dd9-968c-4373-94f7-c7e60386bad3))
    (fp_line (start -6.5 -4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2a9cc1be-423b-4537-a901-2d756797a1f7))
    (fp_line (start -6.5 4.75) (end -6.5 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3071ca79-3ce2-48bb-b1e6-f0f1d201111c))
    (fp_line (start -6.5 4.75) (end 4.85 4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1a3c9d4a-767b-4980-994b-6c5209c7aa95))
    (fp_line (start 4.85 4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d55d2713-3425-48b3-96cf-60312692fd82))
    (fp_circle (center 0 0) (end 0 -3.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 20551ba6-95b8-407e-a649-53789a3392e2))
    (pad "" thru_hole circle (at 0 -4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp e5d7217f-499a-4c54-8ffa-77806ba4173f))
    (pad "" thru_hole circle (at 0 4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp d812e784-e521-460f-835e-3979ab02696b))
    (pad "1" thru_hole rect (at -7.5 -2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "1") (pintype "passive") (tstamp d5064625-d115-49d9-b36c-3bba39ae9eb7))
    (pad "2" thru_hole circle (at -7.5 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R4-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 89dea78a-6ec5-4ca0-91ac-c0b39781aa01))
    (pad "3" thru_hole circle (at -7.5 2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(R2-Pad1)") (pinfunction "3") (pintype "passive") (tstamp a8ac8e0b-cc34-4d7c-8ff6-7175d9c4ef13))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 14baadda-01d4-465f-92e8-fbff253e8246)
    (at 163.93 90.15 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c9d64c4d-d97e-4c7d-8600-8db4c7ddc736")
    (attr through_hole)
    (fp_text reference "R21" (at 3.5 -0.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60891aee-3897-4a85-a2c2-2a42283a9968)
    )
    (fp_text value "1K" (at 6.75 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 957b6eeb-b775-4df3-95d0-3e2d555b4025)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42a140f4-af68-4713-b26e-563ee4c08c66)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0fe01782-6768-4e6c-bc76-f792308c8316))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7cf15086-fa3c-4b30-99d0-15feff375037))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f319ec2-b3f8-46c2-b600-217020ee1a6c))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a298ceb8-f2d0-40f1-8072-9ac77d79ba93))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 90961539-653c-4fe9-86d2-ea7f6164178e))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 97dad12f-f35e-4bc4-b08e-049a98a6f47d))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea498dff-8f7d-463b-9ee1-0e4dea6cd99d))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 75165694-21ad-4110-b528-630a9e2decce))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1f1306c1-4348-4064-9ed1-0ab9786975bd))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0457f3ac-f4dd-450f-833c-dd11abababb3))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f82eb779-7d76-4013-b3cd-bc4df228bdbe))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65a42335-4ced-4474-b316-4de88fdbf2a4))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c1c97de-a4ee-4076-833d-f1291b1b866f))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15a0537c-384a-45a8-b626-a48792096cf0))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc305dd4-09aa-4c8b-93c9-09caff1d0a7b))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06d223ed-278c-4dea-b722-0700848b9b12))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(J4-PadT)") (pintype "passive") (tstamp 14c4e7d6-7e10-4e3d-a6d7-e8df26535884))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "passive") (tstamp e334e19e-b518-4fe7-8126-036624dfc397))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 22e20e67-328c-471a-bcdf-987911ef7f06)
    (at 181.1 117.9)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/5f2c94f3-ecb7-40d2-a6f9-77ae795f082a")
    (attr through_hole)
    (fp_text reference "J5" (at -4.03 -5.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20b37dbd-fb27-4e5b-9e15-658ffa24a3b5)
    )
    (fp_text value "TRI_OUT" (at 0 -1.48) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c591e4ed-432c-4d88-bdce-294af3fd9824)
    )
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 2764eeb5-5b58-4396-90b6-c43f0b134cc4)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa319366-14b8-4fe3-8503-8af7fbeab773)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c734e203-86b0-4617-9c9f-5f9c2010b977))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8949e3fc-1db5-400b-9d4f-0e976462c918))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21cb8e39-b735-4c25-8531-d73cfd9880c2))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb7f9f8d-8a39-4862-8ac5-e891ee8d46ed))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51a76218-4409-4250-8c7d-d7951608ddc4))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6097fa17-90da-49e6-b4dd-cf1a5ba17b3e))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp baf29bef-9a7f-4374-af5e-cfdefeada41b))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e54a9dc4-bd1a-4c59-8dbd-dd69ed498840))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 8052b94d-aeb4-49c8-94bd-65ca1af01e72))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 251ab195-02f6-4b81-b7bc-952d23f9033f))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5c4b0676-90e4-4f56-901a-0bc3ef03c371))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a6ac182-a63e-423f-83d2-c11572724d08))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dbb9e003-20db-4a36-a1a9-7cb4259b2190))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed70bd5b-7143-431e-96b9-a885fef9ebff))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 74be08c9-e9eb-4e91-b23b-5acc8dd65b91))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab8ab46c-a73f-40a9-8d0f-f26a0eeee9fa))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 772b592f-5bf9-40ef-bbd1-71a930de7050))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 98708628-0638-4acb-b875-f3981f9ffa27))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp fa1baea3-9d02-4abe-acbb-91be0efcf53a))
    (pad "S" thru_hole rect (at 0 -6.48 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 43a10353-f472-4880-a022-ff7af04cb6e7))
    (pad "T" thru_hole circle (at 0 4.92 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(J5-PadT)") (pintype "passive") (tstamp 63b3dda2-4bcc-4fad-91ee-48bfaa8baea7))
    (pad "TN" thru_hole circle (at 0 -3.38 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J5-PadTN)") (pintype "passive") (tstamp 9dd1cdc2-2877-4f09-821e-def1f5de937b))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 75c36cea-9aab-40a3-b8af-e08d8f26c38b) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 182.605141 117.9)
          (xy 182.58493 117.654171)
          (xy 182.524841 117.414945)
          (xy 182.426486 117.188744)
          (xy 182.292508 116.981645)
          (xy 182.126504 116.79921)
          (xy 181.932932 116.646336)
          (xy 181.716992 116.527131)
          (xy 181.484482 116.444794)
          (xy 181.241646 116.401539)
          (xy 180.995007 116.398525)
          (xy 180.751187 116.435835)
          (xy 180.516734 116.512466)
          (xy 180.297946 116.62636)
          (xy 180.100697 116.774458)
          (xy 179.930286 116.952784)
          (xy 179.791288 117.156548)
          (xy 179.687436 117.380278)
          (xy 179.621519 117.617965)
          (xy 179.595308 117.863226)
          (xy 179.609507 118.109475)
          (xy 179.663734 118.350099)
          (xy 179.756532 118.578634)
          (xy 179.885411 118.788945)
          (xy 180.046908 118.975382)
          (xy 180.236687 119.132939)
          (xy 180.44965 119.257385)
          (xy 180.680079 119.345377)
          (xy 180.921785 119.394553)
          (xy 181.168278 119.403592)
          (xy 181.412936 119.37225)
          (xy 181.649191 119.30137)
          (xy 181.870697 119.192856)
          (xy 182.071505 119.049621)
          (xy 182.246223 118.875512)
          (xy 182.390158 118.675205)
          (xy 182.499445 118.454079)
          (xy 182.571149 118.218074)
          (xy 182.603344 117.973526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 2e351837-8844-4256-b6c3-b520cc5ff916)
    (at 125.6 81.32 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/4315d178-8cdf-4d30-945c-c3156914c4c8")
    (attr through_hole)
    (fp_text reference "R6" (at 3 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 451c5015-34f3-4cc6-929f-459db8e23637)
    )
    (fp_text value "100K" (at 6.33 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c485052b-fcf9-46dd-92fb-e942f55e68d7)
    )
    (fp_text user "${REFERENCE}" (at 2.98 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e7623bcd-eebd-4d4f-85d9-e665bf999be8)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 783b3c30-bb00-4913-8390-6b8d97404e0b))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00aba788-0141-4370-8396-6a250e91ff55))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3433120-9205-455d-bd24-7040c7f2a8e6))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 80defed2-a5d6-421a-8947-f39dcf6b4d1a))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eba50b1d-ffef-4e10-bf73-424831de9ae0))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45dea1af-c930-408f-8889-248562397ae6))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2288b49a-064e-4086-b4fe-87045bad7c58))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a7a8d1db-1f4f-412a-a433-b6853c3aba99))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0f1e2c58-d199-4465-ae33-952565b5e5c9))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b316c067-a4a7-4de3-9d16-622c0b8611d2))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49fe3658-c2fd-44d8-9ede-93d1bf9d72e1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6fe737b-04d7-456f-8d0f-1e9ef4ddc927))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e7d4070-890f-47d2-8f78-ad7fcfbfde6f))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aca479ca-5434-421e-a5b5-e7e78bc5e2d5))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56dc39cf-64b1-4805-bd76-7d8da6a484ef))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9815eeae-e901-44b9-9b42-6d4a359ab7f3))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(R6-Pad1)") (pintype "passive") (tstamp 0895eec5-822a-4c68-85fe-eb825b96ea7b))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(R6-Pad2)") (pintype "passive") (tstamp ba404367-4b13-48c8-bc73-4e271cae850f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 3c615ced-b6c1-4896-9a6a-c2b62b9c23eb)
    (at 136.05 97.4)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/e0d6e8bc-a0de-4311-9fae-55de74d1ecca")
    (attr through_hole)
    (fp_text reference "J7" (at -4.03 -5.4 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30e737df-0449-4586-bce3-006993f6a1e6)
    )
    (fp_text value "SYNC_IN" (at 0 -1.48 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5e9d5d51-2468-45c6-b60a-94cadb8e41fb)
    )
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 06a21806-ed2a-4cce-b369-2bbd82a0664a)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b08cb89c-60f6-4a0e-9e71-0a6c8cc1527d)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2e2e9b00-6f22-4ca4-9534-4920708d4b03))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e358c455-9cbc-4947-8c6e-22b516282bfe))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0fca50d9-9a13-4e85-afec-e67b64cbd600))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b610becb-de8f-491e-afdf-2fafb1a45ae6))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a92069f-d83a-411a-8b0b-5a4fc28819f2))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 663fdff0-37ac-4152-a2a5-0b76bb2fafc6))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0bd0306-22f2-4028-acf6-f19bf0e41fd2))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a599ae7c-d540-4e18-b704-607c3c22fbb4))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 440dcc2f-3240-4a48-8b03-89223846c4d7))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 589d45b9-3914-409f-8ac1-a8b96fa38f90))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5315206f-168f-4b2f-9278-7c79d7365c0d))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd283216-e4b2-4cfa-ae38-f4d67456f7dc))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b19c1e5d-06b1-41be-bc39-a43f3e478679))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 85137f7d-4bd9-4adb-810c-146eaab46c60))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69354fba-ad4d-45b0-b8c7-eac6b02b6ea0))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b5241ad-ccaf-4278-aac2-6966bbe90188))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d278be0a-4981-483c-8e93-86beeccc5434))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 44513dc7-e5b0-4af1-9f07-15c54c9d4261))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp fe53da05-d3a4-4ddb-b2fd-372b02154882))
    (pad "S" thru_hole rect (at 0 -6.48 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 17f732bf-3cb5-4cf7-860c-67114e8c9c29))
    (pad "T" thru_hole circle (at 0 4.92 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J7-PadT)") (pintype "passive") (tstamp 8fffc3fa-97e7-4794-a456-3ced90912dd5))
    (pad "TN" thru_hole circle (at 0 -3.38 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 76a07985-170d-48f0-bdda-4ea9dfcae1f5))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 74cb9f43-b4e9-4ffc-9db1-c18af2d12319) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 137.555141 97.4)
          (xy 137.53493 97.154171)
          (xy 137.474841 96.914945)
          (xy 137.376486 96.688744)
          (xy 137.242508 96.481645)
          (xy 137.076504 96.29921)
          (xy 136.882932 96.146336)
          (xy 136.666992 96.027131)
          (xy 136.434482 95.944794)
          (xy 136.191646 95.901539)
          (xy 135.945007 95.898525)
          (xy 135.701187 95.935835)
          (xy 135.466734 96.012466)
          (xy 135.247946 96.12636)
          (xy 135.050697 96.274458)
          (xy 134.880286 96.452784)
          (xy 134.741288 96.656548)
          (xy 134.637436 96.880278)
          (xy 134.571519 97.117965)
          (xy 134.545308 97.363226)
          (xy 134.559507 97.609475)
          (xy 134.613734 97.850099)
          (xy 134.706532 98.078634)
          (xy 134.835411 98.288945)
          (xy 134.996908 98.475382)
          (xy 135.186687 98.632939)
          (xy 135.39965 98.757385)
          (xy 135.630079 98.845377)
          (xy 135.871785 98.894553)
          (xy 136.118278 98.903592)
          (xy 136.362936 98.87225)
          (xy 136.599191 98.80137)
          (xy 136.820697 98.692856)
          (xy 137.021505 98.549621)
          (xy 137.196223 98.375512)
          (xy 137.340158 98.175205)
          (xy 137.449445 97.954079)
          (xy 137.521149 97.718074)
          (xy 137.553344 97.473526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 3d660348-830e-42e0-945f-aef90159d0b5)
    (at 182.27 126.15)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c10f4bdc-d1b6-491b-b016-4d2989012f0a")
    (attr through_hole)
    (fp_text reference "R32" (at 3.5 -0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11b32c22-b336-487e-aaf2-dc1262902042)
    )
    (fp_text value "1K" (at 6.25 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92a799b2-846f-474c-8153-1fd3c6e64aac)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c75ce8da-0b8f-4a31-8ce2-b1a7b9e4b0c2)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp adc2f7b5-d40a-4fee-885b-a164703d649c))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fea9972d-33c1-4902-a2c4-1c365c13a0bd))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee47e275-a60a-4097-b216-136c1ab96b2d))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp db71a785-f8cf-489b-b28f-7e80c7cbe56d))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7822ac8a-4815-4449-9266-981a45371f26))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 334c44d7-4085-4844-ba6f-29504e8648e5))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 44222534-617d-40e2-8ed5-b3975e0d883c))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8a4acfbc-192c-47d9-8f0e-e8b2825a3860))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 96382378-2ba0-4f65-b933-66758732bc49))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fddc5fff-9c0c-4574-9083-9890be5a8985))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7760c169-507a-4ca4-81dc-a9ab71f011a9))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff06ae3e-a583-48d1-929d-8dae68c773c9))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5681c34d-d94e-475f-8aed-d98f12ce09d6))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a261d2a-cf5e-450e-b0a8-4f7d45994ebc))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a7e9355b-e620-4d77-8947-b6f1d58d4fa5))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 75e5ed43-aeee-4eb2-8abc-aec7d1b3558c))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(J5-PadT)") (pintype "passive") (tstamp 6fb6c74a-4b63-422e-b3b0-7d88de60ec12))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(R31-Pad1)") (pintype "passive") (tstamp 1697d08b-9c16-410f-b51e-5ade6d7c283f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 48017128-8de0-469a-b8bf-4f590af47ceb)
    (at 181.1 138.4 90)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/0449179c-4b8b-4907-b000-447f961b9fc4")
    (attr through_hole)
    (fp_text reference "J6" (at -4.03 -5.4 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8f3ac756-5f71-4fd9-a03f-6c1de98d9db7)
    )
    (fp_text value "SQ_OUT" (at 0 -1.48 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c194b632-ac8f-4a45-8bb6-81aaf3764040)
    )
    (fp_text user "KEEPOUT" (at 0 0 90) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 571014d2-4a3d-4760-9b77-aa3613a6cb01)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f79312f-686a-4ebe-b54e-1bd70c1e6940)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7fde706-442f-41fe-ad15-c5dcf1a5237b))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 53cad44d-0bb4-4d2d-b4df-f9ed29e0e7ef))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e66f57a9-66c3-482e-87f6-102b5de1fcaa))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0a6d6643-a303-400a-bcb7-d3dd1a7c7de8))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42d89100-fd8d-4d3f-990b-7c8ac8e7eea9))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 660a852a-9fe7-49dc-89b0-3dc672b9750a))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e340b1e-a0f6-47dd-a7fb-49fa2136537c))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1dd02f92-fde1-4011-8e94-2a6a30457699))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 8d6467e6-1e9d-4c17-95b0-e126025a36aa))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b237e83b-1721-4995-a3f7-6565467ffb48))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cc8012b1-752f-47de-8abb-7b1bf49feed3))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a52553f3-caa4-4e20-a655-a86cc8e607c2))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0814eef5-a2e5-4774-99bc-f055ee6d3566))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dd03553f-fcac-47c8-b22d-185a479470ba))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d8bea0f-3363-4d08-b4ec-c32a245ef342))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93a122a6-2ac7-4f9d-9525-2c66f89cff49))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49d441ed-2521-4e59-8a5d-ee9ff3ea0667))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b679ca13-fb69-407f-88fd-c29960e0e3da))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp d568ef93-a382-4e85-b61e-869d7ad3b183))
    (pad "S" thru_hole rect (at 0 -6.48 270) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 75f8133a-3d55-486f-bd18-e41d8e09bc32))
    (pad "T" thru_hole circle (at 0 4.92 270) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(J6-PadT)") (pintype "passive") (tstamp 240e6db2-1621-4490-a281-0d8afe741679))
    (pad "TN" thru_hole circle (at 0 -3.38 270) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(J6-PadTN)") (pintype "passive") (tstamp 966357be-beb4-4fcf-87ad-49b6ff498a7b))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 629fc181-fec4-4fbf-9fbb-532eee06df03) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 181.1 136.894859)
          (xy 180.854171 136.91507)
          (xy 180.614945 136.975159)
          (xy 180.388744 137.073514)
          (xy 180.181645 137.207492)
          (xy 179.99921 137.373496)
          (xy 179.846336 137.567068)
          (xy 179.727131 137.783008)
          (xy 179.644794 138.015518)
          (xy 179.601539 138.258354)
          (xy 179.598525 138.504993)
          (xy 179.635835 138.748813)
          (xy 179.712466 138.983266)
          (xy 179.82636 139.202054)
          (xy 179.974458 139.399303)
          (xy 180.152784 139.569714)
          (xy 180.356548 139.708712)
          (xy 180.580278 139.812564)
          (xy 180.817965 139.878481)
          (xy 181.063226 139.904692)
          (xy 181.309475 139.890493)
          (xy 181.550099 139.836266)
          (xy 181.778634 139.743468)
          (xy 181.988945 139.614589)
          (xy 182.175382 139.453092)
          (xy 182.332939 139.263313)
          (xy 182.457385 139.05035)
          (xy 182.545377 138.819921)
          (xy 182.594553 138.578215)
          (xy 182.603592 138.331722)
          (xy 182.57225 138.087064)
          (xy 182.50137 137.850809)
          (xy 182.392856 137.629303)
          (xy 182.249621 137.428495)
          (xy 182.075512 137.253777)
          (xy 181.875205 137.109842)
          (xy 181.654079 137.000555)
          (xy 181.418074 136.928851)
          (xy 181.173526 136.896656)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 49ef2a75-2e10-4083-a3f6-5312d3f892ae)
    (at 136.05 55.2)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/40927805-ddd9-4832-9cfa-124d7beeaa55")
    (attr through_hole)
    (fp_text reference "J2" (at -4.03 -5.4 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c9543b48-4c51-4db4-80e3-c9c7cb2c12c5)
    )
    (fp_text value "CV_IN" (at 0 -1.48 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e969788-85e4-4613-b1a7-ed85eabab6ef)
    )
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 3e9b490e-9a57-4868-a01d-795ce4e50298)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a0c0b5f4-37b7-45ed-bb1f-e3a3e765ce14)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f4f312b-fa49-4672-900b-e9d783938882))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6c8ca92-e448-44ac-a05e-3195bc572e86))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3445729-3e47-4715-a547-0199e45fd623))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb0e5431-bc6f-43aa-9392-19e7e3f09860))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 730b5a95-34b9-4cc3-a33f-278d4b72790e))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1db067b-6c31-4714-9873-9be0129776e8))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp efbd208a-dec5-47e6-a6a7-6d5926c2058e))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1a32f676-71c9-42a4-ac8c-31d3cf6de3b9))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 55d6e31f-543a-4fa8-b4d1-27d2384d1382))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01c2e735-0638-462f-bde8-5e4e7528edf9))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71c6558d-f8c0-418e-b42c-54e4565d6bf2))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp baa29258-3634-4b13-b063-63c57931596f))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 848cb197-7170-4fbd-a975-5cae53a83bbd))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49dc9c79-f8da-4408-9e73-6d891f0e2479))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 67fddf12-4017-4acd-a71f-a06b8fd3e0d0))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ef508e58-82af-441e-9112-8650c34917e0))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db9d871f-7281-47a9-aacd-d637bd0b6312))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 73844c29-90d7-4757-ad55-3b319d5d2ed3))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 60a2a357-bff7-45ea-8b23-08145d73b3a0))
    (pad "S" thru_hole rect (at 0 -6.48 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 41e05fa2-2e04-4519-898e-7577a581b872))
    (pad "T" thru_hole circle (at 0 4.92 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J2-PadT)") (pintype "passive") (tstamp 54c67054-db4a-496a-a9bb-77a3e8dab4f8))
    (pad "TN" thru_hole circle (at 0 -3.38 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 352991c7-2d1d-4b29-8499-cf37f76d82af))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 813c2f0a-35c4-45fd-931e-2b9f62fde48c) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 137.555141 55.2)
          (xy 137.53493 54.954171)
          (xy 137.474841 54.714945)
          (xy 137.376486 54.488744)
          (xy 137.242508 54.281645)
          (xy 137.076504 54.09921)
          (xy 136.882932 53.946336)
          (xy 136.666992 53.827131)
          (xy 136.434482 53.744794)
          (xy 136.191646 53.701539)
          (xy 135.945007 53.698525)
          (xy 135.701187 53.735835)
          (xy 135.466734 53.812466)
          (xy 135.247946 53.92636)
          (xy 135.050697 54.074458)
          (xy 134.880286 54.252784)
          (xy 134.741288 54.456548)
          (xy 134.637436 54.680278)
          (xy 134.571519 54.917965)
          (xy 134.545308 55.163226)
          (xy 134.559507 55.409475)
          (xy 134.613734 55.650099)
          (xy 134.706532 55.878634)
          (xy 134.835411 56.088945)
          (xy 134.996908 56.275382)
          (xy 135.186687 56.432939)
          (xy 135.39965 56.557385)
          (xy 135.630079 56.645377)
          (xy 135.871785 56.694553)
          (xy 136.118278 56.703592)
          (xy 136.362936 56.67225)
          (xy 136.599191 56.60137)
          (xy 136.820697 56.492856)
          (xy 137.021505 56.349621)
          (xy 137.196223 56.175512)
          (xy 137.340158 55.975205)
          (xy 137.449445 55.754079)
          (xy 137.521149 55.518074)
          (xy 137.553344 55.273526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 5883673a-7880-42b3-97d1-3affdb389c2e)
    (at 150.1 98.07 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/e92b8667-f8ca-4b81-b2d9-dff4b91ab131")
    (attr through_hole)
    (fp_text reference "R24" (at 3.33 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e917111-4fa1-4c2a-8018-7fb13332c248)
    )
    (fp_text value "100K" (at 6.33 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61b2f5ec-0b14-40cb-9459-fdb2ebba2645)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa22c3c9-422e-42f9-82da-55e68937a678)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f7a65c7-3dc2-4a7a-a141-3b63a747201f))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ca9cefd-f1a1-431a-bbb5-954303e328eb))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 111f581b-ec21-42d5-b115-d31b98be3053))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b24d3f04-1403-4756-a4a7-b1600fe27407))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f32da5c-e454-40b9-a930-c0552c69dad4))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0aeec3c-e60d-488e-ac97-83dd20e26e7a))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1b09b8cb-7ab4-451f-939e-d3333307af7d))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c651d6ad-1918-4816-857e-959ed9df4c70))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7285c32d-67c2-4c8f-9b81-849c8381e8b6))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc0bc9ef-34fc-4bc0-b94f-c9603671edb7))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16977e53-5ee9-423a-b4ab-0353cb730faa))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed684e05-95a2-4b4d-ae59-3847555c4274))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff66006b-e13a-4be1-9d92-6c9660de79d9))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c66d5171-9965-433d-8b9a-c405b436af6b))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33fa7494-c6b1-4050-a457-668cf37afd07))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e97c9ae1-473b-4a40-aa88-e7cf68097018))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(R23-Pad1)") (pintype "passive") (tstamp 12d58878-ca99-4a37-8be0-27d01439d50a))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(R24-Pad2)") (pintype "passive") (tstamp 6c0ae560-13c9-4bf0-a2af-56bd52072a0c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 5949fef2-1641-426c-a2bd-92a596567612)
    (at 191.6 142.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/7f86f1af-aa51-48df-b254-37b6556d9b08")
    (attr through_hole)
    (fp_text reference "R33" (at 3.58 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp acbabd2f-6a0f-4fbf-a0ca-d060cc9b5ee1)
    )
    (fp_text value "1K" (at 7.08 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 65aba65b-a769-4cef-9aa3-d3959e5b2f18)
    )
    (fp_text user "${REFERENCE}" (at 3.58 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5558a8d-660f-4d52-b241-03846abb4430)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f459c8fc-8524-4101-87b7-c4d0b3382690))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42576a82-e309-438a-a090-e4fffd32608d))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6549046c-4b04-4f46-8e75-51292b6afd71))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7733410d-86f2-4849-8f32-47dae4f30027))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7cfc628-a408-46b4-9259-d9501c8ec468))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 541b2225-a7a7-46fb-9a79-4b516907a8bd))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cfa41882-d9aa-49d8-92da-4271733506fd))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 17621896-724b-445c-9b61-5cd0510e8a60))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 243e9d31-aa98-40ab-b2f0-58a1176f9437))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c45dd6fe-282e-491f-a9f7-bdd023f11151))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a3500f8e-b441-4ddb-b932-678e64df6966))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2152982c-0967-4243-b53f-a346f7675936))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dbcdd812-dcec-4f6c-94db-43232f16a0d1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd4cdf1a-2498-4e1a-ae86-b405d3b1873f))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 32d13d1c-5051-4e12-8f7d-7a82504e21f4))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5af3038a-9e43-46aa-b726-d1235e8c8afc))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(J6-PadT)") (pintype "passive") (tstamp 999af84b-a868-4040-ad45-6d43457be0b4))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(R33-Pad2)") (pintype "passive") (tstamp cef8d008-033c-46e1-b34f-6fa97fcc85ef))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 69ef77bb-d2ff-4baf-9cd8-1877d1a4fb25)
    (at 191.85 108.9 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/b2019e55-7428-42e3-9104-e54a773ca7c1")
    (attr through_hole)
    (fp_text reference "R29" (at 3.5 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef190d6d-d0cf-422d-acfb-545883f56f50)
    )
    (fp_text value "**" (at 6.5 0.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9cfaf4c5-9eeb-472f-9ae7-dd4c147acc20)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad38e939-3e5a-4d83-b293-234553a9c9fb)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e38bc5e-e755-464a-aa2a-ae4571657948))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42400aeb-7269-4592-92f0-dc406a7dc982))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d91927b-8aff-446c-9fd3-f06a95e0d456))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 968a9b85-0a99-4045-8aa5-6c982b0d551d))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c5fc7b4-a6de-4a22-9f8e-6a8c74a777bf))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e0ea655-e4d9-41c8-ba2d-a7f355bd927d))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22ec714d-75e9-4d16-a261-fae3c9474523))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4502634f-067b-41ff-a3d4-1a42b7685918))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 933075bb-e5c1-43ff-bb01-3bda1fe60da3))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a2e63a17-741a-4284-9e01-db6c88d8b1c9))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c2d1cf1-e598-406c-8626-6eaaec0f40c8))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 72af529f-a00d-40e1-934f-7c377686d068))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 51b8cf06-51c3-4ebb-911a-3b9d06fdb504))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15853ed7-0103-4f4e-a862-fd64ce7de10e))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af4da348-0ff1-4ad1-8d9f-d8933f92bc5a))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b351d249-21f7-4884-8c43-041005af07df))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R29-Pad1)") (pintype "passive") (tstamp 3db3a945-301b-44c2-b04a-f439dc002b05))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 3d61204c-1645-48f6-821f-2ad14bad665b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tstamp 6c623fce-9316-4374-b18f-9836dbb74d06)
    (at 143.85 109.9)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/7fb3ceba-a964-4432-a72b-9aff5710a991")
    (attr through_hole)
    (fp_text reference "C15" (at 1.25 -2.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3093f66-ec80-4e2e-8303-bc1a78dababc)
    )
    (fp_text value ".1uF" (at 1.25 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 80613d5f-23c2-4347-a9fa-e050acd66346)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp baba9d46-9c29-4526-a31c-6d8accab29b0)
    )
    (fp_line (start -1.37 -1.37) (end -1.37 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51537cd7-5584-4e61-bd5f-de2c30f85305))
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2610ffcf-fdaf-4d72-8719-7f1853521e62))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cefe35f7-5867-48cf-a407-fbc5a31de49f))
    (fp_line (start 3.87 -1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1e7b255-b52c-4e7e-a748-eb2da756c001))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ff3c824e-22fb-461d-a312-a14889706192))
    (fp_line (start -1.5 1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7c8641a5-d9c2-442d-bc44-531a483cb5e0))
    (fp_line (start 4 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a029d22-3361-440b-b8c7-85811123d7a4))
    (fp_line (start 4 1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 148d2a5b-57c6-44ac-8440-86cb5e3344bd))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cce2cfdf-28a4-48db-b491-609ddd281dc7))
    (fp_line (start -1.25 1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4ca33c91-fae9-4b0c-9832-45c9c13ff6cb))
    (fp_line (start 3.75 -1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp df01c8f7-2dcc-4d7f-a85a-5980e16f39b9))
    (fp_line (start 3.75 1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f86897e4-3bee-4c99-8e75-0480164d5199))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp 8c181660-a9b9-452e-81f6-e9dd24235e1b))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp f4398722-cbba-407f-bd0b-5f5f8797edba))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tstamp 703403b3-027b-4a21-b16a-43011b704f4f)
    (at 161.6 126.15)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/1a250a36-f5de-4042-9d30-567ead176c50")
    (attr through_hole)
    (fp_text reference "C4" (at -0.5 2.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 08d9819c-678b-4f9a-bff9-6e86623ada7c)
    )
    (fp_text value ".1uF" (at 2.25 2.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9c67da8e-3f66-46d5-8cd5-81780eab51aa)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b94156a-89ce-4a39-8dd7-22d9e032963c)
    )
    (fp_line (start -1.37 -1.37) (end -1.37 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d897edcc-134f-4b22-ae96-e78e6c5b1022))
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5ab683d8-ac19-49ed-b994-8e715746f19b))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 865ff1e7-d7de-4273-a25f-375586229247))
    (fp_line (start 3.87 -1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 03d68a92-0a12-46c0-88c9-34deae6f9105))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc05a55e-fb5c-4631-9248-913fcf9877c0))
    (fp_line (start -1.5 1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 253d2026-65d3-4ff3-a476-022f25445c81))
    (fp_line (start 4 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 142ddb1e-25a0-4faa-9970-6a2a2f0c2ef1))
    (fp_line (start 4 1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c948215-9acb-42bd-9c00-390032fa3204))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2abb40b8-3ecb-4d41-adcd-1f63396d01b6))
    (fp_line (start -1.25 1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eafa907f-78b7-458c-b047-598f55c97288))
    (fp_line (start 3.75 -1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db075aa6-c05c-42d4-9275-b4f3d0bb358b))
    (fp_line (start 3.75 1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cfff3698-9f3a-4217-83df-467cbe5a42d0))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 1d388508-8964-4810-b4ae-1960f429ee32))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp dd7bbc26-af86-4b24-b2aa-f77cfffbb4a2))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 79cffb50-ee73-4787-849b-27ad0de0ec7f)
    (at 177.02 87.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/8cccf5a0-cdb8-4fc8-b59a-35d7c9681368")
    (attr through_hole)
    (fp_text reference "R15" (at 3.245113 -0.36) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f285032b-8bdd-432b-b690-dee3edffdef5)
    )
    (fp_text value "100k" (at 6.245113 0.64) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed0bab0e-d85d-47fb-8303-e102979090eb)
    )
    (fp_text user "${REFERENCE}" (at 3.245113 -0.36) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e11a705b-1f34-48f8-aaa9-8c563588d538)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d51cc26-939e-4979-92c5-8fd23058d725))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f596704a-9e46-402b-9eea-078bf1c2ec4a))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51c9e1a9-81d6-4a2f-87ac-6650fb9e14ab))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9dc3a696-ba50-4c19-b5fb-cd424cb98138))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b3132a22-b9e8-4fd2-ac64-ff0e6317c56a))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b79a920f-44e1-4ec0-9b9c-774d45f10d04))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55746c9a-f838-406d-92bf-7eb8a8509ac4))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3950237d-fb3f-456c-95c1-ae1480b4b7a3))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 680e54b4-5ec3-4f7d-ba27-fa2fa95a394d))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp adf96669-ec94-45a0-8982-56842db057fc))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ae58bb5-93e6-4c93-9a51-bbea1fd565fb))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3188d087-1bf1-4ffe-aac6-2c642583f866))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e3a7fbc7-268d-4312-a3d0-0990ac26d7ab))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15f648fd-2350-4672-9667-7519a6f882d8))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9fd21951-3e4b-46de-9351-3559a091b48e))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e856066c-619a-44e2-94ac-b7a41ddb41a2))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C10-Pad2)") (pintype "passive") (tstamp 87ef3c94-17c0-4e74-bc62-559eba6c6e03))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp b454a492-50e1-423a-bc2f-0bafcc52ca33))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (layer "F.Cu")
    (tstamp 7b16c215-3200-4c55-acd8-4d22f5b9e983)
    (at 158.6 117.9 -90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/05a69210-bdd3-4b43-9397-212eac96b88f")
    (attr through_hole)
    (fp_text reference "RV5" (at -5.25 -5.75 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 24a642c6-0629-4596-8d0b-615831673eff)
    )
    (fp_text value "100K" (at -5 5.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53c6be2d-b34b-4a71-b208-ff1acf36d58d)
    )
    (fp_text user "${REFERENCE}" (at 0.12 0.04 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 87350b4b-6ff7-4fc8-bbd7-2f9d433feda5)
    )
    (fp_line (start -6.62 -4.88) (end -1.9 -4.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d759b80b-ee9c-4bdb-8d0e-35b725221d66))
    (fp_line (start -6.62 -3.69) (end -6.62 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5b6097de-5c39-47c8-9fb7-577ca551fa23))
    (fp_line (start -6.62 -0.79) (end -6.62 -1.32)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3074b7d-e7a4-4093-a5ff-2526d0149786))
    (fp_line (start -6.62 1.66) (end -6.62 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e491d5d3-cebe-47fa-9bbd-9a2c62b51ae0))
    (fp_line (start -6.62 4.87) (end -6.62 3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35c14cb3-7f05-45a1-ae58-34487320e51f))
    (fp_line (start -6.62 4.87) (end -1.9 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c3bd968-767f-46dc-969f-a7d33a4384a3))
    (fp_line (start 1.91 -4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de3f5f43-9ea2-40a1-8cfd-26d5eccd623a))
    (fp_line (start 1.91 4.87) (end 4.97 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee211b3b-33c6-4996-bd2a-62654826ec82))
    (fp_line (start 4.97 4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4b75abae-e3eb-4dc5-84fe-72d2c9cdda39))
    (fp_line (start -8.65 -6.67) (end -8.65 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fdcf7d97-3083-42f9-b918-406e39cc1f79))
    (fp_line (start -8.65 6.67) (end 5.1 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5929f4ff-99dd-422e-8ea0-d25555cfda72))
    (fp_line (start 5.1 -6.67) (end -8.65 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a1f0593-959c-4059-8912-0375afcedd6e))
    (fp_line (start 5.1 6.67) (end 5.1 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71a8f3a1-9a60-4c7f-b3d1-46866aa876bd))
    (fp_line (start -6.5 -4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f0cd6218-e743-4071-b26b-d8ee3db2dc97))
    (fp_line (start -6.5 4.75) (end -6.5 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 47fdbaa5-5dd3-454b-8a53-12ae9175ec76))
    (fp_line (start -6.5 4.75) (end 4.85 4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e575e397-f8cc-4573-9720-ab22ed4a690c))
    (fp_line (start 4.85 4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c9959db-2c37-41ea-bd73-b7d266f5a1cd))
    (fp_circle (center 0 0) (end 0 -3.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 0d4dd2c9-e21f-4e04-b735-1c27bd5de7fb))
    (pad "" thru_hole circle (at 0 -4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 8ef7f909-862f-400f-a1a3-fc4a1c5d7234))
    (pad "" thru_hole circle (at 0 4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp bff31919-06fd-4a18-8257-75407e9eb6dc))
    (pad "1" thru_hole rect (at -7.5 -2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(R19-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 89411efa-db2d-461c-8ac6-2f1d30dfcf3f))
    (pad "2" thru_hole circle (at -7.5 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(R23-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 3e1bccf6-24c6-421c-87a0-2c4e5da5cc4a))
    (pad "3" thru_hole circle (at -7.5 2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(R20-Pad1)") (pinfunction "3") (pintype "passive") (tstamp 0b5cb5ab-f901-4cf2-a012-3725689206d0))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 875eb827-68e8-4f85-b1f0-15547f0fd904)
    (at 176.68 68.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/515aae10-aab2-4227-ab18-3be09190d2b3")
    (attr through_hole)
    (fp_text reference "R12" (at 3.5 -0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7508db9c-4356-48fc-9d48-4c803759cb61)
    )
    (fp_text value "100k" (at 6.5 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 147a0cb8-1b30-40b4-813a-1ed877d32f9b)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 18416ef0-f9f1-491e-9fa4-8883333837f3)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bfc0bf46-e5b6-4bfe-9d54-1dbc9d90fcb4))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9521851-1431-47c3-a0f8-43f3dc09536d))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4903159-7b7c-4e43-9a78-9f43395f785f))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c0051d1a-023d-4fbe-977c-6397e7500318))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b06673be-9603-49ce-b4db-530ca16b58cb))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9e11cf5d-219b-47b0-b0e8-287b23327df3))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8fd5f04e-34d3-45ba-b860-bd5f3bea8d8b))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7b114399-cdf2-4a94-9cac-15f3a42e2b6a))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 445e17df-955a-45cf-a77d-f6feb369b38f))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 677db1e6-0709-489e-9241-f096d99b3a99))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18ee179a-d0b7-4033-bb38-30a76d9ceb27))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d61e910-e0fb-4b17-87ee-ef2318563de4))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7cc0de8-2636-4f73-baf6-9599f50a488a))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9697f67f-e79a-4452-9635-421122e38c21))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d408a226-8c24-4949-aac6-22bea27a295c))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp da058e18-19fe-4da6-8ec0-c8c3138d04e8))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp be8a50cd-a7d0-43cd-a1a4-934aa9450190))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(R12-Pad2)") (pintype "passive") (tstamp 9eb107fb-04f2-4a8a-bcce-7684979cd064))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 8a621a45-2ff0-457b-ab02-cd3b0ccceeb4)
    (at 192.1 66.9 180)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/cbfbbf7a-dd7f-4e06-927f-304167ceb7a0")
    (attr through_hole)
    (fp_text reference "VD2" (at 5.45 0) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp edb69ce5-c20e-4b25-a433-7a70087c810e)
    )
    (fp_text value "1N5819" (at 5.08 -2.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f39186c7-097d-40a7-b532-e5e8bf09d23e)
    )
    (fp_text user "K" (at 0 -1.9) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 963eccbd-2ca7-481e-9d10-eb52ebcb9742)
    )
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f5b34b5-09b2-496f-8ac8-58e7478862f2)
    )
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5199e2eb-3f99-48d7-be81-85361c3e2337)
    )
    (fp_line (start 1.14 0) (end 2.36 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ae0388e-bf19-4640-a024-e793501e503a))
    (fp_line (start 2.36 -1.47) (end 2.36 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40594118-682f-4ec5-b151-45e9a05aca36))
    (fp_line (start 2.36 1.47) (end 7.8 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e31d2d9-902f-40ed-95c1-b9238b4e46c8))
    (fp_line (start 3.14 -1.47) (end 3.14 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dac2272d-434e-4e4c-a2a3-19b0a6818d48))
    (fp_line (start 3.26 -1.47) (end 3.26 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f145a5c-1e35-4090-94d3-224c56924cd5))
    (fp_line (start 3.38 -1.47) (end 3.38 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c609e958-b178-4e1c-a7fe-b108a773d111))
    (fp_line (start 7.8 -1.47) (end 2.36 -1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cde1cf99-94a8-4b2e-9714-062984534bd4))
    (fp_line (start 7.8 1.47) (end 7.8 -1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 91a051fc-9860-4b4a-abce-2aa84a4ee3bf))
    (fp_line (start 9.02 0) (end 7.8 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6cb39c1d-ff36-44c6-9b07-4ec5d09b89ae))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dd2d2ac1-76e6-4086-adcc-bf2ab6b925a7))
    (fp_line (start -1.15 1.6) (end 11.31 1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8b0de59-6abe-4e15-9d4d-480cf0af4c86))
    (fp_line (start 11.31 -1.6) (end -1.15 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3b93530a-13ce-445d-8cbf-f2854713e4de))
    (fp_line (start 11.31 1.6) (end 11.31 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 202f94e3-09ba-414a-bda6-402564247b35))
    (fp_line (start 0 0) (end 2.48 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1063b581-528d-43e3-b143-08a92c98ef89))
    (fp_line (start 2.48 -1.35) (end 2.48 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d24abac-3292-4560-8983-ebd62b14bc02))
    (fp_line (start 2.48 1.35) (end 7.68 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d763466-1eb7-4348-8281-325f4485ea35))
    (fp_line (start 3.16 -1.35) (end 3.16 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b29faeb-015f-4aa1-9050-a217048cedcf))
    (fp_line (start 3.26 -1.35) (end 3.26 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ca37b81-2a5b-49b4-ac7b-0d1053d3cec7))
    (fp_line (start 3.36 -1.35) (end 3.36 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 75e9c763-d6c1-40b9-89e1-b5c97b8aa30d))
    (fp_line (start 7.68 -1.35) (end 2.48 -1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd7925e9-f4f1-43c0-bf58-c4510cd6c1b0))
    (fp_line (start 7.68 1.35) (end 7.68 -1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d9346d8-4c37-462c-ae25-3d5f49b0fcf8))
    (fp_line (start 10.16 0) (end 7.68 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 574ea41b-f050-4288-87a2-865d4b95af62))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(VD2-Pad1)") (pinfunction "K") (pintype "passive") (tstamp edbe2d93-e1cb-4ee1-b92b-204fe7335c78))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(R11-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 1f9a8e27-b22c-43ec-a33a-798b0f8ba7b9))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tstamp 8a6347f9-342c-4f57-89f5-1691cc775b8e)
    (at 176.85 126.65)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/3016c27b-8d50-49e7-bd06-4f93bdf92b3b")
    (attr through_hole)
    (fp_text reference "C3" (at -0.25 2.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53467752-89fa-4ff7-aeed-08b4bda29a93)
    )
    (fp_text value ".1uF" (at 2.5 2.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f1ecfa00-b9d2-4a10-9cdc-b676dd609359)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 990e3ec7-60d1-4d71-9b53-d5e5fffc5db8)
    )
    (fp_line (start -1.37 -1.37) (end -1.37 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 427c89ec-adae-4b27-a023-2c2b45ce02af))
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa60a177-4392-40d1-914e-90c16d338742))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d108f5b4-a73c-4601-bcb5-61c6c5b9cea8))
    (fp_line (start 3.87 -1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9d6e5f9-510f-4bf5-b435-8e46f33c3258))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7dfea32b-d97d-471a-9beb-911ae0d1adc5))
    (fp_line (start -1.5 1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ac3e1f84-b35b-4e5d-8cc4-ce2bc23e118f))
    (fp_line (start 4 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6b47b875-04f3-4721-b962-1bcba0516372))
    (fp_line (start 4 1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6f61ef1-4d6c-4579-bb10-0386255cbffd))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e39042d0-b73e-4b3f-9ab1-ba3f44c4e3c6))
    (fp_line (start -1.25 1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9896c15c-182a-4d90-bc0e-0da18977dafa))
    (fp_line (start 3.75 -1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b8eda1f-e435-4fa3-be9c-d7b93e93e3d6))
    (fp_line (start 3.75 1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3ce6bd0e-7817-45cc-a95f-28fdcf4f127d))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp d08dcdcf-7dc7-4e7e-a2b6-964268ff1a0f))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 9de8531a-5e6b-4f4f-a321-8b0505ded4b7))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_T-1_P5.08mm_Horizontal" (layer "F.Cu")
    (tstamp 8b7e7144-e7a5-44d0-b191-3634ede0defa)
    (at 167.81 115.4)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/34f89165-7ab4-416d-aef9-c49468062b63")
    (attr through_hole)
    (fp_text reference "D2" (at 2.79 0) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5855557d-72f5-47b1-877e-4768d8b84a05)
    )
    (fp_text value "1N4148" (at 2.54 2.42) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d284ea39-4306-465c-9f93-14335d5e49a9)
    )
    (fp_text user "K" (at 0 -2) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp edfa5d1b-c825-4bc1-8f91-7461ca8100f8)
    )
    (fp_text user "K" (at 0 -2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 405373a2-ca7b-4a57-b2a7-8e096ac6bd1f)
    )
    (fp_text user "${REFERENCE}" (at 2.78 0) (layer "F.Fab")
        (effects (font (size 0.64 0.64) (thickness 0.096)))
      (tstamp fc271480-1129-42cc-9fcf-2ed05a0a892f)
    )
    (fp_line (start 0.82 -1.42) (end 4.26 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e05c387-1995-4e45-8358-6160f036b217))
    (fp_line (start 0.82 -1.24) (end 0.82 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2859d447-5b57-4650-a43d-74985af7423d))
    (fp_line (start 0.82 1.24) (end 0.82 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2620817-973b-43f9-95dc-dc4a4fe0368a))
    (fp_line (start 0.82 1.42) (end 4.26 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b0e6e538-e19e-4ea0-84c9-c502a1d5df78))
    (fp_line (start 1.3 -1.42) (end 1.3 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 277145a8-9169-45a5-b337-aee3ffb2f873))
    (fp_line (start 1.42 -1.42) (end 1.42 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fef6c6cf-8a0f-43ba-b5d9-ce77eef138c7))
    (fp_line (start 1.54 -1.42) (end 1.54 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f80cbb2-9092-4003-a24f-e25c36a51dd3))
    (fp_line (start 4.26 -1.42) (end 4.26 -1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dfe22afb-126f-45ca-8ec7-dd1b9628f50d))
    (fp_line (start 4.26 1.42) (end 4.26 1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e0436d1-2218-465f-8632-cfa12accaaf1))
    (fp_line (start -1.25 -1.55) (end -1.25 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e63e546c-dcb6-46cc-9eba-bef4ee226a71))
    (fp_line (start -1.25 1.55) (end 6.33 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a009c7a8-acb0-4b1e-b581-5dae42e027b8))
    (fp_line (start 6.33 -1.55) (end -1.25 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 58606dc3-2065-48d7-adc7-3fff31eadb6d))
    (fp_line (start 6.33 1.55) (end 6.33 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 72eeee6d-48b6-4030-90d8-31f06cf62910))
    (fp_line (start 0 0) (end 0.94 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a43fd723-8cbf-45bc-b694-8494b6240249))
    (fp_line (start 0.94 -1.3) (end 0.94 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ecfb62e-49c9-4b12-838b-0fbf20f24348))
    (fp_line (start 0.94 1.3) (end 4.14 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d54dd09-3e0b-4d08-bb0c-701e6aa46973))
    (fp_line (start 1.32 -1.3) (end 1.32 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce83586c-5d9a-4f3f-b96e-c670a8187e82))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae60e88a-3bb7-47ac-a197-66b93a93a14f))
    (fp_line (start 1.52 -1.3) (end 1.52 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b319b58-fa43-45bc-9223-611233feb7de))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9879a78c-ed61-4cb3-9e54-8ab039e96733))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed01a10e-359b-46d6-97b3-495fe582fcdd))
    (fp_line (start 5.08 0) (end 4.14 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 78d4ef45-f6cc-4d90-a94b-3e42f2bebd71))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp e2fc99d8-f7db-47cf-845e-587231c920ba))
    (pad "2" thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp b1c21662-3858-42cb-8b35-b684bef18d8e))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp 8f960550-065c-40b7-ac8d-9c7f27d4408e)
    (at 136.05 138.4 90)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/f014435b-331f-455f-9b31-4a41a48742b3")
    (attr through_hole)
    (fp_text reference "J3" (at -4.03 -5.4 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3d0163c-cb9e-47d9-870c-baf33bb71e95)
    )
    (fp_text value "PWM_DUTY_IN" (at 0 -1.48 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13d5c5c3-1a33-4679-85ad-860b73967dba)
    )
    (fp_text user "KEEPOUT" (at 0 0 90) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 97ffe7ec-c522-4d64-b4de-262ec94da548)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c77d158a-7c98-46c7-b903-370390877abd)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8bc4d10-16ae-43ff-9995-3748ee4393e6))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 84716b75-3a6a-43e0-a391-6bc3c6d372bb))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca58c628-8b15-4494-81bb-9659e6fa326b))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83b0a0f7-1770-4690-96ce-1d7e49d0c8e2))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0846a58-01a4-46f2-b2c0-e18de8a2aef1))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b858a449-c9e2-4d2c-a592-6e8fca1b4d12))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d88297e3-c057-4f55-8b23-dbfbf3be31ec))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41cb01b3-0197-4231-919b-14c5def52641))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 53694d7a-d2e9-41f8-b40a-30b546710c71))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9914cae2-a401-4d19-a39d-ec3abe568d17))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 02aff472-5450-411d-a2ca-adfd56e4fb1f))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 23fe037d-09b2-481a-9a48-ec919b80a6c6))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f7b4d28-ed83-4f8c-b561-d923c574a708))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6125aaba-175c-4daa-ab20-a858bc21e020))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c376bdd-b41a-4d39-82bc-2f5a6b0efe4f))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 670b2ef2-507d-4390-8add-e7a20a9963e2))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dda8345d-a685-40c6-bb62-b574253507b4))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 98499e26-389d-43c1-adc7-45a0d7cb49ba))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2bbac9d0-a491-415c-97a6-be88ec9f8429))
    (pad "S" thru_hole rect (at 0 -6.48 270) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 4ae73539-f9c3-4603-91bc-5579423c9a9d))
    (pad "T" thru_hole circle (at 0 4.92 270) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J3-PadT)") (pintype "passive") (tstamp b9d215f3-8f90-4693-a70b-a5f9179350eb))
    (pad "TN" thru_hole circle (at 0 -3.38 270) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 5b5fb8a1-3fac-46b4-bc0f-42b1ee72205a))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp c5c41a0a-1731-41fa-b100-66a87a902c7a) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 136.05 136.894859)
          (xy 135.804171 136.91507)
          (xy 135.564945 136.975159)
          (xy 135.338744 137.073514)
          (xy 135.131645 137.207492)
          (xy 134.94921 137.373496)
          (xy 134.796336 137.567068)
          (xy 134.677131 137.783008)
          (xy 134.594794 138.015518)
          (xy 134.551539 138.258354)
          (xy 134.548525 138.504993)
          (xy 134.585835 138.748813)
          (xy 134.662466 138.983266)
          (xy 134.77636 139.202054)
          (xy 134.924458 139.399303)
          (xy 135.102784 139.569714)
          (xy 135.306548 139.708712)
          (xy 135.530278 139.812564)
          (xy 135.767965 139.878481)
          (xy 136.013226 139.904692)
          (xy 136.259475 139.890493)
          (xy 136.500099 139.836266)
          (xy 136.728634 139.743468)
          (xy 136.938945 139.614589)
          (xy 137.125382 139.453092)
          (xy 137.282939 139.263313)
          (xy 137.407385 139.05035)
          (xy 137.495377 138.819921)
          (xy 137.544553 138.578215)
          (xy 137.553592 138.331722)
          (xy 137.52225 138.087064)
          (xy 137.45137 137.850809)
          (xy 137.342856 137.629303)
          (xy 137.199621 137.428495)
          (xy 137.025512 137.253777)
          (xy 136.825205 137.109842)
          (xy 136.604079 137.000555)
          (xy 136.368074 136.928851)
          (xy 136.123526 136.896656)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 92eddf35-1159-4cea-801e-71974f982bd2)
    (at 125.6 78.48 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/6277a9b8-86c0-4f6a-8ceb-afb42af0ac18")
    (attr through_hole)
    (fp_text reference "R36" (at 3.5 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 441a1137-59f2-47a5-87a3-fca53ecea859)
    )
    (fp_text value "100" (at 6.75 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0b2bda6-0b44-4400-91bb-858d20b7649f)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 02817cfe-577b-4ebf-8291-0b55b62f48b6)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4514e76-04af-4ee5-9ee8-54ca82b371d6))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0e215bb7-468d-4faa-857e-62a5d3758203))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41f13e8c-c400-4b42-b7f3-104121507f57))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bbd66aec-ed42-4184-9dfe-c3b85b169ad5))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b5d9eae-d74a-4819-b502-60bc7a6fb9c6))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ffefafcb-e5a0-4463-934c-4e9c42ff2326))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b87c930-e957-4755-9fb8-5e29f7c3d020))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e99c883e-b8b7-43d2-ad3a-c781b3c5c584))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp afc7aa35-8e2a-434a-8ade-f4e5cc8662af))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 03b09c4e-b701-405e-9d8c-26bcf0548769))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 083e98e9-f3dd-4068-99a5-bb57e9c9e3aa))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5f7fbad-314c-4b1a-83b6-2ffa9dce4acc))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f71dcee9-cf05-4dfa-be18-bb70ea8a8609))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc18fb6d-a4eb-4d77-948b-d5f7cbf4f260))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ad90c33-5d10-462a-b4de-14a44f045895))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18467a38-2658-410c-aa98-a5a78d365ef2))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(Q3-Pad3)") (pintype "passive") (tstamp 1420a629-04e7-4a18-bc2c-312c24815d37))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 1fcabca9-e5ce-48aa-94ac-717eed0bd18e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_T-1_P5.08mm_Horizontal" (layer "F.Cu")
    (tstamp 932774c5-b1a7-4039-ab64-a68f9bfe4a4b)
    (at 140.06 72.65)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/80b0a6be-c24f-4565-9798-aeccaa4203ac")
    (attr through_hole)
    (fp_text reference "D1" (at 2.54 -0.05) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19d796d3-9c71-4043-afc7-18fd7b6d21ed)
    )
    (fp_text value "1N4148" (at 2.54 2.42) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c8234a8e-4525-454d-8eee-0075196babaf)
    )
    (fp_text user "${REFERENCE}" (at 2.78 0) (layer "F.Fab")
        (effects (font (size 0.64 0.64) (thickness 0.096)))
      (tstamp fe547f57-b624-42c6-b62c-ec935ccee9a4)
    )
    (fp_line (start 0.82 -1.42) (end 4.26 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 19da9477-5019-459b-a924-37a2ac25cd84))
    (fp_line (start 0.82 -1.24) (end 0.82 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3491a69e-7ad1-4f11-bfee-e9b3aa9983dc))
    (fp_line (start 0.82 1.24) (end 0.82 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e530a042-2de6-4fde-8bd6-f4e7ca0c433a))
    (fp_line (start 0.82 1.42) (end 4.26 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a36b5990-6ce0-43b4-a859-bea7dfaca5be))
    (fp_line (start 1.3 -1.42) (end 1.3 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b8f446b-8ecd-421d-b489-c372c856a697))
    (fp_line (start 1.42 -1.42) (end 1.42 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 701515df-812a-419f-824b-41c9c96181ec))
    (fp_line (start 1.54 -1.42) (end 1.54 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f27fb94-b5fc-4243-a68b-9b31016e0d04))
    (fp_line (start 4.26 -1.42) (end 4.26 -1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a570bf5b-27d5-4dd5-9979-e0df9914d9b8))
    (fp_line (start 4.26 1.42) (end 4.26 1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b24e945a-9c57-48c0-8f33-1a6afb96f4c7))
    (fp_line (start -1.25 -1.55) (end -1.25 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81d05ef3-0721-4f66-b00a-c9430addba5d))
    (fp_line (start -1.25 1.55) (end 6.33 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d633b74a-759b-4536-95c5-51546b5dab18))
    (fp_line (start 6.33 -1.55) (end -1.25 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4354043f-5486-4179-a91e-f72c88c54ac9))
    (fp_line (start 6.33 1.55) (end 6.33 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 309035b7-c41b-4207-b855-7e9972a447ab))
    (fp_line (start 0 0) (end 0.94 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4237a335-f364-4fd3-9743-d042e5beb3e8))
    (fp_line (start 0.94 -1.3) (end 0.94 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49727a4c-e82c-4403-9853-def660260593))
    (fp_line (start 0.94 1.3) (end 4.14 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a0c464dc-83fd-4041-961f-2663841912b7))
    (fp_line (start 1.32 -1.3) (end 1.32 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff1368a3-5f03-4eee-8d15-498a9fdd75b9))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64b90d42-f262-4fc7-a71e-4fbae7a78296))
    (fp_line (start 1.52 -1.3) (end 1.52 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 13b6492c-5a9a-4623-bbef-315fef86293c))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12ef016b-e5af-4c1e-8a86-ca647f6daf7c))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8809acfc-cba3-4f08-97f8-228cd26f7647))
    (fp_line (start 5.08 0) (end 4.14 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b3fed110-dc29-4652-b629-59faac882bdd))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pinfunction "K") (pintype "passive") (tstamp f46af421-24a7-4408-a6a3-aa65c472381d))
    (pad "2" thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 5e4049d2-f554-4c6c-a054-834211f7f852))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 96e10bd0-fba7-4f3c-8575-5b1fcd41a653)
    (at 166.52 72.15)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/6a823c88-b116-4c03-b4ec-28be3d014d76")
    (attr through_hole)
    (fp_text reference "R2" (at 3 -0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bf627ce7-ea41-4a48-80cb-1d4e318c0266)
    )
    (fp_text value "47K" (at 6.5 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b517c19e-0703-4614-b40b-2b1cd0c6b19a)
    )
    (fp_text user "${REFERENCE}" (at 3 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 530c0860-b496-4964-86ae-fc4ec7182785)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e95c7b7-5f74-478c-b655-76600b7daa7f))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba8f2c48-51a3-4560-8f24-4844993cce20))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 221bfa27-2622-4439-8824-7e9c97e158a8))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09c6aeda-8771-4a05-b63b-7ef1f7dcc2bc))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c37aec8f-dbac-4535-9582-57c23466e01e))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dda794e6-67b9-496e-80f9-134d8a754c7e))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 593e3b4c-21b0-4ba1-b169-ae51613510e3))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3d2ccce4-2311-42e6-baf3-ac03dabf2637))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e0a756b-3423-42ac-b7ea-2d9f178bfe9a))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41fbd254-2aad-476e-a9de-8523babb7d16))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84ac7d54-fdd6-4533-bd35-ce4af8299f94))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec21b57a-054d-4523-9531-0f31ec109d12))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aab7ce1c-b68d-4d29-b1ff-7f1838859015))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e2e28d46-a1bb-4db0-aa4e-bf13ea814d28))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3ab3f27b-3829-4ed3-a581-9abe5b2c5989))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb820c7e-744f-461e-a5d5-b9bd5c1d0aac))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(R2-Pad1)") (pintype "passive") (tstamp 33e23b20-941e-4412-a798-68e4d8742501))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp f4cfd481-87c0-4789-a182-b03c9edea219))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 9f47491d-5877-4f82-9bea-657eb74933fb)
    (at 129.1 127.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/089e9e41-d7d2-4c99-9a27-34d0405b524a")
    (attr through_hole)
    (fp_text reference "R37" (at 3.5 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f51d11ee-efdd-428c-9b16-ab4f6810e60e)
    )
    (fp_text value "1K" (at 6.75 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2faf39b2-c7c7-473b-bfa7-ca3d2ccb4387)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1bef00a3-9c5e-4692-a684-cd25577915db)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aacb8cac-f8ef-4dbd-b30e-0f4b204d3181))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2a0867c-08e2-49f7-91cf-f97dae4b0d4b))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 39780fb2-1990-4945-8f7d-9180dcda62ba))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5e157cd-1a00-4cee-8958-f7d1d102afb0))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1d96718-0b17-4c0c-a339-3d0b3d85a026))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fdaabf35-fdc8-4179-b2fe-572a6266b396))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9cad3675-7218-435e-967e-ee07295aa5b6))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d255aa00-3be1-4f98-990d-cc860cbfdc09))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c6c20560-4220-4796-ac37-1b20075c84e9))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 06019840-a14a-491b-9e50-7519ebc8f190))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2d4519e-8d33-4702-bcbc-5b1400a4c8cc))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6698302f-f1ad-4a90-9b27-645bed321c55))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c2c1298-e36e-4689-a3da-00157949730a))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d9d45bef-44a6-4ee7-ad54-89b47006c4dc))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7359856-3ee5-455a-94e5-6f6e0f955bff))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2cb20377-ab19-4b47-8a6f-6a1cde412905))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(R37-Pad1)") (pintype "passive") (tstamp d9eb115f-5610-4390-ae3c-76144680c877))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J7-PadT)") (pintype "passive") (tstamp a0c550f1-f025-4338-a8c3-3222c196d281))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp a3e403c0-9a45-4ccb-80a4-1ce81c4275a5)
    (at 125.6 102.07 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/1827756f-7ff2-46f2-bbdd-22a1ae5c00b8")
    (attr through_hole)
    (fp_text reference "R35" (at 3.5 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 260e82f8-9bcd-4c5b-83b7-297d3d0afdc5)
    )
    (fp_text value "100k" (at 6.25 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f861e2e-5357-4eed-8a40-b7a0dee9e56f)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ffa83369-92f5-4b9c-a1d6-9ccca23aeb44)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4d0ba890-3228-4fd3-9ca4-1e0eba05acfd))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 601af6dd-577f-4a6c-a11d-4fa2f47fc0ee))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a87d5b71-62c8-4537-b9a8-124b2d9ad6ec))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12a5e231-33bb-4a4e-bab3-f64ab6ee2d65))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6168b61-b8ba-41f5-a945-819e284a720d))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 556060d3-c5ae-4f58-90f5-189ada9a9094))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1994427-cd60-4df4-a5f9-5191dfd5b5bf))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f04a318-44d5-433d-a107-fb5125d78cd2))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0d21774c-2924-4693-83c5-ddbebd5aef84))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 397924f9-d440-4b66-8101-ae78cca5c584))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b03f6548-c792-4484-82e4-82e619d0dfd6))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d322956-dff9-4a27-ad05-90c9c139164d))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d74ac93e-c492-4cb6-afc6-10a2483465b3))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d8aee7a2-4955-43d2-b457-0190cbdc5f9d))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7358c195-c240-47d0-a217-d384dde22f78))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5bba8d97-2f3e-464b-b2f0-36169e3ccc05))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(D4-Pad1)") (pintype "passive") (tstamp 594d9b9d-11ed-4696-85ec-263401d7b9ab))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 193232df-5689-4234-95e2-dc693c24dc0c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (layer "F.Cu")
    (tstamp ae8ebda0-a78e-4cc9-9c5f-c7384669d529)
    (at 158.6 55.3 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c8fb07c7-7f90-4338-8473-f0fd7002cc83")
    (attr through_hole)
    (fp_text reference "RV1" (at -7.1 5.75 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c634c28-d84e-4c27-8e29-814f8fae606a)
    )
    (fp_text value "100K" (at -3.85 5.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5fdd6a6e-725c-4659-91fa-540dd1d9c9ea)
    )
    (fp_text user "${REFERENCE}" (at 0.12 0.04 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8cb86e58-e31b-4121-b5bb-30880ebc2515)
    )
    (fp_line (start -6.62 -4.88) (end -1.9 -4.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c0d23f7-6a7a-4695-a572-13502f06a982))
    (fp_line (start -6.62 -3.69) (end -6.62 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 440e2980-4a45-4b7b-8965-d473e147a1b0))
    (fp_line (start -6.62 -0.79) (end -6.62 -1.32)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ebd98b0-8e88-4b06-8741-608d4f18ceb9))
    (fp_line (start -6.62 1.66) (end -6.62 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21f89053-5bb0-44dc-98c2-aeead6368e16))
    (fp_line (start -6.62 4.87) (end -6.62 3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f92b7ef-f9db-4cb3-abca-c9370dab8ce0))
    (fp_line (start -6.62 4.87) (end -1.9 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3dae215a-f2f5-4ef9-9785-0b584dfe5cba))
    (fp_line (start 1.91 -4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0887c8f-1050-4cd8-b923-6e2818d75e8e))
    (fp_line (start 1.91 4.87) (end 4.97 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f267054-45df-4739-a615-a0e74f707d88))
    (fp_line (start 4.97 4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aac77fe3-cd66-424c-9407-8900455097a9))
    (fp_line (start -8.65 -6.67) (end -8.65 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5ddb06ea-ad37-43fd-af66-30a3abb38601))
    (fp_line (start -8.65 6.67) (end 5.1 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f3e26a70-e10f-48e9-bb5b-2e178fec225b))
    (fp_line (start 5.1 -6.67) (end -8.65 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e34eab8f-7bca-4492-bb30-f8dcc1e78dcc))
    (fp_line (start 5.1 6.67) (end 5.1 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bddb99c5-dfbb-4320-b361-06906e7d5b21))
    (fp_line (start -6.5 -4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9210f292-0ccf-4629-ba44-86998e578ff3))
    (fp_line (start -6.5 4.75) (end -6.5 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b28edfd-4833-4507-bc40-f2d368412628))
    (fp_line (start -6.5 4.75) (end 4.85 4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77ffb8a5-107d-4d38-add2-99bf21e2d427))
    (fp_line (start 4.85 4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9b2f853e-d337-4611-b2c2-40dc2b454fa9))
    (fp_circle (center 0 0) (end 0 -3.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 45c43f6d-8cc3-43b0-90ee-b2db0d06c90e))
    (pad "" thru_hole circle (at 0 -4.8 180) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp eed7fa52-670c-4ac0-8247-557811da9aff))
    (pad "" thru_hole circle (at 0 4.8 180) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 783b97ca-c255-4aad-a39f-fc6caf47803f))
    (pad "1" thru_hole rect (at -7.5 -2.5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "1") (pintype "passive") (tstamp fa53491b-e868-4670-8d4c-ef79e17fa47e))
    (pad "2" thru_hole circle (at -7.5 0 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(R3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp cf813bdb-ce72-4d83-9d7c-12a3444f4a42))
    (pad "3" thru_hole circle (at -7.5 2.5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(R1-Pad1)") (pinfunction "3") (pintype "passive") (tstamp 5668678c-989d-44cb-9a8a-bd175f181bb6))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp b17d6625-4c63-401c-9d1c-9a69029cfbfb)
    (at 188.1 122.65 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/9a13e11d-8a81-4b9c-a73d-3a2c1a246ee0")
    (attr through_hole)
    (fp_text reference "R30" (at 3.33 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16404283-913f-4473-b7a8-f76f47306126)
    )
    (fp_text value "~200K" (at 5.83 0.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50abc65c-f2b8-4318-b906-543c44238f70)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a151e9f2-68c5-44ce-8d02-18c1e1e2e1f4)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ece8538-287e-49ea-ad48-760e4b5a1441))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c25e8087-2710-4192-90cf-09492fa5137e))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89992520-78ff-49a0-9a3c-bdc3a80b4839))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f9c3d71-463e-4620-a5fc-a720255d1d40))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be63282e-99b2-48f6-a639-ef61ad6bb1b7))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1762aac6-858f-45f2-bd92-8145b14c6d7b))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c6da1bb6-21f6-403b-b275-ba5e13301e1b))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a03d6ea3-7d88-4196-93c3-e3350a767556))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4f56daf0-67b0-49a2-abe5-5bc670f8322b))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6445203e-9853-45e8-b402-3baf6198f5f1))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 71d82d8b-2b19-45e1-abb4-5a6d75d8e058))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86ae1e17-50c2-45fa-9336-49b1a7bbd100))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4945bb25-ab69-44f1-b32b-1fb5745c3d73))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dcea7eec-adb5-481e-9137-550be211cc9e))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d3c0a25c-7aa5-4d00-b6ce-f37a9b649345))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b433b6d6-9c02-4d8e-a8d4-514815494dae))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C13-Pad2)") (pintype "passive") (tstamp 64e5d5f3-5ced-446a-bcfa-56697c0e7d39))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 915cd7a9-2b81-4472-8ce7-47d5299fc743))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp b4f1900c-47a0-463c-80ed-5fa1621f796d)
    (at 154.85 127.15 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/52dde8a6-ae82-45b7-81d1-29e9e9bcb45e")
    (attr through_hole)
    (fp_text reference "R20" (at 6.83 0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22e55e77-5d98-4de9-ae0f-e44eb5a41364)
    )
    (fp_text value "100K" (at 3.83 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8649acee-ca42-4de0-8e48-91eef4fc50af)
    )
    (fp_text user "${REFERENCE}" (at 6.83 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b44a1274-a7b4-46e6-96f9-2a5ca0185e73)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 399d19c6-3bba-4cd6-abe7-876b258493d2))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a018f766-4ced-4e8b-87d2-5e45365f4d9b))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c101e091-5f9a-48d3-a3ea-653818fae655))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c5f52bf-1f94-494a-90eb-ddb5cc1803e7))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7185c8fa-21ed-4741-9e73-20e3f2a8273b))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 07e5a3fc-88ff-4995-bcac-412479b0b21d))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1aa273b-ac4b-4380-a23f-0d5796f72ef3))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f53147f7-398e-47fc-b589-eb74b8b7cf21))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3db0d3e4-c042-4b10-a5d4-ff321702cbd5))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1cffe150-7812-412c-a83b-75d95fac9cd1))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4d27c356-8bef-4edb-b564-b3fa4442715e))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cfb8ab4-6a6e-40dc-80bc-d57b737dc0ae))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8f0a12d-d511-4c5a-9b41-9a11de5ac339))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b11b46c-a979-4413-bb41-17ae22f711e6))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c70e91cb-4127-4f4a-898a-473b5fa080fa))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15075c73-1daa-4d05-861d-17375b7356a5))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(R20-Pad1)") (pintype "passive") (tstamp ea8e5340-bd0f-4328-a9f4-53957244cf2d))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp 45a2d46a-47d3-4c3d-8175-a2052ec45cee))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp b54e5d59-a0bf-436f-ba87-f4d06d291cb1)
    (at 149.85 51.32 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/b6846fec-9c0c-4ec7-865a-3de831406157")
    (attr through_hole)
    (fp_text reference "R8" (at 3.02 -0.51 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee148811-835f-43d3-ad3b-546774320db4)
    )
    (fp_text value "1M" (at 7.02 0.49 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e8828b3-c308-43c4-9ca1-0710dbb6fd96)
    )
    (fp_text user "${REFERENCE}" (at 3.02 -0.51 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 196130f2-1a07-47bf-ba54-e6a87e6bd511)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5a940890-4ac6-40cb-83d8-ef854f0cc316))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 714e28b9-c1d5-445a-958f-3f32deefa23d))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp df20f813-191a-471a-a5d7-fc38b8abcc67))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0489a20c-7cbf-49cb-834c-e5722ec5c84b))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 28ad1530-2810-430f-afd3-57dfb68d1679))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de51ae1f-49a5-4e86-abb8-3ae73c2fe36c))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp baed9903-4fbb-4ea1-9ccc-ae6795ae4bc1))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b6571338-83f9-42d4-a565-d15526f24f6e))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fe02e5da-aff6-4dc2-890e-179d0ae6b31a))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f4c89ad-6505-4c06-955f-24e0e8358937))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 966458b7-1424-4f8f-9927-15213c6a135c))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ca267e0-a56a-4c66-8a7a-638c6dbf9ca4))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d2de15a-205d-4708-a63b-8734e554a787))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38ef2688-cc09-4033-bef2-a4c749f139fc))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afc59a5d-71ac-419e-b052-df71638026cf))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9c7e5d5a-c77b-4f8e-aabf-8ee5b7ce45f2))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp 55a263e5-4cd7-4761-80a9-9e35aae47829))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(Q1-Pad3)") (pintype "passive") (tstamp d5f3b04d-b201-434b-8337-cdb68a12448d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_T-1_P5.08mm_Horizontal" (layer "F.Cu")
    (tstamp b978f245-9155-477f-9774-42ea9be46759)
    (at 125.35 133.36 -90)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/20042917-94e3-46e6-b59d-8308e1585666")
    (attr through_hole)
    (fp_text reference "D4" (at 2.75 0 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af4ec658-0f60-4dd8-a6c1-9cfa94218a07)
    )
    (fp_text value "1N4148" (at 2.54 -2.25 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e64a9eff-8df9-4902-a0b9-6e985142ba06)
    )
    (fp_text user "K" (at 0 -2 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae860f60-0855-49c3-befc-0cd7702f5c5c)
    )
    (fp_text user "${REFERENCE}" (at 2.78 0 90) (layer "F.Fab")
        (effects (font (size 0.64 0.64) (thickness 0.096)))
      (tstamp 755eaeb2-f94a-4378-b3cf-14d011c5545e)
    )
    (fp_line (start 0.82 -1.42) (end 4.26 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3028c2c3-7943-4a05-ba5f-85f31f416041))
    (fp_line (start 0.82 -1.24) (end 0.82 -1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 147428f9-b3eb-4a89-a661-d2b7346cdc5e))
    (fp_line (start 0.82 1.24) (end 0.82 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46cce1cc-a371-4cd4-b7ab-8f49bad52de8))
    (fp_line (start 0.82 1.42) (end 4.26 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dabd9587-ce0a-43bd-ba93-dda90fe47a0c))
    (fp_line (start 1.3 -1.42) (end 1.3 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fea5f107-77db-4ea9-909f-678078e7b28c))
    (fp_line (start 1.42 -1.42) (end 1.42 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4fa194e-358a-4bdc-82ca-32a8e70bad56))
    (fp_line (start 1.54 -1.42) (end 1.54 1.42)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 461bb3f3-5742-4fa9-b740-b25bd9d59814))
    (fp_line (start 4.26 -1.42) (end 4.26 -1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c154cdd-d0b3-481f-94db-caf0643d5926))
    (fp_line (start 4.26 1.42) (end 4.26 1.24)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 06018644-7dcf-48d2-9a90-e38b270596fa))
    (fp_line (start -1.25 -1.55) (end -1.25 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4fbc5a92-b9d5-4309-ad1b-a5fd9c312966))
    (fp_line (start -1.25 1.55) (end 6.33 1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5721bc36-c9f8-4624-b449-a45aea6b82cc))
    (fp_line (start 6.33 -1.55) (end -1.25 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e6bcd724-6960-4eb9-b461-6bcede3be004))
    (fp_line (start 6.33 1.55) (end 6.33 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f82af888-a8ce-4ef8-abc7-dae5171838fc))
    (fp_line (start 0 0) (end 0.94 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 11e8f602-36fd-4597-a3d5-1df1423e21c4))
    (fp_line (start 0.94 -1.3) (end 0.94 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 559c5711-d087-40ed-90cf-47022040fc2b))
    (fp_line (start 0.94 1.3) (end 4.14 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 229a3b12-c177-4826-ac15-502644bb2684))
    (fp_line (start 1.32 -1.3) (end 1.32 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b2305ca-75ec-4664-9154-20e716a38515))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 094f5f28-7f46-4548-9d70-e15070316066))
    (fp_line (start 1.52 -1.3) (end 1.52 1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c9916098-72b0-4393-b11c-3768f3d48e80))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9230e32a-4e04-49ef-aa75-e078b88299f1))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37f904ce-975b-4d95-b9f5-c7fcee897434))
    (fp_line (start 5.08 0) (end 4.14 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dc9445d-f6f4-40ba-a553-9f5a7756141b))
    (pad "1" thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive") (tstamp dd9d35b5-29a6-4785-828a-2abd53b76370))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C14-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a2ae4071-d8cb-4229-909e-aca33284f0ee))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp bd2f8159-2cdd-4775-b4b6-4aa9736a00f0)
    (at 177.02 83.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/a41bb707-3991-4640-b536-537d7b137aa2")
    (attr through_hole)
    (fp_text reference "R13" (at 3.33 -0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d75bbc94-7f2b-49bc-90a5-a0975b678ec2)
    )
    (fp_text value "100k" (at 6.33 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5239f97e-f135-4286-a328-80d9a8c0e9b3)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6f0a9df-8485-4ea0-af2b-4af7f8937330)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 115d3ff1-cb23-4e4e-adc8-8922f9f65694))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74217209-b83b-49fe-ad55-ccd23a5bdddd))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 553a97e5-5d22-42de-8775-750c5b98fc0c))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a9860ac-e84c-42a7-85d6-538b91cb73a2))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6bd6f935-7d41-4370-995c-daa3118faba0))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3da42785-dea5-40ab-8734-38f3ffc98bb7))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 72438d0c-069b-429e-a8f0-c5b324f904e6))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 98730d61-1753-4df4-ba68-1f7b2989b2a5))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4b3795ea-7837-46b9-8222-5dc3fc377cc2))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 59eaa4cd-ef9e-4f65-97eb-37d3a848ce57))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ac0ba5e-dc7d-46cd-98c4-26070dd61f5d))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b2f718f-5d7d-40b7-8227-7a406f47e735))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a76f7854-ec63-409a-8efc-0a4c1e9e4f1b))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a42ddd37-71fd-4194-863a-6ad3e41b064e))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 71d493fd-1e12-4312-afdb-8437c35bdf1d))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43db05ab-3237-462a-b254-da6da45f5069))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(R12-Pad2)") (pintype "passive") (tstamp ed4e85a8-cad1-406d-b865-bb25874976ba))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 35f11b8e-432b-4bed-89ef-d9163830687f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp ce15444a-18b3-4980-9c25-9b43f30cb275)
    (at 172.6 108.98 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/b58a557c-5890-4779-be88-a40bfd257fcb")
    (attr through_hole)
    (fp_text reference "R25" (at 3.33 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0294d5a9-72b6-42aa-975b-caded45f5f02)
    )
    (fp_text value "1M" (at 6.83 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2f8cd7c-e9de-4dd6-a14d-a0dfdf5ca5dc)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13107357-afa7-4dcd-bbb9-4c3b881553da)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc2b919a-53f8-4239-99d8-c36114f6a30d))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdef0fa3-91ee-4e0b-bd14-53deec6872cc))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9e8fe86-7cdc-458b-a665-8cd1dd303bda))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5b03ea43-5712-4a93-8abc-ba6d2efad06d))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc77ff8c-2976-43ce-90ab-6ba31dea6077))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a521dc78-a8b0-4ff7-bd78-d2e93eed19ea))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea4ed1c1-25f5-478d-8be9-c618d538c5a1))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 501aa904-ad35-401e-967c-328a680b09ee))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c782d722-a62d-4f9d-8375-aa11ee57d9aa))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1605c621-fa9c-49bb-8a2a-a5a9a60b2d64))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dd8bfc6-5195-4cb1-bb92-c3f13618039f))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f39c690d-192f-435b-834c-1e6cf797d9da))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8bed95c-c28c-4e0f-ae26-a05aeac7d223))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b0eb2a43-bafd-4c0c-bbd6-510b735efca0))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6671210b-8d7c-499a-a581-801b208ec4de))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c74ecd7-d640-44b0-97be-eae6103d5a18))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "passive") (tstamp f4417a0d-5adb-4579-a00c-2263b79353a5))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(R25-Pad2)") (pintype "passive") (tstamp eb0a6637-6977-43e6-8983-267ee6cf8ac2))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (layer "F.Cu")
    (tstamp d6ac69b1-fcf7-45de-89da-73824e8ec112)
    (at 158.6 97.4 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/ae0d137f-993e-4304-b7e6-42edb9d64ef8")
    (attr through_hole)
    (fp_text reference "RV3" (at -3.45 -5.7 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 736c1128-9167-4e18-9b02-0a70cea78317)
    )
    (fp_text value "100K" (at -6 5.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2394f8f7-5fc6-4bfc-b4c1-16b2ef8e278e)
    )
    (fp_text user "${REFERENCE}" (at 0.12 0.04 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e13a1b4-9aa3-4474-9ec4-bed1c7319a87)
    )
    (fp_line (start -6.62 -4.88) (end -1.9 -4.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b66ea8f-f889-4dba-9e47-8bd0422f2c0b))
    (fp_line (start -6.62 -3.69) (end -6.62 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b92e143d-fc66-45fe-ab88-c4970c357f73))
    (fp_line (start -6.62 -0.79) (end -6.62 -1.32)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab28388d-e4c7-4725-bab8-df5ae86be92a))
    (fp_line (start -6.62 1.66) (end -6.62 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0185cce9-7c49-40c6-ac78-4cf0ab172c94))
    (fp_line (start -6.62 4.87) (end -6.62 3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 354c6932-0ae8-405b-adde-a3016f3f0829))
    (fp_line (start -6.62 4.87) (end -1.9 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a35bd13-5460-47c4-a788-b915baff8706))
    (fp_line (start 1.91 -4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4508aa9a-b51a-442e-b085-ee6c7046e1fd))
    (fp_line (start 1.91 4.87) (end 4.97 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3cc69709-2757-4471-8457-8d1f5a4afe4e))
    (fp_line (start 4.97 4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09a1383a-4a9a-4292-b83e-79aa0be046f8))
    (fp_line (start -8.65 -6.67) (end -8.65 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f33b435-6eaf-49f1-ae8f-91910544f88e))
    (fp_line (start -8.65 6.67) (end 5.1 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1971fe2-c1f0-47b3-913f-d3e75cfe7cef))
    (fp_line (start 5.1 -6.67) (end -8.65 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30540c81-0948-4aea-ae54-3208f4005e42))
    (fp_line (start 5.1 6.67) (end 5.1 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a7f7325-c346-4a01-bef9-68bf45620d87))
    (fp_line (start -6.5 -4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9b751ee-4cae-45fd-9ff4-e6bf28adc150))
    (fp_line (start -6.5 4.75) (end -6.5 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e259724d-6051-4f78-91e1-90b91d0b07e1))
    (fp_line (start -6.5 4.75) (end 4.85 4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa1e3f97-4cdd-4842-8359-2c3be3d884c5))
    (fp_line (start 4.85 4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 680a8e8b-d67e-4d42-a262-22b10a632630))
    (fp_circle (center 0 0) (end 0 -3.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c57f09e4-0d95-4ecf-a19b-ef3efa108830))
    (pad "" thru_hole circle (at 0 -4.8 180) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 4fb22dc8-c3b5-463e-a25a-9af21fc334f3))
    (pad "" thru_hole circle (at 0 4.8 180) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp a68f2770-43f7-45f6-b17d-c7a7d46d6730))
    (pad "1" thru_hole rect (at -7.5 -2.5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/FM IN LVL") (pinfunction "1") (pintype "passive") (tstamp e31c44d3-905b-4af2-bbc8-8a59c47a2667))
    (pad "2" thru_hole circle (at -7.5 0 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(R6-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 223e533c-3411-4dfc-b417-1090c95207c8))
    (pad "3" thru_hole circle (at -7.5 2.5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "3") (pintype "passive") (tstamp 6993ef25-5767-4441-aced-bf1510f52e5d))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp d6c435cc-5411-4ddb-a2b6-ba7441464a37)
    (at 129.35 84.23 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/7b3ac2e2-3fad-4e50-8e50-cbe4457942f0")
    (attr through_hole)
    (fp_text reference "R9" (at 3 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3070c489-379d-451c-ab3f-6f0974565696)
    )
    (fp_text value "1K" (at 7 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 331da234-064c-4c79-b356-800965552395)
    )
    (fp_text user "${REFERENCE}" (at 3 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c89601c5-6b26-48a1-8402-ea2ff09ea856)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d201b7e-b8ed-4474-8b60-a0c97ced3f95))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f7cf052-9b7a-4234-86b4-d1901910f6b0))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9232defe-6941-4a01-a5ec-b3db1a8be9dd))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c44ca3a-8680-4451-9f4e-79461cfa5e92))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 05b63f26-8848-42b4-bd41-86b832558436))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 189760de-9929-4154-a17e-e8253ce73299))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28a44df6-9532-4a33-ba8b-c8211e72d58f))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ace61fe7-c732-4767-9255-6352df4e8f9b))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 72346be2-fbcd-4d0e-a6ba-45a17dd56c26))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 77c885f5-2a6e-4c4e-8f80-0262d7478cfb))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1322ea8c-7a56-44d3-a03d-676a97d3e5b9))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9331906-e7bc-45aa-8c65-b7b2f1932332))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c87bb2f-d0c8-4c86-a81c-a532cdb9c0d1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ebd40221-18ba-499a-9042-b2b996923305))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37408fae-5a04-478e-b057-4ab1d55b49ba))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eed8f33c-f6a0-415e-b713-41a073758427))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pintype "passive") (tstamp 9a809e8e-c392-403d-8ebc-3a7259a02900))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Q2-Pad1)") (pintype "passive") (tstamp c7caee0b-b512-4705-9f09-532f2be7c2e8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp d6e05f90-8f51-40b2-a0a3-3e7b071b74bc)
    (at 129.1 100.07 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/0ed5b4a8-3b0d-4d72-a546-1a5b230ffc9a")
    (attr through_hole)
    (fp_text reference "R23" (at 3.33 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b519b16b-1d23-4b50-b160-48fa270c6d7f)
    )
    (fp_text value "100K" (at 6.33 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c3787d31-d18a-4993-ab23-39f8c3241872)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8063566-c09b-42f4-ac48-f95ac5ca4346)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5096d022-4399-43b9-80b5-a6da5ec669fc))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41d03d66-e711-43a9-b6d6-73922a5643c4))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89b7314a-75dc-475b-9ab7-89b6342e53dc))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1de9ad51-79dd-42cd-b5f1-26fe5d3556d3))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ebee96b-b0e9-4234-a194-bcea2cf11dfe))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a4f1a8b-a8aa-44fb-bd15-3d03b24aef21))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 66fb00dd-307a-4f6e-94df-6f6c23c5c07d))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2df17ca5-fb58-49fc-89b3-0242c73ad928))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 042b45f1-3d8c-4243-9e5a-2ad828db7dea))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 02a8ff82-f5d3-4857-8913-f09d5dd215b1))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 238d8ae0-cf84-4e8f-852a-ecfb26c13871))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ce5b549-8bb1-40a5-a15b-83f8f0a764bf))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5547c18-18a1-411f-b252-622804bbc538))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6430799-9a71-46fd-8b3d-5ef21eae4017))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 182e1269-a258-46c9-8a4d-605d9405063d))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3ba985c-7171-4f47-9d23-a29faf92d8f0))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(R23-Pad1)") (pintype "passive") (tstamp c68e6f43-81de-4670-9719-8517ab926643))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(R23-Pad2)") (pintype "passive") (tstamp e52b0ada-bb40-443a-8b20-948781bb3a84))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp dcc42f03-eb52-49c6-b570-872604956912)
    (at 173.85 96.48 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/35caf4d1-813b-4ed0-8fbd-28b08103bdda")
    (attr through_hole)
    (fp_text reference "R26" (at 3.42 -0.31 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp abd57132-d532-47a1-b0e5-eccd52fc8300)
    )
    (fp_text value "20K" (at 6.67 0.69 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 622a197e-eb00-4b04-a196-a7e608cb9a07)
    )
    (fp_text user "${REFERENCE}" (at 3.42 -0.31 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97307d67-308a-43c1-ac56-a7a44aea826c)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01c0414b-cfe0-404a-ac73-17f21ef02c0a))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a152768a-a8fb-4e69-849e-999df6b1066e))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4f59b2b-e5c3-4ed7-8408-e50073a0df82))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bbc217f2-cac4-4c5b-b721-506ad1ec71e3))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e09cbdba-2a91-413c-ac19-66e05b736b35))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e1a5a8e-884e-4c7b-834e-b3c6c97c5c9e))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1f9f5b4-cf3c-4df3-a9c2-d0c408af9107))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp acd4db8c-c173-48fc-b0ad-b5205683e061))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 53fa52be-0be0-4dad-9036-af49eabf8b46))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b911af14-9a7e-4c9b-b6ca-5520c1a1303b))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d91d0f4-fd40-4037-af03-cd833eace572))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ad6f6ad1-f46e-4f90-9ba4-916b2a10eb44))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f29708a-41d8-4c04-9c49-38c9f2d07483))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 092a4f1a-2903-4177-a69f-1466c51f5959))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0537c691-7b7d-4464-8543-0bd440748dd7))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c82c91d3-3236-4edf-bbff-7cb059cd3acd))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C13-Pad1)") (pintype "passive") (tstamp e73e3753-aba1-49a3-8638-054d5dfd7c4b))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp 2f072368-8cac-4b55-a8f2-30d4139aafc8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp e45aa296-75dd-4dfc-bde1-afad30c1822f)
    (at 163.32 83.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/d8d5f575-2537-46d6-a422-1abc281c90fd")
    (attr through_hole)
    (fp_text reference "R18" (at 3.33 -0.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b8fdf868-ea52-4a6a-9be2-3e3e8ae62abc)
    )
    (fp_text value "10K" (at 6.58 0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ae1c196-3eb1-4ae7-b820-bf5999c95725)
    )
    (fp_text user "${REFERENCE}" (at 3.33 -0.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b76eeeae-4aa7-41c3-97df-138850ccd16d)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddab19af-320b-463f-a074-c2bbfd21066c))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74ba43dc-cf8b-46b1-992c-e61a34f49d53))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5d95201-4634-4a3f-a27f-199f4070f2cc))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 525a51db-29ad-4713-bc26-f0ed9b2a8e6c))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de942df7-7fc0-4cd3-8130-df83415be264))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c49d957-99f0-4c75-b879-c00d49082c0c))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 49028e15-45cf-4d4f-b18a-ba50256325b7))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7aab4a95-665a-4de9-8cf4-5b412dc941f4))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5b365cd7-a9e7-4c55-92cf-ae56bd93f404))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5cc34881-1f24-4fdf-8d33-4e101d648dfb))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 091d5570-6c35-4acb-a92e-bf65fb1e8bdf))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c64b6a94-2058-4601-84c3-9af6be51a9ca))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5f7a3dd8-0c66-45bf-8d26-b01f23110106))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dbd76b55-8764-4db7-9117-06cf4f2911fd))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b10d022e-7ca7-4e50-930b-c7f6ba6c94c0))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd98e377-3841-48a4-a6f0-ce66b8400249))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R16-Pad1)") (pintype "passive") (tstamp 82e49647-4d08-48dd-b772-eeec3f7371e3))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "passive") (tstamp 8b9f4fdc-df4f-4764-a5e8-704f81e75528))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp ef45aa31-738c-4876-b96b-dfb1cb60936c)
    (at 134.6 74.07 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/5053762d-595d-4786-a0a2-113524060ce2")
    (attr through_hole)
    (fp_text reference "R14" (at 3.5 -0.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 52b70405-5244-4a5f-8725-f2eea049a535)
    )
    (fp_text value "200k" (at 6.5 0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 789b570a-1f51-4f3e-b407-ce5c448c500f)
    )
    (fp_text user "${REFERENCE}" (at 3.5 -0.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 44dadab2-f361-4792-95ee-fdbe74020514)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 22739de0-d9f8-43a4-8620-c7a7251d1c04))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 754c68ee-831c-4b15-90ac-8c25ad082d99))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0e58d29-4305-4b89-99fb-500cf316bf9d))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de82403e-1df3-478e-9689-e73b38baa350))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e67fe6c4-618b-4bd7-85bf-fdb953ec94a6))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3ae7eebe-4e0c-41d2-a3b8-934bd4d0d9d1))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8214c0c3-e6d7-4ba2-b43d-14ea994997eb))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a640e284-ee03-4163-ad33-77184d2db41d))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 95db93c9-3ebf-4672-bfd3-f3107a27f8ff))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 076658fb-2853-4bae-a173-50e5784fe716))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6316c372-3426-4d36-85e3-0342457427d6))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f32ce4c4-7aba-48ed-8288-3de4e4b1f060))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50dbc456-42d7-49ec-af76-9981803b43cd))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b58ff457-5bee-4b3b-a32a-c66820375ca3))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d387c75-fad6-4b33-af03-12710ce8921c))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d2cce8d-058f-4fe1-9cdb-45c77ad3457e))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D1-Pad2)") (pintype "passive") (tstamp d20b06bc-50ec-4116-8b0f-d1c0b7d4a0da))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(R12-Pad2)") (pintype "passive") (tstamp 088f8948-c884-424e-8222-4e3b2c003694))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp f00b4898-b17e-4af6-9d4d-9a2526c30da0)
    (at 168.85 45.9)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/b3dd7f2d-1654-418e-a95b-48dc2b12cac5")
    (attr through_hole)
    (fp_text reference "VD1" (at 5.5 0) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d52b09d-3639-41ce-ad8f-b1b1953bc5c5)
    )
    (fp_text value "1N5819" (at 5.08 2.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 802210df-0d40-4607-97d4-381a71f8b821)
    )
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 29bb0613-6609-4033-bb68-3c8e7355eff5)
    )
    (fp_line (start 1.14 0) (end 2.36 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ab30eaa-6bd5-43ad-9ab0-39b0520b7f38))
    (fp_line (start 2.36 -1.47) (end 2.36 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ce08bc1-a3dc-452f-b1bf-c15d4a5f75ca))
    (fp_line (start 2.36 1.47) (end 7.8 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bbfebc79-9a57-4a6e-a69d-bfde874e69e8))
    (fp_line (start 3.14 -1.47) (end 3.14 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f2566e88-1eed-49fd-acd0-5e898c8a63ca))
    (fp_line (start 3.26 -1.47) (end 3.26 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1052a1ed-a0c7-4ab7-8930-a2231b80c83c))
    (fp_line (start 3.38 -1.47) (end 3.38 1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99505c21-b516-403a-81a1-c203f98c60d3))
    (fp_line (start 7.8 -1.47) (end 2.36 -1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 38be0444-90f9-443d-95c1-15347138ede8))
    (fp_line (start 7.8 1.47) (end 7.8 -1.47)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e62663a-8249-426a-947b-b21fb7266309))
    (fp_line (start 9.02 0) (end 7.8 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 63345d8d-520c-4113-a48c-1a9ffe565186))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 33366131-49ef-43c6-befe-b4e724069581))
    (fp_line (start -1.15 1.6) (end 11.31 1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 63df8a40-5244-4e28-96ba-649d5a1c6c72))
    (fp_line (start 11.31 -1.6) (end -1.15 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fffcc9a7-53be-4438-a451-74febd4e9cdc))
    (fp_line (start 11.31 1.6) (end 11.31 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43e97792-79b8-4981-b417-745cae59290a))
    (fp_line (start 0 0) (end 2.48 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8d7c39c0-1439-4b69-a634-9fccf60b967d))
    (fp_line (start 2.48 -1.35) (end 2.48 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5db2e6cd-8266-4032-8878-c4c753327515))
    (fp_line (start 2.48 1.35) (end 7.68 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 39a3d4cf-81dd-497d-9b66-745dc9b08d1a))
    (fp_line (start 3.16 -1.35) (end 3.16 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 75c8c586-592f-4eb2-b427-4b9c0a418de2))
    (fp_line (start 3.26 -1.35) (end 3.26 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e5dba99-9b95-4116-8d35-2495c30b208b))
    (fp_line (start 3.36 -1.35) (end 3.36 1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6c3b2493-9352-4a8a-ac27-e6f4afb851f4))
    (fp_line (start 7.68 -1.35) (end 2.48 -1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8721f09-261f-48dd-bfcb-f6f1daa45c5b))
    (fp_line (start 7.68 1.35) (end 7.68 -1.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 99db4528-a420-4781-8f6f-1654deebb8eb))
    (fp_line (start 10.16 0) (end 7.68 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88f2a3de-d981-4c78-b8ac-77ebdc371c2d))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(R10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 78f0d071-df27-404f-93f4-547943a6bf0a))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(VD1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 70f6bde0-81cb-4772-a12d-a2399a90ddc3))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles_Socket_Centered" (layer "F.Cu")
    (tstamp f40aadff-3079-4793-b758-372380834aaa)
    (at 181.1 97.4)
    (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/dd316292-8e30-4ad5-b5a2-f93f1c8ccf04")
    (attr through_hole)
    (fp_text reference "J4" (at -4.03 -5.4 180) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 59413e0d-98c4-4d50-a848-946bdeb182c3)
    )
    (fp_text value "SAW_OUT" (at 0 -1.48 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8fa3c8d2-8aea-4405-8cc9-d6b56ab43c0d)
    )
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User")
        (effects (font (size 0.4 0.4) (thickness 0.051)))
      (tstamp 0327f608-1d60-453b-a191-a0a309ad2cf9)
    )
    (fp_text user "${REFERENCE}" (at 0 1.52 180) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 998f0e05-cb99-4157-bb46-c96b285b2fd8)
    )
    (fp_line (start -4.5 -4.5) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c841ed4-fadd-4509-b258-77edf00a65dd))
    (fp_line (start -1.23 -7.65) (end -1.23 -6.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c659833-1eec-4c9a-8652-0af556f377b8))
    (fp_line (start -1.23 -7.65) (end -0.37 -7.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c28fbb9e-8bf6-44e4-bf2c-c16c3428b29d))
    (fp_line (start -0.8 6) (end -4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dbfd0d2a-38da-41ba-95cb-832cd0ac4980))
    (fp_line (start -0.72 -4.5) (end -4.5 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c96ea50-b957-44c0-ad3b-99bcdad3a02d))
    (fp_line (start 4.5 -4.5) (end 0.72 -4.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fe65ea15-8313-4026-96d9-f59e2cf75e44))
    (fp_line (start 4.5 -4.5) (end 4.5 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 77d019cf-5706-4638-864e-058f9d6e5e0a))
    (fp_line (start 4.5 6) (end 0.8 6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 213998f7-6f43-47e5-9d3c-4545ced144c8))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 7a1c3b7d-6ff4-4d92-beff-a418736aa01e))
    (fp_line (start -5 6.5) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 26f95715-cd18-4556-882e-874969a6db89))
    (fp_line (start 5 -7.9) (end -5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22f2fce7-4b8d-4a2e-90c3-7776bd5ef8ab))
    (fp_line (start 5 6.5) (end -5 6.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9408c794-8246-47fd-ae2d-685e566c95da))
    (fp_line (start 5 6.5) (end 5 -7.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a50c868-cdf2-4419-94a0-6082be2ae229))
    (fp_line (start -4.5 6) (end -4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 467fa93a-88f6-4b38-90fc-446b8c6cb503))
    (fp_line (start 0 -6.48) (end 0 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ae0cae3-111e-4533-9f99-cbd7a484a054))
    (fp_line (start 4.5 -4.45) (end -4.5 -4.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 491eef6d-80b1-4e0b-bbf7-eb018aae9bc6))
    (fp_line (start 4.5 6) (end -4.5 6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e930547f-4c24-4c38-8025-9332812f2224))
    (fp_line (start 4.5 6) (end 4.5 -4.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 516f22f7-b636-4118-bd9c-4a346946b57f))
    (fp_circle (center 0 0) (end 1.8 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c5e0ea48-40a7-49ed-8bc5-3dcd1e1c6fb5))
    (pad "S" thru_hole rect (at 0 -6.48 180) (size 1.93 1.83) (drill 1.22) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 449eb1b5-eaf4-4f75-945e-66a5beaf3662))
    (pad "T" thru_hole circle (at 0 4.92 180) (size 2.13 2.13) (drill 1.43) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(J4-PadT)") (pintype "passive") (tstamp 38df9863-761a-4c85-b0ce-c2bf0242b7f8))
    (pad "TN" thru_hole circle (at 0 -3.38 180) (size 2.13 2.13) (drill 1.42) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(J4-PadTN)") (pintype "passive") (tstamp 0ee1c1ff-d742-4933-a077-e851e1d2a26c))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp cf37353c-7f54-4a75-9f45-0fe61d8a4012) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 182.605141 97.4)
          (xy 182.58493 97.154171)
          (xy 182.524841 96.914945)
          (xy 182.426486 96.688744)
          (xy 182.292508 96.481645)
          (xy 182.126504 96.29921)
          (xy 181.932932 96.146336)
          (xy 181.716992 96.027131)
          (xy 181.484482 95.944794)
          (xy 181.241646 95.901539)
          (xy 180.995007 95.898525)
          (xy 180.751187 95.935835)
          (xy 180.516734 96.012466)
          (xy 180.297946 96.12636)
          (xy 180.100697 96.274458)
          (xy 179.930286 96.452784)
          (xy 179.791288 96.656548)
          (xy 179.687436 96.880278)
          (xy 179.621519 97.117965)
          (xy 179.595308 97.363226)
          (xy 179.609507 97.609475)
          (xy 179.663734 97.850099)
          (xy 179.756532 98.078634)
          (xy 179.885411 98.288945)
          (xy 180.046908 98.475382)
          (xy 180.236687 98.632939)
          (xy 180.44965 98.757385)
          (xy 180.680079 98.845377)
          (xy 180.921785 98.894553)
          (xy 181.168278 98.903592)
          (xy 181.412936 98.87225)
          (xy 181.649191 98.80137)
          (xy 181.870697 98.692856)
          (xy 182.071505 98.549621)
          (xy 182.246223 98.375512)
          (xy 182.390158 98.175205)
          (xy 182.499445 97.954079)
          (xy 182.571149 97.718074)
          (xy 182.603344 97.473526)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (layer "F.Cu")
    (tstamp f83a7f04-4d75-4eea-9408-cd7e2e55015f)
    (at 158.6 138.4 -90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/664980ec-659b-4d47-b5f6-7678bdb85a1f")
    (attr through_hole)
    (fp_text reference "RV6" (at 3.5 -5.75 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0db50b06-e9e3-4441-8d83-20c2fc660b4c)
    )
    (fp_text value "250K" (at -6.5 -5.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 57b2ec14-ba0a-4f7d-8608-379d2ec22d69)
    )
    (fp_text user "${REFERENCE}" (at 0.12 0.04 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 05db2c2c-7db7-4b3a-b671-644ebcd0a618)
    )
    (fp_line (start -6.62 -4.88) (end -1.9 -4.88)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d5022ab-df8f-4af7-8a19-b4ad42443dba))
    (fp_line (start -6.62 -3.69) (end -6.62 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f4b8a152-9659-47ed-84de-79e93cd5dd0d))
    (fp_line (start -6.62 -0.79) (end -6.62 -1.32)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 77db6791-3b56-4b8e-a1d2-bab9452359b0))
    (fp_line (start -6.62 1.66) (end -6.62 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 821b48db-a6f2-4b6e-838b-a5a44c02153e))
    (fp_line (start -6.62 4.87) (end -6.62 3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f86dddd7-1c6f-4771-99fe-5e5ab6834bf9))
    (fp_line (start -6.62 4.87) (end -1.9 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f4785a9a-37c6-41eb-9ed3-b1bc89416576))
    (fp_line (start 1.91 -4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56f64ec0-1c4a-4b6c-83d0-ce9d60a00a5d))
    (fp_line (start 1.91 4.87) (end 4.97 4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa95d8ec-dec6-4140-aa90-e36989261436))
    (fp_line (start 4.97 4.87) (end 4.97 -4.87)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 59cd03cd-b502-4d6d-8ced-94b2ca082f6c))
    (fp_line (start -8.65 -6.67) (end -8.65 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d12eb1c-f3e4-49ea-a060-258d815f909f))
    (fp_line (start -8.65 6.67) (end 5.1 6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41403c2b-2a90-4521-9d2c-eb137830cbdf))
    (fp_line (start 5.1 -6.67) (end -8.65 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bd76c72f-bc6d-44ce-a1db-da0244b9d64f))
    (fp_line (start 5.1 6.67) (end 5.1 -6.67)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 39b34baf-c5d5-4670-bfc1-5aaf7ba6d9f9))
    (fp_line (start -6.5 -4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d20acd58-2e79-47fc-8099-53022cfae5bf))
    (fp_line (start -6.5 4.75) (end -6.5 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56f289f4-9edb-4ff7-8c29-af71bf613afd))
    (fp_line (start -6.5 4.75) (end 4.85 4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9103f0b-baec-4a54-8e19-35090111ff64))
    (fp_line (start 4.85 4.75) (end 4.85 -4.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76244db7-3a40-4063-a97b-0056493f8803))
    (fp_circle (center 0 0) (end 0 -3.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 30c22947-acdd-4ae0-9046-a54f8da7e3a0))
    (pad "" thru_hole circle (at 0 -4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp b55c4cb3-78cc-49ac-9ac0-1ce0e9329cb3))
    (pad "" thru_hole circle (at 0 4.8) (size 3.24 3.24) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 7483e5ba-dfda-4907-85cc-2f1307a75cb0))
    (pad "1" thru_hole rect (at -7.5 -2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J3-PadT)") (pinfunction "1") (pintype "passive") (tstamp eec531be-6e6d-4000-94a7-625d5be4f075))
    (pad "2" thru_hole circle (at -7.5 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(R24-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 1d42f96c-c328-44cc-b711-854670821437))
    (pad "3" thru_hole circle (at -7.5 2.5) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(R24-Pad2)") (pinfunction "3") (pintype "passive") (tstamp 34d22375-a1a9-4560-8a6e-7eaccc0093ea))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 06b7a86c-ca60-40d7-8079-06557643af5e)
    (at 179.8 65.97 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/d58d92e2-ed4a-4878-8ea3-f276b9929302")
    (attr through_hole)
    (fp_text reference "R1" (at 7.25 -0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 339fb5f7-e100-4ae5-ac95-0725f11d5643)
    )
    (fp_text value "47K" (at 3.5 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9878ab06-7cfa-4318-9406-8b2913456046)
    )
    (fp_text user "${REFERENCE}" (at 7.25 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d5d4d5d5-295f-40ca-9e3a-a2ca78b34f75)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c0bff18f-4034-4b8f-b86e-e3b9c5202a83))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f7f9e828-96fa-4806-98a9-c752599327be))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 030085df-3090-4f6e-9add-0511206c001b))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d7b8620c-e2e1-4ea9-91e9-1711f5c69263))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 11d2bf75-10dd-478a-926b-d16abf21d458))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1aeb2a5d-1051-49a1-adbc-5354561e1219))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bc027ca5-0861-4861-b057-87f5b3643e0c))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 87a589cd-9993-4cdc-bc1d-985a734aa69e))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 701ae2e9-fef1-46be-bc90-3668638e3a8c))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 622f5c54-9c5a-4050-b03e-e64d3f35cbcc))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 063e25f7-bf2c-475f-a596-a0e31ce74392))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5188036f-6b3a-4083-8034-b0741c414ed2))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4407431c-9b90-4c6b-9169-95f1d6f6699d))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cb8fc9a8-3fa3-478a-af7a-8da3de6232c2))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d21a8095-0024-4831-b9fb-31335050c8f2))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 29b763e5-0513-4131-ada6-16cfd32ed828))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(R1-Pad1)") (pintype "passive") (tstamp 6c5b83aa-57e3-4729-b446-12e90608aead))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp c6c97607-e8f0-4bf4-8e00-125bce0f0b44))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 0c2fc394-c146-48d1-8abc-eb0b016cb0e8)
    (at 142.85 55.73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/46339fab-3b3c-4adb-a4dd-4e63a77c8447")
    (attr through_hole)
    (fp_text reference "R5" (at 3 0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fff06ced-6ac4-416a-a78b-d9ccbafb1a78)
    )
    (fp_text value "100K" (at 6.25 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c3fd0144-e4d6-4c97-aa09-b6ed00cf05d8)
    )
    (fp_text user "${REFERENCE}" (at 3 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 192403eb-7ac3-4883-a5b5-79199a6c1cea)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 609b5d04-434d-46bd-b534-f0752d6d14e9))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 06708b6f-9a14-4946-9405-c95457b409df))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b9e73a26-e7cf-4917-a9a6-35952513fca4))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c94b83b1-eca8-4ede-a934-874cebeb432a))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3e67fd14-2e7a-47d4-9dbb-77b3ddd31089))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9d858b06-13e7-4c6e-bbd8-a1254cc6fe35))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c77588c9-d0c6-4ac9-8c64-e0b93247f454))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c04cc54-f4d9-4a43-968e-15362dffb8fb))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp da95beec-6395-4da4-8b6b-32d3d630724c))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5c594aa7-b690-4da5-8557-63beae382aa2))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4456c864-dc57-4582-9c52-27067572267e))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ab3c7a4d-e2f5-4f5b-929c-14b4a65ba51a))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8014ae32-3001-45af-b3e0-795915d2ea09))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4266ae31-47ad-4946-8c44-722c464f68f3))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 06e250e4-fee5-4055-9c33-dee9c638fd8a))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0f2d0c66-9ce5-49be-b6cb-80589ae2be26))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(R5-Pad1)") (pintype "passive") (tstamp b21bdfcc-54ea-40e2-ad7b-7302801ae9de))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J2-PadT)") (pintype "passive") (tstamp f5916eba-711c-4a1f-ad98-4ad7ac5d2ed5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 0c837902-bf83-4254-85c2-fda7daaea1d4)
    (at 144.18 105.15 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/e4244882-a002-400e-ad47-17508aca0954")
    (attr through_hole)
    (fp_text reference "R17" (at 3.366311 0.619389) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 95c08a97-b64c-4e5d-a00a-71700a91281d)
    )
    (fp_text value "~200K" (at 5.855113 -0.59) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 58f35d89-2abb-4e8d-b756-ddcefe8a33cc)
    )
    (fp_text user "${REFERENCE}" (at 3.355113 0.66) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d9f5ba6a-5686-4ddb-a4a1-334ce919e266)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6bb07254-6067-40b8-94ca-b4ee93178ebf))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 58551fc5-4fec-40eb-8bb5-77e18673da19))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e5d778b0-c861-4795-9770-78e91805ae24))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8856ef3c-9e61-46a4-a555-ef0ca59efc85))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 40e478c0-229e-42e1-af7f-44ea81102e84))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 68c47795-98d3-40aa-9441-b55e16ffcf5f))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 09cad033-31d1-4882-a20e-08bc4991fcbd))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 39cca560-02df-4afb-a821-badb2d037b12))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 32fca1e3-aa3b-40ee-bf25-343c750297bd))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 70cae5b6-9411-4ba0-933a-3e6c0d7031d6))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 09af5323-385a-4b9b-9a3f-1f4f5990db2d))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7048622c-ed6b-4302-8560-f72bbc3c9613))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9b6ce6fb-f43e-4c82-b3b2-a83bd28d3990))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 029da506-239d-4236-b999-32809a69bf23))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ce30bb47-4c7e-4cf6-a865-5a7eaa641f5f))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c02e01a6-bce7-4c69-9cbc-1040836b2fe2))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C11-Pad2)") (pintype "passive") (tstamp ffb29a1f-f7df-4ac4-b20e-a5afee15e377))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 822c75ce-1d22-48d4-bb34-ee831c38780a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 113af8af-bb2c-45b6-adcb-bb42dbd1e7e4)
    (at 178.52 105.4)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/05c328b1-d2a5-4182-86c5-782d9ead3def")
    (attr through_hole)
    (fp_text reference "R16" (at 3.5 0.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 90d2cfd8-4c8e-4efd-9443-865cdf1ebeae)
    )
    (fp_text value "5K6*" (at 6.5 -0.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eac392d7-09a0-4bbd-9fea-d0fb7ced42b5)
    )
    (fp_text user "${REFERENCE}" (at 3.5 0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d0725f30-89b6-485d-b85b-57ff3f5f581c)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dca60d6b-74b2-4fe2-b5be-10408e6042b4))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 552bd161-db3b-40bb-9ba5-170600b5489b))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d11aeb0d-6c4f-4d14-93d5-c1625e32cea2))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7f4c3af2-603d-48d7-ab1d-a2e31126c9fd))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0cbd297c-14f5-43c5-8f8b-bfcc20d702bf))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp adcd6eef-d5bf-4a04-9eec-e3caa62e1d5c))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e54997bc-a32e-4b54-9b8e-eb60781206ae))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a1cf94d3-128a-4ddc-9dec-0da242feda58))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1a633279-a575-41ba-aa54-3964ae758c6f))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b7bfd8bf-b4f4-4a7b-811e-ebc089b3635f))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a47bd879-8d10-49f7-9129-cebd89c6db15))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 92bb839b-f7ee-459b-abe3-17cf65f24cb1))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cdb82baf-570d-4a20-bcf6-7d4dd3523911))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b1736473-5853-4393-a3c6-1f6f84063bcd))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7ec4b63b-2db4-4286-94a2-6a89f8e357b7))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 35056087-d832-4a82-93ea-9751e56b2d22))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R16-Pad1)") (pintype "passive") (tstamp b3fc9632-2699-4b11-9ccb-54e917abaeb1))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp d2c09822-b6ab-4c17-a719-012bf47a0936))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "B.Cu")
    (tstamp 1f6058e3-6d7d-49d2-9d53-c97e3b006a21)
    (at 137.55 85.4)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/44041d77-07c9-4f35-9928-42cdc1158972")
    (attr through_hole)
    (fp_text reference "C2" (at -0.25 -2.25) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 71d11774-8fbe-4cc3-9860-7ac3bdf05c38)
    )
    (fp_text value ".1uF" (at 2.25 -2.25) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4bdd0e0c-7027-46d6-9482-82024e2a588e)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 58ad2682-2ce9-4fd3-bf9e-22959a653ef8)
    )
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 097190d3-8323-4286-bad8-7bc850901aef))
    (fp_line (start -1.37 1.37) (end -1.37 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bf794d7c-dd2a-4970-acca-fbf7d24d51ff))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp eac880fb-632b-4bc6-9af3-56568e269255))
    (fp_line (start 3.87 1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 33973e8c-640d-418c-b7c8-756f9ab9ee96))
    (fp_line (start -1.5 -1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2356ab39-d21f-44dc-b8a4-5a292158c711))
    (fp_line (start -1.5 1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e83906ae-05b5-4a16-bdcb-845abe82c818))
    (fp_line (start 4 -1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 64c24dd6-762c-44b9-8a20-2d2a8686f0df))
    (fp_line (start 4 1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 33b92fa6-044f-41b3-b986-224415b0ad8f))
    (fp_line (start -1.25 -1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5eddb7e4-12d4-434a-9d87-05880c00872d))
    (fp_line (start -1.25 1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 60d5520a-0fbe-46fe-833d-11b753acc876))
    (fp_line (start 3.75 -1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7c97e187-452e-4781-bb1f-85f9a2342070))
    (fp_line (start 3.75 1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9ab21284-0c92-4dc1-88ab-3ff65b2d5e08))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 91108494-ef26-44b0-8b6a-f9007a246660))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp 98be63e9-c671-4765-9756-db752ae24ae1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4" (layer "B.Cu")
    (tstamp 23a55f42-ed3b-4a47-bdaa-5f3dcda95aad)
    (at 177.05 62.64 90)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/561f6d92-ef52-4899-9536-9da04166570f")
    (attr through_hole)
    (fp_text reference "C7" (at 3.75 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 11288e0b-fd51-4b28-9c14-c66bb3de35c0)
    )
    (fp_text value ".1uF" (at 4 1.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5e70103b-025e-499e-ac83-01f8e8e19d3a)
    )
    (fp_text user "${REFERENCE}" (at 3.75 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5695e9f1-7688-4850-a288-87f9435b4d56)
    )
    (fp_line (start -1.52 -2.62) (end 9.02 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 70cb2dd4-8bdc-4f9f-9e3c-72ffd4e9edbb))
    (fp_line (start -1.52 2.62) (end -1.52 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d630e46e-4b92-444a-b2de-7705239181f1))
    (fp_line (start -1.52 2.62) (end 9.02 2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d8f3c3c9-afab-4aaf-ab8c-c5ade72f9c1b))
    (fp_line (start 9.02 2.62) (end 9.02 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fda75ab3-d1f7-492a-b858-f4795195df3c))
    (fp_line (start -1.66 -2.75) (end 9.15 -2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b8fa5ef3-eaf4-4118-b412-b8237c6e0272))
    (fp_line (start -1.66 2.75) (end -1.66 -2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 266db32e-ddd9-413c-8637-50d711d0a852))
    (fp_line (start 9.15 -2.75) (end 9.15 2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 29721abc-7370-4e4d-a9bd-ce66d435607b))
    (fp_line (start 9.15 2.75) (end -1.66 2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 957492e1-9e30-4e4e-8e15-c2195250dee0))
    (fp_line (start -1.4 -2.5) (end 8.9 -2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5adfa9ab-8367-4b0c-979f-f365eac00b8f))
    (fp_line (start -1.4 2.5) (end -1.4 -2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a893c2f8-9bbb-4bfb-8e57-e755b6a2af2e))
    (fp_line (start 8.9 -2.5) (end 8.9 2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5ea04245-6e0b-4d01-b41c-056295fdf7a6))
    (fp_line (start 8.9 2.5) (end -1.4 2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1c0cb015-9d02-4235-970e-b86a665e6ce3))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 23f9332f-0cdf-43b0-b919-4c814e280f8a))
    (pad "2" thru_hole circle (at 7.5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp b9b2d4f0-6ed0-4c2c-8887-d6aa29074ada))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 26ee76ce-a04e-4978-83e0-4c455fb88ef5)
    (at 125.35 130.9 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/6eacb3dd-91e1-4862-bc98-9ffcccd0e997")
    (attr through_hole)
    (fp_text reference "R34" (at 6.75 -0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fc0e36d4-c99d-4dbd-83eb-1b349863747f)
    )
    (fp_text value "10k" (at 3.5 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2ebbdf79-1ad3-488f-bed5-a267c65f64b4)
    )
    (fp_text user "${REFERENCE}" (at 6.75 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f427217-8915-469e-8aa0-0dcbbfea5fb5)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 97046f2f-a203-4029-a1c2-e6fb661c9b18))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp af3f405d-0ed8-4a04-b111-68d29439701a))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 47045932-7770-4101-9fb3-6551a5d11194))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 19984db9-dd84-4bc0-8e68-dcd4dfd80d40))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d283bd5c-47fd-4610-9a3f-3ae163fb5438))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 689e98f5-6078-4bd5-bf5a-f62dd53db2ae))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a6495e05-e2cf-4ede-ba8e-6e50624a0803))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bbc72683-8d63-4823-9d21-cc47339a8efd))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 65c924d1-eacb-4b5c-8f5f-ecdeb42eac9e))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ba922165-1b59-412a-8e33-632cedae63fd))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 33a6c70a-af89-4cec-948b-c12b035f5385))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7c80e19e-9c80-49eb-a0cb-db9eed348283))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 01fa2ca5-d003-4ec9-913b-05edc37e0a60))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 33bea214-fd7a-476c-b738-290b3b85538e))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2a70b69e-030f-4949-b122-517736286f72))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e3c0cd35-6e17-4c43-a9ce-5ef6bffeef46))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C14-Pad2)") (pintype "passive") (tstamp 58ddfb07-ad37-4d6b-8b0a-7ace2a98f275))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp ce7cd2f8-e67e-42a0-b157-55f5e865a53a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "B.Cu")
    (tstamp 32c84aa1-abf3-4ebd-a340-1df4d55c0e1b)
    (at 150.15 113.1 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/a4488099-2f1e-44fa-a43b-a6ae9a1dcad6")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -0.55) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c29452c3-32ab-461d-b177-32d4a9dc5607)
    )
    (fp_text value "TL072" (at 3.81 -7.8) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 50033162-f3c7-467d-ac8c-5a339a79c692)
    )
    (fp_text user "${REFERENCE}" (at 3.81 -3.81) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 253c1030-28be-4ff8-bbbb-d8a731d5d4c4)
    )
    (fp_line (start 1.16 -8.95) (end 6.46 -8.95)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 70c665be-f2df-4890-b4c1-af7d7dd9cbd7))
    (fp_line (start 1.16 1.33) (end 1.16 -8.95)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e4d36fa6-8bc6-4962-b0fa-2f4df1a01b09))
    (fp_line (start 2.81 1.33) (end 1.16 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 68e91ab4-8b72-498f-9255-f71f38bbc48f))
    (fp_line (start 6.46 -8.95) (end 6.46 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4b0f44ee-6777-487a-a1cd-6080ba39ab7a))
    (fp_line (start 6.46 1.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2a8a6454-9d03-4fe0-80e9-f417ea53667c))
    (fp_arc (start 2.81 1.33) (mid 3.81 0.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1fddb0d1-9bce-4943-94a4-15cedabfa36c))
    (fp_line (start -1.1 -9.15) (end 8.7 -9.15)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1fb9df67-5aeb-4c56-b0e2-b10fe2d59ac7))
    (fp_line (start -1.1 1.55) (end -1.1 -9.15)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 76ee9d2d-1d3e-4b38-946c-455b2c9292dd))
    (fp_line (start 8.7 -9.15) (end 8.7 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 289781f3-4d7f-4283-8c3b-ac686226304e))
    (fp_line (start 8.7 1.55) (end -1.1 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 95f7555c-c63c-4d65-9c7b-1e888e7213bf))
    (fp_line (start 0.635 -8.89) (end 0.635 0.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f02e456e-c66c-412e-9d65-8da813b5f944))
    (fp_line (start 0.635 0.27) (end 1.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 497645aa-d21a-46cf-9ba4-9375f086d32e))
    (fp_line (start 1.635 1.27) (end 6.985 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d6544db8-455f-44c3-bde5-8b1dc9d02b03))
    (fp_line (start 6.985 -8.89) (end 0.635 -8.89)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e8161756-65da-4402-89cc-c59a8da373b6))
    (fp_line (start 6.985 1.27) (end 6.985 -8.89)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b8505d2c-55f9-48d8-8dc5-4e0804f8e42a))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C14-Pad1)") (pintype "output") (tstamp 1087e40b-a53b-44fa-bcf9-3215d5015261))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "-") (pintype "input") (tstamp e7bd6f88-f229-4e90-93f0-89783a957e41))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(U3-Pad3)") (pinfunction "+") (pintype "input") (tstamp afde4a2f-a9ea-407f-a189-99ff5ce927e0))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in") (tstamp 8a4e6eca-8280-4391-a367-2b158ecd1036))
    (pad "5" thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(R37-Pad1)") (pinfunction "+") (pintype "input") (tstamp 38b7c97f-f9d6-437e-8b26-fed45e645b92))
    (pad "6" thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(U3-Pad3)") (pinfunction "-") (pintype "input") (tstamp 0b9e9dde-7092-4e28-9cc5-81f903337414))
    (pad "7" thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(U3-Pad3)") (pintype "output") (tstamp ddb75872-d3b4-4937-b4dc-50e43d6bfb83))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in") (tstamp 1064813b-80da-4c6a-ab36-92d5cd981ed7))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 3383168c-a48a-4504-a614-8cf4b0181def)
    (at 146.1 55.73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/53c006ac-0948-46e4-b719-1a4a2eb20268")
    (attr through_hole)
    (fp_text reference "R3" (at 3 0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2f15c922-570d-4e63-9f9b-a4f988f54c22)
    )
    (fp_text value "100K" (at 6.25 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 43a8b339-d5b0-41c7-8ba0-e913818583b4)
    )
    (fp_text user "${REFERENCE}" (at 3 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6d26f9da-2cd4-4709-9251-ca13f8426606)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8fe9fe8a-fff9-4fc2-b93e-0dbd678a8af7))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23d3c111-5d3e-4e74-bec5-384d659134a0))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a82d0178-a138-4089-9c15-d79819390474))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a97bc979-46de-4d77-91c0-c2cb7b0133c7))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6f6bd3b8-5065-45f9-8e43-a492fb575f82))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8082bf17-6ccc-4fdb-b720-f466248b6302))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7b9549b2-af1d-4a19-a2c3-7320d9409a1e))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e63b7bb3-863a-4815-8abc-99d221b77651))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1168436f-f673-44ff-811b-096c5955b5eb))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c64687e8-60a9-4248-8d6f-4353a04f824c))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e55a6261-5f64-4351-af1d-ae4a09ae9633))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e8a41373-05ec-4bb6-9feb-aa0ed3530f45))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3ec72763-8eac-4bfe-8dbc-db04e198e1e6))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fcfa60f4-fd8a-4de8-ba93-0f52818eae5f))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4bc9685d-9361-443b-9ea2-fd92156facc1))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fc5b6222-664e-4910-a496-4b631db034db))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(R3-Pad1)") (pintype "passive") (tstamp fe4f1c2f-8972-4a69-bf31-21e3254fa577))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(R3-Pad2)") (pintype "passive") (tstamp dc6ca505-4453-4935-89d9-6d96303c628d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L9.0mm_W3.9mm_P7.50mm_MKT" (layer "B.Cu")
    (tstamp 367922ed-3317-4f44-8a73-dbea847022d5)
    (at 136.6 130.9 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 9mm width 3.9mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/ed7dbb64-a264-42ee-8100-3ba9c6dd1396")
    (attr through_hole)
    (fp_text reference "C14" (at 2.5 1) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0c6b1f1d-7840-4e08-bad5-831152d01730)
    )
    (fp_text value "4.7nF" (at 4.25 -1) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2da565cc-dfdd-4f1c-8ec5-0d7afeac0617)
    )
    (fp_text user "${REFERENCE}" (at 2.5 1) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4ee117f7-75cb-4e1f-86b9-4cf9cd3042a9)
    )
    (fp_line (start -0.87 -2.07) (end 8.37 -2.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 66cdb629-bafe-4719-b016-5b2c4fd7d225))
    (fp_line (start -0.87 -0.665) (end -0.87 -2.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 17db4e1b-390e-4327-ac7b-1edc4d9065fb))
    (fp_line (start -0.87 2.07) (end -0.87 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fc3181a1-ecca-4993-8c39-6f70790c1e88))
    (fp_line (start -0.87 2.07) (end 8.37 2.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 832ad48f-0851-480b-9891-837738846fff))
    (fp_line (start 8.37 -0.665) (end 8.37 -2.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c0c4461a-8ffc-4d38-a6d1-bb22726dae84))
    (fp_line (start 8.37 2.07) (end 8.37 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 06339e1a-8707-4b9b-94ce-ec125b49e745))
    (fp_line (start -1.05 -2.2) (end 8.55 -2.2)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 17784ef6-2d42-4fa6-a626-d9d63260e941))
    (fp_line (start -1.05 2.2) (end -1.05 -2.2)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d24b5f94-98cb-451d-adcf-f5302d295f40))
    (fp_line (start 8.55 -2.2) (end 8.55 2.2)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bcf5fa13-00fc-4829-b9f4-ffa3f0e40b24))
    (fp_line (start 8.55 2.2) (end -1.05 2.2)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d9795806-0e3d-4009-88e2-4cda95f8aa57))
    (fp_line (start -0.75 -1.95) (end 8.25 -1.95)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 96f583d0-fac0-460b-bc45-6ce614549c5c))
    (fp_line (start -0.75 1.95) (end -0.75 -1.95)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9892a7f1-4cf5-404b-9809-a033f711a5d4))
    (fp_line (start 8.25 -1.95) (end 8.25 1.95)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e5722923-c1bb-4703-8613-52754907470c))
    (fp_line (start 8.25 1.95) (end -0.75 1.95)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7c5f9c67-6b6a-48f0-9821-068fb099f12b))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C14-Pad1)") (pintype "passive") (tstamp 712bb6ee-83ff-4567-9ce5-15070a844547))
    (pad "2" thru_hole circle (at 7.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C14-Pad2)") (pintype "passive") (tstamp 23e9eb98-64e5-4677-af5f-e7814b7acb56))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L9.0mm_W3.9mm_P7.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 378efe53-f087-4bb9-973d-81d65e2d1792)
    (at 191.85 122.73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/127eee70-cbb2-410e-a920-2b1a89f46479")
    (attr through_hole)
    (fp_text reference "R31" (at 3.33 0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c34b4225-4782-4363-9a93-b58d88e592a5)
    )
    (fp_text value "**" (at 6.83 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4c25236c-2f73-4c47-8442-f779d498a190)
    )
    (fp_text user "${REFERENCE}" (at 3.33 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd19d94b-a35b-4f73-a940-80715b6aff90)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da4b06fc-ac98-4541-b26f-92549b747b95))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0669b883-92d2-4a76-afd1-4aaf6048eff0))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp beff11e7-00b9-4c80-a1e8-01a26bd22a68))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48b8e2dd-6ce5-49cb-ba55-90f6552d4955))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 294b6876-1932-44ea-82a7-5d778c9c6e11))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c8aacbba-cd3f-4c54-ab0f-f317a380fecd))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d3322a48-500a-40b7-80f9-792bcc051202))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp caa32412-4e81-4e94-8e8f-f7b5555d4f59))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 54c9e017-cc71-4d1e-a3d1-5e511f3e7788))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp da4ca2b2-7cd9-4e00-b237-f6c8a482ca3d))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d91b7d03-6b38-4c53-9b85-eef9456d7bcd))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e7168fd4-b230-4b5a-b32a-dfb985243c95))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cc8aea86-7196-4125-b82f-c3bec610f02b))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3c49e155-b72d-4e9b-b0a4-62b9783cb71a))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5e0723bd-001b-4aab-81d2-21e0263a5886))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d5645909-7be4-4f2f-91fc-8acdab2385a2))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(R31-Pad1)") (pintype "passive") (tstamp 10715241-fef9-4fa7-8cf4-a5fa67b911f5))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R29-Pad1)") (pintype "passive") (tstamp fe68fd24-8332-4a34-8951-6c91ec5c668d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "B.Cu")
    (tstamp 39f59e98-d18a-4591-af84-7bd4c6d0e464)
    (at 130.1 71.21 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/f131e390-37f0-4436-a67b-c2b177e1cfbf")
    (attr through_hole)
    (fp_text reference "TH4" (at 3.81 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a115fa58-20cd-4283-a5b4-af4f766ce556)
    )
    (fp_text value "10K" (at 9.25 0 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fc1827ef-72e6-45d6-b692-40f86fdf6eb0)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "B.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)) (justify mirror))
      (tstamp 47304647-2da2-4926-bb25-ec59a7d53e32)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6f37b807-2d23-48c7-a24e-4098b3e6466f))
    (fp_line (start 1.89 -0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5f573aed-8542-43cb-9b58-d1613424b3cd))
    (fp_line (start 1.89 0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 488feaad-4bd0-47e9-a21b-41c9b6c57328))
    (fp_line (start 5.73 -0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d19ead61-1a32-44bf-9815-4a899e7d7857))
    (fp_line (start 5.73 0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c99cd3d9-e476-4a77-a3dd-421b9847ac54))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 87025e85-2e4d-4f59-9ac4-f4109aaf1c95))
    (fp_line (start -0.95 -1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2f419836-206d-4a4e-863a-7c94e2c93744))
    (fp_line (start -0.95 1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a74a7e64-5393-4b9a-9f71-af77f6cf01ec))
    (fp_line (start 8.57 -1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 37f2c720-4c13-4b37-8ebd-31ee5a8ee9b4))
    (fp_line (start 8.57 1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b8c04e6c-3a79-4d75-9210-e360315bd110))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 792cc3ac-945e-4126-9c3a-16fb05ae6f50))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3db86094-0961-42a4-acdd-01e706a9f057))
    (fp_line (start 2.01 0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a0ea3e98-e248-4468-b91f-69079faafc4d))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e3da252b-b2c1-4d53-aa72-25f0fee32bcd))
    (fp_line (start 5.61 0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e38dfa45-2a64-4bcd-9eec-0af094cc19e2))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fb5d9316-3f63-4e98-8a3c-730448eea28e))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pintype "passive") (tstamp d669b270-2df0-4d8e-ba49-26f4447d245a))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(R6-Pad1)") (pintype "passive") (tstamp f884ba6d-e2c6-4c35-8a0b-8491bbbb4449))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "B.Cu")
    (tstamp 4422cfe6-6f83-4074-8ad9-8dca987d9bc9)
    (at 134.6 71.27 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/430d76bd-4f18-4d1d-b273-a1679dd725d5")
    (attr through_hole)
    (fp_text reference "TH3" (at 3.81 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1a4d8a07-7993-4edf-8f19-6db8b0b38b4e)
    )
    (fp_text value "10K" (at 9.06 0 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 279369f5-853e-446d-9bfd-aa1769140ef4)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "B.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)) (justify mirror))
      (tstamp 1f637f3f-59d7-4348-bd9b-13b627202d58)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 623c6fe6-08c6-433c-be58-749bd3dc260e))
    (fp_line (start 1.89 -0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f35d86ec-e3df-4959-8465-99c67dac7a53))
    (fp_line (start 1.89 0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3aa541c7-46a4-4645-8c13-b41a9e3c13e3))
    (fp_line (start 5.73 -0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1f222b01-63ca-4966-be79-0bd2179fb614))
    (fp_line (start 5.73 0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1255776a-98f3-4303-85ff-aa5896571c61))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3b9dad53-3ad3-4dbc-978b-ca2de2c5be31))
    (fp_line (start -0.95 -1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 634ae905-73b6-4d64-b089-77c37edb046e))
    (fp_line (start -0.95 1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c0b1eb3b-a13a-481a-a1bc-98f407a4171b))
    (fp_line (start 8.57 -1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 04712201-bc25-4a91-be62-162b341dc871))
    (fp_line (start 8.57 1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2e35f517-dcb0-40aa-94c0-c997bd3b8bc2))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 806a3cba-d586-4bec-9e89-48084463cb93))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7eb6f7a3-2b59-41f5-8e73-57b7c013c4ab))
    (fp_line (start 2.01 0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 401fbc23-3c1c-4315-9d1b-d53c369f5561))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 674814e1-5db4-407d-88c6-2f1a726db426))
    (fp_line (start 5.61 0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bb939791-44d4-40ff-bb14-df853ed5f6a0))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e720bac0-9592-4e62-90e2-2e68e9bcab9e))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pintype "passive") (tstamp 10e79442-860f-4361-bde3-8b43f2b82c58))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(R5-Pad1)") (pintype "passive") (tstamp f38c2770-755c-4a6e-a035-23d0ceeba072))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "B.Cu")
    (tstamp 44b2454a-5abb-404f-a9e7-6e40028f650d)
    (at 136.85 71.21 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c29280ee-97a2-468d-8641-6264855c4431")
    (attr through_hole)
    (fp_text reference "TH1" (at 3.75 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a116547c-8958-4e09-af62-1cf435d62300)
    )
    (fp_text value "10K" (at -2 0.25 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a08cfbf0-a2f6-405a-b92b-45e25783cf11)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "B.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)) (justify mirror))
      (tstamp a244a941-a6e1-45f6-9539-006e3aaa43b2)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8b012720-1d76-48b0-b171-5f4e2d853264))
    (fp_line (start 1.89 -0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d682cc2a-69a1-4374-b30e-a9b9f35d557c))
    (fp_line (start 1.89 0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0090705a-3a08-4865-9e69-ef7384e0b4a1))
    (fp_line (start 5.73 -0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b4ce356f-5c87-499a-a172-05c69c120ba2))
    (fp_line (start 5.73 0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 19e0b103-4f1b-4211-9531-4d9fe2df07c7))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e26b05b7-f7c5-4512-905a-49c1010b7de5))
    (fp_line (start -0.95 -1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 007b4fa0-325c-444d-a4fd-0abc49cfb51b))
    (fp_line (start -0.95 1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c944f552-68c9-4ebc-b643-fd8a05427d37))
    (fp_line (start 8.57 -1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ecc89f72-284d-4c40-8a40-a378e0ceb8a9))
    (fp_line (start 8.57 1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4593f720-e86b-4ddd-bdd0-ce3a5f424234))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp adaefe04-4944-4d9a-9c93-5e6b6de17f74))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0fd96f9d-8ffc-4ceb-bf30-e65db61543cc))
    (fp_line (start 2.01 0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 36c88b39-3a43-413d-a571-6daed91e5744))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fea92e25-547f-4669-920e-c923149c45a3))
    (fp_line (start 5.61 0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6b06c66e-9056-4d71-925c-583cbbfd1c0b))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 682f1ba7-0b83-4a53-9735-b4cdd9ef07df))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pintype "passive") (tstamp 3535cba7-be6c-4f10-9776-853dc3a9d754))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(R3-Pad1)") (pintype "passive") (tstamp 7c4efaa0-90b8-4527-9054-076961da7dcd))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:IDC-Header_2x05_P2.54mm_Vertical_Fixed_Ground_Fill" (layer "B.Cu")
    (tstamp 47783012-1ee9-4647-8aa2-2f08e4345d31)
    (at 187.2 59.95)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/3c23d95e-4d4a-4623-a482-03719377953d")
    (attr through_hole)
    (fp_text reference "XP1" (at 1.27 2.65 180) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1ac598c8-8200-4796-9543-3cdc8dd830e5)
    )
    (fp_text value "IDC_10" (at 1.27 -12.5 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7e35d891-7d0a-4812-aea8-f0114b81c9a2)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 -90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ab6ddeff-2bef-4307-bb07-5103856e0843)
    )
    (fp_line (start -4.68 -0.5) (end -3.68 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp df20152a-96e5-4be8-86fe-fe90fbd130f5))
    (fp_line (start -4.68 0.5) (end -4.68 -0.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e8b5cddd-22c8-492a-8111-3fddf9050bbf))
    (fp_line (start -3.68 0) (end -4.68 0.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ea52dcf7-5dbe-4c32-9234-75f4ae93f355))
    (fp_line (start -3.29 -15.37) (end -3.29 5.21)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a4d49b6b-f1bd-496d-a86e-3f6439db5bad))
    (fp_line (start -3.29 -3.03) (end -1.98 -3.03)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 20f88b22-a7cd-44df-9aff-da13bd54a51f))
    (fp_line (start -3.29 5.21) (end 5.83 5.21)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2e9ec955-25a4-44c4-a656-ca1e53af843c))
    (fp_line (start -1.98 -14.07) (end -1.98 -7.13)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 16c156e1-7f4d-44f9-8c5d-0e543466a9fa))
    (fp_line (start -1.98 -7.13) (end -3.29 -7.13)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bf8124c2-8fd9-47fb-993f-577d3acc5176))
    (fp_line (start -1.98 -7.13) (end -1.98 -7.13)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 665375b9-c3f1-4598-8b8a-70a76674df2a))
    (fp_line (start -1.98 -3.03) (end -1.98 3.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 47643ab3-1f0b-47b2-8b03-fd6a282f2b10))
    (fp_line (start -1.98 3.91) (end 4.52 3.91)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d12b216b-53dd-4b5e-9be9-a1cadc8cc142))
    (fp_line (start 4.52 -14.07) (end -1.98 -14.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp be7171d5-1015-45ad-8ecc-b2aa91e35932))
    (fp_line (start 4.52 3.91) (end 4.52 -14.07)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b04e2de8-c9e4-4afc-ac04-f861d5cd9336))
    (fp_line (start 5.83 -15.37) (end -3.29 -15.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 521996a9-43f5-43ad-bd64-c7655b8b41d0))
    (fp_line (start 5.83 5.21) (end 5.83 -15.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b42bc74b-848f-4a97-b2cd-e1dca52bcad4))
    (fp_line (start -3.68 -15.76) (end 6.22 -15.76)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3c52ce07-2299-46f3-9403-c53302200c8f))
    (fp_line (start -3.68 5.6) (end -3.68 -15.76)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1884f6d3-a99d-433c-b4e8-9446392138bf))
    (fp_line (start 6.22 -15.76) (end 6.22 5.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp efde45a8-d28d-4625-b569-09acbbfe228c))
    (fp_line (start 6.22 5.6) (end -3.68 5.6)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 40b7cdb2-8f0f-4348-a7e4-62566f648a53))
    (fp_line (start -3.18 -15.26) (end -3.18 4.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ac496635-1b88-4ac2-a391-82d151b0ee50))
    (fp_line (start -3.18 -3.03) (end -1.98 -3.03)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fd6dda54-700d-48d7-8c01-9d8546a21fd8))
    (fp_line (start -3.18 4.1) (end -2.18 5.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8971b1e3-2290-4680-8936-9a7a9b31350f))
    (fp_line (start -2.18 5.1) (end 5.72 5.1)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6218fcd3-1633-432b-b357-c81d842a922c))
    (fp_line (start -1.98 -14.07) (end -1.98 -7.13)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 596365f3-0a3a-4130-88a7-1a6b3f60c892))
    (fp_line (start -1.98 -7.13) (end -3.18 -7.13)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dbc2badf-72b8-4ef3-b1c1-fda7887b30d0))
    (fp_line (start -1.98 -7.13) (end -1.98 -7.13)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp aee70a7c-1b86-4006-80df-e648af252c5d))
    (fp_line (start -1.98 -3.03) (end -1.98 3.91)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 10fc51e9-3426-4fbc-b696-7f4b511d4378))
    (fp_line (start -1.98 3.91) (end 4.52 3.91)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 95ee1219-fc8b-4ebc-b632-0a049db1b13b))
    (fp_line (start 4.52 -14.07) (end -1.98 -14.07)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f3ba1e05-8965-4f6b-be0c-d0d0d180b3e7))
    (fp_line (start 4.52 3.91) (end 4.52 -14.07)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3e3d5ab3-d2b1-415c-9385-ebc1b698ea83))
    (fp_line (start 5.72 -15.26) (end -3.18 -15.26)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp aa671d40-2051-4036-a9fb-f93ad475e587))
    (fp_line (start 5.72 5.1) (end 5.72 -15.26)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ebbc2c9a-fd84-4db9-87d5-6c5005831517))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 50 "Net-(VD2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp ca478177-d463-42b5-837f-80ae075acf69))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(VD2-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp fed769e7-7422-45f9-911d-fb24396c4e63))
    (pad "3" thru_hole circle (at 0 -2.54 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_3") (pintype "passive") (tstamp be0e9dd9-b6f8-4e05-a575-7586d836706c))
    (pad "4" thru_hole circle (at 2.54 -2.54 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_4") (pintype "passive") (tstamp a46d379b-535a-454e-ac9b-fce8baad3415))
    (pad "5" thru_hole circle (at 0 -5.08 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_5") (pintype "passive") (tstamp 0fbe36f1-e768-489a-9de2-42a6a9909ef6))
    (pad "6" thru_hole circle (at 2.54 -5.08 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_6") (pintype "passive") (tstamp 0b47013a-38a3-4f7f-ab43-e189018f32fb))
    (pad "7" thru_hole circle (at 0 -7.62 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_7") (pintype "passive") (tstamp ee0b199f-2440-4eb8-93fd-950fe594ee6b))
    (pad "8" thru_hole circle (at 2.54 -7.62 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_8") (pintype "passive") (tstamp fb306944-b3c4-43ec-88d7-2d42222f51b6))
    (pad "9" thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(VD1-Pad2)") (pinfunction "Pin_9") (pintype "passive") (tstamp 1d386fdf-939c-4773-871c-5cb929c67272))
    (pad "10" thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(VD1-Pad2)") (pinfunction "Pin_10") (pintype "passive") (tstamp 90912b6c-832b-49ac-bcc6-808c1a81e2b1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 48715e4e-af21-485b-924b-77fb1f26aa0e)
    (at 175.35 105.32 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/880cb7e1-fff6-421f-bd59-788a7c51a2c9")
    (attr through_hole)
    (fp_text reference "R27" (at 6.75 -0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9480e67f-894d-4647-b8ad-44cbebd450ad)
    )
    (fp_text value "47K" (at 3.5 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e6ccb50b-4d3a-4460-af82-5c7582bf0064)
    )
    (fp_text user "${REFERENCE}" (at 6.75 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 24517332-7b98-4c35-9b19-df06c7680b58)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6d7458bf-202f-4edf-af63-974d2dd270f3))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3333dfec-46d5-49fb-a896-a2c591792890))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bcbebced-98ae-480e-936a-2f164c6a3127))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ad3cfb54-cc7f-423d-89c1-1dc1128056ff))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a4144586-a0e7-4c8a-8ed1-a7cd82aff3e8))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 08635dab-0dbe-4158-8713-8f069a8b3445))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ef94244f-16a3-4153-9108-c6742aec1d9d))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d360713c-33f5-4661-9852-4f1a592f38cd))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ba7d031f-0ce3-40f2-8427-aa04fc1a88c3))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7fe01032-833f-4e45-8353-ce92005db100))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7891a5bd-b1ca-489e-8bb6-23e10963f8d9))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7959c091-b029-4842-b28a-87ce7eb70d5b))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4af76460-860d-4f5f-9a87-967d7316e323))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cb16a4ed-ca0b-43b5-bb8f-2220aa518863))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e1f03102-d613-4ccd-b3fb-94ffd5598a6b))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b3b5a8df-5c1a-40e2-ba1f-5deaa21ad53a))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(R25-Pad2)") (pintype "passive") (tstamp b2c0a1fd-c4a8-4220-bf73-68efc160b1c2))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(R27-Pad2)") (pintype "passive") (tstamp a720d58d-53da-477f-a9e7-cdc56de57dac))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "B.Cu")
    (tstamp 499665df-701c-4248-a0e7-387c6f06cd33)
    (at 132.35 71.27 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/fed241ad-0e46-4b19-8968-d27100afaf50")
    (attr through_hole)
    (fp_text reference "TH2" (at 3.81 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0e296054-979c-41d4-8755-6d54a4c817c0)
    )
    (fp_text value "10K" (at -1.69 0 180) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 53d5e066-9e86-4342-a86b-4f0434063a72)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "B.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)) (justify mirror))
      (tstamp 16cde44b-af89-4129-8095-54af3b462aa5)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e0068daf-8f77-47bd-8f26-e02c36720102))
    (fp_line (start 1.89 -0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d34612ee-c104-4e74-8169-613dedab858e))
    (fp_line (start 1.89 0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9b41d604-2008-4b7d-b8c0-8bb935ec5d46))
    (fp_line (start 5.73 -0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 328b9af0-651d-4213-808e-e91c326ab93b))
    (fp_line (start 5.73 0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8014fbc7-252f-4e8d-a2fc-da53f3ec9940))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e03f41a9-9ae7-40b5-9434-3586803935ab))
    (fp_line (start -0.95 -1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 220635ea-2160-427f-9197-76e5312ddf20))
    (fp_line (start -0.95 1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b18e4452-3b85-4610-afc9-72288489d7fd))
    (fp_line (start 8.57 -1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a377e990-bb53-4183-b36a-9bbd3312a383))
    (fp_line (start 8.57 1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 141204f5-6781-4019-9d52-82e37af1f481))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 88f9e06a-10ce-4803-92ac-774962eac83e))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 73355e02-f5c1-441b-b3c0-6150f4241c65))
    (fp_line (start 2.01 0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 44fb21f8-6a30-48aa-abcf-c075ba44d4b1))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp abc6a663-ec48-4568-94c7-8fc96cfb5fba))
    (fp_line (start 5.61 0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 43320125-6311-400c-9893-2870daf8bfa0))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5c84120d-a7b9-44d5-83af-4e7e8e4dd61c))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pintype "passive") (tstamp 6293256a-2cb6-4cca-bee1-31e86da7ed0c))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R4-Pad1)") (pintype "passive") (tstamp fc7378d1-ae87-4f32-932d-bce2834b0946))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 4c383265-6ead-4b11-8473-81bc0ad8e887)
    (at 142.27 58.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/b45e2be7-1d6e-403a-9d96-ea282670bdcf")
    (attr through_hole)
    (fp_text reference "R4" (at 3 0.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a9253d49-5ac8-4563-ba1a-7b1af116dbdf)
    )
    (fp_text value "1M" (at 6.75 -0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d87e169f-c2f9-42ef-956f-61e893ee47f5)
    )
    (fp_text user "${REFERENCE}" (at 3 0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2796926e-d2d6-4a19-b6de-e87023b27062)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 13ac3d82-c057-4d13-ba42-97b17f3b193c))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 55958351-e989-4b1f-95a9-bc6db9cadfaf))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 00b83534-05e5-4222-8920-33e939a59e9c))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ff0e98d4-fb78-481c-9522-64c9fbc6a068))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9e19a039-af64-4349-84cf-65b2504f0f7e))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 810782bb-3506-41d2-a16d-8de619e70f75))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f64c8e2c-f32b-4daf-a5ad-58ce6f44071a))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e1bb401a-8b8f-4283-a948-bb60307215dd))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bc0c5b5a-1dac-40a0-b1f0-605e9048c958))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2d53ee88-1950-4a5c-8a62-7826cc7dbbad))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 2837b80e-871d-4708-9b6c-70d705819549))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a6a61bac-88ec-49db-a887-28971b1bc1d6))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0f6468af-1d90-45c9-8fe9-4f787e2a0b22))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 94067890-fd89-431e-bd19-ab0cb81c7c99))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d1418a12-252f-4986-918b-9fa3015279d4))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a77da457-c472-4be8-b973-44f129da1597))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R4-Pad1)") (pintype "passive") (tstamp 9343be2b-6908-492a-bef1-5a7de8708108))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R4-Pad2)") (pintype "passive") (tstamp d16de268-87de-40d0-949a-f179724ad46f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 4eaea9f1-03a0-4a54-aac7-92f2f87325b3)
    (at 181.35 50.32 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/2eb13314-ab5e-400e-b601-c6a0e6c223f4")
    (attr through_hole)
    (fp_text reference "R11" (at 3.5 0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 178d91eb-0ce1-45f8-940f-2ae917af18e4)
    )
    (fp_text value "10" (at 6.75 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp afd43132-eab9-42f4-9562-22fb7dbaeeae)
    )
    (fp_text user "${REFERENCE}" (at 3.5 0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c664741a-efcd-4a00-8dd1-18fd431e0ca1)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a9afbd10-74c2-4034-905f-21ec3e592982))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 01d51f16-89b7-4833-9d6c-d2d04c81561c))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bcb4c719-f3bb-4a3c-bfe3-476fe75bf9e4))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9388b69c-5959-450e-9099-78221a8c42a4))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c81d4a7b-90b3-4b52-8b3a-5ef1d792263f))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 39495a07-6afa-4591-a830-1feab6db024f))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 812e0b69-350e-44c6-bfe7-07d8079b8121))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp bc974c18-10aa-4d70-9591-33846e4f59f0))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6142e95c-ceb1-4611-8153-2e1099aaaebe))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0e013314-51e2-4d91-aea6-a851ea69e932))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e3903831-0779-4d9a-b4f7-578ed4b32077))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6153f135-2f69-4861-b1ad-75b4aecc8d64))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1c1543d5-20c5-4307-a262-1068df4f96a6))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7e53cd12-2ad8-44f2-8bab-975123f3c97f))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 86ae6332-2bdb-4354-9ac7-0d6d8da2a0fb))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ecc4824e-ca27-4218-9d5b-030cf68913e5))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp bd8218fd-f7f0-4711-b91a-7167a1638ceb))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(R11-Pad2)") (pintype "passive") (tstamp b3dd1118-25e4-4d34-8d8b-6e35e0737684))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "B.Cu")
    (tstamp 5b931e65-7acd-49d3-950e-aec1cfcb6a28)
    (at 150.35 77.74 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/96c27e14-1c89-4cbb-9382-9b06bdb32c30")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7b91a9d7-e1a9-42e3-afe1-e9d2bdfc7ca8)
    )
    (fp_text value "TL074" (at 3.81 -17.57) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d5660d26-967e-4278-97ae-aab3d5faab93)
    )
    (fp_text user "${REFERENCE}" (at 3.81 -7.62) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9e9f4795-0afd-4bf1-9505-75bf134ea5ef)
    )
    (fp_line (start 1.16 -16.57) (end 6.46 -16.57)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5fcbfbce-41a5-41a5-acad-7e019da18ac6))
    (fp_line (start 1.16 1.33) (end 1.16 -16.57)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1dde31dd-7d2c-4ce6-8019-718954bd630b))
    (fp_line (start 2.81 1.33) (end 1.16 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 30999bbf-6e60-4683-bf65-a314838116bb))
    (fp_line (start 6.46 -16.57) (end 6.46 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e14a7f88-2d30-4594-af02-02ceabfe8a40))
    (fp_line (start 6.46 1.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a05e4260-be37-4793-bdd2-d031aa739a18))
    (fp_arc (start 2.81 1.33) (mid 3.81 0.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d41cee29-a60b-4886-81eb-f8d2f98cfc33))
    (fp_line (start -1.1 -16.8) (end 8.7 -16.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 04b5ea25-198e-4435-bc83-ed8b69b70b35))
    (fp_line (start -1.1 1.55) (end -1.1 -16.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4ea94dd4-dccd-4484-8e44-cb3d45c5d6bc))
    (fp_line (start 8.7 -16.8) (end 8.7 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d4943484-85af-47b0-a905-f8521b453cb6))
    (fp_line (start 8.7 1.55) (end -1.1 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 94555205-1b37-4657-b6d8-1d014c82a995))
    (fp_line (start 0.635 -16.51) (end 0.635 0.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7d162854-3e9e-41a8-8634-a2928e7659e7))
    (fp_line (start 0.635 0.27) (end 1.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 462c4a66-46ec-4501-ad16-c38dc9528463))
    (fp_line (start 1.635 1.27) (end 6.985 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 93799d93-9323-4afb-9806-5b92cf7a9d2a))
    (fp_line (start 6.985 -16.51) (end 0.635 -16.51)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 46831f15-882f-44a8-a84b-3bef78b4f170))
    (fp_line (start 6.985 1.27) (end 6.985 -16.51)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a88ce8be-8c93-4eae-86ed-d0aa2ac7c390))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C10-Pad1)") (pintype "output") (tstamp de2bd9e6-4841-49c7-971e-ec9fbbe097c7))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C10-Pad1)") (pinfunction "-") (pintype "input") (tstamp 96255e61-4519-4965-b1bf-1f10baf1e39f))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pinfunction "+") (pintype "input") (tstamp 3823949e-d7cd-4e06-9c09-ac3b7d3e8fb7))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in") (tstamp 93b58f21-cfa5-4436-9524-a88043ef62a0))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C10-Pad2)") (pinfunction "+") (pintype "input") (tstamp 0ce11b79-b6d1-4f0d-ad3d-2d6ae22367ea))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R16-Pad1)") (pinfunction "-") (pintype "input") (tstamp 0a4b6525-7083-44b4-b6c9-616a94d68527))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "output") (tstamp ac75aef3-d1c6-436d-bc78-eea9136a4b89))
    (pad "8" thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(R25-Pad2)") (pintype "output") (tstamp 93c39bb7-7d5f-4a9c-87a6-dc059f314796))
    (pad "9" thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(R23-Pad1)") (pinfunction "-") (pintype "input") (tstamp de69e67c-a480-4742-ab6d-b6566eb953a7))
    (pad "10" thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pinfunction "+") (pintype "input") (tstamp d79e7bfb-87f6-4f03-995f-838141eb422f))
    (pad "11" thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in") (tstamp 0c5fc9d2-19fd-4896-83ed-0c03b3c37b6e))
    (pad "12" thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(R12-Pad2)") (pinfunction "+") (pintype "input") (tstamp a321cf05-c529-4ee8-a000-4a6d33cd395c))
    (pad "13" thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pinfunction "-") (pintype "input") (tstamp f80bcc2d-291a-4705-a63c-64e4dd19bb45))
    (pad "14" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D1-Pad2)") (pintype "output") (tstamp cfd0e6cd-65c7-4143-bd6e-bcf73d00c533))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (tstamp 5c1b4e7a-bfd9-40c7-9286-b1afbdcc2f33)
    (at 146.63 67.17 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/bbea7ed9-1657-40ae-b60d-84557b5aab09")
    (attr through_hole)
    (fp_text reference "Q1" (at -0.73 3.36 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9af96d15-9fc5-4219-9d28-12362795903f)
    )
    (fp_text value "BC558" (at 2.27 3.36 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fe83ad2f-1e2d-45bc-9603-f4ac1d8609fb)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0156170a-c713-4f47-87ad-7580facf4976)
    )
    (fp_line (start -0.53 -1.85) (end 3.07 -1.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 47adb202-e79f-4a55-9a8b-6460752c292d))
    (fp_arc (start 1.27 2.6) (mid -1.132087 0.994977) (end -0.568478 -1.838478)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6b1f4eed-6ce0-49ac-8d64-ecbbfa8fdf70))
    (fp_arc (start 3.108478 -1.838478) (mid 3.672087 0.994977) (end 1.27 2.6)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 024eba3d-5bfd-465a-9b0b-84e31e950769))
    (fp_line (start -1.46 2.73) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8c036bcf-1e5b-4445-ab8b-76130e300254))
    (fp_line (start -1.46 2.73) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 96285755-45e7-46da-b4ac-f31bc872b209))
    (fp_line (start 4 -2.01) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 5fc4e745-f372-4f26-9e7f-544c5c0c4957))
    (fp_line (start 4 -2.01) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3e24bed9-3329-4401-81b3-a4606a39b25a))
    (fp_line (start -0.5 -1.75) (end 3 -1.75)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 61d2f316-0040-4909-82c0-72abbb960617))
    (fp_arc (start 1.27 2.48) (mid -1.021221 0.949055) (end -0.483625 -1.753625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 90646e6f-6dab-4e43-b4df-68ae416bfe66))
    (fp_arc (start 3.023625 -1.753625) (mid 3.561221 0.949055) (end 1.27 2.48)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 99483e8e-10e5-474c-acf8-ea2fb4f68663))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "C") (pintype "passive") (tstamp 83b4d3a9-3b7a-4571-95d2-342b43ab0621))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input") (tstamp 4cae48ad-d498-4d79-8e86-ce99d518bad8))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(Q1-Pad3)") (pinfunction "E") (pintype "passive") (tstamp d83bbc9b-01c5-4e51-8de1-0ed37bead391))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 656b505c-b964-45d6-a329-5479bb882c70)
    (at 160.18 45.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/d1d12995-6194-44a1-8527-79917432a3eb")
    (attr through_hole)
    (fp_text reference "R10" (at 3.5 0.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 29d2c74f-6db0-4333-8668-3a820d58b1ef)
    )
    (fp_text value "10" (at 7 -0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 95f87b14-109a-4800-9e67-33d96b0dad1d)
    )
    (fp_text user "${REFERENCE}" (at 3.5 0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c3ddcae2-8615-4cd6-ad7f-90940c52702e)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9dfc5a68-7616-4aff-8d39-de02b65f5ec6))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b769833d-cca2-4964-a366-74d3983fa431))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 71d22efd-53fe-41e6-b99a-3db977f68a09))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 61cf7d8b-2be4-43a2-bd4a-eb4c7f2b3d1a))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d4956d7e-d881-4ffb-8845-33b07d0263cc))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1c09e61e-b232-41e4-bbda-3c7a26955fca))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 02156d0d-0369-45f2-aa4b-691829ebdd5f))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 32bdc363-3152-4376-9841-3b3a03f9f682))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp cbbfa308-bcf7-488e-a152-3b069087afcb))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 384b3c2a-67d7-4186-aa54-6c4d7ac8b45a))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 957e6ed6-2a8b-4a51-a9a4-c62725919afc))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5f53bdd4-6c5f-434b-ad0a-3f1368134573))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp db5d4149-9721-47da-9849-2b9da84b1725))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d12e6365-d356-4576-9087-510a50d1bc78))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a2e42546-1c45-4a47-bafa-9f76e1a4ca8f))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b8f62975-4fd1-4521-91c2-5f87cd75874e))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(R10-Pad1)") (pintype "passive") (tstamp 4a892390-86e8-490b-99b4-ad65b924cd4b))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp e49e5dda-bbe8-4172-8169-09d8a9cbaa1e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (tstamp 788249f5-c5e2-4389-9a99-b6cf360fafa0)
    (at 174.534664 50.305113)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/7704204b-13e7-43fc-953e-16f4e8e824d0")
    (attr through_hole)
    (fp_text reference "C9" (at 4.265336 2.294887) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 13b5050e-9f13-4080-8286-4f76a47ab1c1)
    )
    (fp_text value "47uF" (at 1.25 -3.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bc33ab51-927b-4b6b-8c6d-6e1d51c0ddbf)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0bec8652-1bab-435a-af89-bb50da2d64b8)
    )
    (fp_line (start -1.554775 1.475) (end -1.054775 1.475)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 078676e5-1660-4bee-9df3-18d47cd1b702))
    (fp_line (start -1.304775 1.725) (end -1.304775 1.225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ef8b3e7d-c34f-45b3-9cd4-be9a488e572d))
    (fp_line (start 1.25 2.58) (end 1.25 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 990fcba6-e632-4606-b05e-30150bf23dea))
    (fp_line (start 1.29 2.58) (end 1.29 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 525fcf85-ee03-4df8-a80c-47ebddee9ab2))
    (fp_line (start 1.33 2.579) (end 1.33 -2.579)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 355b3d75-b7c7-4c61-be7e-6f330b02a458))
    (fp_line (start 1.37 2.578) (end 1.37 -2.578)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6552add4-29b5-4cb9-ac20-541c87cd2886))
    (fp_line (start 1.41 2.576) (end 1.41 -2.576)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ee7491a8-9aa8-493d-895c-ca7175dd4592))
    (fp_line (start 1.45 2.573) (end 1.45 -2.573)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b0c7f73d-5b13-47ff-914c-e9ea36173e9c))
    (fp_line (start 1.49 -1.04) (end 1.49 -2.569)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5869e72b-988d-4e77-8fde-71b3f1e97d76))
    (fp_line (start 1.49 2.569) (end 1.49 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 60317c31-f141-4956-8be2-48cb0de5d786))
    (fp_line (start 1.53 -1.04) (end 1.53 -2.565)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e81b73d6-ae59-41c9-9f19-8ba384d551cd))
    (fp_line (start 1.53 2.565) (end 1.53 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4fae7cae-382a-4997-8b9b-850a6457887d))
    (fp_line (start 1.57 -1.04) (end 1.57 -2.561)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9dbbc0a5-8fc7-4e0b-aefd-9b7366da36b0))
    (fp_line (start 1.57 2.561) (end 1.57 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c27d585c-881c-4cf2-9ff4-b4e8c6ed4673))
    (fp_line (start 1.61 -1.04) (end 1.61 -2.556)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0679467f-99c3-41b5-bcaa-651e5cdbaf43))
    (fp_line (start 1.61 2.556) (end 1.61 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 69cd5c5c-63a6-4bcd-bf25-e34e6ce31ed9))
    (fp_line (start 1.65 -1.04) (end 1.65 -2.55)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0fe47892-e72d-40bb-876c-ceacb7f6d147))
    (fp_line (start 1.65 2.55) (end 1.65 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48915e56-a62d-436b-a5c1-035ad4d30974))
    (fp_line (start 1.69 -1.04) (end 1.69 -2.543)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6dc57af2-0fb0-478b-96ad-736f9e4b2cd1))
    (fp_line (start 1.69 2.543) (end 1.69 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 62d4a5a4-b2f9-46e3-a42c-1fda9da83ab2))
    (fp_line (start 1.73 -1.04) (end 1.73 -2.536)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4b5db87c-5f5b-4ed4-8151-ac957db6309a))
    (fp_line (start 1.73 2.536) (end 1.73 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 26949266-af44-424a-8b33-48bede2bfa3a))
    (fp_line (start 1.77 -1.04) (end 1.77 -2.528)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 187c2055-f9ca-4fb1-8b9c-4484809c8463))
    (fp_line (start 1.77 2.528) (end 1.77 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7cb6f842-5bb4-4db4-8513-15a779187210))
    (fp_line (start 1.81 -1.04) (end 1.81 -2.52)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 88137610-a269-4091-8d41-42f23b7642bd))
    (fp_line (start 1.81 2.52) (end 1.81 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6846cc53-99fb-46e3-9173-393d262bb799))
    (fp_line (start 1.85 -1.04) (end 1.85 -2.511)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f8936fa1-7b6a-43bc-b2c4-93acd427254a))
    (fp_line (start 1.85 2.511) (end 1.85 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5e3f602c-b6b2-4348-9f37-03f868524be5))
    (fp_line (start 1.89 -1.04) (end 1.89 -2.501)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 22c977e3-5ec6-4924-8280-488c4c275f06))
    (fp_line (start 1.89 2.501) (end 1.89 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c3dd50df-8a30-4370-811e-255c10c4cd13))
    (fp_line (start 1.93 -1.04) (end 1.93 -2.491)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 42bb4c35-0b48-478e-a0dc-531ee3449924))
    (fp_line (start 1.93 2.491) (end 1.93 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 35d02c00-574f-4390-b142-c2a71b7fc610))
    (fp_line (start 1.971 -1.04) (end 1.971 -2.48)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9c6e8dea-7bde-4f89-907a-433bb97f82a3))
    (fp_line (start 1.971 2.48) (end 1.971 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2a150d7c-7fda-4a66-922f-6cb4c1b3225a))
    (fp_line (start 2.011 -1.04) (end 2.011 -2.468)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e590f5b9-7600-4d31-b1fc-a09878e8b855))
    (fp_line (start 2.011 2.468) (end 2.011 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c87c4734-42b5-42eb-95f3-1220a6e92d40))
    (fp_line (start 2.051 -1.04) (end 2.051 -2.455)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp de462ece-95d9-495b-a24a-8c8d9c7da038))
    (fp_line (start 2.051 2.455) (end 2.051 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp aef2cf45-5fac-4861-a022-2854a33b3a5d))
    (fp_line (start 2.091 -1.04) (end 2.091 -2.442)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 92f468ff-5f59-4ae4-9265-6bb7a432f68f))
    (fp_line (start 2.091 2.442) (end 2.091 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 18a1742a-ce17-46ec-8bac-e2625b44f5f9))
    (fp_line (start 2.131 -1.04) (end 2.131 -2.428)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 65a9543d-2945-41d6-bb0e-a9e95f525d97))
    (fp_line (start 2.131 2.428) (end 2.131 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 726653cf-0660-4594-a8e2-74647cca00f8))
    (fp_line (start 2.171 -1.04) (end 2.171 -2.414)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 642d0221-9abf-4130-bfc8-37564abf059a))
    (fp_line (start 2.171 2.414) (end 2.171 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 632a1066-53ab-435c-9c01-d8b4e72a9f56))
    (fp_line (start 2.211 -1.04) (end 2.211 -2.398)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e0fdbfef-a314-4db5-987c-b5415d361f3d))
    (fp_line (start 2.211 2.398) (end 2.211 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 28358ba8-3e38-4b0b-bc0b-2cb9d8f6ce67))
    (fp_line (start 2.251 -1.04) (end 2.251 -2.382)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 05341257-9c0e-45fd-8d16-029cfeb5b16a))
    (fp_line (start 2.251 2.382) (end 2.251 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b5a4f93a-4ad6-4b27-bade-0479796cee44))
    (fp_line (start 2.291 -1.04) (end 2.291 -2.365)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c49e28a8-34c7-4b96-b6c1-7ef8832617f8))
    (fp_line (start 2.291 2.365) (end 2.291 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7cac910b-e3f6-48f6-b38d-bdc4ade36f54))
    (fp_line (start 2.331 -1.04) (end 2.331 -2.348)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ee879c67-cd9b-4d59-8517-369b61d05e6d))
    (fp_line (start 2.331 2.348) (end 2.331 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d405461d-c7d8-42b7-a1ed-d4d11d7ca5b2))
    (fp_line (start 2.371 -1.04) (end 2.371 -2.329)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 347e7910-c030-4a13-8ed2-e28a2cc1037e))
    (fp_line (start 2.371 2.329) (end 2.371 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5a3037d9-31e9-48c7-a564-214c18b06c41))
    (fp_line (start 2.411 -1.04) (end 2.411 -2.31)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9a1a5ca7-bc86-47e4-9871-150836fc49df))
    (fp_line (start 2.411 2.31) (end 2.411 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 816e6fb4-a5a9-41d8-b593-9c8ef07fc91e))
    (fp_line (start 2.451 -1.04) (end 2.451 -2.29)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e7169f77-c523-4a67-863f-524189303ed2))
    (fp_line (start 2.451 2.29) (end 2.451 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4be44b9-e4b4-40a6-82c9-f108ddab4d38))
    (fp_line (start 2.491 -1.04) (end 2.491 -2.268)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp df8660a5-4317-4698-9b3e-7e7775958805))
    (fp_line (start 2.491 2.268) (end 2.491 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dc0e0038-bdd9-4ceb-a599-0b0c693c8536))
    (fp_line (start 2.531 -1.04) (end 2.531 -2.247)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9e8cbb64-575a-4e94-8cd5-cb46900532b7))
    (fp_line (start 2.531 2.247) (end 2.531 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4f8cbe3-accb-4988-9a83-c0135de60b6c))
    (fp_line (start 2.571 -1.04) (end 2.571 -2.224)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a52bb0bd-1d08-4ef9-9eda-800777aa589d))
    (fp_line (start 2.571 2.224) (end 2.571 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a0e52df5-648a-4590-a8fd-4b2201d5223d))
    (fp_line (start 2.611 -1.04) (end 2.611 -2.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 38343a7b-f086-4ed2-bcb1-e2de727e4e00))
    (fp_line (start 2.611 2.2) (end 2.611 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 413ac2b1-39b0-4967-b92b-bf77ebb90e8a))
    (fp_line (start 2.651 -1.04) (end 2.651 -2.175)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f865ca79-8ebc-474a-b51e-f3624acb04d6))
    (fp_line (start 2.651 2.175) (end 2.651 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1b361f3d-552d-4b4d-9efe-7c442ea1659d))
    (fp_line (start 2.691 -1.04) (end 2.691 -2.149)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c04b2bab-acac-41a9-b681-e4eb0833b41c))
    (fp_line (start 2.691 2.149) (end 2.691 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp da2b531a-b4c9-4a61-bc53-e98f0fa2f02f))
    (fp_line (start 2.731 -1.04) (end 2.731 -2.122)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f493dd64-53ce-4fd6-9d47-7a611fabdef2))
    (fp_line (start 2.731 2.122) (end 2.731 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 57236aeb-e8d8-489e-9a0a-f180a606f1bd))
    (fp_line (start 2.771 -1.04) (end 2.771 -2.095)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8657cddc-3eb8-4256-91c9-c143208ed28f))
    (fp_line (start 2.771 2.095) (end 2.771 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f2d4eed4-76a8-4c85-a2ad-bcb6f9885116))
    (fp_line (start 2.811 -1.04) (end 2.811 -2.065)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bbaee259-d979-49cf-b126-6092a8b976c6))
    (fp_line (start 2.811 2.065) (end 2.811 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4734707a-e9b7-4e3c-9449-a982b2c4f7ef))
    (fp_line (start 2.851 -1.04) (end 2.851 -2.035)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 11b45896-6e30-42e9-a5e0-babc46767acf))
    (fp_line (start 2.851 2.035) (end 2.851 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ffb5fa9e-dc36-4de9-94b9-84af7119b15f))
    (fp_line (start 2.891 -1.04) (end 2.891 -2.004)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6d7851a7-ce26-4904-b28c-3a4cbb5efffb))
    (fp_line (start 2.891 2.004) (end 2.891 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 50952822-58de-4f1f-bdfb-58adb030d70b))
    (fp_line (start 2.931 -1.04) (end 2.931 -1.971)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8fa9d928-5b9a-4ed1-b573-2046e0532577))
    (fp_line (start 2.931 1.971) (end 2.931 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c473a047-7867-47d9-9b87-2b230d1a3653))
    (fp_line (start 2.971 -1.04) (end 2.971 -1.937)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 174cec19-afd4-4e6d-b161-65ea8387a63c))
    (fp_line (start 2.971 1.937) (end 2.971 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4246ecbd-5c22-446f-b530-f4ea9c81a5c6))
    (fp_line (start 3.011 -1.04) (end 3.011 -1.901)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c2a3f4d2-d261-4a1f-9dc2-7fbda26baada))
    (fp_line (start 3.011 1.901) (end 3.011 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ee6d14eb-3849-4d87-9479-adba9fd87f99))
    (fp_line (start 3.051 -1.04) (end 3.051 -1.864)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7acf9ad2-2934-4fd7-9e19-db66bc52c7a3))
    (fp_line (start 3.051 1.864) (end 3.051 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 59b09b86-3575-41ea-b326-e058937dd325))
    (fp_line (start 3.091 -1.04) (end 3.091 -1.826)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 48a13d68-9dfb-44b1-9159-0ce7a936abb2))
    (fp_line (start 3.091 1.826) (end 3.091 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 383fb21d-f791-4814-8d2f-e236faa8f4cc))
    (fp_line (start 3.131 -1.04) (end 3.131 -1.785)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 13357e06-0e3e-4a7b-a6c1-fc14de892021))
    (fp_line (start 3.131 1.785) (end 3.131 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fac79455-8cec-453e-b53e-c84777571690))
    (fp_line (start 3.171 -1.04) (end 3.171 -1.743)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8553c742-bfff-4728-ac0f-f11c45deb26d))
    (fp_line (start 3.171 1.743) (end 3.171 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c9e3a609-ddbf-4984-93f7-6ca3a1b2c107))
    (fp_line (start 3.211 -1.04) (end 3.211 -1.699)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b68bac29-109a-4c07-a47e-203bab72b669))
    (fp_line (start 3.211 1.699) (end 3.211 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2ee890db-cd83-4bde-a9cf-8e8bb0e425be))
    (fp_line (start 3.251 -1.04) (end 3.251 -1.653)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ffa0ff8b-8b05-41d0-924a-9d36f61a8bd4))
    (fp_line (start 3.251 1.653) (end 3.251 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d432c8b2-07cd-45ee-ba31-4bc702e4eadc))
    (fp_line (start 3.291 -1.04) (end 3.291 -1.605)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ade466ce-8f1d-4905-9cf1-54bdea9f2ca4))
    (fp_line (start 3.291 1.605) (end 3.291 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9ae95696-9a72-42c9-a36a-e3c84c45c3f1))
    (fp_line (start 3.331 -1.04) (end 3.331 -1.554)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cef56fe6-9336-4901-a42c-c4720afc934d))
    (fp_line (start 3.331 1.554) (end 3.331 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c1e56835-4155-4cc0-a327-ec2b121554c5))
    (fp_line (start 3.371 -1.04) (end 3.371 -1.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8d01090b-bee0-4c8f-85ca-35e884082cc1))
    (fp_line (start 3.371 1.5) (end 3.371 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 419b1cf7-0f1e-4f98-8c00-b6e79c80a471))
    (fp_line (start 3.411 -1.04) (end 3.411 -1.443)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4f53939f-394b-4ff5-be28-15ab6dba3b32))
    (fp_line (start 3.411 1.443) (end 3.411 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8b4accc9-7f89-4830-91a8-e974a043c4e4))
    (fp_line (start 3.451 -1.04) (end 3.451 -1.383)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp abcd4264-cb75-42df-be53-3721149e5426))
    (fp_line (start 3.451 1.383) (end 3.451 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d6c6bf02-e872-4cd8-b3a5-f721dfac130a))
    (fp_line (start 3.491 -1.04) (end 3.491 -1.319)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 41d613fb-9b01-438a-aacf-11febb573897))
    (fp_line (start 3.491 1.319) (end 3.491 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7a4a9761-0727-47ff-9610-6b13e67c3856))
    (fp_line (start 3.531 -1.04) (end 3.531 -1.251)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 67beb68f-3dfa-4b9c-b80f-87cb645e6fe2))
    (fp_line (start 3.531 1.251) (end 3.531 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b1f350d4-af40-4cc3-a1ce-efbe212b18e8))
    (fp_line (start 3.571 1.178) (end 3.571 -1.178)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 60481ad6-3329-4f9c-831b-d0202ddc23c7))
    (fp_line (start 3.611 1.098) (end 3.611 -1.098)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 986411f1-ef22-4775-aba8-0e87e907688c))
    (fp_line (start 3.651 1.011) (end 3.651 -1.011)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 47593485-eee0-4956-a44c-5fdf5013bb83))
    (fp_line (start 3.691 0.915) (end 3.691 -0.915)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 09888752-a4fb-45b2-a851-e9a3ba6a05e7))
    (fp_line (start 3.731 0.805) (end 3.731 -0.805)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7f596438-4163-4fca-a901-882d10d0128c))
    (fp_line (start 3.771 0.677) (end 3.771 -0.677)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cfc6fb4d-05d9-4560-a541-6909272fb230))
    (fp_line (start 3.811 0.518) (end 3.811 -0.518)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7fdb5a04-f97b-46cb-81ed-15c17a6397b1))
    (fp_line (start 3.851 0.284) (end 3.851 -0.284)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1fc517e8-80e8-49f3-bc19-22201fc91c53))
    (fp_circle (center 1.25 0) (end 3.87 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "B.SilkS") (tstamp 50526337-52b3-4906-95f4-5460cc427669))
    (fp_circle (center 1.25 0) (end 4 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "B.CrtYd") (tstamp d8ff8e1c-690e-4d84-bd70-c71df290300c))
    (fp_line (start -0.883605 1.0875) (end -0.383605 1.0875)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 72144b2c-a644-47b0-82af-576f6595528c))
    (fp_line (start -0.633605 1.3375) (end -0.633605 0.8375)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 438bc8d9-8242-41a0-aa98-c1108fee9353))
    (fp_circle (center 1.25 0) (end 3.75 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "B.Fab") (tstamp 82a8f625-f852-4931-9f31-d5bf1e42d8d6))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp c43b649f-62e3-4ccc-a070-39643f7c5d7e))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive") (tstamp 50501f47-b584-49c7-9c5e-3b2ab7edeb80))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_T-1_P5.08mm_Horizontal" (layer "B.Cu")
    (tstamp 7f258a5e-1127-45a2-bb09-3894d7427b0f)
    (at 171.64 111.65 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/52e2960e-4f2d-4503-bee6-968a4851223d")
    (attr through_hole)
    (fp_text reference "D3" (at 2.54 0) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6ed981b7-3e81-4548-a7ca-b30fbbcfa70b)
    )
    (fp_text value "1N4148" (at 2.54 -2.42) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c91fbd08-3bde-4baf-952e-bb220e1fa25a)
    )
    (fp_text user "${REFERENCE}" (at 2.78 0) (layer "B.Fab")
        (effects (font (size 0.64 0.64) (thickness 0.096)) (justify mirror))
      (tstamp 85ca745d-b516-4b7a-948b-3264fd479cf5)
    )
    (fp_line (start 0.82 -1.42) (end 4.26 -1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a5cd1225-9c5e-4373-82f4-4f0df54556bf))
    (fp_line (start 0.82 -1.24) (end 0.82 -1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5199bd6d-5f2d-484b-9206-f8e0c8322952))
    (fp_line (start 0.82 1.24) (end 0.82 1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ce89471d-34f3-44df-acc0-fb3d199b7233))
    (fp_line (start 0.82 1.42) (end 4.26 1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7dde69d4-a3c9-4482-be4d-5d1dda880741))
    (fp_line (start 1.3 1.42) (end 1.3 -1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ccd6b049-0f93-4a07-9ee8-a07a7e8d6078))
    (fp_line (start 1.42 1.42) (end 1.42 -1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e0de402c-ebb9-46a5-869e-392c61363ea9))
    (fp_line (start 1.54 1.42) (end 1.54 -1.42)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 190ebd0d-cb2b-45cd-ad23-46d73db80c0a))
    (fp_line (start 4.26 -1.42) (end 4.26 -1.24)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a1e40044-fbf2-48eb-bcb0-a2abeec8b0d3))
    (fp_line (start 4.26 1.42) (end 4.26 1.24)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f2753bc6-b073-40f8-a314-f667734a0d93))
    (fp_line (start -1.25 -1.55) (end 6.33 -1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d47d0483-602f-43a7-b3ab-21be61d0b776))
    (fp_line (start -1.25 1.55) (end -1.25 -1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 2722bd42-cc4f-4be3-b86f-c3b5e521dcca))
    (fp_line (start 6.33 -1.55) (end 6.33 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ddcbc34a-3f9a-4b93-8350-17706aeba265))
    (fp_line (start 6.33 1.55) (end -1.25 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1ad72904-abab-4272-863a-38894437b3aa))
    (fp_line (start 0 0) (end 0.94 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9c941e36-cce3-4406-8aa0-dab8d84d4f4f))
    (fp_line (start 0.94 -1.3) (end 4.14 -1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5a3cf9d9-43a1-482a-af37-6f6cd4aa73d4))
    (fp_line (start 0.94 1.3) (end 0.94 -1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 14441ec6-a6f3-47cc-baa5-7b4f8cdaddb3))
    (fp_line (start 1.32 1.3) (end 1.32 -1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 729f5c8a-8d9c-472b-825c-d3213d78b5e0))
    (fp_line (start 1.42 1.3) (end 1.42 -1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5accf043-f5ac-4aac-9a99-b4cdc3f4a3e9))
    (fp_line (start 1.52 1.3) (end 1.52 -1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 62beb700-865c-4d0b-b750-87c7ca3f6737))
    (fp_line (start 4.14 -1.3) (end 4.14 1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8a50eb02-c0d2-4881-8697-fc3bf9881989))
    (fp_line (start 4.14 1.3) (end 0.94 1.3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e369faff-51d7-4943-90f5-baa23c2a6329))
    (fp_line (start 5.08 0) (end 4.14 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 696ae390-e8d4-41dc-82e5-7e1764d1c3d2))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 9f5dbebc-bcb2-49a9-9cb9-9137a6ca51db))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C12-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 12b3747a-db67-45d5-8cc4-8377d36927bc))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:C_Rect_L22.0mm_W6.1mm_P20mm_MKT_BIG_RED_CAP" (layer "B.Cu")
    (tstamp 7f5c789c-503c-41b8-b3ef-f77eade140b9)
    (at 166.85 102.9 180)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 24mm width 7mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/68b25ead-85b7-44d1-9592-013a47714efa")
    (attr through_hole)
    (fp_text reference "C11" (at 4.25 1.75) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6004b504-54f4-44f0-9320-7372b39e9f5a)
    )
    (fp_text value "1uF" (at 17.5 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 413a310a-f610-4000-8990-8dd5b2fa055d)
    )
    (fp_text user "${REFERENCE}" (at 3.5 1.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 71de996c-1e84-45b9-87b3-0779d152c43e)
    )
    (fp_line (start -0.87 -3.06) (end 21.13 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 01425d55-d59b-4207-8cf8-23e5d57fbf5f))
    (fp_line (start -0.87 -1.185) (end -0.87 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a69a124f-d5cc-4319-b161-d4709f8f2afd))
    (fp_line (start -0.87 3.06) (end -0.87 1.185)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 71d38163-051f-4695-8cdf-9118e41d3999))
    (fp_line (start -0.87 3.06) (end 21.13 3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 77b47eff-27de-4fd7-9dff-c618379c43e8))
    (fp_line (start 21.13 -1.185) (end 21.13 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 45da66fe-9ce2-488d-94bb-a73259d34825))
    (fp_line (start 21.13 3.06) (end 21.13 1.185)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 92a7669c-1030-4de4-89ac-39d38d9c0fc4))
    (fp_line (start -1.45 -3.19) (end 21.45 -3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f6602d00-9c88-4590-9ca7-15e7bdb0fbb9))
    (fp_line (start -1.45 3.19) (end -1.45 -3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a29525c9-be3a-4ecd-b2ae-d39d178522da))
    (fp_line (start 21.45 -3.19) (end 21.45 3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4150cdb2-c44d-44ec-9e4e-b5dabb6c0da1))
    (fp_line (start 21.45 3.19) (end -1.45 3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 80eabd8d-a64b-4a13-9972-495fa343ab2a))
    (fp_line (start -0.75 -2.94) (end 21.01 -2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 438a3f17-182d-4eae-917e-fa386f5e8ea3))
    (fp_line (start -0.75 2.94) (end -0.75 -2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp eaa9e3f0-43f2-4ccb-bd71-7119c229be4e))
    (fp_line (start 21.01 -2.94) (end 21.01 2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0842f03f-ec9f-4aac-995f-44c255f10c99))
    (fp_line (start 21.01 2.94) (end -0.75 2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cfc5db26-962e-4b9c-b36e-92901c7ccc18))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "passive") (tstamp 5bd39168-853f-435d-8de5-a8f291718301))
    (pad "2" thru_hole circle (at 20 0 180) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C11-Pad2)") (pintype "passive") (tstamp 670192b3-4474-481f-9309-c05114e8c24f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L24.0mm_W7.0mm_P22.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp 8565fe8f-311e-45f0-a247-3389e4c7a7cc)
    (at 178.52 108.4)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/de822feb-cb80-46f8-a1f4-c7cb04a882dc")
    (attr through_hole)
    (fp_text reference "R28" (at 3.5 0.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9e0b4c78-e17f-4556-b922-23e9c84a2d09)
    )
    (fp_text value "47K*" (at 6.25 -0.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fa030976-f0eb-4b27-82ca-d253daa263e5)
    )
    (fp_text user "${REFERENCE}" (at 3.5 0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 68adb8c4-9443-4229-869a-f58b1348d24f)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 30b82c81-b498-469c-b93e-3e51b823fa12))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7a71f3e5-852e-46f7-9ff6-7633a702e905))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a80d8c43-5118-4b88-90a5-e4ae93440932))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0364d13f-2825-482f-91bc-174f7a87759f))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 243d07e5-9ad5-46d6-9459-d19da14136b8))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3ab2b31c-e723-4498-a744-776544121d28))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 1d678cf2-5ab2-41a1-abc2-cd4ffc8b9703))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6f9481aa-d93c-4aa1-8d21-f04e9a16ff1b))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp dab29002-9b7f-4f45-8661-9c9e33a69c4e))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 39b9cccc-27b5-4a22-a3f6-e54e55a4346b))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0cce2075-5f21-4a3c-b4d0-b914e07ab6a3))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 830fce5b-2b45-4798-98af-d36341474f45))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9378c79f-b620-405b-afa2-dd459516d4a9))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5b85a3f4-c1d0-4700-8684-ece2f34a00e1))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6b09ae8d-37f9-4856-8aa8-acf254d69f9a))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3c6c5c9a-9cbf-4c8d-8bb9-b28f63fb1c06))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(R27-Pad2)") (pintype "passive") (tstamp 9cecde5a-ea0e-4836-9693-5fe7102824c8))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 029d5590-ccb3-44cd-be63-fed28da146a6))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "SynthMages:C_Rect_L22.0mm_W6.1mm_P20mm_MKT_BIG_RED_CAP" (layer "B.Cu")
    (tstamp 8d6c6d6e-1f7d-49cd-bdb4-c6338091f121)
    (at 168.85 75.4 -90)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 24mm width 7mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/d34b8242-92e1-4fb0-b6aa-ea21c49381f8")
    (attr through_hole)
    (fp_text reference "C10" (at 2.915113 2.01 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f170f38d-2c90-45fc-bf98-9a21f340111c)
    )
    (fp_text value "1uF" (at 16.415113 2.01 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b7271244-0303-40de-a746-bfd38ff4750f)
    )
    (fp_text user "${REFERENCE}" (at 2.915113 2.01 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5ede372a-3121-474a-b0c2-782d97bae80a)
    )
    (fp_line (start -0.87 -3.06) (end 21.13 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 06b21f7a-8e46-4855-ac30-0bfc2cb6641f))
    (fp_line (start -0.87 -1.185) (end -0.87 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 73e1281e-269f-4298-ac16-e85f7e8e2e5e))
    (fp_line (start -0.87 3.06) (end -0.87 1.185)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1ba78357-f2bc-4651-a563-c512a5cd63fd))
    (fp_line (start -0.87 3.06) (end 21.13 3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4933d3c2-7d47-47fe-a635-5332ebae73e3))
    (fp_line (start 21.13 -1.185) (end 21.13 -3.06)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bb1207a1-2019-4b70-b559-4046a1da8bf2))
    (fp_line (start 21.13 3.06) (end 21.13 1.185)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c9025069-7522-42d0-961b-13aecfa9f907))
    (fp_line (start -1.45 -3.19) (end 21.45 -3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 46585ec3-2e96-4125-a89e-6412656c1b00))
    (fp_line (start -1.45 3.19) (end -1.45 -3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0d948659-f11b-4a39-bbda-7d6ebc9c9670))
    (fp_line (start 21.45 -3.19) (end 21.45 3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp db657822-f0a3-42cf-b4a5-78e0809c8ad7))
    (fp_line (start 21.45 3.19) (end -1.45 3.19)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp dafd958c-69cc-46c5-a206-608f0604aea4))
    (fp_line (start -0.75 -2.94) (end 21.01 -2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cbc607ef-355b-4c99-a114-7054ca751adc))
    (fp_line (start -0.75 2.94) (end -0.75 -2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fe30a91a-496a-41ef-a594-45de9ca50717))
    (fp_line (start 21.01 -2.94) (end 21.01 2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 246e15db-5444-4651-a2de-ed9ff92a9191))
    (fp_line (start 21.01 2.94) (end -0.75 2.94)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 65dba6fb-8924-4772-8737-41f9b12b375d))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C10-Pad1)") (pintype "passive") (tstamp e85ad2c3-9a3b-41f2-8873-5b2dba65ac14))
    (pad "2" thru_hole circle (at 20 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C10-Pad2)") (pintype "passive") (tstamp 2a83e6df-edc4-4740-ae0d-e347eb1492cb))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L24.0mm_W7.0mm_P22.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Bourns_3386C_Horizontal" (layer "B.Cu")
    (tstamp 929cc8ce-e1b9-44d4-9842-36ee1eb295ed)
    (at 140.85 127.4 180)
    (descr "Potentiometer, horizontal, Bourns 3386C, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer horizontal Bourns 3386C")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/29221eea-0ae6-49b2-a8c1-1aa9570840a1")
    (attr through_hole)
    (fp_text reference "RV7" (at 1 1.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a0dc5a92-0304-422e-a407-63a72c74e7c9)
    )
    (fp_text value "20K*" (at 0.5 -6.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e45f4473-92a4-4a59-8af8-43611094d75c)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2483f420-f94e-4fc0-967d-285f85b69aa1)
    )
    (fp_line (start -2.535 -7.425) (end 2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 94e40186-41f7-455d-bb72-015c57bf2b48))
    (fp_line (start -2.535 2.345) (end -2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9a37c275-ffc9-414c-95a4-9509c07e9582))
    (fp_line (start -2.535 2.345) (end 2.535 2.345)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 67d30bcd-340f-4aca-8aba-b7973a07be65))
    (fp_line (start 2.535 2.345) (end 2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 82fa2620-eaee-4128-93cd-c58428dff6a4))
    (fp_line (start -2.67 -7.56) (end 2.67 -7.56)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 42ccf623-e03a-49b2-9139-bfe94fe2545e))
    (fp_line (start -2.67 2.48) (end -2.67 -7.56)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 775010cb-565b-4e63-b454-f196b5b943c5))
    (fp_line (start 2.67 -7.56) (end 2.67 2.48)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 36cda423-7f6f-45aa-a5dc-1b2af3fe866a))
    (fp_line (start 2.67 2.48) (end -2.67 2.48)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3f0b6606-4e92-4a70-bdf8-07f5d0175e73))
    (fp_line (start -2.415 -7.305) (end -2.415 2.225)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b84a4de5-2c7f-4e62-a4f1-ff387b019de7))
    (fp_line (start -2.415 2.225) (end 2.415 2.225)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9db2579f-b0ff-4184-81bf-fae2e30ca13a))
    (fp_line (start 2.415 -7.305) (end -2.415 -7.305)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 26124275-f824-452f-b67c-31dce853a68d))
    (fp_line (start 2.415 2.225) (end 2.415 -7.305)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 947b90d8-1d6e-4d03-b09d-de2e4170977d))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(RV7-Pad1)") (pinfunction "1") (pintype "passive") (tstamp f3ec0c5d-8084-4217-9c71-94067cad76cc))
    (pad "2" thru_hole circle (at 0 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C12-Pad1)") (pinfunction "2") (pintype "passive") (tstamp d6e2dea2-f56c-471e-be02-1a7bf6e3e2fc))
    (pad "3" thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C12-Pad2)") (pinfunction "3") (pintype "passive") (tstamp f899d199-5f14-44fb-83bf-ac797bfec70e))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386C_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (tstamp 98bf333f-a675-49f1-8187-8a7226bb29cd)
    (at 142.6 64.65 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/cda01354-7601-4564-ac11-f0eea574c84b")
    (attr through_hole)
    (fp_text reference "Q2" (at 3.52 3.36 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cf8031aa-8a16-4724-9519-27c7917dfd83)
    )
    (fp_text value "BC548" (at 0.27 3.36 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 05b6dee3-aa69-472f-850e-db360d74dde7)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7c225b6d-55c9-4336-aa9c-e8dee881e972)
    )
    (fp_line (start -0.53 -1.85) (end 3.07 -1.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 12652350-d3f0-46cf-bf85-01e17e54922a))
    (fp_arc (start 1.27 2.6) (mid -1.132087 0.994977) (end -0.568478 -1.838478)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 632de01a-9a9c-4e5f-ae9c-fa9c35dadebd))
    (fp_arc (start 3.108478 -1.838478) (mid 3.672087 0.994977) (end 1.27 2.6)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c86948de-430a-4751-bbf4-3813ff477b1c))
    (fp_line (start -1.46 2.73) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4bd75ec6-678c-449d-926c-fcf814561aa8))
    (fp_line (start -1.46 2.73) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp df5883ef-c934-42c2-8804-928486b8608b))
    (fp_line (start 4 -2.01) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 54d43523-e34a-43b1-a3eb-586ed52480e2))
    (fp_line (start 4 -2.01) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a7717899-d6e2-44c3-8e5d-9c42538af4aa))
    (fp_line (start -0.5 -1.75) (end 3 -1.75)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3a100f0b-4c4b-4063-9813-5f65793c410a))
    (fp_arc (start 1.27 2.48) (mid -1.021221 0.949055) (end -0.483625 -1.753625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7bc67e0f-6202-49ed-a301-033a67517661))
    (fp_arc (start 3.023625 -1.753625) (mid 3.561221 0.949055) (end 1.27 2.48)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ed9f7b95-16e1-4def-93d9-8249f41dd789))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Q2-Pad1)") (pinfunction "C") (pintype "passive") (tstamp ac145b5e-6948-4628-a8b3-fe929a81c1ad))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(Q1-Pad3)") (pinfunction "B") (pintype "input") (tstamp 59ef8ad9-c5f1-4b8b-9595-8dc44987a23f))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "E") (pintype "passive") (tstamp 469a14a1-10d8-4349-b022-248a329329fc))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT" (layer "B.Cu")
    (tstamp 9d9238cf-2ffe-4d64-8419-2265ba60e67d)
    (at 151.1 131.15 90)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 9mm width 5.1mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/e758fc45-f028-4b32-a3d8-88c4aaa840b0")
    (attr through_hole)
    (fp_text reference "C12" (at 6.25 -1.75 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eb580a97-68cd-4ed4-8f42-c6292211c6a4)
    )
    (fp_text value "10nF*" (at 1.75 -1.75 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8945ab31-963c-49e7-bf41-5d864106b8ce)
    )
    (fp_text user "${REFERENCE}" (at 6.25 -1.75 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6ba642e2-092d-4c66-9fbc-6c7f719b4a7f)
    )
    (fp_line (start -0.87 -2.67) (end 8.37 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a8ca4a77-cf79-4e98-8490-87b75563c212))
    (fp_line (start -0.87 -0.665) (end -0.87 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2d225d53-a9d5-416a-a417-a68065be6de7))
    (fp_line (start -0.87 2.67) (end -0.87 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a96017e9-528f-4779-acc7-8fca071dfe19))
    (fp_line (start -0.87 2.67) (end 8.37 2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b24f281e-21bd-47c1-bfc6-517bc11ccb9b))
    (fp_line (start 8.37 -0.665) (end 8.37 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b12dc786-7222-4b70-9cad-5ce2f1a66ecc))
    (fp_line (start 8.37 2.67) (end 8.37 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dc6c8cd6-d13d-4fa6-bfd8-bac180171931))
    (fp_line (start -1.05 -2.8) (end 8.55 -2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b8613ca8-2ada-4b47-b63f-7beb3110df59))
    (fp_line (start -1.05 2.8) (end -1.05 -2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 0650a5a9-687e-4a68-ade5-4f00127150a1))
    (fp_line (start 8.55 -2.8) (end 8.55 2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4e23f37c-ee37-4f8d-8f44-c5cec21d456d))
    (fp_line (start 8.55 2.8) (end -1.05 2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ebbd3519-f4cb-46ac-a5a3-9bda56591601))
    (fp_line (start -0.75 -2.55) (end 8.25 -2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bff7881b-6a72-4da1-badb-663a45a6b159))
    (fp_line (start -0.75 2.55) (end -0.75 -2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d57b7e57-6aee-4089-b8bf-189c446f616a))
    (fp_line (start 8.25 -2.55) (end 8.25 2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 58be721e-23ee-4001-b3e8-dd4b4d74d6f4))
    (fp_line (start 8.25 2.55) (end -0.75 2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ee625c49-2975-4eab-b3a6-45819bd491ff))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C12-Pad1)") (pintype "passive") (tstamp a96509bc-5ed1-42a4-bcba-78cc9dfd8fac))
    (pad "2" thru_hole circle (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C12-Pad2)") (pintype "passive") (tstamp 0e8bf6b8-04ba-429d-91cc-65915fb00216))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (tstamp a8bd9e0d-0965-4a87-8d6f-aefd75681269)
    (at 126.96 94.38 -90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c4b41c78-2e4c-446f-807c-a6e5b001c6dd")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.22098 1.717321 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d0d7e762-c3a7-47cd-a4d2-0102a0e8d429)
    )
    (fp_text value "NPN*" (at 1.27 -2.79 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6d7722eb-07b9-4bad-823e-4f78b4f2f1f2)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0f5e4770-031b-4310-bec7-2938140f4829)
    )
    (fp_line (start -0.53 -1.85) (end 3.07 -1.85)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c7d0247b-10cd-4bd2-9e48-0f3bd1b98786))
    (fp_arc (start 1.27 2.6) (mid -1.132087 0.994977) (end -0.568478 -1.838478)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7a6e6bd1-4a85-43c2-8067-90faaa8869a4))
    (fp_arc (start 3.108478 -1.838478) (mid 3.672087 0.994977) (end 1.27 2.6)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7ca9d0a4-0307-4b5d-89f4-6d006113c65a))
    (fp_line (start -1.46 2.73) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp f467d56a-fd7a-48bd-ad18-f352b7e4203d))
    (fp_line (start -1.46 2.73) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 23b2ba5c-5d88-4dbd-820a-69ab48feb490))
    (fp_line (start 4 -2.01) (end -1.46 -2.01)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4efb8b34-c591-4775-9b1d-3cf815f26d7b))
    (fp_line (start 4 -2.01) (end 4 2.73)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3525ac42-3dcf-4cb6-8e24-af1bc668a70a))
    (fp_line (start -0.5 -1.75) (end 3 -1.75)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp cbfbebb4-9a7a-466b-93e8-aa5c76c4ac7a))
    (fp_arc (start 1.27 2.48) (mid -1.021221 0.949055) (end -0.483625 -1.753625)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3a0673e8-088b-40f2-82ed-d0c9484808a2))
    (fp_arc (start 3.023625 -1.753625) (mid 3.561221 0.949055) (end 1.27 2.48)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 9b0e5dda-63fd-479c-8fc7-9daec74e0de5))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pinfunction "C") (pintype "passive") (tstamp 6989a07b-75bf-4a9a-9709-dcbc50688dde))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(D4-Pad1)") (pinfunction "B") (pintype "input") (tstamp e8e61631-b7f2-4574-8990-776e3062984c))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(Q3-Pad3)") (pinfunction "E") (pintype "passive") (tstamp ef17553f-2de3-4600-8aff-2c61b578e7c0))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Bourns_3386C_Horizontal" (layer "B.Cu")
    (tstamp b748d5d3-2e67-4a6d-bec1-4508bf5799eb)
    (at 126.6 51.94)
    (descr "Potentiometer, horizontal, Bourns 3386C, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer horizontal Bourns 3386C")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/f0f04dcf-5fb4-4b91-a4ed-6e36e8bde82f")
    (attr through_hole)
    (fp_text reference "RV4" (at 0 1.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2dab8563-610b-4d33-bccf-4e96581bc128)
    )
    (fp_text value "2K" (at 0 -6.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8d6f4950-d0a3-47ba-bbcf-028e27434a81)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 09d99ba3-c554-4494-aaa5-5418069c3db4)
    )
    (fp_line (start -2.535 -7.425) (end 2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dadde4b9-335d-46ea-a15d-414201856b71))
    (fp_line (start -2.535 2.345) (end -2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c531de9f-c500-40a9-ab53-014b2610ce04))
    (fp_line (start -2.535 2.345) (end 2.535 2.345)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 07c09e13-a41d-43c9-8efa-ffe05d188822))
    (fp_line (start 2.535 2.345) (end 2.535 -7.425)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 369af149-7e02-4e2b-b218-a8d9c352e171))
    (fp_line (start -2.67 -7.56) (end 2.67 -7.56)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 57906894-2247-4797-9903-02b5c1410b5a))
    (fp_line (start -2.67 2.48) (end -2.67 -7.56)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7f04ddad-f767-4bae-b1a3-c8b494051341))
    (fp_line (start 2.67 -7.56) (end 2.67 2.48)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 3790d0db-d1f2-4e70-b3f5-370084aacfea))
    (fp_line (start 2.67 2.48) (end -2.67 2.48)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e0b0a576-fdd8-40e5-8709-9ea8dbb0e10f))
    (fp_line (start -2.415 -7.305) (end -2.415 2.225)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c0cb1c7f-a978-44e9-9882-497d4816d306))
    (fp_line (start -2.415 2.225) (end 2.415 2.225)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6bed4d03-1e39-4ce8-8d73-66588f7b7598))
    (fp_line (start 2.415 -7.305) (end -2.415 -7.305)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1839b583-0b5b-48e4-988b-aea3e5c1789d))
    (fp_line (start 2.415 2.225) (end 2.415 -7.305)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 01929da4-fd8a-40d0-afa3-0d5aa8601a44))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(R7-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 9c4c68d8-b69e-42a2-ac8f-d39a5151d021))
    (pad "2" thru_hole circle (at 0 -2.54) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "2") (pintype "passive") (tstamp f1e87536-4f4f-4b0a-b497-32f9d03408d5))
    (pad "3" thru_hole circle (at 0 -5.08) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "3") (pintype "passive") (tstamp b183baea-fb23-489b-8015-20985283b4df))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386C_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT" (layer "B.Cu")
    (tstamp cb8881fa-74aa-4c3f-ae15-2adbbc417928)
    (at 139.6 78.15 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 9mm width 5.1mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/ef071772-c583-43e7-bdbd-e142e779fbb0")
    (attr through_hole)
    (fp_text reference "C5" (at 1.25 1.75) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2aaea98c-15b2-4f52-8d2d-287a003a4fb6)
    )
    (fp_text value "1nF*" (at 6.25 1.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b6e275ae-ccc2-4e73-ae8b-c40159f05b0f)
    )
    (fp_text user "${REFERENCE}" (at 1.25 1.75) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97c5b3bc-38b6-44f3-9467-a14b2032eb26)
    )
    (fp_line (start -0.87 -2.67) (end 8.37 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4c27b2f0-802c-4cf2-bf17-fe44481f587c))
    (fp_line (start -0.87 -0.665) (end -0.87 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bbfeaa62-03fe-4182-8c36-9183df1e1a43))
    (fp_line (start -0.87 2.67) (end -0.87 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2ae369b5-d5f0-4d0e-8f39-9c2484f22917))
    (fp_line (start -0.87 2.67) (end 8.37 2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 28b3a1f5-bb1a-479a-95c2-21676058b494))
    (fp_line (start 8.37 -0.665) (end 8.37 -2.67)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 04783a12-12a2-49ea-b616-e723d9a93a9a))
    (fp_line (start 8.37 2.67) (end 8.37 0.665)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8be57cf4-9cfe-4a54-a1aa-b2da83b790e2))
    (fp_line (start -1.05 -2.8) (end 8.55 -2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp ea013e53-8fe0-447d-891d-42f568f49adc))
    (fp_line (start -1.05 2.8) (end -1.05 -2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 860eade4-7b36-4271-b16d-fc7078e42042))
    (fp_line (start 8.55 -2.8) (end 8.55 2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 27439160-c314-4408-8425-8224eae52d32))
    (fp_line (start 8.55 2.8) (end -1.05 2.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp d49f6e3b-fc3e-46ee-a818-b8ab1dd98083))
    (fp_line (start -0.75 -2.55) (end 8.25 -2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 8fc73c7c-7c2c-4eb3-ac42-68008960e1e7))
    (fp_line (start -0.75 2.55) (end -0.75 -2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 36e809a7-27dc-4fa9-b2fa-a8c20a3083b4))
    (fp_line (start 8.25 -2.55) (end 8.25 2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f3fadeb5-fb54-4958-b34b-3d45b7242e3d))
    (fp_line (start 8.25 2.55) (end -0.75 2.55)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4e2ee77f-de3b-4e2b-8ce7-b05f019266c1))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C5-Pad1)") (pintype "passive") (tstamp 7a02c210-92b5-4a3b-add7-90d376a5cfc0))
    (pad "2" thru_hole circle (at 7.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 36e06866-3936-4adb-894b-1a3e0f436ea0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp cbe4eb0f-7ca7-4cc1-82a6-a5e80b2fe237)
    (at 125.6 65.98 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/201f0370-ce38-4e7f-9e38-2b5d7d0ef2b5")
    (attr through_hole)
    (fp_text reference "R7" (at 7.25 -0.5 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 48017262-2dd9-4727-b111-292d4d6f5de7)
    )
    (fp_text value "1K5" (at 3.5 0.25 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bd2edd3b-527f-4d2d-9abd-b42523758d04)
    )
    (fp_text user "${REFERENCE}" (at 7.25 -0.5 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4eb2ef0f-19f6-46ab-83de-9b2814fb3379)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 09cfcbdd-f7fd-41ee-8d20-2b3d5d6f6de2))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 10499e32-b886-454e-898b-57605f1d84eb))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 787180a8-cf12-4aaf-b77b-d312be20b4d8))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 56c5512f-5b6c-4b96-88f2-696486a01d76))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c5ba462e-1d40-4385-8040-ec0897abbf28))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bf674ddc-ce41-4487-9416-c770b7b009e2))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e9d54beb-23a1-4c40-b742-be63a2e3c806))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b3ff8174-40d2-4edd-b471-9b00dab171ae))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a63b6ef0-321f-4693-acad-c499f47254d7))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8c390589-ed7a-48ad-b62d-2d49538470a0))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 67cc5672-3c31-41b4-b0b6-0fb4c4a94df1))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 994f1a95-a5c5-4051-94ef-135d88a61307))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 26b41b0c-1b2f-4398-afae-8ebdd8099ed1))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c7d3287d-2efe-4a03-80d5-be2fc26110e8))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp c654e39d-0582-46cc-a233-c6e19f013414))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e76e67c7-0fee-4d82-b23f-41bc685b7ae5))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(Q1-Pad2)") (pintype "passive") (tstamp fd5ef6a2-a796-45e4-9265-75ae5db580e1))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(R7-Pad2)") (pintype "passive") (tstamp 99c466c4-9c4b-4719-a5ee-99a2831cca6a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4" (layer "B.Cu")
    (tstamp cf86ac48-14b9-40a5-85e3-7e80f35aa529)
    (at 187.35 132.15 180)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c66aeb6b-d8cb-46ee-820e-9aa05f1001bd")
    (attr through_hole)
    (fp_text reference "C13" (at 1.5 2) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b89575e0-9e13-427d-9a41-c0625ead5fe5)
    )
    (fp_text value "470nF" (at 7.5 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0c36e8d6-b12c-4b9e-b604-ae74f04c73fe)
    )
    (fp_text user "${REFERENCE}" (at 1.5 2) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f42d9cc-94c5-4adf-80cd-8b1c98c35dc0)
    )
    (fp_line (start -1.62 -3.12) (end 11.62 -3.12)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5a47ccdd-44bf-408f-baae-11a3cc4084e2))
    (fp_line (start -1.62 3.12) (end -1.62 -3.12)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4f2102c3-3bb7-4a4b-801c-4d259f5c3627))
    (fp_line (start -1.62 3.12) (end 11.62 3.12)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 91feb1a5-88bd-43a3-b354-3cd3fb1e02f4))
    (fp_line (start 11.62 3.12) (end 11.62 -3.12)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 497c8f14-6bdb-4f12-bb0c-48644623ac69))
    (fp_line (start -1.75 -3.25) (end 11.75 -3.25)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 445128b6-1fc2-408f-9fd7-69d71d160529))
    (fp_line (start -1.75 3.25) (end -1.75 -3.25)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4af3b9fa-b41e-42e9-ad66-52d5275e1171))
    (fp_line (start 11.75 -3.25) (end 11.75 3.25)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp e1b280d6-9b2c-4d71-8811-a2506bfe2002))
    (fp_line (start 11.75 3.25) (end -1.75 3.25)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 836c4cf1-df84-4010-a114-26a1e304849b))
    (fp_line (start -1.5 -3) (end 11.5 -3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5602407d-b390-444a-8b49-c595a034eff9))
    (fp_line (start -1.5 3) (end -1.5 -3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp bd7d7647-efc3-459b-8932-0055eb62d9d9))
    (fp_line (start 11.5 -3) (end 11.5 3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp d8a5da18-2fbe-4051-9b21-dde8622340d2))
    (fp_line (start 11.5 3) (end -1.5 3)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 88ed374c-dc47-4587-a50d-f0db47266bfd))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C13-Pad1)") (pintype "passive") (tstamp e5183fb7-24ab-4dec-99ae-d0c3a66f2535))
    (pad "2" thru_hole circle (at 10 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C13-Pad2)") (pintype "passive") (tstamp 911d324d-9425-41e3-9c04-ac5b8fcdd938))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (tstamp da6a2420-d799-4ddc-a8be-e105445f4e47)
    (at 168.65 49.144888 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/c648a4d9-afc0-4ace-a0ed-4c5ac558a8b2")
    (attr through_hole)
    (fp_text reference "C8" (at 3.455112 -3.05 180) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e6c001af-82d9-4ae0-9d1e-fecfe362e9ee)
    )
    (fp_text value "47uF" (at 1.25 -3.75 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ee9a4b1d-bc4a-4694-a8fe-98fd6355b1c6)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5acbabf-8a1b-41ff-8a57-430b0866e685)
    )
    (fp_line (start -1.554775 1.475) (end -1.054775 1.475)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d8b82d0c-5f1e-4d5c-982d-0aef6f2a387f))
    (fp_line (start -1.304775 1.725) (end -1.304775 1.225)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5f9b89f3-f84c-42b9-bacd-f988102cf68e))
    (fp_line (start 1.25 2.58) (end 1.25 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 28b2d35c-f656-49b6-8430-f787fc0b9c08))
    (fp_line (start 1.29 2.58) (end 1.29 -2.58)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0e47a824-c3de-4848-8ba6-abd0f55db199))
    (fp_line (start 1.33 2.579) (end 1.33 -2.579)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 37a30ea3-75a4-49d3-bda6-6e8733aee1ce))
    (fp_line (start 1.37 2.578) (end 1.37 -2.578)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp deb9a048-7dd4-4633-a8c0-c35ff7a2eb96))
    (fp_line (start 1.41 2.576) (end 1.41 -2.576)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6398f7c7-bf76-4eb1-97a6-6db9f081c13b))
    (fp_line (start 1.45 2.573) (end 1.45 -2.573)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 64961151-9697-40a9-81f5-5d72d7814a40))
    (fp_line (start 1.49 -1.04) (end 1.49 -2.569)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f010f725-e541-42c1-b951-a71cf0e94dd9))
    (fp_line (start 1.49 2.569) (end 1.49 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 79f1d7c5-d59f-4e72-8252-2396f10fbdad))
    (fp_line (start 1.53 -1.04) (end 1.53 -2.565)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 24b3e20f-f8fa-4b4e-8784-d65be9d992df))
    (fp_line (start 1.53 2.565) (end 1.53 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a093bd6d-1e0a-49ce-9c25-a3ad77ddd38e))
    (fp_line (start 1.57 -1.04) (end 1.57 -2.561)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2691bab6-ca4a-43d5-a994-209289532d12))
    (fp_line (start 1.57 2.561) (end 1.57 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d6445e96-63ff-4a64-8f75-0add509a6554))
    (fp_line (start 1.61 -1.04) (end 1.61 -2.556)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d64c9b1d-8e02-4a8b-85dd-cc224813c45d))
    (fp_line (start 1.61 2.556) (end 1.61 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c2aa15e8-ebd7-4199-a898-e45cd9ebcf49))
    (fp_line (start 1.65 -1.04) (end 1.65 -2.55)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ab05ef3d-6936-4e3c-95d3-4a1f7afa45bd))
    (fp_line (start 1.65 2.55) (end 1.65 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23ef3d65-d216-44ee-8cef-4c911d2e3b94))
    (fp_line (start 1.69 -1.04) (end 1.69 -2.543)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d8990c80-c64f-44df-b454-91d6e42ba4f1))
    (fp_line (start 1.69 2.543) (end 1.69 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ba94d136-1b3f-4469-bfb1-d3782025f4aa))
    (fp_line (start 1.73 -1.04) (end 1.73 -2.536)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a167a4b1-fe04-4877-80ad-879975ef8c99))
    (fp_line (start 1.73 2.536) (end 1.73 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b7accdb9-2199-41e0-b6c0-48b1731c8d47))
    (fp_line (start 1.77 -1.04) (end 1.77 -2.528)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 99ed89c2-d5be-4a1a-9195-4a233a7a7365))
    (fp_line (start 1.77 2.528) (end 1.77 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 137e7c59-a536-479d-a331-ba36ab7b562b))
    (fp_line (start 1.81 -1.04) (end 1.81 -2.52)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e1d7b38d-e7c7-4a05-9d4b-a85252132699))
    (fp_line (start 1.81 2.52) (end 1.81 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c6a64637-1be7-4216-ba52-22e74e69e17d))
    (fp_line (start 1.85 -1.04) (end 1.85 -2.511)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 22dc5a79-24f8-4fb3-8af2-437fb13b3f46))
    (fp_line (start 1.85 2.511) (end 1.85 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 23ecdff0-830e-4292-9658-245f525b39a0))
    (fp_line (start 1.89 -1.04) (end 1.89 -2.501)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 443323d3-681e-42aa-aecc-8d4199eb3191))
    (fp_line (start 1.89 2.501) (end 1.89 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 356a6a10-fef3-435e-982c-8a944a5e2790))
    (fp_line (start 1.93 -1.04) (end 1.93 -2.491)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bb8e86e9-a1bb-4796-8237-a4bd1cb1488b))
    (fp_line (start 1.93 2.491) (end 1.93 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e201b4f9-051c-4c12-84e3-e9124b07f00f))
    (fp_line (start 1.971 -1.04) (end 1.971 -2.48)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f4c89871-4c3a-406e-b4b9-49600e3b8dbd))
    (fp_line (start 1.971 2.48) (end 1.971 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6426512a-70c1-431a-99b4-3ec688a57e5d))
    (fp_line (start 2.011 -1.04) (end 2.011 -2.468)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a82140aa-c794-44a2-8a36-042c521808c6))
    (fp_line (start 2.011 2.468) (end 2.011 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8b6ed163-c3ca-41bf-8aa7-f24481ec2bb0))
    (fp_line (start 2.051 -1.04) (end 2.051 -2.455)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c59040e9-fe4d-47ac-9b06-05cfc31068dc))
    (fp_line (start 2.051 2.455) (end 2.051 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d3892a16-50de-45be-922a-54b933383c6d))
    (fp_line (start 2.091 -1.04) (end 2.091 -2.442)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 437f0507-d909-49d7-9c60-00ccee26edea))
    (fp_line (start 2.091 2.442) (end 2.091 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f97eb1fe-6d23-4e20-bcfc-350ab0c37e42))
    (fp_line (start 2.131 -1.04) (end 2.131 -2.428)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4a41fbdb-1e1d-4a8d-8e2f-fea089dc7645))
    (fp_line (start 2.131 2.428) (end 2.131 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 956ff5f3-5847-40b1-b1c5-2c5374bf3a5e))
    (fp_line (start 2.171 -1.04) (end 2.171 -2.414)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1b8b4d7d-79a0-406c-a72c-31d04d8a6e95))
    (fp_line (start 2.171 2.414) (end 2.171 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0f6d82d7-a962-45f1-aee0-e85e5b01dedd))
    (fp_line (start 2.211 -1.04) (end 2.211 -2.398)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e90fc102-2676-49ef-9425-43aac391cc9b))
    (fp_line (start 2.211 2.398) (end 2.211 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1bdaf636-4759-43d6-8f83-f273b2c67b56))
    (fp_line (start 2.251 -1.04) (end 2.251 -2.382)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8f583284-8c7f-43fc-9df0-9c31bac19b95))
    (fp_line (start 2.251 2.382) (end 2.251 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ba17c44d-254a-4874-8c0f-1bc27ba944b1))
    (fp_line (start 2.291 -1.04) (end 2.291 -2.365)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4676c3bb-9162-48c6-96a6-d1f629c011da))
    (fp_line (start 2.291 2.365) (end 2.291 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f1785cf1-374b-44c0-9215-f936585a5eab))
    (fp_line (start 2.331 -1.04) (end 2.331 -2.348)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b526dc9a-76fb-4f5f-9a11-dd339c83d259))
    (fp_line (start 2.331 2.348) (end 2.331 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f2684fc4-91ed-45a7-abce-f0f8ccfcc7b5))
    (fp_line (start 2.371 -1.04) (end 2.371 -2.329)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5cac17d3-f251-4c09-8928-674b65308806))
    (fp_line (start 2.371 2.329) (end 2.371 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 904bd7be-66d0-4ec1-acea-250620dee310))
    (fp_line (start 2.411 -1.04) (end 2.411 -2.31)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2291c833-3ee7-4419-aec7-406fbbd609b0))
    (fp_line (start 2.411 2.31) (end 2.411 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b9ca12e8-8791-4deb-9110-a7fb732a6834))
    (fp_line (start 2.451 -1.04) (end 2.451 -2.29)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f663c479-929b-4965-aeb2-10b7eb69ecdd))
    (fp_line (start 2.451 2.29) (end 2.451 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3e9d33cd-3705-48b5-a33b-5688c63cebda))
    (fp_line (start 2.491 -1.04) (end 2.491 -2.268)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp de985688-4e75-4a50-a760-8a0f829849b4))
    (fp_line (start 2.491 2.268) (end 2.491 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5999f4ec-48f4-48a2-af96-d2d1514eeca7))
    (fp_line (start 2.531 -1.04) (end 2.531 -2.247)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f056e093-735d-4598-8219-6b2de64f3412))
    (fp_line (start 2.531 2.247) (end 2.531 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 402a47ef-a541-4e00-993f-7bb84f5131b6))
    (fp_line (start 2.571 -1.04) (end 2.571 -2.224)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3371d39d-9505-4877-8199-1a03d3842891))
    (fp_line (start 2.571 2.224) (end 2.571 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c811816e-0219-407a-b342-1c05836c8961))
    (fp_line (start 2.611 -1.04) (end 2.611 -2.2)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp c70e9eb1-506a-49f9-a62d-d9568f059c0c))
    (fp_line (start 2.611 2.2) (end 2.611 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0f7cba37-cb06-4c4d-bfaa-491c6a09ba33))
    (fp_line (start 2.651 -1.04) (end 2.651 -2.175)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 54e3d04a-9ecc-4599-850e-c781825b7878))
    (fp_line (start 2.651 2.175) (end 2.651 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6bab1744-cea4-4a50-abbb-61a226013f7b))
    (fp_line (start 2.691 -1.04) (end 2.691 -2.149)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2000d49c-c1d6-44f5-a2c2-24dc26215227))
    (fp_line (start 2.691 2.149) (end 2.691 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 108c0713-df8a-42ed-b21a-51d780eba7e7))
    (fp_line (start 2.731 -1.04) (end 2.731 -2.122)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ca0ab72f-945a-414d-83be-7ad16af46593))
    (fp_line (start 2.731 2.122) (end 2.731 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 816eb129-55d2-4314-a01a-6899293e989d))
    (fp_line (start 2.771 -1.04) (end 2.771 -2.095)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4473020f-faa8-41d8-9182-246619db4ab6))
    (fp_line (start 2.771 2.095) (end 2.771 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bb0c7921-0d09-4525-b0e7-e967d410a46e))
    (fp_line (start 2.811 -1.04) (end 2.811 -2.065)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7b81bb7c-3016-413d-ac96-b9d48363a952))
    (fp_line (start 2.811 2.065) (end 2.811 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f092ed07-4c58-4302-9de5-2ce76f63b326))
    (fp_line (start 2.851 -1.04) (end 2.851 -2.035)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9dfb8884-bbdb-4ebd-b579-7a7affd85a52))
    (fp_line (start 2.851 2.035) (end 2.851 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 12c84e7b-14f8-475a-87df-6d09468233cf))
    (fp_line (start 2.891 -1.04) (end 2.891 -2.004)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7671ed16-728e-4d92-a2e6-59dfd998a7eb))
    (fp_line (start 2.891 2.004) (end 2.891 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1e2cdfc6-7dc2-426b-bb09-154d8c93118c))
    (fp_line (start 2.931 -1.04) (end 2.931 -1.971)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8e380384-26a8-46e0-a5c5-df41672d6836))
    (fp_line (start 2.931 1.971) (end 2.931 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a6edaaab-a7d8-41d9-bb17-e82e7aa8992c))
    (fp_line (start 2.971 -1.04) (end 2.971 -1.937)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1aa915a8-d723-450a-9b03-f21efd16000e))
    (fp_line (start 2.971 1.937) (end 2.971 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ac395c4d-abcb-4d9b-9dcf-49bc048bf54c))
    (fp_line (start 3.011 -1.04) (end 3.011 -1.901)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp be494c29-2dff-4404-85bd-290b0986304e))
    (fp_line (start 3.011 1.901) (end 3.011 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a7ce35df-1ffa-405a-affe-45c8490bbfa7))
    (fp_line (start 3.051 -1.04) (end 3.051 -1.864)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp dca2e1ac-d233-4cad-aefc-a7afd0ce50c3))
    (fp_line (start 3.051 1.864) (end 3.051 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b8c51922-cc75-4008-8a1d-9f60ca1c06cf))
    (fp_line (start 3.091 -1.04) (end 3.091 -1.826)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 66e485fb-cd71-4a94-aa48-cb08fd8c5cf0))
    (fp_line (start 3.091 1.826) (end 3.091 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp aca915d2-e9a1-43a3-a3db-335feb1dcacd))
    (fp_line (start 3.131 -1.04) (end 3.131 -1.785)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4ce71d71-c595-4e77-94c5-1863a5bba7be))
    (fp_line (start 3.131 1.785) (end 3.131 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9e243228-1909-461f-ba02-27e95f34378a))
    (fp_line (start 3.171 -1.04) (end 3.171 -1.743)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0317606f-d1cd-4fa3-8651-e631d6a5714e))
    (fp_line (start 3.171 1.743) (end 3.171 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0ec99e0b-a596-43f4-9771-2543da9a0539))
    (fp_line (start 3.211 -1.04) (end 3.211 -1.699)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 310abef1-5c77-45a3-81f6-d52f8cdaa36d))
    (fp_line (start 3.211 1.699) (end 3.211 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 77722a5b-98cb-46b0-acf2-9f43ba4e0e7a))
    (fp_line (start 3.251 -1.04) (end 3.251 -1.653)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6782dcfb-5bc6-410f-9943-125d10022eae))
    (fp_line (start 3.251 1.653) (end 3.251 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 03b93500-5164-4326-8268-3d2a5031b8a0))
    (fp_line (start 3.291 -1.04) (end 3.291 -1.605)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ada47bdb-d332-4b54-bb41-da89e3b1264c))
    (fp_line (start 3.291 1.605) (end 3.291 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9ec68965-adb4-4fdb-aaf1-68b552b9f74a))
    (fp_line (start 3.331 -1.04) (end 3.331 -1.554)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp fd63af15-7c7d-4b69-a070-c8ea1a7388e9))
    (fp_line (start 3.331 1.554) (end 3.331 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ac26b4f1-eefe-4991-a7bc-508d36810a3a))
    (fp_line (start 3.371 -1.04) (end 3.371 -1.5)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cc1b5871-d929-4402-9d5a-f1a4de30ffaa))
    (fp_line (start 3.371 1.5) (end 3.371 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 94583a16-42db-427a-9487-29a7b2640d08))
    (fp_line (start 3.411 -1.04) (end 3.411 -1.443)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9170e509-e6fd-4eab-9558-7ac5f2d83094))
    (fp_line (start 3.411 1.443) (end 3.411 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp d2fe6ea8-beaa-40a4-a5b7-667ba24b6f31))
    (fp_line (start 3.451 -1.04) (end 3.451 -1.383)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 085bf28d-90ff-4ce1-99cd-8fd9eebefe8c))
    (fp_line (start 3.451 1.383) (end 3.451 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 14553f6f-e946-4efc-8743-3c2afd6ec95e))
    (fp_line (start 3.491 -1.04) (end 3.491 -1.319)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 64af88ad-7a39-4b1e-a904-c098e5b8ce0d))
    (fp_line (start 3.491 1.319) (end 3.491 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 62a0c8e3-d382-4d89-8302-120e0ed433a2))
    (fp_line (start 3.531 -1.04) (end 3.531 -1.251)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 4d5d8594-8e84-4ef4-8f52-e1df6b7a2555))
    (fp_line (start 3.531 1.251) (end 3.531 1.04)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 10d37415-1c65-45e6-bf1a-564d7ebdb0c6))
    (fp_line (start 3.571 1.178) (end 3.571 -1.178)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 71f5442a-1a9b-482d-bd94-1cec13edbafd))
    (fp_line (start 3.611 1.098) (end 3.611 -1.098)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 3d3dd634-1f47-4d7d-b6a9-9b0201ee998b))
    (fp_line (start 3.651 1.011) (end 3.651 -1.011)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bf1c424d-5b93-4616-8c81-e6e9ba14a101))
    (fp_line (start 3.691 0.915) (end 3.691 -0.915)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ca688b9e-6173-4e39-bb00-8dd9320164cb))
    (fp_line (start 3.731 0.805) (end 3.731 -0.805)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bd33a15c-a1e6-43b4-a54a-0f3034b27729))
    (fp_line (start 3.771 0.677) (end 3.771 -0.677)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 7b36d442-8fdd-4de2-b04b-e410bf22694c))
    (fp_line (start 3.811 0.518) (end 3.811 -0.518)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 88036e61-b654-4dc3-bd02-417f9b017374))
    (fp_line (start 3.851 0.284) (end 3.851 -0.284)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp bc00976b-c0eb-4457-bf4a-9fb24157f525))
    (fp_circle (center 1.25 0) (end 3.87 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "B.SilkS") (tstamp 5bbfd822-8af9-4bce-a8eb-4be2e245eb56))
    (fp_circle (center 1.25 0) (end 4 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "B.CrtYd") (tstamp 8ee54246-eb33-4e19-84db-0482290d48f4))
    (fp_line (start -0.883605 1.0875) (end -0.383605 1.0875)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 21140d5b-4a64-41fb-89df-af11d2316c68))
    (fp_line (start -0.633605 1.3375) (end -0.633605 0.8375)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dbd1cef5-8f45-4c79-bbc0-94e3af0859db))
    (fp_circle (center 1.25 0) (end 3.75 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "B.Fab") (tstamp 665da681-efdb-4747-b4b0-366fadd98660))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp 49ea62f3-bfb4-4af8-a888-e3493cc70cf8))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 3ae3a194-1b2f-469c-87e9-78fa6bb70d51))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4" (layer "B.Cu")
    (tstamp e03fc1f0-ed16-408d-9a2a-36c8e24290f9)
    (at 168.7 55.15 -90)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/19f04210-d881-47d2-a78a-019985ff0681")
    (attr through_hole)
    (fp_text reference "C6" (at 3.75 0 90) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 29737c18-6cea-4b02-ab5a-f3d0a074dffa)
    )
    (fp_text value ".1uF" (at 3.75 -1.75 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8c82d9bb-cc2a-4e46-8607-4e5bd168c276)
    )
    (fp_text user "${REFERENCE}" (at 3.75 0 90) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f12bd55e-ca0d-4a6e-8145-041b02a92297)
    )
    (fp_line (start -1.52 -2.62) (end 9.02 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 6cd05ecd-f478-457c-bc19-f57e38dc73da))
    (fp_line (start -1.52 2.62) (end -1.52 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2a1e169a-3d99-4083-82b4-49af8085bc58))
    (fp_line (start -1.52 2.62) (end 9.02 2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 344baffe-faad-4c3b-aa34-201dc9416e59))
    (fp_line (start 9.02 2.62) (end 9.02 -2.62)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b72e4489-3e2c-467e-90fa-1d31dfd2b001))
    (fp_line (start -1.66 -2.75) (end 9.15 -2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4ad27710-1c9b-40ec-bfdf-76b07a0696ae))
    (fp_line (start -1.66 2.75) (end -1.66 -2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 50f60447-393c-4bf4-80b0-b4c346eea5a8))
    (fp_line (start 9.15 -2.75) (end 9.15 2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp fb3f414f-e3d4-4152-b7de-84f76085dccf))
    (fp_line (start 9.15 2.75) (end -1.66 2.75)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b228c05e-e4d3-4e25-a349-8af6be345475))
    (fp_line (start -1.4 -2.5) (end 8.9 -2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 93d8ce6a-083a-48de-b79f-d24c08be1821))
    (fp_line (start -1.4 2.5) (end -1.4 -2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 3ba3c7d6-7362-4e10-a917-ca3b9115362b))
    (fp_line (start 8.9 -2.5) (end 8.9 2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e724bae5-5467-44be-a16a-ec46b5f84850))
    (fp_line (start 8.9 2.5) (end -1.4 2.5)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 19e0a47f-9747-4f2a-951c-649921ea2d7a))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp 8f4818ce-d542-4eca-b757-3e5958f5a265))
    (pad "2" thru_hole circle (at 7.5 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp da51c726-9b43-48f1-b389-6d11bb6f0157))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "B.Cu")
    (tstamp e35fb82d-237a-416c-af78-c8d27d2c5466)
    (at 153.1 85.4)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/42095387-7b5f-4fc7-b561-de75877450ec")
    (attr through_hole)
    (fp_text reference "C1" (at 3 -2.25) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d1a36d4e-1336-4b9e-9d24-5221fda9fed0)
    )
    (fp_text value ".1uF" (at 0.5 -2.25) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bef12426-7f64-419b-ba96-0eed81459558)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3393d3cc-aab1-4a53-b97d-17f44ae57a0a)
    )
    (fp_line (start -1.37 -1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b477f6d1-2370-42f5-b41c-3f1f1e17dcda))
    (fp_line (start -1.37 1.37) (end -1.37 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5150c384-3ecf-428f-8579-9bdfa916656d))
    (fp_line (start -1.37 1.37) (end 3.87 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 41a0362a-7d82-4e40-9779-083cd2215a73))
    (fp_line (start 3.87 1.37) (end 3.87 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp e3a0066f-8d46-432f-95b1-cb05dfa4ac9e))
    (fp_line (start -1.5 -1.5) (end 4 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp c474b706-6b9c-43b0-84be-a71538773f02))
    (fp_line (start -1.5 1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp fab872d8-f573-4bc5-bdf8-8875465c37f1))
    (fp_line (start 4 -1.5) (end 4 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 34b14672-4a04-4ef8-bd86-ceff661777d1))
    (fp_line (start 4 1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7f298787-03a9-4505-8690-b3ee9f41ccc0))
    (fp_line (start -1.25 -1.25) (end 3.75 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp fbae6317-4e30-48fb-823d-d50a03a0a458))
    (fp_line (start -1.25 1.25) (end -1.25 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 7a3a9fa9-cc4b-417f-b4fc-4e3b949d4dbf))
    (fp_line (start 3.75 -1.25) (end 3.75 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e420e003-e988-4724-b2d3-9fc7dbbceffd))
    (fp_line (start 3.75 1.25) (end -1.25 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 92e82ce3-234c-4f68-a964-222250971aad))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp f06b0008-eeff-4f00-83dc-e6f5434c8916))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive") (tstamp 9ed4851a-5373-4702-a804-cb865b7e91f8))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "B.Cu")
    (tstamp e3eba64f-81b1-463c-8178-99cffec742b5)
    (at 174.35 119.025 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/9e42bf79-6e11-43d7-8ea0-a63aae613bac")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 2.33) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4a6f1692-1ddf-40e4-b9cc-01a663e20c73)
    )
    (fp_text value "TL074" (at 3.81 -17.57) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a4ff7a79-5c30-42ca-afa4-3a605b20c759)
    )
    (fp_text user "${REFERENCE}" (at 3.81 -7.62) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d4101173-f58b-43a9-b357-55cb1dc024d7)
    )
    (fp_line (start 1.16 -16.57) (end 6.46 -16.57)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 0bbcc89b-b3fb-4d24-b32b-37af676da5b0))
    (fp_line (start 1.16 1.33) (end 1.16 -16.57)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2fc80725-e318-4234-8c73-68a0b4223bc4))
    (fp_line (start 2.81 1.33) (end 1.16 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp a565bcc5-481f-4ab7-9b71-8e6240b46181))
    (fp_line (start 6.46 -16.57) (end 6.46 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f9d2e919-05ec-47ec-ae11-7925931ba4d0))
    (fp_line (start 6.46 1.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 1fe1e1c2-7561-46dc-b07e-96d5b0e990ed))
    (fp_arc (start 2.81 1.33) (mid 3.81 0.33) (end 4.81 1.33)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 5d09f412-62b5-4a7b-a780-77beb74e031d))
    (fp_line (start -1.1 -16.8) (end 8.7 -16.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 73869f95-77c1-48c0-bcb1-c3c1838eee09))
    (fp_line (start -1.1 1.55) (end -1.1 -16.8)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4b8db025-3b9c-4bfd-aaf7-05697f7ee58a))
    (fp_line (start 8.7 -16.8) (end 8.7 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 008f6b1a-aaa8-42b3-9e30-3fa8abbd3255))
    (fp_line (start 8.7 1.55) (end -1.1 1.55)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp a2a4f1b2-966a-4028-ad0c-beca2fe4d14f))
    (fp_line (start 0.635 -16.51) (end 0.635 0.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 322ae608-6dc0-4d3e-8f9d-7c369c80eb3a))
    (fp_line (start 0.635 0.27) (end 1.635 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e16491bc-306f-4fe6-a7fa-e558f2e57214))
    (fp_line (start 1.635 1.27) (end 6.985 1.27)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 5eb6f1ab-4cc2-4cb5-81f2-9ec5c78419ef))
    (fp_line (start 6.985 -16.51) (end 0.635 -16.51)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f6502afd-9fbf-4fed-95f1-06c2649de341))
    (fp_line (start 6.985 1.27) (end 6.985 -16.51)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp dd329ecc-4355-453f-ba7b-56c1878035cc))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(R33-Pad2)") (pintype "output") (tstamp 38faaa1c-ff5a-45ca-a789-de8b3dbddf9e))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(R33-Pad2)") (pinfunction "-") (pintype "input") (tstamp 75288178-aea8-4ff6-ad4e-9f03d52768ca))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(R27-Pad2)") (pinfunction "+") (pintype "input") (tstamp 3910cdf7-6fd4-43c0-8946-02577a571e2d))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in") (tstamp 1e1f52b6-e0ae-4860-a107-7adbc7aa1ef7))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C13-Pad2)") (pinfunction "+") (pintype "input") (tstamp 6b49c192-98a3-49c3-97af-ebc159e7a488))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R29-Pad1)") (pinfunction "-") (pintype "input") (tstamp 4dbba241-0a2e-4dc2-9619-52a08227cb1a))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(R31-Pad1)") (pintype "output") (tstamp 77c9c415-c6a9-469b-b7b3-05ac4a5d9487))
    (pad "8" thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D2-Pad2)") (pintype "output") (tstamp 4b13ddb9-f68f-49d1-bc2b-bb4a14c4eeb9))
    (pad "9" thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D2-Pad2)") (pinfunction "-") (pintype "input") (tstamp 378c9ac9-eee6-4062-baeb-2db0786b3a1a))
    (pad "10" thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C11-Pad2)") (pinfunction "+") (pintype "input") (tstamp 429cc7b8-0de7-4593-94ec-3d039bf668b5))
    (pad "11" thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in") (tstamp 976049d4-0f70-45e8-b30c-22e1667c8697))
    (pad "12" thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "+") (pintype "input") (tstamp dd80e559-7bb6-406a-9b3a-bbdfb5038545))
    (pad "13" thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C12-Pad1)") (pinfunction "-") (pintype "input") (tstamp 74dbb27b-f455-4526-bf0a-4cea3a366bfd))
    (pad "14" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C12-Pad2)") (pintype "output") (tstamp 5280c7f1-c88a-4474-8e0d-68df22926de9))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tstamp fe61447a-b5bf-4027-99ef-bdccd5174004)
    (at 169.68 107.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Fireball.kicad_sch")
    (property "Sheetname" "")
    (path "/66be33fa-335a-4444-9eb9-aa52ea4477de")
    (attr through_hole)
    (fp_text reference "R19" (at 3.33 0.5) (layer "B.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1ef0ef43-a82c-40e6-b905-e3ff500db175)
    )
    (fp_text value "100K" (at 6.33 -0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d1dbd6eb-ef43-4cfe-8799-33dfe3c90469)
    )
    (fp_text user "${REFERENCE}" (at 3.33 0.5) (layer "B.Fab")
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9b4a85bd-30aa-4a48-81b0-1a777df0aa86)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 8e1d7d87-41c5-4767-9787-62683f80fa1d))
    (fp_line (start 1.81 -1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 31638aa2-41e1-46b2-8287-b2d7afb19810))
    (fp_line (start 1.81 1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 22416ffb-0abc-4196-a84c-ca379efe8dac))
    (fp_line (start 8.35 -1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp cafa09a2-0076-4738-801f-d99992564b18))
    (fp_line (start 8.35 1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ac06b02a-09c7-4903-aa48-4d45ac508481))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b3563145-7a05-4c89-8d33-0c8e64076884))
    (fp_line (start -1.05 -1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4025eaeb-9b56-405d-a061-fc2cb58b34b7))
    (fp_line (start -1.05 1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 7a41cb39-49b8-4b11-834f-90a5c1afa8ef))
    (fp_line (start 11.21 -1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8e5b35d1-2365-4a19-9335-15de5723359d))
    (fp_line (start 11.21 1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp b001eda3-b67a-47e2-8ae2-6569dd2cdc15))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f460fcfc-614e-4bb3-99ee-ce7e5fa20d96))
    (fp_line (start 1.93 -1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1d95d0c0-624a-4224-a6dc-42e50f3b036a))
    (fp_line (start 1.93 1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 1ca6a77a-1994-474a-9d6f-f1e5cdd4821d))
    (fp_line (start 8.23 -1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b02469b4-771b-46c0-8a91-90bec930902d))
    (fp_line (start 8.23 1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 74c8d118-5f22-4678-80a4-a13d0abbd41d))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 04b2f2d1-b328-4b5a-9de4-e7cd7c5a17aa))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive") (tstamp 9497df61-29fe-4296-9eac-497867341b29))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(R19-Pad2)") (pintype "passive") (tstamp f901222b-ea96-4500-ab6b-33717e6847f4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 123.6 43.9) (end 193.6 143.9)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp e08301ac-3c6e-4659-8763-975d2b4cb450))
  (gr_text "JLCJLCJLCJLC" (at 192 71.7 90) (layer "B.SilkS") (tstamp 9f7076e8-7bde-4158-870e-9db1c07f924b)
    (effects (font (size 1 1) (thickness 0.15)) (justify left bottom mirror))
  )

  (segment (start 168.7 55.15) (end 170.025 56.475) (width 0.6) (layer "F.Cu") (net 1) (tstamp 08c03e40-94c6-49f1-8424-4e40feb91247))
  (segment (start 168.7 55.15) (end 166.6 53.05) (width 0.6) (layer "F.Cu") (net 1) (tstamp 17c200da-f7b4-46bd-a17c-a5ae3866889c))
  (segment (start 167.6 107.9) (end 161.85 102.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp 180be161-6a9e-44c6-947b-530d6d525f55))
  (segment (start 161.45779 61.4) (end 162.45 61.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp 2a674d0a-3e79-42c0-a3af-37f77a29b22f))
  (segment (start 161.45779 61.4) (end 158.35 61.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp 2b3310f4-7595-45b3-8c62-bb3444ea8d6a))
  (segment (start 151.855 86.495) (end 151.485 86.495) (width 0.6) (layer "F.Cu") (net 1) (tstamp 3319509f-cb6b-4e70-84d1-9100c487a83a))
  (segment (start 154.1 51.44221) (end 154.05779 51.44221) (width 0.6) (layer "F.Cu") (net 1) (tstamp 4164873d-bb71-4b32-b4ae-62334381082e))
  (segment (start 151.1 51.4) (end 154.01558 51.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp 48a50273-8379-46c3-a374-16bbd909b1da))
  (segment (start 176.845 126.645) (end 176.85 126.65) (width 0.6) (layer "F.Cu") (net 1) (tstamp 4f887ac7-071a-4dec-b3d2-688a6dd10a1c))
  (segment (start 151.68 101.48) (end 151.68 86.67) (width 0.6) (layer "F.Cu") (net 1) (tstamp 5165c4ba-522d-4045-aeb9-03191fb11dbb))
  (segment (start 170.025 56.475) (end 170.025 61.075) (width 0.6) (layer "F.Cu") (net 1) (tstamp 53ad6f0b-48d1-4f22-ab76-4a4da5714bf9))
  (segment (start 174.35 126.645) (end 176.845 126.645) (width 0.6) (layer "F.Cu") (net 1) (tstamp 5bfd3f51-1e86-4702-a60d-8e90f0f2b55c))
  (segment (start 149.93 51.4) (end 149.85 51.32) (width 0.6) (layer "F.Cu") (net 1) (tstamp 6740dae7-0a70-44d0-bd73-48699df88c52))
  (segment (start 152.35 102.15) (end 151.68 101.48) (width 0.4) (layer "F.Cu") (net 1) (tstamp 676c2e97-2b16-4ea6-a2fe-b09d4a8a23ee))
  (segment (start 157.5 54.84221) (end 154.1 51.44221) (width 0.6) (layer "F.Cu") (net 1) (tstamp 6ec0636d-7a15-44b3-a714-bf62753783dd))
  (segment (start 152.1 102.15) (end 151.76 102.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp 71792462-24af-4035-a907-782c2a259819))
  (segment (start 143.85 109.9) (end 143.85 111.78) (width 0.6) (layer "F.Cu") (net 1) (tstamp 72e23d80-63de-4662-b084-ddad15f686ab))
  (segment (start 151.837701 70.637701) (end 158.35 77.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp 7473a88c-f012-4f1c-8f7f-b1e9c2125e86))
  (segment (start 167.9 55.95) (end 168.7 55.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp 7530a08b-31c4-4c42-a8f9-436290d575df))
  (segment (start 170.025 61.075) (end 173.85 64.9) (width 0.6) (layer "F.Cu") (net 1) (tstamp 7e6ebea3-ebca-4d61-ab3f-ae12038f797f))
  (segment (start 151.68 102.07) (end 151.68 101.48) (width 0.6) (layer "F.Cu") (net 1) (tstamp 81d05f92-7142-456d-a3fa-827331d8fbf3))
  (segment (start 166.6 53.05) (end 166.6 51.194888) (width 0.6) (layer "F.Cu") (net 1) (tstamp 86a1d370-f0a7-4876-9149-a86f4690c96c))
  (segment (start 158.35 61.4) (end 157.5 61.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp 9f34545b-9160-4269-b2ea-1bf277165fb2))
  (segment (start 173.85 64.9) (end 175.85 64.9) (width 0.6) (layer "F.Cu") (net 1) (tstamp a05636ec-34d1-431d-ace6-d6da1ca2bc04))
  (segment (start 154.1 51.44221) (end 154.1 51.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp b2a32f1a-d2c9-4549-a9ad-6daa04a8f257))
  (segment (start 162.45 61.4) (end 167.9 55.95) (width 0.6) (layer "F.Cu") (net 1) (tstamp b3cd247d-8ab0-4618-a9f7-56ec7d37fba9))
  (segment (start 151.68 86.67) (end 151.855 86.495) (width 0.6) (layer "F.Cu") (net 1) (tstamp b63c10d5-956f-470c-89da-671358d31f24))
  (segment (start 151.485 86.495) (end 150.35 85.36) (width 0.6) (layer "F.Cu") (net 1) (tstamp b835d77e-6b52-459a-b45e-1ce79fb66dd7))
  (segment (start 152.005 86.495) (end 153.1 85.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp c6da55a9-b856-4a5e-ba24-b08fdc7476a6))
  (segment (start 157.5 60.55) (end 157.5 54.84221) (width 0.6) (layer "F.Cu") (net 1) (tstamp c8d7bc7c-6dca-4ed3-9e8e-89a0387058f7))
  (segment (start 143.85 111.78) (end 142.53 113.1) (width 0.6) (layer "F.Cu") (net 1) (tstamp c9bf883e-66cf-4ebc-9d5c-fd851ddc72d4))
  (segment (start 152.1 102.15) (end 152.35 102.15) (width 0.25) (layer "F.Cu") (net 1) (tstamp cc4d86ae-8bf9-4e64-bf97-a451ffd34612))
  (segment (start 157.5 60.55) (end 158.35 61.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp ccdaa719-2c9a-4b03-be99-967d98a6d72c))
  (segment (start 176.68 65.73) (end 176.68 68.9) (width 0.6) (layer "F.Cu") (net 1) (tstamp ced6e24d-72ba-4d48-ac78-7a5713429077))
  (segment (start 166.6 51.194888) (end 168.65 49.144888) (width 0.6) (layer "F.Cu") (net 1) (tstamp d1972185-e65f-41d6-bfb8-24267cd74959))
  (segment (start 151.855 86.495) (end 152.005 86.495) (width 0.6) (layer "F.Cu") (net 1) (tstamp d1fe57f2-8fe6-415a-b613-26a717ff78a9))
  (segment (start 150.02 51.15) (end 149.85 51.32) (width 0.6) (layer "F.Cu") (net 1) (tstamp db88b935-6adf-441b-ad01-5d569ff88ffa))
  (segment (start 154.01558 51.4) (end 154.05779 51.44221) (width 0.6) (layer "F.Cu") (net 1) (tstamp db8a0ade-037a-4711-9942-4b1b17cb291f))
  (segment (start 143.85 109.9) (end 151.68 102.07) (width 0.6) (layer "F.Cu") (net 1) (tstamp de6de016-f4bb-4948-a113-b6d258c69a8e))
  (segment (start 151.1 51.4) (end 149.93 51.4) (width 0.6) (layer "F.Cu") (net 1) (tstamp e1fa53d1-a603-4960-b7d0-a877b92e2e4a))
  (segment (start 151.76 102.15) (end 151.68 102.07) (width 0.25) (layer "F.Cu") (net 1) (tstamp e6a55229-b3a1-47ae-a423-106ebac07514))
  (segment (start 161.85 102.15) (end 152.1 102.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp eef4de2a-0c05-4bff-a23d-dadfcdfc7fc5))
  (segment (start 175.85 64.9) (end 176.68 65.73) (width 0.6) (layer "F.Cu") (net 1) (tstamp f1268508-a64f-4623-8355-58ed8ea19403))
  (segment (start 169.68 107.9) (end 167.6 107.9) (width 0.6) (layer "F.Cu") (net 1) (tstamp f1f9890b-10b1-4da7-bcbc-5d353d4c1d53))
  (segment (start 157.5 61.4) (end 157.5 60.55) (width 0.6) (layer "F.Cu") (net 1) (tstamp f3c964af-888b-4903-ae10-0a16675ae3d6))
  (segment (start 157.5 61.4) (end 156.1 62.8) (width 0.6) (layer "F.Cu") (net 1) (tstamp f5fe29fb-a803-4313-95a6-6bc62ac8dce0))
  (segment (start 150.02 45.9) (end 150.02 51.15) (width 0.6) (layer "F.Cu") (net 1) (tstamp f906ecfa-a787-4746-97ea-116f6c06005a))
  (via (at 158.35 77.15) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 1) (tstamp 195ff72b-2ba2-4e46-8e37-fdc601d5e0ff))
  (via (at 151.837701 70.637701) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 1) (tstamp d83e97c9-ce29-4dfb-8fd2-1f91993506b7))
  (segment (start 171.1 114.11) (end 171.1 123.4) (width 0.6) (layer "B.Cu") (net 1) (tstamp 33fb6cab-07f6-4a3e-b3ab-07a42de9ebd5))
  (segment (start 151.837701 68.912299) (end 156.1 64.65) (width 0.6) (layer "B.Cu") (net 1) (tstamp 349c2d55-3739-416e-973c-539a582209b3))
  (segment (start 169.68 112.69) (end 171.1 114.11) (width 0.6) (layer "B.Cu") (net 1) (tstamp 573557f6-f4ea-404d-9caa-688e24ca0982))
  (segment (start 156.1 64.65) (end 156.1 62.8) (width 0.6) (layer "B.Cu") (net 1) (tstamp 64fc3a60-ed81-4507-9f59-4cc83c627bba))
  (segment (start 153.1 85.4) (end 153.1 83.9) (width 0.6) (layer "B.Cu") (net 1) (tstamp 7c9b7ec5-85a0-4fa6-9ffa-60afb3e0bce3))
  (segment (start 169.68 107.9) (end 169.68 112.69) (width 0.6) (layer "B.Cu") (net 1) (tstamp 901b6cfd-2102-47af-9df5-50d23d762158))
  (segment (start 174.345 126.645) (end 174.35 126.645) (width 0.6) (layer "B.Cu") (net 1) (tstamp aaad1f1f-6a57-43c1-8dba-f20c55e0d2b8))
  (segment (start 151.837701 70.637701) (end 151.837701 68.912299) (width 0.6) (layer "B.Cu") (net 1) (tstamp c39dbfd2-83a8-4e62-a0d2-50af9e81dd4c))
  (segment (start 153.1 83.9) (end 158.35 78.65) (width 0.6) (layer "B.Cu") (net 1) (tstamp d71bb67b-45fa-4a2a-9ceb-4a5265cbedd6))
  (segment (start 171.1 123.4) (end 174.345 126.645) (width 0.6) (layer "B.Cu") (net 1) (tstamp e8e78193-db5d-4fb9-80ae-8b11720773a4))
  (segment (start 158.35 78.65) (end 158.35 77.15) (width 0.6) (layer "B.Cu") (net 1) (tstamp f026d778-d4fe-4e49-86a4-bed13a5470fe))
  (segment (start 136.05 111.42) (end 136.05 114.52) (width 0.25) (layer "F.Cu") (net 2) (tstamp aff22eae-c55e-493a-97a3-31233f73769c))
  (segment (start 176.68 72.15) (end 176.015 72.815) (width 0.6) (layer "F.Cu") (net 3) (tstamp 04101a17-63e6-41f8-a8cb-e4a2c4814946))
  (segment (start 150.15 120.72) (end 155.18 120.72) (width 0.6) (layer "F.Cu") (net 3) (tstamp 0bd5629b-00d1-4f87-8bcd-a778f063797a))
  (segment (start 175.1 85.07) (end 175.1 82.65) (width 0.6) (layer "F.Cu") (net 3) (tstamp 0d3f4b11-2b70-4d35-bc5b-f3f4fd1643d7))
  (segment (start 179.8 77.95) (end 179.8 76.13) (width 0.6) (layer "F.Cu") (net 3) (tstamp 10b8cd52-0c6a-45e4-ac5f-03ecb48ca74a))
  (segment (start 177.05 50.320449) (end 177.05 55.14) (width 0.6) (layer "F.Cu") (net 3) (tstamp 16040901-bb4c-4703-aad2-5b682103e58b))
  (segment (start 166.73 126.645) (end 165.595 126.645) (width 0.6) (layer "F.Cu") (net 3) (tstamp 17f60ab9-abbd-4302-b127-ac57ce3f00fb))
  (segment (start 164.95 100.9) (end 165.85 100) (width 0.6) (layer "F.Cu") (net 3) (tstamp 18e2b0c9-1779-45e3-a053-57528bca91a4))
  (segment (start 164.595 126.645) (end 165.595 126.645) (width 0.6) (layer "F.Cu") (net 3) (tstamp 1c2f8a50-8111-4e03-b8bc-db5877982071))
  (segment (start 146.6 127.15) (end 147.35 126.4) (width 0.6) (layer "F.Cu") (net 3) (tstamp 25b4058a-0ece-4df0-9271-09181c0f8393))
  (segment (start 177.034664 50.305113) (end 181.335113 50.305113) (width 0.6) (layer "F.Cu") (net 3) (tstamp 2c023324-6eda-4fa7-b2dc-3a5c488d16c7))
  (segment (start 140.09 85.36) (end 140.05 85.4) (width 0.25) (layer "F.Cu") (net 3) (tstamp 3e271698-94ac-4698-8370-ed21cd0658c6))
  (segment (start 156.3 119.6) (end 157 118.9) (width 0.6) (layer "F.Cu") (net 3) (tstamp 4120ae9f-4876-4322-813c-5277c62bbde0))
  (segment (start 175.1 82.65) (end 179.8 77.95) (width 0.6) (layer "F.Cu") (net 3) (tstamp 469be06c-af36-4e97-adbc-daf58076ab82))
  (segment (start 173.85 86.32) (end 175.1 85.07) (width 0.6) (layer "F.Cu") (net 3) (tstamp 48dd91cd-1a27-4a43-8d67-5f3613883b93))
  (segment (start 165.85 82.98) (end 165.85 86.15) (width 0.6) (layer "F.Cu") (net 3) (tstamp 532bed1b-2dc7-4a2e-a51e-f2f10988bb22))
  (segment (start 165.85 100) (end 165.85 86.15) (width 0.6) (layer "F.Cu") (net 3) (tstamp 5a11d960-add5-4bd3-8ea0-9caf519114bc))
  (segment (start 150.15 121.35) (end 150.15 120.72) (width 0.6) (layer "F.Cu") (net 3) (tstamp 5e3efe83-a2ce-413e-95f2-cda002ee0546))
  (segment (start 177.034664 50.305113) (end 177.05 50.320449) (width 0.6) (layer "F.Cu") (net 3) (tstamp 6245d704-d9eb-4848-bce2-437ae3771ae5))
  (segment (start 147.35 124.15) (end 150.15 121.35) (width 0.6) (layer "F.Cu") (net 3) (tstamp 64ef431d-98cc-4351-a507-4a09050f784f))
  (segment (start 144.69 127.15) (end 146.6 127.15) (width 0.6) (layer "F.Cu") (net 3) (tstamp 679fa549-9f5d-48ed-abce-0629f00f12b5))
  (segment (start 175.85 73.01) (end 176.68 73.01) (width 0.6) (layer "F.Cu") (net 3) (tstamp 7b2fc8b6-5508-41f3-997e-481e28a073be))
  (segment (start 147.35 126.4) (end 147.35 124.15) (width 0.6) (layer "F.Cu") (net 3) (tstamp 7f2e0430-f00c-4fbd-a6d6-a307b7bbf38c))
  (segment (start 181.335113 50.305113) (end 181.35 50.32) (width 0.25) (layer "F.Cu") (net 3) (tstamp 7ff0d46f-7a66-4e80-b908-9bdead9da991))
  (segment (start 176.015 72.815) (end 165.85 82.98) (width 0.6) (layer "F.Cu") (net 3) (tstamp 8c811ae1-7dfa-4c7d-99eb-6ca0ffac7adc))
  (segment (start 142.73 85.36) (end 140.09 85.36) (width 0.6) (layer "F.Cu") (net 3) (tstamp 8e31687e-2ccd-4fec-a197-65f97fdc7f87))
  (segment (start 179.8 76.13) (end 176.68 73.01) (width 0.6) (layer "F.Cu") (net 3) (tstamp 95c5829a-c97d-4bbb-9ab1-294721ebc6d8))
  (segment (start 164.1 126.15) (end 164.595 126.645) (width 0.25) (layer "F.Cu") (net 3) (tstamp baad5a09-1811-4e64-b576-ac30420050da))
  (segment (start 155.18 120.72) (end 156.3 119.6) (width 0.6) (layer "F.Cu") (net 3) (tstamp e622c047-9db4-49d6-a6d5-0b05afc5e477))
  (segment (start 177.049551 50.32) (end 177.034664 50.305113) (width 0.6) (layer "F.Cu") (net 3) (tstamp e7671a1a-41bf-4534-bd45-401334af95f7))
  (segment (start 176.68 73.01) (end 176.68 72.15) (width 0.6) (layer "F.Cu") (net 3) (tstamp efa3ec59-cf0c-45e0-a39a-1e1420870c5d))
  (via (at 157 118.9) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp 810f13b7-a8fb-4ef3-9e7f-0f7a39f15afd))
  (via (at 164.95 100.9) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp fb0f300e-4c55-484e-ac7b-5a86399da9d2))
  (segment (start 174.6 59.15) (end 174.6 59.25) (width 0.25) (layer "B.Cu") (net 3) (tstamp 08b8cf9b-f156-4ed4-9b21-6d2d816efc7a))
  (segment (start 157.475 119.525) (end 164.1 126.15) (width 0.6) (layer "B.Cu") (net 3) (tstamp 0e175b0f-b70b-4f74-978e-643e0d697ea3))
  (segment (start 175.25 59.25) (end 175.25 58.4) (width 0.6) (layer "B.Cu") (net 3) (tstamp 15914e4a-9e37-4e06-b22d-f7c1b4e63666))
  (segment (start 174.6 59.15) (end 175.15 59.15) (width 0.6) (layer "B.Cu") (net 3) (tstamp 1ea77696-48d7-4c4d-8102-89d10d28b9da))
  (segment (start 157 118.9) (end 157.425 118.475) (width 0.6) (layer "B.Cu") (net 3) (tstamp 29153efc-c1e3-45ea-8ba2-2d27d06fcf49))
  (segment (start 164.3 101.55) (end 164.95 100.9) (width 0.6) (layer "B.Cu") (net 3) (tstamp 2a72a6bd-2be5-4006-a8de-2f7cc7f1f997))
  (segment (start 175.555 71.005) (end 175.25 70.7) (width 0.6) (layer "B.Cu") (net 3) (tstamp 35c4ffb0-b7b7-45b6-b8bf-76cda90a4606))
  (segment (start 175.25 59.9) (end 175.25 59.25) (width 0.6) (layer "B.Cu") (net 3) (tstamp 3ed67b8c-1b80-4c9e-b527-9af3600768b9))
  (segment (start 142.73 85.36) (end 144.8 83.29) (width 0.6) (layer "B.Cu") (net 3) (tstamp 48095e01-316f-4007-b4ff-97b00918373f))
  (segment (start 143.2 70.6) (end 146.63 67.17) (width 0.6) (layer "B.Cu") (net 3) (tstamp 5262808e-eb60-4f2d-9429-ee193c6e9223))
  (segment (start 175.25 56.94) (end 177.05 55.14) (width 0.6) (layer "B.Cu") (net 3) (tstamp 576c6fff-6a5e-401a-8ee7-64ccb1aad410))
  (segment (start 174.6 59.25) (end 175.25 59.9) (width 0.6) (layer "B.Cu") (net 3) (tstamp 5899ca76-fc09-4986-9cd6-12869f99fca6))
  (segment (start 144.8 83.29) (end 144.8 75.8) (width 0.6) (layer "B.Cu") (net 3) (tstamp 5d915aea-88b2-4c27-a37a-e6066447f6ac))
  (segment (start 157.425 118.475) (end 157.475 118.525) (width 0.25) (layer "B.Cu") (net 3) (tstamp 6e48cdc8-8014-4add-9ceb-d3e631dc401c))
  (segment (start 147.58 67.17) (end 155.6 59.15) (width 0.6) (layer "B.Cu") (net 3) (tstamp 79285d28-31b8-4c58-bba6-9c3221f3c51e))
  (segment (start 175.25 58.5) (end 174.6 59.15) (width 0.6) (layer "B.Cu") (net 3) (tstamp 855f29a4-08e6-4861-b76a-69869ff1e13c))
  (segment (start 157 119.05) (end 157.475 119.525) (width 0.6) (layer "B.Cu") (net 3) (tstamp 8f269208-7394-42ec-800e-c93ae92f19c2))
  (segment (start 175.555 71.025) (end 175.555 71.005) (width 0.6) (layer "B.Cu") (net 3) (tstamp 8f6898f8-aeee-4c90-abaf-958545e94ebf))
  (segment (start 157.475 118.525) (end 157.475 119.525) (width 0.25) (layer "B.Cu") (net 3) (tstamp 9116d63d-85b3-4dc8-a185-47d2ec4f6553))
  (segment (start 157.425 118.475) (end 164.3 111.6) (width 0.6) (layer "B.Cu") (net 3) (tstamp a2d28dcb-a29c-4ec6-b3cb-153612935b00))
  (segment (start 175.25 58.4) (end 175.25 56.94) (width 0.6) (layer "B.Cu") (net 3) (tstamp a5d1c837-e1be-4133-a234-56ed0ba1495c))
  (segment (start 175.25 70.7) (end 175.25 59.9) (width 0.6) (layer "B.Cu") (net 3) (tstamp a80ba965-d6bb-445d-a268-9e18f131e6bd))
  (segment (start 175.15 59.15) (end 175.25 59.25) (width 0.6) (layer "B.Cu") (net 3) (tstamp a8abec49-85df-4476-afa2-2f882f59e729))
  (segment (start 176.68 72.15) (end 175.555 71.025) (width 0.6) (layer "B.Cu") (net 3) (tstamp b3b3fc5c-e844-48c0-9b76-03dc004db956))
  (segment (start 155.6 59.15) (end 174.6 59.15) (width 0.6) (layer "B.Cu") (net 3) (tstamp b51d2519-a9f4-40b2-a5f3-e28c46edfe6b))
  (segment (start 146.63 67.17) (end 147.58 67.17) (width 0.6) (layer "B.Cu") (net 3) (tstamp b6569a31-9bea-4c50-9048-3ca3c768ccd0))
  (segment (start 143.2 74.2) (end 143.2 70.6) (width 0.6) (layer "B.Cu") (net 3) (tstamp b7908e84-45ce-4f55-b852-90193d8ebe83))
  (segment (start 175.25 58.4) (end 175.25 58.5) (width 0.25) (layer "B.Cu") (net 3) (tstamp cbc1dcc9-55fc-437e-ba4f-008cf183171a))
  (segment (start 164.3 104.05) (end 164.3 101.55) (width 0.6) (layer "B.Cu") (net 3) (tstamp ec39b05d-daee-4478-a584-51e5674b126d))
  (segment (start 144.8 75.8) (end 143.2 74.2) (width 0.6) (layer "B.Cu") (net 3) (tstamp efc888e4-ac71-45d3-ad61-0aa949ef7695))
  (segment (start 164.3 111.6) (end 164.3 104.05) (width 0.6) (layer "B.Cu") (net 3) (tstamp ffd7ebdd-86e4-413c-882a-b1a3bfb0228b))
  (segment (start 141.73 80.28) (end 142.73 80.28) (width 0.25) (layer "F.Cu") (net 4) (tstamp 0da8f546-140d-4512-ac87-a09b4b6d9428))
  (segment (start 126.96 94.38) (end 126.96 92.94) (width 0.25) (layer "F.Cu") (net 4) (tstamp 5645998b-2477-4215-a6fd-da3349077192))
  (segment (start 126.96 92.94) (end 129.35 90.55) (width 0.25) (layer "F.Cu") (net 4) (tstamp 607a3e9a-2cdb-4aee-b7ed-d989e4647816))
  (segment (start 139.6 78.15) (end 141.73 80.28) (width 0.25) (layer "F.Cu") (net 4) (tstamp 79a015c2-e5ac-4c96-99be-f147a347161e))
  (segment (start 142.73 80.28) (end 147.81 80.28) (width 0.25) (layer "F.Cu") (net 4) (tstamp a8cbb528-f698-4f16-99db-6f6f5c830dcb))
  (segment (start 147.81 80.28) (end 150.35 82.82) (width 0.25) (layer "F.Cu") (net 4) (tstamp d53fbd7d-0c43-4751-bbe5-d82984be00a1))
  (segment (start 129.35 90.55) (end 129.35 84.23) (width 0.25) (layer "F.Cu") (net 4) (tstamp f2618565-882e-43fd-85f5-b689a6f33d12))
  (segment (start 139.6 78.15) (end 139.6 73.11) (width 0.25) (layer "B.Cu") (net 4) (tstamp 2905af3f-c600-4491-93c8-f7bc2b5803b8))
  (segment (start 135.43 78.15) (end 139.6 78.15) (width 0.25) (layer "B.Cu") (net 4) (tstamp 743b56ab-f60d-4085-9fca-ef41b98b8a64))
  (segment (start 129.35 84.23) (end 135.43 78.15) (width 0.25) (layer "B.Cu") (net 4) (tstamp 82228cd6-3186-40cd-b0fd-118d2003720a))
  (segment (start 139.6 73.11) (end 140.06 72.65) (width 0.25) (layer "B.Cu") (net 4) (tstamp f8500594-6620-40c7-8ebb-98d93d7c92e8))
  (segment (start 150.35 80.28) (end 150.35 77.74) (width 0.25) (layer "F.Cu") (net 5) (tstamp 79d16e42-81e9-4c1e-990c-df5856e8bbdb))
  (segment (start 167.85 74.4) (end 153.3 74.4) (width 0.25) (layer "B.Cu") (net 5) (tstamp 1cfe04e8-1ffe-4f9d-92c9-c76eb2a74215))
  (segment (start 168.85 75.4) (end 167.85 74.4) (width 0.25) (layer "B.Cu") (net 5) (tstamp 654708d6-8868-4a26-a740-e992ab917eb3))
  (segment (start 150.35 77.35) (end 150.35 77.74) (width 0.25) (layer "B.Cu") (net 5) (tstamp 71c5bec0-4205-42f8-bee3-0db37565f878))
  (segment (start 153.3 74.4) (end 150.35 77.35) (width 0.25) (layer "B.Cu") (net 5) (tstamp 932ff6f3-ad40-428a-ab7f-2bf5caf46e15))
  (segment (start 168.85 95.4) (end 177.02 87.23) (width 0.25) (layer "F.Cu") (net 6) (tstamp ab51481b-c650-499f-8f07-51df1f243ea1))
  (segment (start 177.02 87.23) (end 177.02 87.2) (width 0.25) (layer "F.Cu") (net 6) (tstamp ea768dfb-637f-4745-b58f-8571afe8c1e8))
  (segment (start 148.4 89.85) (end 148.4 93.5) (width 0.25) (layer "B.Cu") (net 6) (tstamp 131fede5-c200-4a30-bd4e-d818c09edeb2))
  (segment (start 167.1 93.65) (end 168.85 95.4) (width 0.25) (layer "B.Cu") (net 6) (tstamp 1b1ba089-62b1-4288-b510-b23f2e94da61))
  (segment (start 149.45 94.55) (end 151.05 94.55) (width 0.25) (layer "B.Cu") (net 6) (tstamp 31a5c17a-7ddf-47f9-8d08-8b6bade9b7c5))
  (segment (start 148.4 93.5) (end 149.45 94.55) (width 0.25) (layer "B.Cu") (net 6) (tstamp 389d01b7-d336-457c-a202-cd3cde6ec6c3))
  (segment (start 151.05 94.55) (end 151.95 93.65) (width 0.25) (layer "B.Cu") (net 6) (tstamp b5157df6-5d47-4a6d-8b6e-47506742e771))
  (segment (start 150.35 87.9) (end 148.4 89.85) (width 0.25) (layer "B.Cu") (net 6) (tstamp cf6d2d07-2524-4f33-ad84-9c8daca4687a))
  (segment (start 151.95 93.65) (end 167.1 93.65) (width 0.25) (layer "B.Cu") (net 6) (tstamp f4c4c390-874f-48e5-b81c-1d2d5496376c))
  (segment (start 149.13 92.98) (end 144.05 87.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp 28b0f4eb-0a3b-445e-97f1-312cb2cf4ca8))
  (segment (start 166.85 102.9) (end 166.85 90.23) (width 0.25) (layer "F.Cu") (net 7) (tstamp 33337f47-edc0-4337-a978-e7386ff62f6c))
  (segment (start 165.38863 102.9) (end 166.85 102.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp 6462b23b-1e33-4c90-8815-8c054775822a))
  (segment (start 153.77 91.28137) (end 165.38863 102.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp 9bc4a97a-bf33-4504-bbe5-e059d45d816c))
  (segment (start 150.35 92.98) (end 149.13 92.98) (width 0.25) (layer "F.Cu") (net 7) (tstamp a46cb9e6-1d57-4b35-89ed-462e762c3caa))
  (segment (start 173.48 83.6) (end 166.85 90.23) (width 0.25) (layer "F.Cu") (net 7) (tstamp ab118024-8965-4a10-82db-9e7607ad8e98))
  (segment (start 144.05 87.9) (end 142.73 87.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp e312ccbf-181f-4509-9ff8-b4043aecf2e9))
  (segment (start 153.77 90.15) (end 153.77 91.28137) (width 0.25) (layer "F.Cu") (net 7) (tstamp f5286612-3b36-49ec-8ed9-c06bb42ce801))
  (segment (start 153.65 90.15) (end 153.77 90.15) (width 0.25) (layer "B.Cu") (net 7) (tstamp 623ad2b7-28d5-4b29-b21e-2309fd6b5901))
  (segment (start 150.82 92.98) (end 153.65 90.15) (width 0.25) (layer "B.Cu") (net 7) (tstamp 7224852b-4667-4928-943f-792e2eb58ba0))
  (segment (start 166.85 102.9) (end 172.6 108.65) (width 0.25) (layer "B.Cu") (net 7) (tstamp aabb632b-73c8-4570-98f7-96bbb5848185))
  (segment (start 150.35 92.98) (end 150.82 92.98) (width 0.25) (layer "B.Cu") (net 7) (tstamp ab049414-a492-49cb-b85d-64cb75bfd205))
  (segment (start 172.6 108.65) (end 172.6 108.98) (width 0.25) (layer "B.Cu") (net 7) (tstamp b6988c26-baca-4870-ad70-4cddf08617ed))
  (segment (start 144.6 105.15) (end 144.18 105.15) (width 0.25) (layer "F.Cu") (net 8) (tstamp 4348c400-d00e-4bb1-a96e-724eb0bed42d))
  (segment (start 146.85 102.9) (end 144.6 105.15) (width 0.25) (layer "F.Cu") (net 8) (tstamp 4fb72aa6-60ae-4d5b-af4f-d4de775ce3f3))
  (segment (start 132.85 122.7) (end 134.81 124.66) (width 0.25) (layer "B.Cu") (net 8) (tstamp 096690eb-1407-4f4a-a5ec-1d1ea3967e75))
  (segment (start 134.81 124.66) (end 141.36 124.66) (width 0.25) (layer "B.Cu") (net 8) (tstamp 21267af1-fbfb-4a99-ad92-2bfe051abeb1))
  (segment (start 138.2 105.15) (end 132.85 110.5) (width 0.25) (layer "B.Cu") (net 8) (tstamp 55976e93-0ec7-49d8-aa48-86b8a739c741))
  (segment (start 142.4 125.7) (end 142.4 132.2) (width 0.25) (layer "B.Cu") (net 8) (tstamp 95b80aaa-805b-45c5-b4e5-9cb846460a6d))
  (segment (start 142.4 132.2) (end 143.85 133.65) (width 0.25) (layer "B.Cu") (net 8) (tstamp 97effeda-78d0-4a85-93de-6f4c5cd1262e))
  (segment (start 143.85 133.65) (end 162.265 133.65) (width 0.25) (layer "B.Cu") (net 8) (tstamp b3e264f3-abae-4f30-a45c-b7b9ebe4a3cb))
  (segment (start 141.36 124.66) (end 142.4 125.7) (width 0.25) (layer "B.Cu") (net 8) (tstamp bf77ae70-6008-4452-a2a5-90654fc28831))
  (segment (start 144.18 105.15) (end 138.2 105.15) (width 0.25) (layer "B.Cu") (net 8) (tstamp c1e83281-4d0b-4f69-95b5-e459e9fd37e1))
  (segment (start 162.265 133.65) (end 166.73 129.185) (width 0.25) (layer "B.Cu") (net 8) (tstamp ccae2db2-74b1-4c51-ac35-02c14d67e83f))
  (segment (start 132.85 110.5) (end 132.85 122.7) (width 0.25) (layer "B.Cu") (net 8) (tstamp df1514db-77da-4686-a58e-7c6fd04d5df3))
  (segment (start 154.825 129.675) (end 161.1 123.4) (width 0.25) (layer "F.Cu") (net 9) (tstamp 33cd0719-319c-4bce-a8c3-643b17be36ad))
  (segment (start 145.85 130.07) (end 140.98 130.07) (width 0.25) (layer "F.Cu") (net 9) (tstamp 5b8fd325-2d3e-401b-852d-bd0c24e495c4))
  (segment (start 164.895 123.4) (end 166.73 121.565) (width 0.25) (layer "F.Cu") (net 9) (tstamp 7a0fed92-e5eb-4ed9-b3df-f0f7ff832c9b))
  (segment (start 152.575 129.675) (end 154.825 129.675) (width 0.25) (layer "F.Cu") (net 9) (tstamp c5bf4836-4a70-4a38-bb49-83f011787015))
  (segment (start 151.1 131.15) (end 152.575 129.675) (width 0.25) (layer "F.Cu") (net 9) (tstamp da5239be-91f7-4796-9f91-009d17c588ae))
  (segment (start 161.1 123.4) (end 164.895 123.4) (width 0.25) (layer "F.Cu") (net 9) (tstamp e32b2cc6-1331-4b55-b7a5-eb491a537d83))
  (segment (start 140.98 130.07) (end 140.85 129.94) (width 0.25) (layer "F.Cu") (net 9) (tstamp ed707ab0-e67f-40c1-a1c3-4982a4ae2c12))
  (segment (start 145.85 130.07) (end 150.02 130.07) (width 0.25) (layer "B.Cu") (net 9) (tstamp 086f8dfc-7d53-43de-ae50-a485be7b471d))
  (segment (start 150.02 130.07) (end 151.1 131.15) (width 0.25) (layer "B.Cu") (net 9) (tstamp 5e8a7e63-c8e7-45c5-958d-f684d67d1635))
  (segment (start 151.1 123.65) (end 152.95 121.8) (width 0.25) (layer "F.Cu") (net 10) (tstamp 13a173bd-b07e-4109-a414-e642e12e0dac))
  (segment (start 151.1 127.15) (end 151.1 123.65) (width 0.25) (layer "F.Cu") (net 10) (tstamp 3a6ea42a-9078-4019-8314-866d1164fb94))
  (segment (start 163.25 121.8) (end 166.025 119.025) (width 0.25) (layer "F.Cu") (net 10) (tstamp 4edf2947-5792-419d-baeb-68333bd491f3))
  (segment (start 166.56 111.65) (end 165.75 112.46) (width 0.25) (layer "F.Cu") (net 10) (tstamp 84e409af-f3cc-48d3-94b4-b976d4ad06ac))
  (segment (start 166.025 119.025) (end 166.73 119.025) (width 0.25) (layer "F.Cu") (net 10) (tstamp a7630f5b-0ffb-413d-89b0-413b9273dbbc))
  (segment (start 152.95 121.8) (end 163.25 121.8) (width 0.25) (layer "F.Cu") (net 10) (tstamp b05b7013-09e6-46ef-914f-b909580addbd))
  (segment (start 145.77 132.48) (end 151.1 127.15) (width 0.25) (layer "F.Cu") (net 10) (tstamp b2bd058b-f0b7-4078-8b69-71e2be2ed8b5))
  (segment (start 165.75 112.46) (end 165.75 118.045) (width 0.25) (layer "F.Cu") (net 10) (tstamp b8097490-88a9-40ae-a1bc-8d13c2e1cc54))
  (segment (start 165.75 118.045) (end 166.73 119.025) (width 0.25) (layer "F.Cu") (net 10) (tstamp c3e405a4-ad20-4f9e-ad88-4d4d832e5392))
  (segment (start 140.85 132.48) (end 145.77 132.48) (width 0.25) (layer "F.Cu") (net 10) (tstamp f9fea834-af29-4c4a-a81b-67eee87ddc21))
  (segment (start 172.71863 96.48) (end 173.85 96.48) (width 0.25) (layer "F.Cu") (net 11) (tstamp 199441ab-e053-437e-883f-059d675b4609))
  (segment (start 171.64 111.65) (end 171.05 111.06) (width 0.25) (layer "F.Cu") (net 11) (tstamp 2ebe6996-4a01-42e2-9498-a3b37f2cbcff))
  (segment (start 171.05 111.06) (end 171.05 98.14863) (width 0.25) (layer "F.Cu") (net 11) (tstamp 3b0f9a15-30e2-4af3-ac34-08ecde3a776e))
  (segment (start 171.64 111.65) (end 171.56 111.65) (width 0.25) (layer "F.Cu") (net 11) (tstamp 5e0debdc-b6c9-4797-a6e9-a810db5a8243))
  (segment (start 171.05 98.14863) (end 172.71863 96.48) (width 0.25) (layer "F.Cu") (net 11) (tstamp 855755a3-6952-4cc0-95e2-ab9bfd3db344))
  (segment (start 171.56 111.65) (end 167.81 115.4) (width 0.25) (layer "F.Cu") (net 11) (tstamp fe3db2da-604a-46a0-858f-753b2a372bb2))
  (segment (start 173.6 136.15) (end 183.35 136.15) (width 0.25) (layer "B.Cu") (net 11) (tstamp 0f2ac112-7426-46bd-8b95-711ed6f416f8))
  (segment (start 172.35 126.9) (end 172.35 134.9) (width 0.25) (layer "B.Cu") (net 11) (tstamp 131e6c1d-cdd0-4dc0-a923-c781453ac945))
  (segment (start 172.35 134.9) (end 173.6 136.15) (width 0.25) (layer "B.Cu") (net 11) (tstamp 1ce0052f-58eb-4372-a92b-7c35478b84b1))
  (segment (start 169.85 117.44) (end 169.85 124.4) (width 0.25) (layer "B.Cu") (net 11) (tstamp 59d4a6c4-455b-4a39-87e3-9b76ab9e5969))
  (segment (start 167.81 115.4) (end 169.85 117.44) (width 0.25) (layer "B.Cu") (net 11) (tstamp 749ec279-665d-4da9-b27c-2de703c7e6a8))
  (segment (start 183.35 136.15) (end 187.35 132.15) (width 0.25) (layer "B.Cu") (net 11) (tstamp 7faac092-90cd-423b-a41c-748212dd9f5b))
  (segment (start 169.85 124.4) (end 172.35 126.9) (width 0.25) (layer "B.Cu") (net 11) (tstamp a381f240-66a1-405d-9a40-290181a030a3))
  (segment (start 177.35 132.15) (end 174.385 129.185) (width 0.25) (layer "F.Cu") (net 12) (tstamp bc1acbcc-a66b-42aa-834c-d119ccd8ed42))
  (segment (start 174.385 129.185) (end 174.35 129.185) (width 0.25) (layer "F.Cu") (net 12) (tstamp fa3842f8-ef1a-4e92-9187-a5c624d05864))
  (segment (start 188.1 127.9) (end 188.1 122.65) (width 0.25) (layer "B.Cu") (net 12) (tstamp 76232155-9b21-4276-82b8-8180c061bb08))
  (segment (start 177.35 132.15) (end 183.85 132.15) (width 0.25) (layer "B.Cu") (net 12) (tstamp 8601ab6e-a8ba-44ff-a0ba-c4849ee74b4a))
  (segment (start 183.85 132.15) (end 188.1 127.9) (width 0.25) (layer "B.Cu") (net 12) (tstamp c1300a2b-f668-4d2f-b72b-da699e1acb16))
  (segment (start 142.73 77.74) (end 142.73 75.06) (width 0.25) (layer "F.Cu") (net 13) (tstamp 07f6a5fa-dfb0-4253-82ae-e93f7c018d15))
  (segment (start 142.73 75.06) (end 145.14 72.65) (width 0.25) (layer "F.Cu") (net 13) (tstamp 1aa95ad8-9638-45b4-90cb-15006af7a173))
  (segment (start 140.15 75.35) (end 142.54 77.74) (width 0.25) (layer "F.Cu") (net 13) (tstamp 31865cfb-fbfe-4470-b3c0-e553154f2913))
  (segment (start 142.54 77.74) (end 142.73 77.74) (width 0.25) (layer "F.Cu") (net 13) (tstamp 470a2227-8fc9-46ab-a300-c36dae8632de))
  (segment (start 134.6 74.07) (end 135.88 75.35) (width 0.25) (layer "F.Cu") (net 13) (tstamp 5338aa33-2c7a-425b-be9f-dbb0d1c9ab9f))
  (segment (start 135.88 75.35) (end 140.15 75.35) (width 0.25) (layer "F.Cu") (net 13) (tstamp 89cf796d-89b3-4ecc-b11f-f247d6632637))
  (segment (start 166.73 131.725) (end 166.73 134.265) (width 0.25) (layer "F.Cu") (net 14) (tstamp 5d2d6072-a3ea-4046-9de2-98a79877a696))
  (segment (start 172.89 125.565) (end 166.73 131.725) (width 0.25) (layer "F.Cu") (net 14) (tstamp 778c713b-adf1-452a-a8c6-f7572692de44))
  (segment (start 163.985 134.265) (end 166.73 134.265) (width 0.25) (layer "F.Cu") (net 14) (tstamp 7b35699b-c467-4981-a988-e62e14dd9c3d))
  (segment (start 147.47 141.85) (end 156.4 141.85) (width 0.25) (layer "F.Cu") (net 14) (tstamp 7f2201a0-f23f-44a5-859e-f880875484bd))
  (segment (start 156.4 141.85) (end 163.985 134.265) (width 0.25) (layer "F.Cu") (net 14) (tstamp 8396d983-ae5b-4eb3-ba7c-42bdcf7427b0))
  (segment (start 145.85 140.23) (end 147.47 141.85) (width 0.25) (layer "F.Cu") (net 14) (tstamp 99c081de-3475-49e6-ac87-a2f7f8514e01))
  (segment (start 172.89 115.4) (end 172.89 125.565) (width 0.25) (layer "F.Cu") (net 14) (tstamp bd6cb45e-e4ac-4d0c-a492-29b1bab8593a))
  (segment (start 145.85 115.4) (end 148.15 113.1) (width 0.25) (layer "F.Cu") (net 15) (tstamp 14e581bb-ea4c-48c5-b97d-2b6d87f2eae4))
  (segment (start 145.85 119.65) (end 145.85 115.4) (width 0.25) (layer "F.Cu") (net 15) (tstamp 626515c5-5f13-4017-8610-f4faffb4ef13))
  (segment (start 148.15 113.1) (end 150.15 113.1) (width 0.25) (layer "F.Cu") (net 15) (tstamp 81738253-1d4d-42a4-98e6-e185bfa55df6))
  (segment (start 136.6 128.9) (end 145.85 119.65) (width 0.25) (layer "F.Cu") (net 15) (tstamp c4e5baec-d9bb-4577-bda9-8d72c681b956))
  (segment (start 136.6 130.9) (end 136.6 128.9) (width 0.25) (layer "F.Cu") (net 15) (tstamp fc53a824-5250-440b-9cf7-7b296c46a45c))
  (segment (start 146.63 64.63) (end 146.7 64.63) (width 0.25) (layer "F.Cu") (net 16) (tstamp 0ec19e72-3881-44f7-87cc-c9ea06a69f51))
  (segment (start 146.7 64.63) (end 149.85 61.48) (width 0.25) (layer "F.Cu") (net 16) (tstamp 8a695272-a277-464b-8aca-bb25091c5aaa))
  (segment (start 145.115 65.92) (end 142.6 65.92) (width 0.25) (layer "F.Cu") (net 16) (tstamp a9b35e2f-cc20-4a01-82d9-047647eb5f30))
  (segment (start 146.63 64.63) (end 146.405 64.63) (width 0.25) (layer "F.Cu") (net 16) (tstamp acc01f55-96a9-4a01-a58b-0c18d6bd111d))
  (segment (start 146.405 64.63) (end 145.115 65.92) (width 0.25) (layer "F.Cu") (net 16) (tstamp ea9df021-b0ce-486c-b0fb-3a22069a00c7))
  (segment (start 142.375 64.65) (end 138.5 68.525) (width 0.25) (layer "B.Cu") (net 17) (tstamp 177eb878-2599-4898-a11e-9e6e247f23c2))
  (segment (start 130.67 72.75) (end 129.35 74.07) (width 0.25) (layer "B.Cu") (net 17) (tstamp 701255a9-3f60-4b0e-a870-25806c0dec48))
  (segment (start 137.85 72.75) (end 130.67 72.75) (width 0.25) (layer "B.Cu") (net 17) (tstamp b17ba51e-eec5-4735-96e7-fd03656984b4))
  (segment (start 138.5 68.525) (end 138.5 72.1) (width 0.25) (layer "B.Cu") (net 17) (tstamp b1e6578a-262c-456c-920c-bd23aef60d82))
  (segment (start 138.5 72.1) (end 137.85 72.75) (width 0.25) (layer "B.Cu") (net 17) (tstamp b95e20ff-fa50-41af-9685-7ad21f2a4fb2))
  (segment (start 142.6 64.65) (end 142.375 64.65) (width 0.25) (layer "B.Cu") (net 17) (tstamp e2791f78-7f4c-4e97-88d0-16518f370200))
  (segment (start 175.8 74.4) (end 164.2 62.8) (width 0.25) (layer "B.Cu") (net 18) (tstamp 0cba6e0a-0c68-4e95-b511-8cb17e85af9c))
  (segment (start 179.8 65.97) (end 179.8 72.5) (width 0.25) (layer "B.Cu") (net 18) (tstamp a11a8682-d0c5-48d1-a6bb-3508b2d3ed5f))
  (segment (start 179.8 72.5) (end 177.9 74.4) (width 0.25) (layer "B.Cu") (net 18) (tstamp a2a965da-4992-4093-9be5-634da76b5ed1))
  (segment (start 177.9 74.4) (end 175.8 74.4) (width 0.25) (layer "B.Cu") (net 18) (tstamp b563b8c2-9c00-49f7-ba5f-ab0859baa631))
  (segment (start 164.2 62.8) (end 161.1 62.8) (width 0.25) (layer "B.Cu") (net 18) (tstamp bf546e98-6c31-43d3-a31b-cec1f80cb1e0))
  (segment (start 157.15 72.15) (end 166.52 72.15) (width 0.25) (layer "B.Cu") (net 19) (tstamp 18db8bfa-1dfc-4b47-80bc-a7069ce15337))
  (segment (start 156.1 71.1) (end 157.15 72.15) (width 0.25) (layer "B.Cu") (net 19) (tstamp 6477825d-1dcc-43eb-942b-34ce574b3a08))
  (segment (start 156.1 69.4) (end 156.1 71.1) (width 0.25) (layer "B.Cu") (net 19) (tstamp 9bec49d5-74ee-444d-b381-f90188b6b57d))
  (segment (start 146.1 58.25) (end 140.76 63.59) (width 0.25) (layer "B.Cu") (net 20) (tstamp 6388a97a-7b3c-44f2-a595-df09a2cd8cb7))
  (segment (start 146.1 55.73) (end 146.1 58.25) (width 0.25) (layer "B.Cu") (net 20) (tstamp cda95c1c-105e-4371-8d5f-487bbaa8e2a0))
  (segment (start 140.76 63.59) (end 136.85 63.59) (width 0.25) (layer "B.Cu") (net 20) (tstamp f2223bc5-3816-4d07-99b3-1f384f2aa56b))
  (segment (start 146.1 50.695) (end 146.1 45.57) (width 0.25) (layer "F.Cu") (net 21) (tstamp 08a00886-ad04-4e64-bae3-d8c46641965b))
  (segment (start 153.555 58.15) (end 146.1 50.695) (width 0.25) (layer "F.Cu") (net 21) (tstamp 4bffd8e1-a662-4970-9348-bee587deff83))
  (segment (start 153.555 62.555) (end 153.555 58.15) (width 0.25) (layer "F.Cu") (net 21) (tstamp 58512c59-4e7c-4047-9725-fd338b3381ad))
  (segment (start 157.35 64.05) (end 155.05 64.05) (width 0.25) (layer "F.Cu") (net 21) (tstamp 7c19035e-e843-4d57-a66c-a0c197679b86))
  (segment (start 155.05 64.05) (end 153.555 62.555) (width 0.25) (layer "F.Cu") (net 21) (tstamp a7776dc7-ddbd-484d-b743-6d5a0c496cce))
  (segment (start 158.6 62.8) (end 157.35 64.05) (width 0.25) (layer "F.Cu") (net 21) (tstamp dbb6942f-c540-4122-bf7b-abd358e21292))
  (segment (start 136.85 66.85) (end 142.27 61.43) (width 0.25) (layer "F.Cu") (net 22) (tstamp 03530831-aed4-46c1-9362-d5aaa2474505))
  (segment (start 142.27 61.43) (end 142.27 58.9) (width 0.25) (layer "F.Cu") (net 22) (tstamp 676f9dc9-a232-47af-92a3-bc4d3fc52202))
  (segment (start 132.35 63.65) (end 132.35 66.3) (width 0.25) (layer "F.Cu") (net 22) (tstamp 975247e4-7a85-4dd1-a907-655f8d10c048))
  (segment (start 132.35 66.3) (end 132.9 66.85) (width 0.25) (layer "F.Cu") (net 22) (tstamp a29874df-95a6-422f-824d-f150a2d9dff3))
  (segment (start 132.9 66.85) (end 136.85 66.85) (width 0.25) (layer "F.Cu") (net 22) (tstamp cde2f436-8e7e-4f21-9d1f-82d6ffbabf17))
  (segment (start 152.43 63.23) (end 158.6 69.4) (width 0.25) (layer "F.Cu") (net 23) (tstamp cbdd530f-04ab-4064-91d6-30c15418b513))
  (segment (start 152.43 58.9) (end 152.43 63.23) (width 0.25) (layer "F.Cu") (net 23) (tstamp d58cb3d6-e8c5-43b5-b6d9-2cd20829e84c))
  (segment (start 134.85 63.65) (end 142.77 55.73) (width 0.25) (layer "B.Cu") (net 24) (tstamp 821b093e-4589-41e7-8993-948d46322e0a))
  (segment (start 142.77 55.73) (end 142.85 55.73) (width 0.25) (layer "B.Cu") (net 24) (tstamp 84c8c370-fb4b-4b8e-9bed-8417e1e69e70))
  (segment (start 134.6 63.65) (end 134.85 63.65) (width 0.25) (layer "B.Cu") (net 24) (tstamp dd3f904b-ae05-4dc2-965e-b6a85081242f))
  (segment (start 136.05 58.5) (end 142.85 51.7) (width 0.25) (layer "F.Cu") (net 25) (tstamp 418c1086-16e0-4db5-9a82-18e64d729e58))
  (segment (start 142.85 51.7) (end 142.85 45.57) (width 0.25) (layer "F.Cu") (net 25) (tstamp 4f40a940-6151-4662-a277-8e5a48935fc2))
  (segment (start 136.05 60.12) (end 136.05 58.5) (width 0.25) (layer "F.Cu") (net 25) (tstamp e3b7fa47-11d4-4d39-b285-23e49cbf5fd1))
  (segment (start 127.6 71.15) (end 127.6 79.32) (width 0.25) (layer "B.Cu") (net 26) (tstamp 11fe2f31-47b9-468c-aea3-db036d6b20f2))
  (segment (start 130.1 68.65) (end 127.6 71.15) (width 0.25) (layer "B.Cu") (net 26) (tstamp 3c9d65c5-a957-4c42-808e-2c16aa1b76a8))
  (segment (start 130.1 63.59) (end 130.1 68.65) (width 0.25) (layer "B.Cu") (net 26) (tstamp 6b933462-ca6e-48ce-b020-eb9b5c815a3c))
  (segment (start 127.6 79.32) (end 125.6 81.32) (width 0.25) (layer "B.Cu") (net 26) (tstamp ef64cc85-b5af-4e71-ae15-5450f78116a0))
  (segment (start 128.33 88.75) (end 137.75 88.75) (width 0.25) (layer "B.Cu") (net 27) (tstamp 1924a364-c64d-4089-90bf-2f7a688b82e3))
  (segment (start 137.75 88.75) (end 139.5 90.5) (width 0.25) (layer "B.Cu") (net 27) (tstamp 2cd9090d-8a97-4607-a10d-a42b032544c3))
  (segment (start 125.6 91.48) (end 128.33 88.75) (width 0.25) (layer "B.Cu") (net 27) (tstamp 2dce01c8-c283-41e2-ab48-49cd50c8ea16))
  (segment (start 145.25 99.5) (end 153.2 99.5) (width 0.25) (layer "B.Cu") (net 27) (tstamp 8a270795-724c-4a88-91b3-dae9f7e1e5c7))
  (segment (start 139.5 93.75) (end 145.25 99.5) (width 0.25) (layer "B.Cu") (net 27) (tstamp 99defa32-f9a2-4c34-bdf2-98994eff73ad))
  (segment (start 153.2 99.5) (end 158.6 104.9) (width 0.25) (layer "B.Cu") (net 27) (tstamp b2bb88b2-91b0-4944-b6ae-23031cfa3cf4))
  (segment (start 139.5 90.5) (end 139.5 93.75) (width 0.25) (layer "B.Cu") (net 27) (tstamp bdc9fc88-2cdf-4a93-98b5-7d7480dfdf02))
  (segment (start 125.6 55.82) (end 125.6 52.94) (width 0.25) (layer "F.Cu") (net 28) (tstamp 30464bee-50c0-4dfe-85b7-cacca162db13))
  (segment (start 125.6 52.94) (end 126.6 51.94) (width 0.25) (layer "F.Cu") (net 28) (tstamp 9cc4bf30-8173-495f-8431-ee4800ec0175))
  (segment (start 160.18 45.9) (end 168.85 45.9) (width 0.6) (layer "F.Cu") (net 29) (tstamp 547f20f5-054d-4029-bc6f-5ed6a2075f6a))
  (segment (start 181.94 66.9) (end 181.94 61.07) (width 0.25) (layer "F.Cu") (net 30) (tstamp 471f6247-3b17-4664-9c00-01aec7f5344b))
  (segment (start 181.94 61.07) (end 181.35 60.48) (width 0.25) (layer "F.Cu") (net 30) (tstamp fcb8aed7-5d2d-4fa4-896c-4dfbfcb2d2c0))
  (segment (start 146.88 82.82) (end 142.73 82.82) (width 0.25) (layer "F.Cu") (net 31) (tstamp 09634e26-a8be-475d-9b28-f49854259fc0))
  (segment (start 146.9 82.8) (end 146.88 82.82) (width 0.25) (layer "F.Cu") (net 31) (tstamp 302d7a25-b786-4d5e-a45b-a916d68d1b7d))
  (via (at 146.9 82.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 31) (tstamp 1cac1b14-1723-4b89-af31-57aa3c0cfaa2))
  (segment (start 136.6 82.8) (end 136.62 82.82) (width 0.25) (layer "B.Cu") (net 31) (tstamp 090e35cc-2b8b-435d-a799-961cc08eb03f))
  (segment (start 147.6 77.3) (end 147.6 82.1) (width 0.25) (layer "B.Cu") (net 31) (tstamp 189f5b17-8d27-4252-bf0a-dc5b3e277ac0))
  (segment (start 136.62 82.82) (end 142.73 82.82) (width 0.25) (layer "B.Cu") (net 31) (tstamp 1b85befa-e1fb-4cd7-bbac-906063abd43d))
  (segment (start 154.35 70.55) (end 147.6 77.3) (width 0.25) (layer "B.Cu") (net 31) (tstamp 32fbf2bd-792e-4efb-a33a-c2e208d7c4c4))
  (segment (start 163.72 66.1) (end 157.45 66.1) (width 0.25) (layer "B.Cu") (net 31) (tstamp 385bf589-3206-49f6-8679-44b1536fe7e9))
  (segment (start 177.02 79.4) (end 166.52 68.9) (width 0.25) (layer "B.Cu") (net 31) (tstamp 5b9667f5-43ab-4f46-a4e3-d23da8390718))
  (segment (start 154.35 69.2) (end 154.35 70.55) (width 0.25) (layer "B.Cu") (net 31) (tstamp 69585d9e-53ea-47e8-84e6-31bc0e5fcbfe))
  (segment (start 166.52 68.9) (end 163.72 66.1) (width 0.25) (layer "B.Cu") (net 31) (tstamp 795fb4b2-5f70-41d8-b118-2536528afbd7))
  (segment (start 157.45 66.1) (end 154.35 69.2) (width 0.25) (layer "B.Cu") (net 31) (tstamp 87e85142-0798-40b6-9a72-8558080d3e0c))
  (segment (start 136.03 82.8) (end 136.6 82.8) (width 0.25) (layer "B.Cu") (net 31) (tstamp 952544d9-a3a5-427e-8695-ee8ac989645a))
  (segment (start 177.02 83.85) (end 177.02 79.4) (width 0.25) (layer "B.Cu") (net 31) (tstamp 9e55e520-fb4a-4592-bf2d-a3df44bd8518))
  (segment (start 134.6 84.23) (end 136.03 82.8) (width 0.25) (layer "B.Cu") (net 31) (tstamp a660d89f-ab2c-447e-9df5-e234ff03551a))
  (segment (start 147.6 82.1) (end 146.9 82.8) (width 0.25) (layer "B.Cu") (net 31) (tstamp a912d890-4143-4cfa-ba8f-055abd9f280e))
  (segment (start 152.39 88.4) (end 157.27 88.4) (width 0.25) (layer "B.Cu") (net 32) (tstamp 15d241f0-0a6c-4033-982d-86d9bdaf9563))
  (segment (start 157.27 88.4) (end 157.685 88.815) (width 0.25) (layer "B.Cu") (net 32) (tstamp 53e9e9c0-6560-4749-998e-4b47f8d784e0))
  (segment (start 178.52 105.4) (end 178.52 97.97) (width 0.25) (layer "B.Cu") (net 32) (tstamp 7f5201b6-c45d-4ac2-8fe3-4f2c895162a7))
  (segment (start 150.35 90.44) (end 152.39 88.4) (width 0.25) (layer "B.Cu") (net 32) (tstamp 96e90774-4f24-4f77-b344-c3d335cbec90))
  (segment (start 172.65 92.1) (end 159.8 92.1) (width 0.25) (layer "B.Cu") (net 32) (tstamp 9d6ff610-2c74-4965-b254-72a19a07464b))
  (segment (start 157.895 90.195) (end 157.895 89.025) (width 0.25) (layer "B.Cu") (net 32) (tstamp b104dde6-02c2-4284-8f2c-17b5e5f30443))
  (segment (start 163.32 83.6) (end 158.185 88.735) (width 0.25) (layer "B.Cu") (net 32) (tstamp b3458ce7-1d81-4d78-ac06-d3dda80f0ea2))
  (segment (start 158.185 88.735) (end 157.895 89.025) (width 0.25) (layer "B.Cu") (net 32) (tstamp bed1108d-d1ee-4f9f-ac6b-c3d63df4935f))
  (segment (start 158.105 88.815) (end 158.185 88.735) (width 0.25) (layer "B.Cu") (net 32) (tstamp c49882db-60c1-436b-808b-58580151d342))
  (segment (start 157.685 88.815) (end 157.895 89.025) (width 0.25) (layer "B.Cu") (net 32) (tstamp d34a777b-1170-4442-b895-51ce790f2ed3))
  (segment (start 178.52 97.97) (end 172.65 92.1) (width 0.25) (layer "B.Cu") (net 32) (tstamp d8103df7-a940-436a-a00b-28a929252f61))
  (segment (start 157.685 88.815) (end 158.105 88.815) (width 0.25) (layer "B.Cu") (net 32) (tstamp db6b7bfe-74b6-42ca-8ee8-574cc6ff9551))
  (segment (start 159.8 92.1) (end 157.895 90.195) (width 0.25) (layer "B.Cu") (net 32) (tstamp eb99e775-1bf4-4fca-858e-219a5cdb5f9c))
  (segment (start 159.52 107.9) (end 161.1 109.48) (width 0.25) (layer "F.Cu") (net 33) (tstamp 5c2cf187-4146-4e2e-96f6-d0a2614db1ff))
  (segment (start 161.1 109.48) (end 161.1 110.4) (width 0.25) (layer "F.Cu") (net 33) (tstamp c3289e72-716e-4ba9-82c1-4b5381dfb5e1))
  (segment (start 154.85 127.15) (end 156.1 125.9) (width 0.25) (layer "B.Cu") (net 34) (tstamp 6f7c4c6a-8ca2-450d-b981-054e8893f99e))
  (segment (start 156.1 125.9) (end 156.1 110.4) (width 0.25) (layer "B.Cu") (net 34) (tstamp e2348d3f-3086-4be1-81c6-870afad20def))
  (segment (start 173.8 90.15) (end 181.1 97.45) (width 0.25) (layer "B.Cu") (net 35) (tstamp a91827d1-7625-4a57-ad33-de3802404fad))
  (segment (start 163.93 90.15) (end 173.8 90.15) (width 0.25) (layer "B.Cu") (net 35) (tstamp b7bf694d-acf7-40db-8f76-a270c33075bf))
  (segment (start 181.1 97.45) (end 181.1 102.32) (width 0.25) (layer "B.Cu") (net 35) (tstamp de911b72-6db2-4a61-8671-08d6b3fa9258))
  (segment (start 142.73 90.44) (end 150.1 97.81) (width 0.25) (layer "F.Cu") (net 36) (tstamp 28c7e806-e2b3-4b65-b673-8f9fb5af9f12))
  (segment (start 139.85 93.32) (end 142.73 90.44) (width 0.25) (layer "F.Cu") (net 36) (tstamp 2bafeced-56f6-46a4-b3e6-09f953230e22))
  (segment (start 129.1 100.07) (end 136.23 100.07) (width 0.25) (layer "F.Cu") (net 36) (tstamp 550a23ab-9ac7-4985-8064-d1f4007db920))
  (segment (start 136.23 100.07) (end 139.85 96.45) (width 0.25) (layer "F.Cu") (net 36) (tstamp a3984fc5-afba-4967-8c47-25621de06eb7))
  (segment (start 139.85 96.45) (end 139.85 93.32) (width 0.25) (layer "F.Cu") (net 36) (tstamp f023c516-999d-4055-b6c0-09c8260d76bd))
  (segment (start 149.375305 101.1) (end 138.9 101.1) (width 0.25) (layer "B.Cu") (net 37) (tstamp 275299a4-2ce4-4cbe-b13a-dcd758d689da))
  (segment (start 129.1 105.7) (end 129.1 110.23) (width 0.25) (layer "B.Cu") (net 37) (tstamp 47f58eb6-f2f2-4c76-9c3e-7207b1f19afc))
  (segment (start 158.6 110.4) (end 158.6 110.324695) (width 0.25) (layer "B.Cu") (net 37) (tstamp 52507ba6-8a6b-4eb9-980f-4851e0eb9ecb))
  (segment (start 137.8 100) (end 134.8 100) (width 0.25) (layer "B.Cu") (net 37) (tstamp 5708ecfa-f870-4c8b-a2a0-802d0ee17788))
  (segment (start 158.6 110.324695) (end 149.375305 101.1) (width 0.25) (layer "B.Cu") (net 37) (tstamp 5bd6e380-8513-48b7-ae73-6a69eb74ea6e))
  (segment (start 138.9 101.1) (end 137.8 100) (width 0.25) (layer "B.Cu") (net 37) (tstamp b7a09fe5-167d-4ffa-86b5-85d19a129f73))
  (segment (start 134.8 100) (end 129.1 105.7) (width 0.25) (layer "B.Cu") (net 37) (tstamp da325b66-c466-4c99-9be1-3b130a8d5aca))
  (segment (start 156.1 130.9) (end 158.6 130.9) (width 0.25) (layer "F.Cu") (net 38) (tstamp 4f88b3b2-4ad0-47b7-8e2d-8276bc24bc5c))
  (segment (start 152.85 127.65) (end 152.85 122.15) (width 0.25) (layer "B.Cu") (net 38) (tstamp 04c341bb-93bc-4ee7-a22c-af53e046f040))
  (segment (start 150.1 110.132412) (end 150.1 108.23) (width 0.25) (layer "B.Cu") (net 38) (tstamp 1900d105-e1a8-4113-b657-3573b0c0cf85))
  (segment (start 151.75 120.65) (end 151.75 111.782412) (width 0.25) (layer "B.Cu") (net 38) (tstamp 5a6e296d-9c91-414b-8bf8-f3df50a4f649))
  (segment (start 151.75 121.05) (end 151.75 120.65) (width 0.25) (layer "B.Cu") (net 38) (tstamp 5a748611-c80f-4344-b1f0-9be67a21d414))
  (segment (start 156.1 130.9) (end 152.85 127.65) (width 0.25) (layer "B.Cu") (net 38) (tstamp 77bad093-f045-4c51-bf0d-1c81f8989f9f))
  (segment (start 151.75 111.782412) (end 150.1 110.132412) (width 0.25) (layer "B.Cu") (net 38) (tstamp cc532b7d-bba9-4b89-ba66-5b3d6cea69ff))
  (segment (start 152.85 122.15) (end 151.75 121.05) (width 0.25) (layer "B.Cu") (net 38) (tstamp e00d55b8-b977-4f71-8ab7-db8ceebd84cb))
  (segment (start 172.6 102.57) (end 175.35 105.32) (width 0.25) (layer "F.Cu") (net 39) (tstamp 51a72ddb-62cb-4a5a-a4ac-86934c9bdff8))
  (segment (start 172.6 98.82) (end 172.6 102.57) (width 0.25) (layer "F.Cu") (net 39) (tstamp 9b9979b7-621a-4aac-87c2-ab73a89dec54))
  (segment (start 151.5 96.25) (end 152.45 95.3) (width 0.25) (layer "B.Cu") (net 39) (tstamp 00ad6936-efb8-4ac4-986d-09f8c88b6da1))
  (segment (start 142.73 92.98) (end 146 96.25) (width 0.25) (layer "B.Cu") (net 39) (tstamp 6d2f75c4-c892-4706-841a-5f4329390e2f))
  (segment (start 152.45 95.3) (end 165 95.3) (width 0.25) (layer "B.Cu") (net 39) (tstamp 6fc84e45-bf8e-4da4-97a6-0115f8d035ce))
  (segment (start 165 95.3) (end 168.52 98.82) (width 0.25) (layer "B.Cu") (net 39) (tstamp af11787c-ef21-4596-97ba-899a68917e3b))
  (segment (start 168.52 98.82) (end 172.6 98.82) (width 0.25) (layer "B.Cu") (net 39) (tstamp d44f3948-57ec-4993-b4c1-4e7ed6aadfcc))
  (segment (start 146 96.25) (end 151.5 96.25) (width 0.25) (layer "B.Cu") (net 39) (tstamp eb1ca506-53d0-4ed0-9da9-9250db639c19))
  (segment (start 175.35 111.57) (end 178.52 108.4) (width 0.25) (layer "F.Cu") (net 40) (tstamp 0c2803cc-4027-4952-bd9c-e2dd4e14b014))
  (segment (start 176.4 122.055) (end 174.35 124.105) (width 0.25) (layer "F.Cu") (net 40) (tstamp 54fbf4ad-e955-48fd-8727-cf78d05e7e39))
  (segment (start 175.35 115.48) (end 176.37 116.5) (width 0.25) (layer "F.Cu") (net 40) (tstamp a79eafac-0dcc-4dc7-b0cf-87f9e891c8ad))
  (segment (start 176.4 116.5) (end 176.4 122.055) (width 0.25) (layer "F.Cu") (net 40) (tstamp ab23e484-3bc0-4c72-a7d5-9803c3bea76e))
  (segment (start 176.37 116.5) (end 176.4 116.5) (width 0.25) (layer "F.Cu") (net 40) (tstamp af6535ce-1398-4bbc-8ae2-81698b877604))
  (segment (start 175.35 115.48) (end 175.35 111.57) (width 0.25) (layer "F.Cu") (net 40) (tstamp b34b8d0b-4691-4b27-8663-c1af3b46f762))
  (segment (start 191.85 115.1) (end 191.85 112.57) (width 0.25) (layer "F.Cu") (net 41) (tstamp 31239a29-b7c9-4ad6-b13f-06e8a5b91159))
  (segment (start 186.15 120.8) (end 191.85 115.1) (width 0.25) (layer "F.Cu") (net 41) (tstamp c2ae3f82-1d34-4841-89a7-cfab20d6977e))
  (segment (start 191.85 112.57) (end 191.85 108.9) (width 0.25) (layer "F.Cu") (net 41) (tstamp ee39135f-ee7a-462a-a100-ef2234dcbf35))
  (via (at 186.15 120.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 41) (tstamp 742589e9-57d7-4608-a38a-472d68ec993b))
  (segment (start 185.1 121.85) (end 186.15 120.8) (width 0.25) (layer "B.Cu") (net 41) (tstamp 648f856c-c8e4-46be-bd4e-307d92475377))
  (segment (start 185.1 126.5) (end 185.1 121.85) (width 0.25) (layer "B.Cu") (net 41) (tstamp 77bb44a1-6072-4c34-8576-7f2ba8298dbc))
  (segment (start 182.15 129.45) (end 185.1 126.5) (width 0.25) (layer "B.Cu") (net 41) (tstamp 82b68e9e-16f1-4aa6-88bc-d2d290750859))
  (segment (start 174.35 131.725) (end 176.625 129.45) (width 0.25) (layer "B.Cu") (net 41) (tstamp 93aa3047-8ce8-4225-8bd5-4bd4cafd8998))
  (segment (start 176.625 129.45) (end 182.15 129.45) (width 0.25) (layer "B.Cu") (net 41) (tstamp a1062bba-2083-4df6-a237-e4d0c7264ab2))
  (segment (start 188.85 126.15) (end 192.43 126.15) (width 0.25) (layer "F.Cu") (net 42) (tstamp 13f57a1b-34e3-4d2c-8e0f-0071319c5d6d))
  (segment (start 192.43 123.31) (end 191.85 122.73) (width 0.25) (layer "F.Cu") (net 42) (tstamp 5f61d856-912f-4d64-a73d-6f0cb1e41d37))
  (segment (start 192.43 126.15) (end 192.43 123.31) (width 0.25) (layer "F.Cu") (net 42) (tstamp 67130052-b2e7-4892-8f6b-71e0d24d5f66))
  (segment (start 180.735 134.265) (end 188.85 126.15) (width 0.25) (layer "F.Cu") (net 42) (tstamp 8d3e3e06-659d-44f1-9509-b734f4460707))
  (segment (start 174.35 134.265) (end 180.735 134.265) (width 0.25) (layer "F.Cu") (net 42) (tstamp d90a4191-6a3c-4438-af8b-bb7a0cd603a4))
  (segment (start 182.27 126.15) (end 182.27 123.99) (width 0.25) (layer "F.Cu") (net 43) (tstamp 1b1745bc-b4ac-4621-8c63-d6be93f7e4d8))
  (segment (start 182.27 123.99) (end 181.1 122.82) (width 0.25) (layer "F.Cu") (net 43) (tstamp 622555ab-f32b-4861-84da-89fc3f47e546))
  (segment (start 189.85 142.23) (end 186.02 138.4) (width 0.25) (layer "F.Cu") (net 44) (tstamp 00e941e8-bbb1-4dfa-ab51-2dee3d8db30f))
  (segment (start 191.6 142.23) (end 189.85 142.23) (width 0.25) (layer "F.Cu") (net 44) (tstamp ea83bdda-b617-4cad-8038-5a80b580c985))
  (segment (start 174.35 119.025) (end 174.35 121.565) (width 0.25) (layer "F.Cu") (net 45) (tstamp f8cbddda-5bc0-4315-835c-a2ba72a2c8de))
  (segment (start 190.05 122.05) (end 186.7 118.7) (width 0.25) (layer "B.Cu") (net 45) (tstamp 0d568279-c63c-4d1d-bc28-40091229d492))
  (segment (start 191.6 127.85) (end 190.05 126.3) (width 0.25) (layer "B.Cu") (net 45) (tstamp 27ad656e-d32b-44b6-8256-b09a26c164b0))
  (segment (start 191.6 132.07) (end 191.6 127.85) (width 0.25) (layer "B.Cu") (net 45) (tstamp 3b68a719-898d-4409-9acf-18b127e6c50d))
  (segment (start 190.05 126.3) (end 190.05 122.05) (width 0.25) (layer "B.Cu") (net 45) (tstamp bf95de25-d0bb-4fbf-b760-0c69383fa64f))
  (segment (start 186.7 118.7) (end 174.675 118.7) (width 0.25) (layer "B.Cu") (net 45) (tstamp c0e560a6-3861-4ba7-b2fb-e88f0989abec))
  (segment (start 174.675 118.7) (end 174.35 119.025) (width 0.25) (layer "B.Cu") (net 45) (tstamp d17dd24d-7a56-46dc-9b66-13f3de6fc066))
  (segment (start 152.25 104.9) (end 156.1 104.9) (width 0.25) (layer "F.Cu") (net 46) (tstamp 39ca955f-a713-426f-9288-008f9fdef8de))
  (segment (start 152.2 104.95) (end 152.25 104.9) (width 0.25) (layer "F.Cu") (net 46) (tstamp f51201c2-63ef-46ef-b29b-3b495dd92cac))
  (via (at 152.2 104.95) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 46) (tstamp 0e8ed71c-b250-4373-afb3-75fa0143c340))
  (segment (start 147.4 111.6) (end 141.7 111.6) (width 0.25) (layer "B.Cu") (net 46) (tstamp 0e650484-75ef-4376-a9f9-82c5a9d4afea))
  (segment (start 148.1 110.9) (end 147.4 111.6) (width 0.25) (layer "B.Cu") (net 46) (tstamp 14774be5-ca8c-4588-a94b-c89fecd83ff0))
  (segment (start 139.45 119.42) (end 136.05 122.82) (width 0.25) (layer "B.Cu") (net 46) (tstamp 20400a84-5022-478f-b036-c75288e9ea94))
  (segment (start 152.2 104.95) (end 149.3 104.95) (width 0.25) (layer "B.Cu") (net 46) (tstamp 36c1040e-480d-4460-9e18-bf7212d07c75))
  (segment (start 149.3 104.95) (end 148.1 106.15) (width 0.25) (layer "B.Cu") (net 46) (tstamp 44b3a038-cdf9-411f-9f8d-6dae8b26b0e9))
  (segment (start 139.45 113.85) (end 139.45 119.42) (width 0.25) (layer "B.Cu") (net 46) (tstamp 76a789be-2741-4791-8115-1b9e3fcb72d4))
  (segment (start 141.7 111.6) (end 139.45 113.85) (width 0.25) (layer "B.Cu") (net 46) (tstamp 7ddaef24-4d7d-4792-8159-e7f710bd3646))
  (segment (start 148.1 106.15) (end 148.1 110.9) (width 0.25) (layer "B.Cu") (net 46) (tstamp f133950f-e409-4945-9e83-006e4fda85ea))
  (segment (start 144.32 135.05) (end 156.95 135.05) (width 0.25) (layer "F.Cu") (net 47) (tstamp 5b7fea74-58d7-4db1-b718-248d011f72d8))
  (segment (start 140.97 138.4) (end 144.32 135.05) (width 0.25) (layer "F.Cu") (net 47) (tstamp a36ed1f7-87a3-4ed8-9343-8b9220faec4b))
  (segment (start 156.95 135.05) (end 161.1 130.9) (width 0.25) (layer "F.Cu") (net 47) (tstamp eae3c2bc-b39e-4a8b-8ff3-4279129e1f1e))
  (segment (start 189.74 49.79) (end 187.2 49.79) (width 0.6) (layer "F.Cu") (net 49) (tstamp 51d86972-461b-4b41-a135-164122608b0a))
  (segment (start 187.2 49.79) (end 183.31 45.9) (width 0.6) (layer "F.Cu") (net 49) (tstamp 98963c5e-78d3-40a8-b81b-f8e30c9af5f8))
  (segment (start 183.31 45.9) (end 179.01 45.9) (width 0.6) (layer "F.Cu") (net 49) (tstamp a7bd116a-17f1-4e85-a7d4-5c1804281ab7))
  (segment (start 189.74 64.54) (end 192.1 66.9) (width 0.6) (layer "F.Cu") (net 50) (tstamp 598a7bd4-2d1e-463e-89d5-092d3c5d4ffa))
  (segment (start 189.74 59.95) (end 187.2 59.95) (width 0.6) (layer "F.Cu") (net 50) (tstamp 81260e88-3d61-4201-a038-fbd637eb190e))
  (segment (start 189.74 59.95) (end 189.74 64.54) (width 0.6) (layer "F.Cu") (net 50) (tstamp a58217ed-40ce-4ce8-ac05-27312440aabc))
  (segment (start 125.35 130.9) (end 129.1 130.9) (width 0.25) (layer "F.Cu") (net 51) (tstamp e268ef32-acef-4078-a6ee-4529ffb5a126))
  (segment (start 129.1 134.69) (end 129.1 130.9) (width 0.25) (layer "B.Cu") (net 51) (tstamp 65499bcb-f47a-4aad-b314-266406c9fd47))
  (segment (start 125.35 138.44) (end 129.1 134.69) (width 0.25) (layer "B.Cu") (net 51) (tstamp 82b88a39-c9b1-40d3-bd31-b23a4fbffbbc))
  (segment (start 125.35 133.36) (end 127.25 131.46) (width 0.25) (layer "B.Cu") (net 52) (tstamp 29522946-f4c0-40d3-bf9d-c1bcafce4bf6))
  (segment (start 125.6 96.46) (end 125.6 102.07) (width 0.25) (layer "B.Cu") (net 52) (tstamp 450ee621-bc87-4555-b4db-5c37b76681b8))
  (segment (start 127.25 131.46) (end 127.25 103.72) (width 0.25) (layer "B.Cu") (net 52) (tstamp 5f9336f4-6927-445e-8a3b-0c6a431beb6b))
  (segment (start 126.96 95.65) (end 126.41 95.65) (width 0.25) (layer "B.Cu") (net 52) (tstamp 75e2e101-752b-44cc-ab96-6b2f2b3d96e2))
  (segment (start 127.25 103.72) (end 125.6 102.07) (width 0.25) (layer "B.Cu") (net 52) (tstamp b8ca4f5f-13c7-4667-ba7a-49c895651856))
  (segment (start 126.41 95.65) (end 125.6 96.46) (width 0.25) (layer "B.Cu") (net 52) (tstamp c02fc4fd-8ec3-4e94-9b6c-b2e64b7d25c2))
  (segment (start 127.45 107.15) (end 132.28 102.32) (width 0.25) (layer "F.Cu") (net 56) (tstamp 43d6e497-155e-4780-9593-84fc55ce2ae8))
  (segment (start 127.45 115.42) (end 127.45 107.15) (width 0.25) (layer "F.Cu") (net 56) (tstamp 481a2f1d-c461-4f89-baa6-82b367a7ebc9))
  (segment (start 129.1 117.07) (end 127.45 115.42) (width 0.25) (layer "F.Cu") (net 56) (tstamp 65a0279c-b55e-484c-bb18-803502f76cd4))
  (segment (start 132.28 102.32) (end 136.05 102.32) (width 0.25) (layer "F.Cu") (net 56) (tstamp bda22866-8268-4cde-8a88-925497edc071))
  (segment (start 134.6 71.27) (end 136.79 71.27) (width 0.25) (layer "F.Cu") (net 57) (tstamp 0852aaff-c790-42a4-ab74-5da1124ac1cb))
  (segment (start 127.95 69.4) (end 128.29 69.4) (width 0.25) (layer "F.Cu") (net 57) (tstamp 09ca6a8e-c268-4892-bccc-bd6b1380c20e))
  (segment (start 130.1 71.21) (end 132.29 71.21) (width 0.25) (layer "F.Cu") (net 57) (tstamp 1e9c3f23-fac4-4064-b442-24aee1937a3a))
  (segment (start 147.63 65.9) (end 146.63 65.9) (width 0.25) (layer "F.Cu") (net 57) (tstamp 21365bc3-067e-41d1-9014-2ca5462935ad))
  (segment (start 128.29 69.4) (end 130.1 71.21) (width 0.25) (layer "F.Cu") (net 57) (tstamp 561b5119-5db3-412f-aea0-ee40aeba75d3))
  (segment (start 149.1 68.9) (end 149.1 67.37) (width 0.25) (layer "F.Cu") (net 57) (tstamp 57f17f9d-1f37-40ce-a6d0-3ec6144df9cd))
  (segment (start 146.79 71.21) (end 149.1 68.9) (width 0.25) (layer "F.Cu") (net 57) (tstamp 690656dd-a65e-43b3-b7e3-f7aaa76ded64))
  (segment (start 132.29 71.21) (end 132.35 71.27) (width 0.25) (layer "F.Cu") (net 57) (tstamp 70f3501b-1b37-4d5d-a4e2-f60a80420786))
  (segment (start 132.35 71.27) (end 134.6 71.27) (width 0.25) (layer "F.Cu") (net 57) (tstamp 7cd53749-d785-48bc-bfd6-5c0bbd22fc77))
  (segment (start 136.79 71.27) (end 136.85 71.21) (width 0.25) (layer "F.Cu") (net 57) (tstamp a74a46dc-2364-4bc1-b752-ace902cb942a))
  (segment (start 149.1 67.37) (end 147.63 65.9) (width 0.25) (layer "F.Cu") (net 57) (tstamp a85b437e-0ad0-4512-9c53-5b86486d0bfc))
  (segment (start 136.85 71.21) (end 146.79 71.21) (width 0.25) (layer "F.Cu") (net 57) (tstamp e309450d-54b5-469e-9241-e5980daceb63))
  (via (at 127.95 69.4) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 57) (tstamp 0b19a0c1-60e6-445f-9394-0537cab38726))
  (segment (start 127.95 68.33) (end 127.95 69.4) (width 0.25) (layer "B.Cu") (net 57) (tstamp 6f23daae-2d48-4258-870d-b9a88921e37f))
  (segment (start 125.6 65.98) (end 127.95 68.33) (width 0.25) (layer "B.Cu") (net 57) (tstamp dd8b3a24-bda9-44d0-8f06-8686e8f3a52e))
  (segment (start 127.58 78.48) (end 125.6 78.48) (width 0.25) (layer "F.Cu") (net 58) (tstamp 5efd1e59-2d56-4e40-807f-dbe1b2336f9b))
  (segment (start 132.3 83.2) (end 127.58 78.48) (width 0.25) (layer "F.Cu") (net 58) (tstamp 67351ef0-ef13-4e05-bcdf-550b938189df))
  (segment (start 127.51 96.92) (end 132.3 92.13) (width 0.25) (layer "F.Cu") (net 58) (tstamp 778e4bfc-f0a9-4301-b399-e47c93b5e123))
  (segment (start 132.3 92.13) (end 132.3 83.2) (width 0.25) (layer "F.Cu") (net 58) (tstamp 81bc9be5-a3c0-48f4-a2f3-677c2602daa1))
  (segment (start 126.96 96.92) (end 127.51 96.92) (width 0.25) (layer "F.Cu") (net 58) (tstamp ba87afa7-0a89-4545-8845-437c35c752fe))
  (segment (start 129.1 127.23) (end 136.02 127.23) (width 0.25) (layer "F.Cu") (net 59) (tstamp b2cd9aa6-69ac-431c-89b8-a0ed026228c2))
  (segment (start 136.02 127.23) (end 142.53 120.72) (width 0.25) (layer "F.Cu") (net 59) (tstamp cc4679ff-f25f-46cb-a140-2fe11fe0984f))
  (segment (start 142.53 115.64) (end 142.53 118.18) (width 0.25) (layer "F.Cu") (net 60) (tstamp 7438bbf2-6fbe-4874-a631-cac395881c9f))
  (segment (start 142.53 118.18) (end 150.15 118.18) (width 0.25) (layer "B.Cu") (net 60) (tstamp 957a3bf0-d489-42b8-a04e-22852b94833c))

  (zone (net 2) (net_name "GNDREF") (layers "F&B.Cu") (tstamp b86f7216-0d2b-4fa6-875c-a041c9c102a6) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.6 143.9)
        (xy 123.6 143.9)
        (xy 123.6 43.9)
        (xy 193.6 43.9)
      )
    )
  )
)
