(module Potentiometer_Alpha_RA6020F_Single_Slide (layer F.Cu) (tedit 6047AE4E)
  (descr "Bourns single-gang slide potentiometer, 60.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
  (tags "Bourns single-gang slide potentiometer 60.0mm")
  (fp_text reference REF** (at 36.62 -5.68) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Potentiometer_Alpha_RA6020F_Single_Slide (at 36.35 10.17) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -5 2) (end -3.5 2) (layer F.Fab) (width 0.1))
  (fp_circle (center 75 2) (end 76.5 2) (layer F.Fab) (width 0.1))
  (fp_line (start -8.1 -4.25) (end 79.1 -4.25) (layer F.Fab) (width 0.1))
  (fp_line (start 79.1 -4.25) (end 79.1 8.25) (layer F.Fab) (width 0.1))
  (fp_line (start 79.1 8.25) (end -9.1 8.25) (layer F.Fab) (width 0.1))
  (fp_line (start -9.1 8.25) (end -9.1 -3.25) (layer F.Fab) (width 0.1))
  (fp_line (start -9.1 -3.25) (end -8.1 -4.25) (layer F.Fab) (width 0.1))
  (fp_line (start -9.22 -4.37) (end 79.22 -4.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.22 8.37) (end 79.22 8.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.22 -4.37) (end -9.22 8.37) (layer F.SilkS) (width 0.12))
  (fp_line (start 79.22 -4.37) (end 79.22 8.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.585 0) (end -2.085 -0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.085 -0.5) (end -2.085 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.085 0.5) (end -1.585 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 5 2) (end 65 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 5 0.5) (end 5 3.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.72 1.22) (end 5 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 5 2) (end 5.75 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 65 0.5) (end 65 3.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 64.25 1.25) (end 65 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 65 2) (end 64.25 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.6 -4.75) (end -9.6 8.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.6 8.75) (end 79.6 8.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 79.6 8.75) (end 79.6 -4.74) (layer F.CrtYd) (width 0.05))
  (fp_line (start 79.6 -4.74) (end -9.6 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 36.75 1.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.75) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5 5) (size 2.5 2.5) (drill 1.75) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 70 0) (size 2.5 2.5) (drill 1.75) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA6043_Single_Slide.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
