(module 3PDT-toggle-switch-1M-seriesx (layer F.Cu) (tedit 6080751D)
  (fp_text reference REF** (at 0 -7.8) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value DPDT-toggle-switch-1M-series (at 0.1 9.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.415 -2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 8.13 -6.35) (end 8.13 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.13 6.35) (end -8.13 6.34) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.13 6.34) (end -8.13 -6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.13 -6.35) (end 8.13 -6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.835 -6.35) (end 5.835 -6.34) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.415 -6.6) (end 8.415 -6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start 8.415 -6.6) (end 8.415 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start 8.415 6.6) (end -8.415 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start -8.415 6.6) (end -8.415 -6.6) (layer F.CrtYd) (width 0.12))
  (pad 4 thru_hole circle (at 0 4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 -4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -4.83 4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -4.83 0) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -4.83 -4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 4.83 4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 4.83 -4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 4.83 0) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
)
