(module PPTC_RXEF025 (layer F.Cu) (tedit 5FE3676B)
  (descr "Fuse, Resettable, Radial, pin pitch=5.00mm, , diameter*width=7.0*3.0mm^2, Fuse, https://www.littelfuse.com/~/media/electronics/datasheets/resettable_ptcs/littelfuse_ptc_radial_leaded_rxef_datasheet.pdf.pdf")
  (tags "Fuse Resettable Radial pin pitch 5.00mm  diameter 7.0mm width 3.0mm ")
  (fp_text reference REF** (at 0 -2.4) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value "PPTC RXEF025" (at 0 2.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4 -1.6) (end -4 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4 1.6) (end 4 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 1.6) (end 4 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 -1.6) (end -4 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.87 -1.5) (end 3.87 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.87 -1.5) (end -3.87 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.87 1.5) (end 3.87 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.87 -1.5) (end 3.87 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.75 -1.4) (end -3.75 -1.4) (layer F.Fab) (width 0.1))
  (fp_line (start 3.75 1.4) (end 3.75 -1.4) (layer F.Fab) (width 0.1))
  (fp_line (start -3.75 1.4) (end 3.75 1.4) (layer F.Fab) (width 0.1))
  (fp_line (start -3.75 -1.4) (end -3.75 1.4) (layer F.Fab) (width 0.1))
  (fp_text user %V (at 0 0.635) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P5.00mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
