(module SPDT-toggle-switch-1M-series (layer F.Cu) (tedit 602FC394)
  (fp_text reference REF** (at 0 -7.4) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value SPDT-toggle-switch-1M-series (at 0 9.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.43 -6.35) (end 3.43 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.43 6.35) (end -3.43 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.43 6.34) (end -3.43 -6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.43 -6.35) (end 3.42 -6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.42 -6.35) (end 3.42 -6.34) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.7 -6.6) (end 3.7 -6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.7 -6.6) (end 3.7 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.7 6.6) (end -3.7 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.7 6.6) (end -3.7 -6.6) (layer F.CrtYd) (width 0.12))
  (fp_text user %R (at 0 -2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 -4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 4.7) (size 3.1 3.1) (drill 2.1) (layers *.Cu *.Mask))
)
