(module PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 602FC2C7)
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (fp_text reference REF** (at 0 -2.33) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value PinHeader_1x03_P2.54mm_Vertical (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.77 0.635) (end -3.77 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -3.77 -1.27) (end 3.85 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 3.85 -1.27) (end 3.85 1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 3.85 1.27) (end -3.135 1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -3.135 1.27) (end -3.77 0.635) (layer F.Fab) (width 0.1))
  (fp_line (start 3.91 1.33) (end 3.91 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.23 1.33) (end 3.91 1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.23 -1.33) (end 3.91 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.23 1.33) (end -1.23 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 1.33) (end -3.83 1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.83 1.33) (end -3.83 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.3 1.8) (end 4.35 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.35 1.8) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.35 -1.8) (end -4.3 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.3 -1.8) (end -4.3 1.8) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0.04 0 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at -2.5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0.04 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 2.58 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
    (offset (xyz 2.5 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
