(module Kosmo_Panel_Dual_Slotted_Mounting_Hole (layer F.Cu) (tedit 5F6CB982)
  (descr "Mounting Hole 3.2mm, M3")
  (tags "mounting hole 3.2mm m3")
  (attr virtual)
  (fp_text reference REF** (at 1.4 -4.2) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Kosmo_Panel_Dual_Slotted_Mounting_Hole (at 1.4 4.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 3.25) (end 2.8 3.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -3.25) (end 2.8 -3.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 3) (end 2.8 3) (layer Cmts.User) (width 0.12))
  (fp_line (start 0 -3) (end 2.8 -3) (layer Cmts.User) (width 0.12))
  (fp_line (start 0 -197.25) (end 2.8 -197.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -190.75) (end 2.8 -190.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -197) (end 2.8 -197) (layer Cmts.User) (width 0.12))
  (fp_line (start 0 -191) (end 2.8 -191) (layer Cmts.User) (width 0.12))
  (fp_text user %R (at 1.7 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 2.8 0) (end 2.8 3) (angle -180) (layer Cmts.User) (width 0.12))
  (fp_arc (start 0 0) (end 0 -3) (angle -180) (layer Cmts.User) (width 0.12))
  (fp_arc (start 2.8 0) (end 2.8 3.25) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end 0 3.25) (angle 180) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 -194) (end 0 -190.75) (angle 180) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 1.7 -194) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 2.8 -194) (end 2.8 -190.75) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 -194) (end 0 -197) (angle -180) (layer Cmts.User) (width 0.12))
  (fp_arc (start 2.8 -194) (end 2.8 -191) (angle -180) (layer Cmts.User) (width 0.12))
  (pad 1 thru_hole oval (at 1.4 0) (size 6.8 4) (drill oval 6 3.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 1.4 -194) (size 6.8 4) (drill oval 6 3.2) (layers *.Cu *.Mask))
)
