(footprint "SOCKET_2_PIN_Header" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A420)
  (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x02 2.54mm single row")
  (property "Sheetfile" "Fireball.kicad_sch")
  (property "Sheetname" "")
  (attr through_hole)
  (fp_text reference "J6" (at 0 -2.77 180) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b683601e-7d12-49ff-b63f-13f8f52988cc)
  )
  (fp_text value "SQ_OUT" (at 0 5.31 180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dd2cd960-b90d-4114-b007-a4beffc931d0)
  )
  (fp_text user "${REFERENCE}" (at 0 1.27 270) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9284bf63-32d6-499e-a26e-0e18aaf6de9f)
  )
  (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 181701de-bd2a-49f1-8e35-9602b8713b6c))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 53c9ee13-5cd7-497a-8573-392c94bd1bbc))
  (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 94fc3446-0438-40a3-9d12-6dcdbacca54a))
  (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp bf141fc8-2dbf-4c7b-a12f-5a9640882866))
  (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp bf2c95c6-d183-48f1-a89b-d07f72d68e8a))
  (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp d40e2fee-9975-4fd9-b8d0-0be1f21ca733))
  (fp_line (start 1.75 -1.8) (end 1.75 4.3) (layer "F.CrtYd") (width 0.05) (tstamp 27cbef69-43c4-4406-b7f5-16a26eb3726d))
  (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 33e41341-8a3f-4253-b42f-10183e3cb892))
  (fp_line (start -1.8 4.3) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 55e725ad-a52b-42b9-ba34-59e826d46546))
  (fp_line (start 1.75 4.3) (end -1.8 4.3) (layer "F.CrtYd") (width 0.05) (tstamp cd3b147f-0c31-40bc-acb1-bab8cea7763a))
  (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 12c3d017-2ed4-48da-aaf4-f39a3bd5e0eb))
  (fp_line (start 1.27 -0.635) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 311a374b-50fc-4552-ab71-b8930f4933c9))
  (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 9c24c51d-bd6f-48b5-af9a-27309e0e960b))
  (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e53e94ee-a456-4eb5-886d-6033fb57b06b))
  (fp_line (start -1.27 3.81) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp fcc2d4ea-d6a8-4bb2-b6ce-11cb4e0758b3))
  (pad "S" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp fbacd2b2-ad11-4133-8e7e-febf013ce0ea))
  (pad "T" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 053520a8-ee36-4c2a-9a4a-37c4d730756e))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
