(footprint "SOCKET_3_PIN_HEADER_NORMAL" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A429)
  (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x03 2.54mm single row")
  (property "Sheetfile" "Fireball.kicad_sch")
  (property "Sheetname" "")
  (attr through_hole)
  (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c42b512b-0342-404b-9a55-c98caf9bb946)
  )
  (fp_text value "FM_IN" (at 0 7.85) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 74b00f8b-365a-4b15-96f2-4c7b8984c806)
  )
  (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4067d837-381d-495a-af86-ba540d9cf26a)
  )
  (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 245e220b-e4ea-4554-af29-5bea2dada8e6))
  (fp_line (start -1.33 1.27) (end -1.33 6.41) (layer "F.SilkS") (width 0.12) (tstamp 38c6da96-cdc0-4de9-8d2c-abd4a316aeac))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 3a285137-6835-4978-96b7-2c1e817d26ac))
  (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 4952ebe2-99a6-49f4-96f5-86c44a3d3f4a))
  (fp_line (start 1.33 1.27) (end 1.33 6.41) (layer "F.SilkS") (width 0.12) (tstamp 8739eccd-7781-4f79-b5ca-bab6eb64c471))
  (fp_line (start -1.33 6.41) (end 1.33 6.41) (layer "F.SilkS") (width 0.12) (tstamp fd1bdffa-10cd-4529-a2e9-31e3c118c429))
  (fp_line (start -1.8 6.85) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 51f06611-6d23-43ed-8f67-977a68147dca))
  (fp_line (start 1.75 6.85) (end -1.8 6.85) (layer "F.CrtYd") (width 0.05) (tstamp 6c7901d3-8777-4685-80df-de5e1c770ef3))
  (fp_line (start 1.75 -1.8) (end 1.75 6.85) (layer "F.CrtYd") (width 0.05) (tstamp 8cb51de3-71b2-4760-a164-fe84a7f9bd34))
  (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c147c77d-d813-45a2-9ee5-138b49b32fd6))
  (fp_line (start 1.27 -0.635) (end 1.27 6.35) (layer "F.Fab") (width 0.1) (tstamp 5eb5809d-026a-488c-b801-9892dac5da66))
  (fp_line (start 1.27 6.35) (end -1.27 6.35) (layer "F.Fab") (width 0.1) (tstamp 92c267b2-7747-4fdb-b0c1-6ac64d16c677))
  (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp a1b1a422-1683-45f0-af95-909b6c069be5))
  (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp b9a635ee-b164-4b48-8201-388778b92c18))
  (fp_line (start -1.27 6.35) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp d0366112-eb9a-4e64-a52b-5ce1bc359290))
  (pad "S" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 573ff460-828a-4d09-9f6b-5bf26ea158cc))
  (pad "T" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp c4f64d4c-d73f-4367-a993-0e115c3f8e69))
  (pad "TN" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 1c983375-972d-47c3-91d9-00e9533bc509))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
