(footprint "6.3mm_NPTH_MAXJLCPCB" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Mounting Hole 6.4mm, no annular, M6, DIN965")
  (tags "mounting hole 6.4mm no annular m6 din965")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -2.54) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp edd0c009-7997-48f2-8d20-06e533afbbe9)
  )
  (fp_text value "6.3mm_NPTH_MAXJLCPCB" (at 0 6.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 69182475-0bd6-470c-b768-25f122b918d7)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a5cd39bd-2e50-4366-9543-e28087f8607a)
  )
  (fp_circle (center 0 0) (end 5.5 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 8a50cbe6-0e3f-4ca3-a22b-f168efe2ac67))
  (fp_circle (center 0 0) (end 5.75 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 334b1007-5d7a-4edd-9983-155c70a9aa00))
  (pad "" np_thru_hole circle (at 0 0) (size 6.3 6.3) (drill 6.3) (layers "F&B.Cu" "*.Mask") (tstamp ed373e9a-4d69-48e3-9e6f-2312c63f86e5))
)
