(footprint "3.5mm_jack_hole_nonpcb" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Mounting Hole 8.4mm, no annular, M8")
  (tags "mounting hole 8.4mm no annular m8")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -5.08) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 32fbb37a-7c9c-4309-bda3-1286be42cd00)
  )
  (fp_text value "3.5mm_jack" (at 0 5.08) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4c7aa143-70cb-405c-9c5c-b2badb5a1074)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f9af9f86-0f99-41a1-8da1-2c70df7a09bf)
  )
  (fp_circle (center 0 0) (end 4.2 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 0cdcd992-ac15-4489-8ed9-95e5e1faadbb))
  (fp_circle (center 0 0) (end 4.3 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp b420248a-6c99-40d8-b1e3-b001eee2fa76))
  (pad "" np_thru_hole circle (at 0 0) (size 8.2 8.2) (drill 8.2) (layers "F&B.Cu" "*.Mask") (tstamp 396dd376-1277-4f67-92c6-2ebdba894a6f))
)
