(footprint "SLIDE_POT_0547" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
  (tags "Bourns single-gang slide potentiometer 45.0mm")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a4699170-083b-499a-bdb3-b2682e117d7f)
  )
  (fp_text value "SLIDE_POT_0547" (at 0 2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fba516e7-1049-45b0-8dba-0ae3b2bc2d6f)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 279a77ec-bb4c-42b3-9906-0ade47adceea)
  )
  (fp_line (start -30.4 1) (end -30.4 2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65bf255e-30c7-491d-bd1d-e666fc7677dd))
  (fp_line (start -30.4 2) (end -29.9 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f24260f8-1331-43e2-bff6-abb81e499b67))
  (fp_line (start -30.12 -4.124122) (end -30.12 -2.429122)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f29a92d-11ef-42dd-a987-3bef31d36eeb))
  (fp_line (start -30.12 -0.079122) (end -30.12 1.423878)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c619a347-43e9-4a78-9912-d4fc2de25c81))
  (fp_line (start -30.12 3.068878) (end -30.12 4.124121)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5179b702-18b1-4c0b-88b7-70b264320e2b))
  (fp_line (start -30.12 4.15) (end 30.12 4.15)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1e8a2b8b-d0df-4d90-af84-100d8092f058))
  (fp_line (start -29.9 1.5) (end -30.4 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d7d6dad-d935-4444-b24a-282689ec1a66))
  (fp_line (start -27 -4.124122) (end 30.12 -4.124122)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 75fd8877-17c4-4b41-94ae-561bb503f5a2))
  (fp_line (start -22.5 -1.5) (end -22.5 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6b0e71af-91e1-4387-9d66-66d1d05b933f))
  (fp_line (start -22.5 0) (end -21.75 0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 63cfe93e-ea01-45b1-b131-67492aba5aed))
  (fp_line (start -22.5 0) (end 22.5 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e4018a0-5c04-4c92-bcd9-853a35dfe3a5))
  (fp_line (start -21.75 -0.75) (end -22.5 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 14fcda38-09e8-4cd8-888b-cd8facb1fa99))
  (fp_line (start 21.75 -0.75) (end 22.5 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58f7b580-71c1-4997-ab9f-3e3ed8687f3f))
  (fp_line (start 22.5 -1.5) (end 22.5 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b1b3d19-af08-43b0-a834-67e869a85cfb))
  (fp_line (start 22.5 0) (end 21.75 0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc5e4cec-5c83-4e03-a24f-dd120a363295))
  (fp_line (start 25.536 -4.124122) (end 30.12 -4.124122)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c044948b-39e9-4095-b709-e9a1a6ed63b1))
  (fp_line (start 30.12 -4.124122) (end 30.12 -2.077122)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0a09304c-d389-40eb-aef4-3a71c7d354bc))
  (fp_line (start 30.12 -0.431122) (end 30.12 4.124121)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 33e8e34b-3fd7-49a7-8180-45c8b0fc97e0))
  (fp_line (start -30.5 -4.504122) (end -30.5 4.382747)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f0bfe63-e710-4ee8-8e3e-b8683319158b))
  (fp_line (start -30.5 4.382747) (end 30.5 4.382747)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp de889320-9fb7-4c8f-b5e4-8f62c2c29470))
  (fp_line (start 30.5 -4.504122) (end -30.5 -4.504122)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1a083db0-a788-4bbb-8d77-32ee8f12c4fb))
  (fp_line (start 30.5 4.382747) (end 30.5 -4.504122)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 47741f99-6708-4f25-ae75-5e83fac66a30))
  (fp_line (start -30 -3.004122) (end -29.25 -3.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 59eca3c0-81a2-4b28-8bef-dc347d6657b6))
  (fp_line (start -30 4.054121) (end -30 -3.004122)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c2fe06a-1681-4a48-aa1d-801da50bc4be))
  (fp_line (start -27 -4.004122) (end 30 -4.004122)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ac7e483-d91f-4940-8a9e-167626499dba))
  (fp_line (start 30 -4.004122) (end 30 4.054121)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d4330c89-18bc-4962-a55b-ca9358d36288))
  (fp_line (start 30 4.054121) (end -30 4.054121)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d3c0b5bd-5a14-4367-8d6f-91bacd901d74))
  (fp_circle (center 28 0) (end 29 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp b90b4541-6a84-4d36-9772-fa47aa0c00b7))
  (pad "1" thru_hole rect (at -25.171374 1.5) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 7a2dbd7f-98b4-4cf2-9552-d02ea395684a))
  (pad "2" thru_hole circle (at -25.171374 -1.5) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 18319b92-e737-40e2-b17d-aae23912ded9))
  (pad "3" thru_hole circle (at 25.5 1.5) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 339e3fee-f81c-4e41-b9f2-245e53f532d6))
  (pad "MP" thru_hole circle (at -28.12 -4.195879) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 842bcde6-b67e-4e27-9254-54a1304887b4))
  (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
