(footprint "Pushbutton Switch (PBS105)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0.001344 -6.171835) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4a42150c-e2cb-48c8-8496-6e7fedd454bb)
  )
  (fp_text value "PBS105" (at 0 5.761533) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db29ad0b-b335-4faf-88c7-319c7ace35e3)
  )
  (fp_text user "${REFERENCE}" (at 0.014406 7.115765 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 788c9283-32be-4c0b-b74e-17c5f67f5b7f)
  )
  (fp_circle (center 0 0) (end 4.85 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp d1282e50-3778-4949-8587-669860f91aa6))
  (fp_circle (center 0 0) (end 5 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 9e3ad1dd-4e42-49a9-85a9-445b965c1097))
  (fp_circle (center 0 0) (end 4.75 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp d17b33bd-6640-4d6c-aae2-da8e38ce3b8f))
  (pad "1" thru_hole oval (at 0 -1.75) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask") (tstamp c7351bc0-95e7-4de9-93f8-e2fc166956da))
  (pad "2" thru_hole oval (at 0 1.75) (size 3.25 3.25) (drill 2.5) (layers "*.Cu" "*.Mask") (tstamp 2e14092c-1e97-4b3c-b1f4-9b887ef28570))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
