(footprint "Alpha Rotary 12" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (fp_text reference "REF**" (at 0 -14.245) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b54513e2-df59-4e32-9561-ac9d27fbd2ae)
  )
  (fp_text value "Alpha Rotary 12" (at 0 14.245) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9db02b87-8c23-4abe-9b20-d1636f73c97f)
  )
  (fp_circle (center 0 0) (end 0 13.37)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 468440c6-a5ae-4a31-a960-4f6b8386b33d))
  (fp_circle (center 0 0) (end 0 13.57)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 4b98c5b8-661b-4747-a258-92c523ade94b))
  (fp_circle (center 0 0) (end 0 13.25)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 22a09df8-498a-4e86-9100-b6cce8922620))
  (pad "1" thru_hole oval (at -5.5 -9.526279 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 9cb1c10d-f270-488e-bf73-b25e77353d86))
  (pad "2" thru_hole oval (at 0 -11 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 40bd76c6-5236-43d1-971d-8c86f488a964))
  (pad "3" thru_hole oval (at 5.499999 -9.526279 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 34be17a3-f268-488b-a5d6-3648ff3879fe))
  (pad "4" thru_hole oval (at 9.526279 -5.5 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp af5804eb-e0b5-4ede-af7f-e16ee33b3e5b))
  (pad "5" thru_hole oval (at 11 0 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 63f0e913-613d-4180-a79b-1ec3f4b3bc6c))
  (pad "6" thru_hole oval (at 9.526279 5.499999 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3915f14f-8af1-4495-9192-f5fbfa70532b))
  (pad "7" thru_hole oval (at 5.499999 9.526279 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp c7beafd8-364c-447f-b7d7-6e0e2ceccb43))
  (pad "8" thru_hole oval (at 0 11 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7f9f4c62-5e12-4653-93ff-05a76b7d99a2))
  (pad "9" thru_hole oval (at -5.5 9.526279 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7a4efe19-a54b-44a1-a4f1-2f8abffb9f71))
  (pad "10" thru_hole oval (at -9.526279 5.5 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 396d2ce8-8f70-4699-9e7a-bf2776182cb2))
  (pad "11" thru_hole oval (at -11 0 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 5b6c3b38-2e08-4e9f-a343-e0b8a26a3ed4))
  (pad "12" thru_hole oval (at -9.526279 -5.5 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 75b8d339-68f9-4c8c-9d82-41bce9bada05))
  (pad "A" thru_hole oval (at 0 -3.75 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 022351ed-6722-45a3-84b7-4bb2545bc178))
  (pad "C" thru_hole oval (at 0 3.75 45) (size 4 4) (drill 2.75) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp bdaf5f08-6978-4cec-b530-d8d27fca13ba))
)
