(footprint "Perfboard_1x12" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x12 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7ecb03d8-bd3a-479f-9629-1e10b959c15a)
  )
  (fp_text value "Perfboard_1x12" (at 0 30.27) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1f7e0f69-2318-4ab5-be64-0d2cf92f6c65)
  )
  (fp_text user "${REFERENCE}" (at 0 13.97 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 98661a0d-504e-4522-a4be-0212d43bfa07)
  )
  (fp_line (start -1.33 -1.33) (end 0 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5ac1c824-21f2-431e-bf95-1ec9d090d876))
  (fp_line (start -1.33 0) (end -1.33 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41a2d477-a834-4a90-849f-909444c36252))
  (fp_line (start -1.33 1.27) (end -1.33 29.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 267eff58-d283-4bcf-8d59-7e3c3dc97fdd))
  (fp_line (start -1.33 1.27) (end 1.33 1.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88f63691-19d9-4b40-93d5-4d20a9fd6fd4))
  (fp_line (start -1.33 29.27) (end 1.33 29.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 147ce810-dd63-4afc-a974-a309f92fe335))
  (fp_line (start 1.33 1.27) (end 1.33 29.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 02dac598-8954-4bc6-81fd-166c9ef3141c))
  (fp_line (start -1.8 -1.8) (end -1.8 29.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4aab70e7-6b5d-4627-8366-3f90918395a4))
  (fp_line (start -1.8 29.75) (end 1.8 29.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 02f17198-efde-4ef6-8576-505b8581707f))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f27f1ad4-9f1a-483c-af1b-a7dec364fd00))
  (fp_line (start 1.8 29.75) (end 1.8 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 504d89ac-dbd6-42fd-97ac-b8041dd56a03))
  (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d9edb7a-a616-48e4-83da-1cdf3762e05b))
  (fp_line (start -1.27 29.21) (end -1.27 -0.635)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3072a21-1bec-4b9c-9db8-82f352b4b675))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 333a58a8-9ddf-4bdc-9888-a3c8b866354f))
  (fp_line (start 1.27 -1.27) (end 1.27 29.21)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 130f1777-7e60-4dc5-849d-cc842a8f4001))
  (fp_line (start 1.27 29.21) (end -1.27 29.21)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0f0898ce-edc2-47ed-b3ae-0f7043d8b364))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 54718f7e-4dde-4c07-bc34-f000ebe4676b))
  (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2fbb081b-bf60-4865-a951-f7519f3c97a8))
  (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 03d8d8fc-27c6-4d01-92ee-3c64988c2aa1))
  (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5a431f5a-6c1b-4838-bb0f-59dcd9473439))
  (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 88d6edcd-4ab4-4df9-a6cd-cf1ba99e9237))
  (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 83cfd216-3510-4f2a-b79d-b23af62f15eb))
  (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 4a93ff39-ab42-4cc1-bfe2-62898798f5c1))
  (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7b681f65-5d70-439c-8256-baa98734019a))
  (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ff63ed00-cc7a-4e61-9b46-c05e40297b26))
  (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 85fcc3a9-dc71-44a4-a3ae-a2fb80c99feb))
  (pad "11" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 195a3d86-4e63-40ef-88bf-d4979ac6692a))
  (pad "12" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp c4ea6d5c-6e08-484d-9125-f068d352bba7))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
