(footprint "Micro SPDT (3 pin)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.388232) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4a42150c-e2cb-48c8-8496-6e7fedd454bb)
  )
  (fp_text value "uSPDT" (at 0 7.62) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db29ad0b-b335-4faf-88c7-319c7ace35e3)
  )
  (fp_text user "${REFERENCE}" (at 0 9.158636 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 788c9283-32be-4c0b-b74e-17c5f67f5b7f)
  )
  (fp_line (start -1.605 -1.605) (end -1.605 6.605)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 24199bf2-7a4c-47d7-a9d0-c8212ed52732))
  (fp_line (start -1.605 -1.605) (end 1.605 -1.605)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e0d3fed-d2a2-43ed-ac38-36961c14bfa4))
  (fp_line (start -1.605 6.605) (end 1.605 6.605)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b8d7228-c97e-4f3b-bb80-5394d1336ea8))
  (fp_line (start 1.605 -1.605) (end 1.605 6.605)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 528d64f1-caad-4315-bf88-6b33a6c30761))
  (fp_line (start -1.8 -1.8) (end -1.8 6.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76c67b9f-3f15-4145-bbbc-8312e5795846))
  (fp_line (start -1.8 6.85) (end 1.8 6.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 56a0eaa8-1f42-4824-9fc4-0cbfa375ec08))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 757b6603-0fa3-41f4-942f-2ab155c45604))
  (fp_line (start 1.8 6.85) (end 1.8 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0624b2c1-b80d-48b5-9bf7-4536c6317e1c))
  (fp_line (start -1.545 -1.545) (end 1.545 -1.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5eacb716-3494-462e-bcdc-e6b518f66765))
  (fp_line (start -1.545 6.545) (end -1.545 -1.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4fb5e79-dd44-4947-9d51-22633c17ad61))
  (fp_line (start 1.545 -1.545) (end 1.545 6.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e173d00-babf-4201-8f82-f5030a24fbf9))
  (fp_line (start 1.545 6.545) (end -1.545 6.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a8bc881-5fff-4bac-96c1-41af6ae648ff))
  (pad "1" thru_hole rect (at 0 0) (size 2.25 2.25) (drill 1.75) (layers "*.Cu" "*.Mask") (tstamp c7351bc0-95e7-4de9-93f8-e2fc166956da))
  (pad "2" thru_hole oval (at 0 2.5) (size 2.25 2.25) (drill 1.75) (layers "*.Cu" "*.Mask") (tstamp 2e14092c-1e97-4b3c-b1f4-9b887ef28570))
  (pad "3" thru_hole oval (at 0 5) (size 2.25 2.25) (drill 1.75) (layers "*.Cu" "*.Mask") (tstamp 7072b420-9990-4d8f-a6b8-3c72e84d3433))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
