(footprint "POT_2_PIN_Header" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A420)
  (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x02 2.54mm single row")
  (property "Sheetfile" "Fireball.kicad_sch")
  (property "Sheetname" "")
  (attr through_hole)
  (fp_text reference "J6" (at 0 -2.77 180) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b8b1b5d6-d374-4db8-8197-105b8433dcc6)
  )
  (fp_text value "SQ_OUT" (at 0 5.31 180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1ff3ad9e-d059-41b5-8ffb-b79c09d1ce61)
  )
  (fp_text user "${REFERENCE}" (at 0 1.27 270) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 24b29ac3-cec8-4233-b26b-011f785a6ceb)
  )
  (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 2027a130-58b8-4c5c-82c4-0812381fe609))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 6c70a98e-3374-4a4e-9ebb-4bd25d79d2c4))
  (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 6e736372-0e50-47fb-88fc-c1af2ed5dabf))
  (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 71fc87a6-83cd-4a88-8158-47543b930e8d))
  (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp cdc58dc2-60e0-4878-af9a-e2f3305040bb))
  (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp dee4a1f7-b9af-481d-ab59-bdc26f57e488))
  (fp_line (start -1.8 4.3) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 37f94ecf-8f33-4131-b5f0-e03a8b6092b5))
  (fp_line (start 1.75 -1.8) (end 1.75 4.3) (layer "F.CrtYd") (width 0.05) (tstamp 60ef9c5a-2871-4961-85ba-0af1c08696f9))
  (fp_line (start 1.75 4.3) (end -1.8 4.3) (layer "F.CrtYd") (width 0.05) (tstamp da80d13f-1f31-4610-976f-bc046deaabd4))
  (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp fd0c4886-aa8a-44b5-99c0-4159dc2d6a42))
  (fp_line (start 1.27 -0.635) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 64936ce4-2a12-4bf0-9a3e-bd69ebcf2982))
  (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 65430d86-0566-460f-a0df-d1ef5d8d799d))
  (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 80a0e04b-0e87-4112-a024-0380dd6a19b6))
  (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e98d880f-f7ee-4d86-a52b-a9d2f31c2050))
  (fp_line (start -1.27 3.81) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp fba26dd2-51b3-462a-beaa-d4d039098ee6))
  (pad "S" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f20f8af3-4dbd-46d2-95da-c5266b755df6))
  (pad "T" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a6828931-7dd3-42ea-800c-2dc18d6e09de))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
