(footprint "Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5C6C6C48)
  (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
  (tags "potentiometer vertical 9mm single")
  (attr through_hole)
  (fp_text reference "REF**" (at -1.05 -7.3 180) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2f2629dd-6685-4f2e-ad90-d91a3cd942e1)
  )
  (fp_text value "Potentiometer_Alpha_RD901F-40-00D_Single_Vertical_CircularHoles_Shaft_Centered" (at -7.5 7.61 180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b9ec3328-369c-430c-9e62-6b3943bbe3fa)
  )
  (fp_text user "${REFERENCE}" (at 0.12 0.04) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0475c69a-bc29-4f2f-b8f0-b7af9b731cef)
  )
  (fp_line (start 4.97 4.87) (end 4.97 -4.87) (layer "F.SilkS") (width 0.12) (tstamp 055f4cbb-36d3-45fa-bf7b-df1023c37036))
  (fp_line (start -6.62 4.87) (end -1.9 4.87) (layer "F.SilkS") (width 0.12) (tstamp 52cd90aa-0ad9-41b7-a7a3-83bc5ab21b71))
  (fp_line (start -6.62 -4.88) (end -1.9 -4.88) (layer "F.SilkS") (width 0.12) (tstamp 7c8e6849-9425-41a7-ae31-e4ce2d95e9c9))
  (fp_line (start 1.91 4.87) (end 4.97 4.87) (layer "F.SilkS") (width 0.12) (tstamp 9abaee90-9f6c-4f76-bedf-1b9856950b17))
  (fp_line (start -6.62 4.87) (end -6.62 3.38) (layer "F.SilkS") (width 0.12) (tstamp a1a33286-c167-43ca-95d0-ae63c30daba5))
  (fp_line (start -6.62 1.66) (end -6.62 0.83) (layer "F.SilkS") (width 0.12) (tstamp b0e42afc-ca4a-483b-903a-3319cb1fc454))
  (fp_line (start -6.62 -3.69) (end -6.62 -4.87) (layer "F.SilkS") (width 0.12) (tstamp c9ab225e-5bc2-47ec-abbe-ccae5533084a))
  (fp_line (start -6.62 -0.79) (end -6.62 -1.32) (layer "F.SilkS") (width 0.12) (tstamp d48f9ec3-29d8-46c4-8cb5-e9a8774478dc))
  (fp_line (start 1.91 -4.87) (end 4.97 -4.87) (layer "F.SilkS") (width 0.12) (tstamp d68336fd-4e74-4aa5-955c-2d2983d60088))
  (fp_line (start 5.1 -6.67) (end -8.65 -6.67) (layer "F.CrtYd") (width 0.05) (tstamp 3b8a1984-3f1f-4267-9068-5128190dd9ff))
  (fp_line (start -8.65 -6.67) (end -8.65 6.67) (layer "F.CrtYd") (width 0.05) (tstamp 5bb8bd3d-98d4-412b-89f1-1a5355b28ec4))
  (fp_line (start -8.65 6.67) (end 5.1 6.67) (layer "F.CrtYd") (width 0.05) (tstamp 77903d15-5138-48da-976a-df7ced60833c))
  (fp_line (start 5.1 6.67) (end 5.1 -6.67) (layer "F.CrtYd") (width 0.05) (tstamp d93dc459-cf32-47ec-be16-929c586bf87d))
  (fp_line (start -6.5 4.75) (end 4.85 4.75) (layer "F.Fab") (width 0.1) (tstamp 4ba618f0-119a-4218-b127-ad2aa374e7a4))
  (fp_line (start -6.5 4.75) (end -6.5 -4.75) (layer "F.Fab") (width 0.1) (tstamp 83f77ef8-e070-4976-a7d4-d98ff44f2398))
  (fp_line (start 4.85 4.75) (end 4.85 -4.75) (layer "F.Fab") (width 0.1) (tstamp c1da84e6-cd61-4d7d-b265-d0d27b3c2a39))
  (fp_line (start -6.5 -4.75) (end 4.85 -4.75) (layer "F.Fab") (width 0.1) (tstamp d46a092e-6486-42f0-9848-b1ded34db426))
  (fp_circle (center 0 0) (end 0 -3.5) (layer "F.Fab") (width 0.1) (fill none) (tstamp c8ca4e9f-a89b-4fc0-8b36-0440d19ed1df))
  (pad "" thru_hole circle (at 0 4.8 90) (size 3.24 3.24) (drill 1.8) (layers *.Cu *.Mask) (tstamp 24adb1fb-e367-4d32-a5d1-afb70741f95f))
  (pad "" thru_hole circle (at 0 -4.8 90) (size 3.24 3.24) (drill 1.8) (layers *.Cu *.Mask) (tstamp 45f1b02e-55c2-4587-8b07-6ec9f97580e8))
  (pad "1" thru_hole rect (at -7.5 -2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp c4308013-8eaa-4944-a339-ca7b446f1b98))
  (pad "2" thru_hole circle (at -7.5 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp a2905bf8-4081-43cf-a840-a739bfe95491))
  (pad "3" thru_hole circle (at -7.5 2.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp 518dd386-846a-485b-8f8f-e4f97f3cd1f8))
  (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
