(module Bigger_Push_Switch_Hole_NPTH (layer F.Cu) (tedit 610E962E)
  (descr "Mounting Hole 6mm")
  (tags "mounting hole 6mm")
  (attr virtual)
  (fp_text reference REF** (at 0 -7) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Bigger_Push_Switch_Hole_NPTH (at 0 7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 6.25 0) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 0) (end 6 0) (layer Cmts.User) (width 0.15))
  (fp_text user %R (at 0.3 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at 0 0) (size 15.2 15.2) (drill 15.2) (layers *.Cu *.Mask))
)
