(module Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 602FC354)
  (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
  (tags "Potentiometer vertical Bourns 3296W")
  (fp_text reference REF** (at 0 -3.66) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value Potentiometer_Bourns_3296W_Vertical (at 0 3.67) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 3.495 1.15) (end 4.59 1.15) (layer F.Fab) (width 0.1))
  (fp_line (start -4.765 -2.41) (end -4.765 2.42) (layer F.Fab) (width 0.1))
  (fp_line (start -4.765 2.42) (end 4.765 2.42) (layer F.Fab) (width 0.1))
  (fp_line (start 4.765 2.42) (end 4.765 -2.41) (layer F.Fab) (width 0.1))
  (fp_line (start 4.765 -2.41) (end -4.765 -2.41) (layer F.Fab) (width 0.1))
  (fp_line (start 3.495 2.235) (end 3.496 0.066) (layer F.Fab) (width 0.1))
  (fp_line (start 3.495 2.235) (end 3.496 0.066) (layer F.Fab) (width 0.1))
  (fp_line (start -4.885 -2.53) (end 4.885 -2.53) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.885 2.54) (end 4.885 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.885 -2.53) (end -4.885 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.885 -2.53) (end 4.885 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.06 -2.7) (end -5.06 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.06 2.7) (end 5.04 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.04 2.7) (end 5.04 -2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.04 -2.7) (end -5.06 -2.7) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at -0.635 0.005) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
