(module TerminalBlock_Degson_DG301_1x03_P5.00mm_Vertical (layer F.Cu) (tedit 602FC3BA)
  (descr "terminal block RND 205-00079, vertical (cable from top), 3 pins, pitch 5mm, size 15x10mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00276_DB_EN.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
  (tags "THT terminal block RND 205-00079 vertical pitch 5mm size 15x10mm^2 drill 1.3mm pad 2.5mm")
  (fp_text reference REF** (at 0 -4.2) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value TerminalBlock_Degson_DG301_1x03_P5.00mm_Vertical (at -0.05 7.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8.1 4.5) (end 7.5 4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.1 -3.1) (end 7.5 -3.1) (layer F.Fab) (width 0.1))
  (fp_line (start 7.5 -3.1) (end 7.5 4.5) (layer F.Fab) (width 0.1))
  (fp_line (start 7.5 4.5) (end -6.2 4.5) (layer F.Fab) (width 0.1))
  (fp_line (start -6.2 4.5) (end -8.1 2.6) (layer F.Fab) (width 0.1))
  (fp_line (start -8.1 2.6) (end -8.1 -3.1) (layer F.Fab) (width 0.1))
  (fp_line (start -8.1 -3.1) (end 7.5 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.1 -3.1) (end -8.1 4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.5 -3.1) (end 7.5 4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.05 -1.3) (end -6.49 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.51 -1.3) (end -2.95 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.05 4.1) (end -2.95 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.05 -1.3) (end -7.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.95 -1.3) (end -2.95 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.05 -1.3) (end -7.05 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start -7.05 4.1) (end -2.95 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start -2.95 4.1) (end -2.95 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -2.95 -1.3) (end -7.05 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -2.05 -1.3) (end -0.883 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.884 -1.3) (end 2.05 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 4.1) (end 2.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 -1.3) (end -2.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.05 -1.3) (end 2.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 -1.3) (end -2.05 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start -2.05 4.1) (end 2.05 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.05 4.1) (end 2.05 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 2.05 -1.3) (end -2.05 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 2.95 -1.3) (end 4.117 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.884 -1.3) (end 7.05 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.95 4.1) (end 7.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.95 -1.3) (end 2.95 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.05 -1.3) (end 7.05 4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.95 -1.3) (end 2.95 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.95 4.1) (end 7.05 4.1) (layer F.Fab) (width 0.1))
  (fp_line (start 7.05 4.1) (end 7.05 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 7.05 -1.3) (end 2.95 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -8.3 2.4) (end -8.3 4.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.3 4.7) (end -6.3 4.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.5 -3.5) (end -8.5 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.5 4.9) (end 7.9 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.9 4.9) (end 7.9 -3.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.9 -3.5) (end -8.5 -3.5) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 5.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00277_1x03_P5.00mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
