(module SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 602FC3AB)
  (descr "Wire solder connection")
  (tags connector)
  (attr virtual)
  (fp_text reference REF** (at 0 -2.5) (layer F.SilkS) hide
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_text value SolderWirePad_1x01_Drill1mm (at 0 3.175) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.75) (end -1.75 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 1.75) (end -1.75 1.75) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask))
)
